;PG27FFX2A.inf Ver. 2.0.0.0
;Monitor INF file for ASRock PG27FFX2A
;Copyright 2023 ASRock, All rights reserved.

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%ASRock%
CatalogFile=PG27FFX2A.cat
DriverVer=07/22/2024,2.0.0.4
PnpLockdown=1

;-------------------------------------------------
[ControlFlags]
ExcludeFromSelect.nt=Monitor\ASRABA6
[SourceDisksNames]
1=%DISK%,,,

[SourceDisksFiles]
PG27FFX2A.icm=1

[DestinationDirs]
DefaultDestDir=12
PG27FFX2A.Copyfiles = 23


; Manufacturers
;-------------------------------------------------
[Manufacturer]
%ASRock%=ASRock,NTx86,NTAMD64


 [ASRock.NTx86] 
%PG27FFX2A% = PG27FFX2A.Install, Monitor\ASRABA6

 [ASRock.NTAMD64] 
%PG27FFX2A% = PG27FFX2A.Install, Monitor\ASRABA6

; Install Sections
;-------------------------------------------------
[PG27FFX2A.Install.Services]
AddService = monitor,%SPSVCINST_ASSOCSERVICE%, Monitor_Service.Install

[Monitor_Service.Install]
Display_Name = %Monitor.SVCDESC%
ServiceType = 1;SERVICE_KERNEL_DRIVER
StartType = 3;SERVICE_DEMAND_START
ErrorControl =1;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\monitor.sys

[PG27FFX2A.Install]
DelReg    = DEL_CURRENT_REG
AddReg    = PG27FFX2A.AddReg, 1920, DPMS, DisplayHdrLevel
CopyFiles = PG27FFX2A.CopyFiles


					     
; AddReg & DELReg sections
;-------------------------------------------------

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile
HKR,,DisplayHdrLevel
[1920]
HKR,,MaxResolution,,"1920,1080"

[DPMS]
HKR,,DPMS,,1

[DisplayHdrLevel]
HKR,,DisplayHdrLevel,0x10000,"0D710BC2-6368-4EB2-A829-CBBD45CE3BD2"

; AddReg sections
;---------------------------------------------------------- 

[PG27FFX2A.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-578.0,48.0-520.0,+,+"
HKR,,ICMProfile,0,"PG27FFX2A.icm"



;---------------------------------------------------------- 

[PG27FFX2A.CopyFiles]
PG27FFX2A.icm


;---------------------------------------------------------- 
[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC ="Monitor Class Function Driver Service"
ASRock="ASRock"	
DISK="ASRock Monitor Installation Disk"
PG27FFX2A= "ASRock PG27FFX2A"
