;
; Copyright (c) AVerMedia TECHNOLOGIES, Inc. 
;

[Version]
signature   = "$CHICAGO$" ;all windows os
Class       = MEDIA
ClassGUID   = {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider    = %AVer%
DriverVer   =07/26/2012,1.3.64.107
CatalogFile = AVerBDA716x_x64.cat

[Manufacturer]
%AVer% = AVerMedia,NTamd64,ntamd64.6

[AVerMedia.NTamd64]

;******** AVerMedia A177 ***
%AVer.DeviceDesc22% = AVer_A177_RC.NTamd64 , PCI\VEN_1131&DEV_7162&SUBSYS_011C1461 ; A177

;******** AVerMedia A568 ***

;******** AVerMedia M789 ***
%AVer.DeviceDesc00% = AVer_M789.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_01511461 ; M789 (I)
%AVer.DeviceDesc01% = AVer_M789.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_02511461 ; M789 (II)

;******** AVerMedia M788 ***
%AVer.DeviceDesc02% = AVer_M788.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_01551461 ; M788 (I)

;******** AVerMedia H788 HyBrid DVBT I ***
%AVer.DeviceDesc08% = AVer_H788_HyDVBT_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_0B551461 ; H788 HyBrid DVBT (I)

;******** AVerMedia H788 Pure DVBT***
%AVer.DeviceDesc09% = AVer_H788_PuDVBT_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_0C551461 ; H788 Pure DVBT (I)

;******** AVerMedia H788 Hybrid ATSC***
%AVer.DeviceDesc10% = AVer_H788_HyATSC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_06551461 ; H788 Hybrid ATSC (I)

;******** AVerMedia H788 Hybrid ATSC IR***
%AVer.DeviceDesc10% = AVer_H788_HyATSC_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_1A551461 ; H788 Hybrid ATSC RC(I)

;******** AVerMedia H788 Hybrid ATSC 2 AV-in***
%AVer.DeviceDesc10% = AVer_H788_HyATSC_II.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_11551461 ; H788 Hybrid ATSC 2 AV-in (Ii)

;******** AVerMedia H788 Pure ATSC***
%AVer.DeviceDesc11% = AVer_H788_PuATSC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_07551461 ; H788 Pure ATSC (I)

;******** AVerMedia H788 Pure ATSC IR***
%AVer.DeviceDesc11% = AVer_H788_PuATSC_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_1B551461 ; H788 Pure ATSC RC (I)

;******** AVerMedia H788 Pure Analog***
%AVer.DeviceDesc12% = AVer_H788_Analog_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_08551461 ; H788 Pure Analog (I)

;******** AVerMedia H788 Hybrid DVBT II***
%AVer.DeviceDesc08% = AVer_H788_HyDVBT_II_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_14551461 ; H788 Hybrid DVBT II

;******** AVerMedia H788 Pure DVBT II***
%AVer.DeviceDesc09% = AVer_H788_PuDVBT_II_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_15551461 ; H788 Pure DVBT II

;******** AVerMedia H788 Pure Analog II***
%AVer.DeviceDesc12% = AVer_H788_Analog_II_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_16551461 ; H788 Pure Analog II

;******** AVerMedia A701 ***
%AVer.DeviceDesc04% = AVer_A701.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_03551461 ; A701 (I)

;******** AVerMedia HC83_ATSC ***
%AVer.DeviceDesc25% = AVer_HC83_ATSC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_28551461 ; HC83_ATSC (I)

;******** AVerMedia HC83_DVBT ***
%AVer.DeviceDesc26% = AVer_HC83_DVBT.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_29551461 ; HC83_DVBT (I)

;******** AVerMedia M799 ***
%AVer.DeviceDesc13% = AVer_M799_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_09551461 ; M799
%AVer.DeviceDesc33% = AVer_M799_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_79911461 ; M799
%AVer.DeviceDesc33% = AVer_M799_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_79921461 ; M799

;******** AVerMedia A707 ***
%AVer.DeviceDesc23% = AVer_A707_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_26551461 ; A707
%AVer.DeviceDesc31% = AVer_A707o.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_36551461 ; A707o

;******** AVerMedia A707 Pure DVBT CI/CA ***
%AVer.DeviceDesc29% = AVer_A707_DVBT.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_2E551461 ; A707_PURE_DVBT_CICA

;******** AVerMedia A750 ***
%AVer.DeviceDesc28% = AVer_A750.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_03511461 ; A750

;******** AVerMedia A717 ***
%AVer.DeviceDesc32% = AVer_A717.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_71711461 ; A717

[AVerMedia.NTamd64.6]

;******** AVerMedia A177 ***
%AVer.DeviceDesc22% = AVer_A177_vistaRC.NTamd64 , PCI\VEN_1131&DEV_7162&SUBSYS_011C1461 ; A177

;******** AVerMedia A568 ***

;******** AVerMedia M789 ***
%AVer.DeviceDesc00% = AVer_M789.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_01511461 ; M789 (I)
%AVer.DeviceDesc01% = AVer_M789.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_02511461 ; M789 (II)

;******** AVerMedia M788 ***
%AVer.DeviceDesc02% = AVer_M788.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_01551461 ; M788 (I)

;******** AVerMedia H788 HyBrid DVBT I ***
%AVer.DeviceDesc08% = AVer_H788_HyDVBT_vistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_0B551461 ; H788 HyBrid DVBT (I)

;******** AVerMedia H788 Pure DVBT***
%AVer.DeviceDesc09% = AVer_H788_PuDVBT_vistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_0C551461 ; H788 Pure DVBT (I)

;******** AVerMedia H788 Hybrid ATSC***
%AVer.DeviceDesc10% = AVer_H788_HyATSC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_06551461 ; H788 Hybrid ATSC (I)

;******** AVerMedia H788 Hybrid ATSC IR***
%AVer.DeviceDesc10% = AVer_H788_HyATSC_vistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_1A551461 ; H788 Hybrid ATSC RC(I)

;******** AVerMedia H788 Hybrid ATSC 2 AV-in***
%AVer.DeviceDesc10% = AVer_H788_HyATSC_II.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_11551461 ; H788 Hybrid ATSC 2 AV-in (Ii)

;******** AVerMedia H788 Pure ATSC***
%AVer.DeviceDesc11% = AVer_H788_PuATSC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_07551461 ; H788 Pure ATSC (I)

;******** AVerMedia H788 Pure ATSC IR***
%AVer.DeviceDesc11% = AVer_H788_PuATSC_vistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_1B551461 ; H788 Pure ATSC RC (I)

;******** AVerMedia H788 Pure Analog***
%AVer.DeviceDesc12% = AVer_H788_Analog_vistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_08551461 ; H788 Pure Analog (I)

;******** AVerMedia H788 Hybrid DVBT II***
%AVer.DeviceDesc08% = AVer_H788_HyDVBT_II_vistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_14551461 ; H788 Hybrid DVBT II

;******** AVerMedia H788 Pure DVBT II***
%AVer.DeviceDesc09% = AVer_H788_PuDVBT_II_vistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_15551461 ; H788 Pure DVBT II

;******** AVerMedia H788 Pure Analog II***
%AVer.DeviceDesc12% = AVer_H788_Analog_II_vistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_16551461 ; H788 Pure Analog II

;******** AVerMedia A701 ***
%AVer.DeviceDesc04% = AVer_A701.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_03551461 ; A701 (I)

;******** AVerMedia HC83_ATSC ***
%AVer.DeviceDesc25% = AVer_HC83_ATSC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_28551461 ; HC83_ATSC (I)

;******** AVerMedia HC83_DVBT ***
%AVer.DeviceDesc26% = AVer_HC83_DVBT.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_29551461 ; HC83_DVBT (I)

;******** AVerMedia M799 ***
%AVer.DeviceDesc13% = AVer_M799_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_09551461 ; M799
%AVer.DeviceDesc33% = AVer_M799_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_79911461 ; M799
%AVer.DeviceDesc33% = AVer_M799_RC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_79921461 ; M799

;******** AVerMedia A707 ***
%AVer.DeviceDesc23% = AVer_A707_VistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_26551461 ; A707
%AVer.DeviceDesc31% = AVer_A707o.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_36551461 ; A707o

;******** AVerMedia A707 Pure DVBT CI/CA ***
%AVer.DeviceDesc29% = AVer_A707_DVBT.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_2E551461 ; A707_PURE_DVBT_CICA

;******** AVerMedia A750 ***
%AVer.DeviceDesc28% = AVer_A750_VistaRC.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_03511461 ; A750

;******** AVerMedia A717 ***
%AVer.DeviceDesc32% = AVer_A717.NTamd64 , PCI\VEN_1131&DEV_7160&SUBSYS_71711461 ; A717

[DestinationDirs]
AVerCap64.CopyFiles.NTamd64 = 10,system32\drivers ; be aware not to use 12 as the drivers directory, 
                                        ; as driver will not work anymore in W98
AverCap64.CopyDll.NTamd64 = 16425
AVer716x.CopyMCMLFiles_SC=24,ProgramData\PBDACN\MCML_Saa716x\SC
AVer716x.CopyMCMLImageFiles_SC=24,ProgramData\PBDACN\MCML_Saa716x\SC\Images
AVer716x.CopyMCMLFiles_TC=24,ProgramData\PBDACN\MCML_Saa716x\TC
AVer716x.CopyMCMLImageFiles_TC=24,ProgramData\PBDACN\MCML_Saa716x\TC\Images

[SourceDisksNames]
1 = %AVSTRM_INSTALLATION_DISK%,,

[SourceDisksFiles]
AVerBDA716x_x64.sys   = 1
MV716x_x64.ax         = 1
CoSetup_x64.ax        = 1
Setup_Signal.mcml                = 1
Setup_FirstPage.mcml             = 1
Setup_DataSource.mcml            = 1
Setup.mcml                       = 1
DiagnosticsPage.mcml             = 1
Diagnostics_Signal.mcml          = 1
Diagnostics_FirstPage.mcml       = 1
Diagnostics_DataSource.mcml      = 1
Setup_Signal_TC.mcml                = 1
Setup_FirstPage_TC.mcml             = 1
Setup_DataSource_TC.mcml            = 1
Setup_TC.mcml                       = 1
DiagnosticsPage_TC.mcml             = 1
Diagnostics_Signal_TC.mcml          = 1
Diagnostics_FirstPage_TC.mcml       = 1
Diagnostics_DataSource_TC.mcml      = 1
WinLogo1.png                     = 1
upbanner.png                     = 1
sqs.png                          = 1
MEDIACENTERLOGO.png              = 1
mCE.png                          = 1
logo.png                         = 1
listframe.png                    = 1
introduction.png                 = 1
footer.png                       = 1
COMMON.LIST.FRAME.png            = 1
COMMON.BUTTON.LEFT.FOCUSOVERLAY.png=1
COMMON.BUTTON.LEFT.FOCUS.png     = 1
COMMON.BUTTON.FIRSTRUN.DORMANT.FULL.png=1
COMMON.BACKGROUND.png            = 1
bg2.png                          = 1
AUTOSCROLL.CHEVRON.TOP.REST.png  = 1
AUTOSCROLL.CHEVRON.BOTTOM.REST.png=1

[AVerCap64.CopyFiles.NTamd64]
AVerBDA716x_x64.sys

[AverCap64.CopyDll.NTamd64]
MV716x_x64.ax
CoSetup_x64.ax

[AVer716x.CopyMCMLFiles_SC]
Setup_Signal.mcml
Setup_FirstPage.mcml
Setup_DataSource.mcml
Setup.mcml
DiagnosticsPage.mcml
Diagnostics_Signal.mcml
Diagnostics_FirstPage.mcml
Diagnostics_DataSource.mcml

[AVer716x.CopyMCMLImageFiles_SC]
WinLogo1.png
upbanner.png
sqs.png
MEDIACENTERLOGO.png
mCE.png
logo.png
listframe.png
introduction.png
footer.png
COMMON.LIST.FRAME.png
COMMON.BUTTON.LEFT.FOCUSOVERLAY.png
COMMON.BUTTON.LEFT.FOCUS.png
COMMON.BUTTON.FIRSTRUN.DORMANT.FULL.png
COMMON.BACKGROUND.png
bg2.png
AUTOSCROLL.CHEVRON.TOP.REST.png
AUTOSCROLL.CHEVRON.BOTTOM.REST.png

[AVer716x.CopyMCMLFiles_TC]
Setup_Signal_TC.mcml
Setup_FirstPage_TC.mcml
Setup_DataSource_TC.mcml
Setup_TC.mcml
DiagnosticsPage_TC.mcml
Diagnostics_Signal_TC.mcml
Diagnostics_FirstPage_TC.mcml
Diagnostics_DataSource_TC.mcml

[AVer716x.CopyMCMLImageFiles_TC]
WinLogo1.png
upbanner.png
sqs.png
MEDIACENTERLOGO.png
mCE.png
logo.png
listframe.png
introduction.png
footer.png
COMMON.LIST.FRAME.png
COMMON.BUTTON.LEFT.FOCUSOVERLAY.png
COMMON.BUTTON.LEFT.FOCUS.png
COMMON.BUTTON.FIRSTRUN.DORMANT.FULL.png
COMMON.BACKGROUND.png
bg2.png
AUTOSCROLL.CHEVRON.TOP.REST.png
AUTOSCROLL.CHEVRON.BOTTOM.REST.png

;======================================
;
;       Initialization Entries
;
;======================================

;******** AVerMedia M789 x64 ***
[AVer_M789.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_M789.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_M789.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_M789.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut


;******** AVerMedia M788 x64 ***
[AVer_M788.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_M788.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_M788.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_M788.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut


;******** AVerMedia H788 HyBrid DVBT_RC ***
[AVer_H788_HyDVBT_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_HyDVBT_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_HyDVBT_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_HyDVBT_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 HyBrid DVBT_vistaRC ***
[AVer_H788_HyDVBT_vistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_HyDVBT_vistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_HyDVBT_vistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_HyDVBT_vistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure DVBT_RC ***
[AVer_H788_PuDVBT_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_PuDVBT_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_PuDVBT_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_PuDVBT_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure DVBT_vistaRC ***
[AVer_H788_PuDVBT_vistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_PuDVBT_vistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_PuDVBT_vistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_PuDVBT_vistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Hybrid ATSC ***
[AVer_H788_HyATSC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_HyATSC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_HyATSC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_HyATSC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Hybrid ATSC_RC ***
[AVer_H788_HyATSC_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_HyATSC_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_HyATSC_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_HyATSC_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Hybrid ATSC_vistaRC ***
[AVer_H788_HyATSC_vistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_HyATSC_vistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_HyATSC_vistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_HyATSC_vistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut


;******** AVerMedia H788 Hybrid ATSC 2 AV-in ***
[AVer_H788_HyATSC_II.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_HyATSC_II.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_HyATSC_II.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_HyATSC_II.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure ATSC ***
[AVer_H788_PuATSC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_PuATSC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_PuATSC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_PuATSC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure ATSC_RC ***
[AVer_H788_PuATSC_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_PuATSC_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_PuATSC_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_PuATSC_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure ATSC_vistaRC ***
[AVer_H788_PuATSC_vistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_PuATSC_vistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_PuATSC_vistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_PuATSC_vistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure Analog_RC ***
[AVer_H788_Analog_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_Analog_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_Analog_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_Analog_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure Analog_vistaRC ***
[AVer_H788_Analog_vistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_Analog_vistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_Analog_vistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_Analog_vistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut


;******** AVerMedia H788 Hybrid DVBT II_RC ***
[AVer_H788_HyDVBT_II_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_HyDVBT_II_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_HyDVBT_II_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_HyDVBT_II_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Hybrid DVBT II_vistaRC ***
[AVer_H788_HyDVBT_II_vistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_HyDVBT_II_vistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_HyDVBT_II_vistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_HyDVBT_II_vistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut


;******** AVerMedia H788 Pure DVBT II_RC ***
[AVer_H788_PuDVBT_II_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_PuDVBT_II_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_PuDVBT_II_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_PuDVBT_II_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure DVBT II_vistaRC ***
[AVer_H788_PuDVBT_II_vistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_PuDVBT_II_vistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_PuDVBT_II_vistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_PuDVBT_II_vistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure Analog II_RC ***
[AVer_H788_Analog_II_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_Analog_II_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_Analog_II_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_Analog_II_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia H788 Pure Analog II_vistaRC ***
[AVer_H788_Analog_II_vistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_H788_Analog_II_vistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_H788_Analog_II_vistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_H788_Analog_II_vistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut


;******** AVerMedia A701 x64 ***
[AVer_A701.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_A701.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_A701.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A701.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia HC83_ATSC x64 ***
[AVer_HC83_ATSC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_HC83_ATSC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64


[AVer_HC83_ATSC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_HC83_ATSC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia HC83_DVBT x64 ***
[AVer_HC83_DVBT.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_HC83_DVBT.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_HC83_DVBT.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_HC83_DVBT.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia A177_RC x64 ***
[AVer_A177_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_A177_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_A177_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A177_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia A177_vistaRC x64 ***
[AVer_A177_vistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_A177_vistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_A177_vistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A177_vistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia A568 x64 ***

;******** AVerMedia M799_RC x64 ***
[AVer_M799_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_M799_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_M799_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_M799_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia A707_DVBT x64 ***
[AVer_A707_DVBT.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_A707_DVBT.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_A707_DVBT.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A707_DVBT.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia A707_RC x64 ***
[AVer_A707_RC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_A707_RC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_A707_RC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A707_RC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia A707_VistaRC x64 ***
[AVer_A707_VistaRC.NTamd64]
Include   = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs     = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg    = AVerCap64.AddReg.NTamd64, AVer_A707_VistaRC.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_A707_VistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A707_VistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia A707o ***
[AVer_A707o.NTamd64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64
AddReg        = AVerCap64.AddReg.NTamd64, AVer_A707o.AddReg
RegisterDlls  = AVerCap64.Register.NTamd64

[AVer_A707o.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A707o.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut


;******** AVerMedia A750 x64 ***
[AVer_A750.NTamd64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64, AVer716x.CopyMCMLFiles_SC, AVer716x.CopyMCMLImageFiles_SC, AVer716x.CopyMCMLFiles_TC, AVer716x.CopyMCMLImageFiles_TC
AddReg        = AVerCap64.AddReg.NTamd64, AVer_A750.AddReg, AVer716x_Win7_MCML.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_A750.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A750.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia A750_VistaRc ***
[AVer_A750_VistaRC.NTamd64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64, AVer716x.CopyMCMLFiles_SC, AVer716x.CopyMCMLImageFiles_SC, AVer716x.CopyMCMLFiles_TC, AVer716x.CopyMCMLImageFiles_TC
AddReg        = AVerCap64.AddReg.NTamd64, AVer_A750_VistaRC.AddReg, AVer716x_Win7_MCML.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_A750_VistaRC.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A750_VistaRC.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

;******** AVerMedia AVer_A717  ***
[AVer_A717.NTamd64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf, machine.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT, PciASPMOptOut
CopyFiles     = AVerCap64.CopyFiles.NTamd64, AverCap64.CopyDll.NTamd64, AVer716x.CopyMCMLFiles_SC, AVer716x.CopyMCMLImageFiles_SC, AVer716x.CopyMCMLFiles_TC, AVer716x.CopyMCMLImageFiles_TC
AddReg        = AVerCap64.AddReg.NTamd64, AVer_A717.AddReg, AVer716x_Win7_MCML.AddReg
RegisterDlls  = AverCap64.Register.NTamd64

[AVer_A717.NTamd64.Services]
AddService = %SERVICE_NAME_X64% , 0x00000002, AVerCap64.ServiceInstall.NTamd64, AVerCap64.EventInstall.NTamd64

[AVer_A717.NTamd64.HW]
Include       = machine.inf
Needs         = PciASPMOptOut

[AVerCap64.ServiceInstall.NTamd64]
DisplayName  = %DISPLAY_NAME%
Description  = %SERVICE_DESCRIPTION%
ServiceType  = %SERVICE_KERNEL_DRIVER%
StartType    = %SERVICE_DEMAND_START%
ErrorControl = %SERVICE_ERROR_IGNORE%
ServiceBinary=%12%\AVerBDA716x_x64.sys

[AVerCap64.EventInstall.NTamd64]
AddReg = PhilCapEvent_AddReg.NTamd64

;======================================
;
;           Registry Entries
;
;======================================

[AverCap64.Register.NTamd64]
16425,,MV716x_x64.ax,1
16425,,CoSetup_x64.ax,1

[PhilCapEvent_AddReg.NTamd64]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\AVerBDA716x_x64.sys"
HKR,,TypesSupported,0x00010001,7


;
;******** General Driver Registry Entries ***
;
[AVerCap64.AddReg.NTamd64]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,AVerBDA716x_x64.sys

; audio capture registry entries
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,AVerBDA716x_x64.sys


; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_PIN%,"Name",,"Capture"
HKLM,%MediaInterfaces%\{6a2e0650-28e4-11d0-A18C-00A0C9118959},,,"Copy Protect Notification Filter"
HKLM,%MediaInterfaces%\{6a2e0650-28e4-11d0-A18C-00A0C9118959},IID,1,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00
HKLM,%MediaInterfaces%\{1704290E-658E-4818-BBE3-A18A8E4ECD2B},,,"CState Control Filter"
HKLM,%MediaInterfaces%\{1704290E-658E-4818-BBE3-A18A8E4ECD2B},IID,1,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

HKR, "Parameters", Prefix,,"AVerMedia 716x BDA"

HKR, "AudioDecoder\Path0", "DefaultDecoderLevel",0x00010001,0x00
HKR, "AudioDecoder\Path0", "DefaultMonoLevel",0x00010001,0x07
HKR, "AudioDecoder\Path0", "DefaultSAPLevel",0x00010001,0x07

HKR, "VideoDecoder\Path0", "AutoBlank",0x00010001,0

HKR, "AudioDecoder\Path0", "VolumeTunerNTSC", 0x00010001, 0x04
HKR, "AudioDecoder\Path0", "VolumeTunerPAL", 0x00010001, 0x04
HKR, "AudioDecoder\Path0", "VolumeTunerSECAM", 0x00010001, 0x04
HKR, "AudioDecoder\Path0", "VolumeExt1",0x00010001,0

HKR, "AudioDecoder", "EnableAudioStdDetectionEx",0x00010001,1

HKR, "Parameters", "SECAML_EMITune", 0x00010001, 1		; Bob_0024_20080407

HKR, "VideoDecoder\Tuner\Path0", "DefaultBrightness",0x00010001,126
HKR, "VideoDecoder\Tuner\Path0", "DefaultContrast",0x00010001,67
HKR, "VideoDecoder\Tuner\Path0", "DefaultHue",0x00010001,129
HKR, "VideoDecoder\Tuner\Path0", "DefaultSaturation",0x00010001,63
HKR, "VideoDecoder\Tuner\Path0", "DefaultSharpness",0x00010001,8

HKR, "VideoDecoder\Tuner\Path1", "DefaultBrightness",0x00010001,126
HKR, "VideoDecoder\Tuner\Path1", "DefaultContrast",0x00010001,67
HKR, "VideoDecoder\Tuner\Path1", "DefaultHue",0x00010001,129
HKR, "VideoDecoder\Tuner\Path1", "DefaultSaturation",0x00010001,63
HKR, "VideoDecoder\Tuner\Path1", "DefaultSharpness",0x00010001,8

HKR, "Parameters", "QAMNode",0x00010001,0x01

[AVer716x_Win7_MCML.AddReg]
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_SC,GPNVConfig,0x00000000,"1"
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_SC,CNMCMLFile,0x00000000,"\??\C:\ProgramData\PBDACN\MCML_Saa716x\SC\"
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_SC,MCMLFilePath,0x00000000,"\??\C:\ProgramData\PBDACN\MCML_Saa716x\SC\"
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_SC,GuideDataType,0x00000000,"{C80C0DF3-6052-4c16-9F56-C44C21F73C45}"
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_SC,PbdaTunerType,0x00000000,"216C62DF-6D7F-4E9A-8571-05F14EDB766A"
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_TC,GPNVConfig,0x00000000,"1"
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_TC,CNMCMLFile,0x00000000,"\??\C:\ProgramData\PBDACN\MCML_Saa716x\TC\"
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_TC,MCMLFilePath,0x00000000,"\??\C:\ProgramData\PBDACN\MCML_Saa716x\TC\"
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_TC,GuideDataType,0x00000000,"{C80C0DF3-6052-4c16-9F56-C44C21F73C45}"
HKLM,System\CurrentControlSet\SERVICES\NXP_SAA716x_TC,PbdaTunerType,0x00000000,"216C62DF-6D7F-4E9A-8571-05F14EDB766A"

;
;******** Board - Specific Registry Entries ***
;

;******** AVerMedia M789 ***
[AVer_M789.AddReg]


;******** AVerMedia M788 ***
[AVer_M788.AddReg]

;******** AVerMedia H788 HyBrid DVBT_RC ***
[AVer_H788_HyDVBT_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 HyBrid DVBT_vistaRC ***
[AVer_H788_HyDVBT_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR, "ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia H788 Pure DVBT_RC***
[AVer_H788_PuDVBT_RC.AddReg]
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 0

;******** AVerMedia H788 Pure DVBT_vistaRC***
[AVer_H788_PuDVBT_vistaRC.AddReg]
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "IRSource", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 0

;******** AVerMedia H788 Hybrid ATSC***
[AVer_H788_HyATSC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Hybrid ATSC_RC***
[AVer_H788_HyATSC_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Hybrid ATSC_vistaRC***
[AVer_H788_HyATSC_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Hybrid ATSC 2 AV-in***
[AVer_H788_HyATSC_II.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Pure ATSC***
[AVer_H788_PuATSC.AddReg]
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Pure ATSC_RC ***
[AVer_H788_PuATSC_RC.AddReg]
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Pure ATSC_vistaRC***
[AVer_H788_PuATSC_vistaRC.AddReg]
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"
HKR, "Parameters", "AVerParam_1",0x00010001,1

;******** AVerMedia H788 Pure Analog_RC***
[AVer_H788_Analog_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 Pure Analog_vistaRC***
[AVer_H788_Analog_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia H788 Hybrid DVBT II_RC***
[AVer_H788_HyDVBT_II_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 Hybrid DVBT II_vistaRC***
[AVer_H788_HyDVBT_II_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia H788 Pure DVBT II_RC***
[AVer_H788_PuDVBT_II_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 Pure DVBT II_vistaRC***
[AVer_H788_PuDVBT_II_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia H788 Pure Analog II_RC***
[AVer_H788_Analog_II_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia H788 Pure Analog II_vistaRC ***
[AVer_H788_Analog_II_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"


;******** AVerMedia A701 ***
[AVer_A701.AddReg]
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,4
HKR, "Parameters", Prefix,,"AVerMedia BDA"

;******** AVerMedia HC83_ATSC ***
[AVer_HC83_ATSC.AddReg]
HKR, "Parameters", "PowerSaveMode",0x00010001,1
HKR, "Parameters", "AVerParam_1",0x00010001,1
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_AnalogIFLevel",0x00010001,3

;******** AVerMedia HC83_DVBT ***
[AVer_HC83_DVBT.AddReg]
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,4
HKR, "Parameters", "PowerSaveMode",0x00010001,1

HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_AnalogIFLevel",0x00010001,3

;******** AVerMedia M799_RC ***
[AVer_M799_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
HKR, "Parameters", ForceTunerStdName,," SBTD-T Tuner"


;******** AVerMedia A177_RC ***
[AVer_A177_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "FMPath",0x00010001,4

; Enable RF frequency offset auto detection for DVB-T, YWLee
HKR, "Parameters","EnableAutoOffset",0x00010001,0x01

; Don't use tuning thread, YWLee
HKR, "Parameters", "TDA8275A_UseTuningThread" , 0x00010001, 0x00

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;******** AVerMedia A177_vistaRC ***
[AVer_A177_vistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "FMPath",0x00010001,4

; Enable RF frequency offset auto detection for DVB-T, 
HKR, "Parameters","EnableAutoOffset",0x00010001,0x01

; Don't use tuning thread, 
HKR, "Parameters", "TDA8275A_UseTuningThread" , 0x00010001, 0x00

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;******** AVerMedia A707_RC ***
[AVer_A707_RC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,1

HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,4000000
HKR, "Parameters", "Afa9033_8M_IF_FREQ",0x00010001,4000000
HKR, "Parameters", "TDA18271_DVBT_8M_STD",0x00010001,0x19
HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_6M",0x00010001,4570000       
HKR, "Parameters", "Afa9033_6M_IF_FREQ",0x00010001,4570000             


;HKR, "Parameters", "TDA18271_AnalogIFLevel_PAL_B",0x00010001,0
;HKR, "Parameters", "TDA18271_AnalogIFLevel_SCEAM_L",0x00010001,1

;HKR, "Parameters", "Gafixd_PAL_B",0x00010001,1
;HKR, "Parameters", "Gafixd_SCEAM_L",0x00010001,1
;HKR, "Parameters", "DTV_GAIN1_PAL_B",0x00010001,5
;HKR, "Parameters", "DTV_GAIN1_SCEAM_L",0x00010001,0
HKR, "Parameters", "SECAML_SSIF_LEVEL",0x00010001,2

HKR, "Parameters", "SECAML_EMITune", 0x00010001, 0

HKR, "Parameters", "I2CBus0Speed",0x00010001,0
HKR, "Parameters", "I2CBus1Speed",0x00010001,4

HKR, "Parameters", "DgtlPacketNumber",0x00010001,312

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

HKR, "Parameters", "DVBS_I2C_DelayTime", 0x00010001, 5

;AVEREth.sys
HKR, "ENUM\Device1",pnpid,,"AVerMedia.EtherNet"		  ; Virtual Network driver for data service.

;CICA Support
;HKR, "Parameters", "CICAEnable", 0x00010001, 1
;HKR, "Parameters", "CICAI2CBus", 0x00010001, 0
HKR, "Parameters", "AVerParam_6", 0x00010001, 1
HKR, "Parameters", "AVerParam_7", 0x00010001, 0
HKR, "Parameters", "AVerParam_9", 0x00010001, 16

;******** AVerMedia A707_DVBT ***
[AVer_A707_DVBT.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,1

HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,4000000
HKR, "Parameters", "Afa9033_8M_IF_FREQ",0x00010001,4000000
HKR, "Parameters", "TDA18271_DVBT_8M_STD",0x00010001,0x19
HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_6M",0x00010001,4570000      
HKR, "Parameters", "Afa9033_6M_IF_FREQ",0x00010001,4570000            
HKR, "Parameters", "SECAML_SSIF_LEVEL",0x00010001,2

HKR, "Parameters", "I2CBus0Speed",0x00010001,0
HKR, "Parameters", "I2CBus1Speed",0x00010001,4

HKR, "Parameters", "DgtlPacketNumber",0x00010001,312

;CICA Support
;HKR, "Parameters", "CICAEnable", 0x00010001, 1
;HKR, "Parameters", "CICAI2CBus", 0x00010001, 0
HKR, "Parameters", "AVerParam_6", 0x00010001, 1
HKR, "Parameters", "AVerParam_7", 0x00010001, 0
HKR, "Parameters", "AVerParam_9", 0x00010001, 16

;******** AVerMedia A707_VistaRC ***
[AVer_A707_VistaRC.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,1

HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,4000000
HKR, "Parameters", "Afa9033_8M_IF_FREQ",0x00010001,4000000
HKR, "Parameters", "TDA18271_DVBT_8M_STD",0x00010001,0x19
HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_6M",0x00010001,4570000    
HKR, "Parameters", "Afa9033_6M_IF_FREQ",0x00010001,4570000         

;HKR, "Parameters", "TDA18271_AnalogIFLevel_PAL_B",0x00010001,0
;HKR, "Parameters", "TDA18271_AnalogIFLevel_SCEAM_L",0x00010001,1
HKR, "Parameters", "SECAML_SSIF_LEVEL",0x00010001,2

;HKR, "Parameters", "Gafixd_PAL_B",0x00010001,1
;HKR, "Parameters", "Gafixd_SCEAM_L",0x00010001,1
;HKR, "Parameters", "DTV_GAIN1_PAL_B",0x00010001,5
;HKR, "Parameters", "DTV_GAIN1_SCEAM_L",0x00010001,0

HKR, "Parameters", "SECAML_EMITune", 0x00010001, 0

HKR, "Parameters", "I2CBus0Speed",0x00010001,0
HKR, "Parameters", "I2CBus1Speed",0x00010001,4

HKR, "Parameters", "DgtlPacketNumber",0x00010001,312

HKR, "Parameters", "DVBS_I2C_DelayTime", 0x00010001, 5

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"

;AVEREth.sys
HKR, "ENUM\Device1",pnpid,,"AVerMedia.EtherNet"		  ; Virtual Network driver for data service.

;CICA Support
;HKR, "Parameters", "CICAEnable", 0x00010001, 1
;HKR, "Parameters", "CICAI2CBus", 0x00010001, 0
HKR, "Parameters", "AVerParam_6", 0x00010001, 1
HKR, "Parameters", "AVerParam_7", 0x00010001, 0
HKR, "Parameters", "AVerParam_9", 0x00010001, 16

;******** AVerMedia A707o ***
[AVer_A707o.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "TDA18271_DigitalIFLevel",0x00010001,1

HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_8M",0x00010001,4000000
HKR, "Parameters", "Afa9033_8M_IF_FREQ",0x00010001,4000000
HKR, "Parameters", "TDA18271_DVBT_8M_STD",0x00010001,0x19
HKR, "Parameters", "TDA18271_DVBT_IF_FREQ_6M",0x00010001,4570000  
HKR, "Parameters", "Afa9033_6M_IF_FREQ",0x00010001,4570000     

HKR, "Parameters", "SECAML_SSIF_LEVEL",0x00010001,2

HKR, "Parameters", "SECAML_EMITune", 0x00010001, 0

HKR, "Parameters", "I2CBus0Speed",0x00010001,0
HKR, "Parameters", "I2CBus1Speed",0x00010001,4

HKR, "Parameters", "DgtlPacketNumber",0x00010001,312

HKR, "Parameters", "DVBS_I2C_DelayTime", 0x00010001, 5

HKR, "AudioDecoder\Path0", "VolumeTunerNTSC", 0x00010001, 4
HKR, "AudioDecoder\Path0", "VolumeTunerPAL", 0x00010001, 3
HKR, "AudioDecoder\Path0", "VolumeTunerSECAM", 0x00010001, 4

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1

;AVEREth.sys
HKR, "ENUM\Device1",pnpid,,"AVerMedia.EtherNet"		  ; Virtual Network driver for data service.

;CICA Support
;HKR, "Parameters", "CICAEnable", 0x00010001, 1
;HKR, "Parameters", "CICAI2CBus", 0x00010001, 0
HKR, "Parameters", "AVerParam_6", 0x00010001, 1
HKR, "Parameters", "AVerParam_7", 0x00010001, 0
HKR, "Parameters", "AVerParam_9", 0x00010001, 16

HKR, "Parameters", "TunerAddIn", 0x00010001, 0x00100102


;******** AVerMedia A750 ***
[AVer_A750.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 1

HKR, "Parameters", "I2CBus0Speed",0x00010001,1	; 400KHz
HKR, "Parameters", "I2CBus1Speed",0x00010001,3	; 75KHz
HKR, "Parameters", ForceTunerStdName,," DTMB Tuner"
HKR, "Parameters", "PBDA Tuner",0x00010001,1

;******** AVerMedia A750_VistaRc ***
[AVer_A750_VistaRc.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "IRSource", 0x00010001, 1
HKR, "Parameters", "RemoteICI2CBus", 0x00010001, 1

HKR, "Parameters", "I2CBus0Speed",0x00010001,1	; 400KHz
HKR, "Parameters", "I2CBus1Speed",0x00010001,3	; 75KHz
HKR, "Parameters", ForceTunerStdName,," DTMB Tuner"
HKR, "Parameters", "PBDA Tuner",0x00010001,1

;IR Support
HKR, "Parameters", "IREnable", 0x00010001, 1
;HKR,"ENUM\CIR",pnpid,,"AVerIR"
;

;******** AVerMedia A717 ***
[AVer_A717.AddReg]
HKR, "Parameters", "UseDecoderRegistry",0x00010001,1
HKR, "Parameters", "I2CBus0Speed",0x00010001,3
HKR, "Parameters", "I2CBus1Speed",0x00010001,3

HKR, "Parameters", "PowerSaveMode",0x00010001,0
HKR, "Parameters", "AVerParam_2",0x00010001,1

HKR, "Parameters", "SECAML_EMITune", 0x00010001, 0

HKR, "Parameters", "DgtlPacketNumber",0x00010001,312


;CICA Support
HKR, "Parameters", "AVerParam_6", 0x00010001, 2
HKR, "Parameters", "AVerParam_7", 0x00010001, 1
HKR, "Parameters", "AVerParam_8", 0x00010001, 0
HKR, "Parameters", "AVerParam_9", 0x00010001, 14
HKR, "Parameters", "AVerParam_10", 0x00010001, 14

;AVEREth.sys
HKR, "ENUM\Device1",pnpid,,"AVerMedia.EtherNet"		  ; Virtual Network driver for data service.

;RELockMachine
HKR, "Parameters", "RELOCKMachineEnable", 0x00010001, 0

HKR, "Parameters", "TunerAddIn", 0x00010001, 0x01100102

HKR, "Parameters", "Afa9033_6M_IF_FREQ",0x00010001,4570000
HKR, "Parameters", "Afa9033_7M_IF_FREQ",0x00010001,3500000
HKR, "Parameters", "Afa9033_8M_IF_FREQ",0x00010001,4000000

;*** strings, GUIDs and names
;

[Strings]

SERVICE_NAME_X64         = "AVerBDA6x_x64"

; Proxy GUIDs

KSProxy.CLSID            = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSXBar.CLSID             = "{71F96460-78F3-11d0-A18C-00A0C9118956}"
KSTVAudio.CLSID          = "{71F96462-78F3-11d0-A18C-00A0C9118956}"
KSTvTune.CLSID           = "{266EEE40-6C63-11cf-8A03-00AA006ECB65}"

; Category GUIDs

KSCATEGORY_MULTIPLEXER   = "{7A5DE1D3-01A1-452c-B481-4FA2B96271E8}"
KSCATEGORY_ENCODER       = "{19689BF6-C384-48fd-AD51-90E58C79F70B}"
KSCATEGORY_CAPTURE       = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO         = "{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_AUDIO         = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}"

; Our Pin Name GUIDs

AVSTREAM_ANLG_AUDIO_IN_PIN   = "{7BB284B9-714D-493d-A101-B1B028E782BD}"
AVSTREAM_ANLG_AUDIO_OUT_PIN  = "{5582E657-E596-42b5-9DB3-541B27A2355F}"
AVSTREAM_ANLG_VIDEO_ITU_PIN  = "{82631A2E-403C-4581-A4B0-EC173D004410}"
AVSTREAM_ANLG_AUDIO_I2S_PIN  = "{C2E46358-F032-4d88-B802-06B59D162730}"
AVSTREAM_ANLG_VIDEO_PIN      = "{16FFBD0A-F770-4692-A2FF-DD394DFE9564}"
AVSTREAM_ANLG_AUDIO_PIN      = "{BA9E27B1-CF44-490e-8EAB-5F662E5FFE74}"

; Our Filter GUIDs


; system defines

SERVICE_BOOT_START     = 0x0 
SERVICE_SYSTEM_START   = 0x1 
SERVICE_AUTO_START     = 0x2 
SERVICE_DEMAND_START   = 0x3 
SERVICE_DISABLED       = 0x4 

SERVICE_KERNEL_DRIVER  = 0x1 
SERVICE_ERROR_IGNORE   = 0x0 
SERVICE_ERROR_NORMAL   = 0x1 
SERVICE_ERROR_SEVERE   = 0x2
SERVICE_ERROR_CRITICAL = 0x3 

FLG_REGSVR_DLLREGISTER = 0x00000001

;Our strings

AVer                     = "AVerMedia TECHNOLOGIES, Inc."
60Hybrid.DeviceDesc      = "Philips SAA7160, Hybrid Capture Device"
61Hybrid.DeviceDesc      = "Philips SAA7161, Hybrid Capture Device"
62Hybrid.DeviceDesc      = "Philips SAA7162, Hybrid Capture Device"
63Hybrid.DeviceDesc      = "Philips SAA7163  Hybrid Capture Device"

AVer.DeviceDesc00        = "AVerMedia M789 PCIe Pure DVBT"
AVer.DeviceDesc01        = "AVerMedia M789 PCIe Dual DVBT"
AVer.DeviceDesc02        = "AVerMedia M788 PCIe Hybrid Analog/ATSC"
AVer.DeviceDesc03        = "AVerMedia A317 Mini-Card Hybrid Analog/ATSC"
AVer.DeviceDesc04        = "AVerMedia A701 PCIe Hybrid Analog/DVBT, Combo DVBS"
AVer.DeviceDesc05        = "AVerMedia HC82 Express-Card Hybrid Analog/ATSC"
AVer.DeviceDesc06        = "AVerMedia HC82 Express-Card Hybrid Analog/DVBT"
AVer.DeviceDesc07        = "AVerMedia A316 Mini-Card Hybrid Analog/DVBT"
AVer.DeviceDesc08        = "AVerMedia H788 PCIe Hybrid Analog/DVBT"
AVer.DeviceDesc09        = "AVerMedia H788 PCIe DVBT"
AVer.DeviceDesc10        = "AVerMedia H788 PCIe Hybrid Analog/ATSC"
AVer.DeviceDesc11        = "AVerMedia H788 PCIe ATSC"
AVer.DeviceDesc12        = "AVerMedia H788 PCIe Analog"
AVer.DeviceDesc13        = "AVerMedia M799 PCIe Hybrid SBTD-T"
AVer.DeviceDesc14        = "AVerMedia A317D Mini-Card ATSC"
AVer.DeviceDesc15        = "AVerMedia A327 Mini-Card Hybrid Analog/ATSC"
AVer.DeviceDesc16        = "AVerMedia A326 Mini-Card Hybrid Analog/DVBT"
AVer.DeviceDesc17        = "AVerMedia A188 PCIe Duo Hybrid Analog/DVBT"
AVer.DeviceDesc18        = "AVerMedia A188C PCIe Duo Hybrid Analog/ATSC"
AVer.DeviceDesc19        = "AVerMedia A188 PCIe Analog"
AVer.DeviceDesc20        = "AVerMedia A188 PCIe Pure DVBT"
AVer.DeviceDesc21        = "AVerMedia A188C PCIe Pure ATSC"
AVer.DeviceDesc22        = "AVerMedia A177 PCIe Dual Hybrid Analog/DVBT"
AVer.DeviceDesc23        = "AVerMedia A707 PCIe Dual Hybrid Analog/DVBT/DVBS"
AVer.DeviceDesc24        = "AVerMedia A188O PCIe Duo Hybrid Analog/DVBT"
AVer.DeviceDesc25        = "AVerMedia HC83 Express-Card Hybrid Analog/ATSC"
AVer.DeviceDesc26        = "AVerMedia HC83 Express-Card Hybrid Analog/DVBT"
AVer.DeviceDesc27        = "AVerMedia A311 Mini-Card Dual DVBT"
AVer.DeviceDesc28        = "AVerMedia A750 PCIe DTMB"
AVer.DeviceDesc29        = "AVerMedia A707 PCIe Pure DVBT"
AVer.DeviceDesc31        = "AVerMedia A707o PCIe Dual Hybrid Analog/DVBT/DVBS"
AVer.DeviceDesc32        = "AVerMedia A717 PCIe Dual Hybrid Analog/DVBT/DVBC/DVBS"
AVer.DeviceDesc33        = "AVerMedia M799 PCIe Analog"

AVSTRM_INSTALLATION_DISK = "AVerBDA6x installation disk"
DISPLAY_NAME             = "AVerMedia SAA716x BDA Service"
SERVICE_DESCRIPTION      = "The PCIe capture driver"
MediaInterfaces          = "System\CurrentControlSet\Control\MediaInterfaces"
