
[version]
Signature="$Chicago$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%AirgoNet%
Compatible=1
DriverVer=09/21/2004, 1.2.0.80
MillenniumPreferred=.ME
CatalogFile=AniNet.cat
[SourceDisksNames]
1= %Disk_1%,,,
[SourceDisksFiles]
WNIhdd51.sys=1
WNIhdd50.sys=1
[DestinationDirs]
DefaultDestDir=11
Airgo_Driver.Copyfiles=12
Airgo_Driver.NT.5.1.Copyfiles=12
[Manufacturer]
%Airgo%=Airgo,NT.5.1
[ControlFlags]
ExcludeFromSelect=PCI\VEN_17CB&DEV_0001&SUBSYS_000117CB, \
PCI\VEN_17CB&DEV_0001&SUBSYS_80101799
[Airgo]
%Belkin.DeviceDesc%=Airgo.ndi, PCI\VEN_17CB&DEV_0001&SUBSYS_80101799
%Belkin.DeviceDesc%=Airgo.ndi, PCI\VEN_17CB&DEV_0001&SUBSYS_000117CB
[Airgo.NT.5.1]
%Belkin.DeviceDesc%=Airgo.ndi.NT.5.1, PCI\VEN_17CB&DEV_0001&SUBSYS_80101799
%Belkin.DeviceDesc%=Airgo.ndi.NT.5.1, PCI\VEN_17CB&DEV_0001&SUBSYS_000117CB
[Airgo.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8
AddReg=Airgo.NT.reg, AdvancedParms, StaticParms
;CpyFiles=Airgo_Driver.CopyFiles
[Airgo.ndi.NT.Services]
AddService=Airgo, 2, Airgo.Service, Airgo.EventLog
[Airgo.Service]
DisplayName=%Airgo.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\wnihdd50.sys
LoadOrderGroup=NDIS
[Airgo.EventLog]
AddReg=Airgo.AddEventLog.reg
[Airgo.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\wnihdd50.sys"
HKR, , TypesSupported, 0x00010001, 7
[Airgo.ndi.NT.5.1]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8
AddReg=Airgo.NT.reg, AdvancedParms, StaticParms
;CpyFiles=Airgo_Driver.NT.5.1.CopyFiles
[Airgo.ndi.NT.5.1.Services]
AddService=Airgo, 2, Airgo.NT.5.1.Service, Airgo.EventLog
[Airgo.NT.5.1.Service]
DisplayName=%Airgo.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\wnihdd51.sys
LoadOrderGroup=NDIS
[Airgo.EventLog]
AddReg=Airgo.NT.5.1.AddEventLog.reg
[Airgo.NT.5.1.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\wnihdd51.sys"
HKR, , TypesSupported, 0x00010001, 7
[Airgo.NT.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis5"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi, Service, 0, "Airgo"
[Airgo_Driver.Copyfiles]
wnihdd50.sys,,,2
[Airgo_Driver.NT.5.1.CopyFiles]
wnihdd51.sys,,,2
[AdvancedParms]
HKR,,MonBufSize,,"2600"
HKR,,MonBufCount,,"12"
HKR,,MBMsgBufSize,,"4096"
HKR,,MBMsgBufCount,,"6"
HKR,,RxBufferCount,,"100"
HKR,NDI\params\RxBufferCount, ParamDesc, 0, "Rx Buffer Count"
HKR,NDI\params\RxBufferCount, type, 0, "dword"
HKR,NDI\params\RxBufferCount, default, 0, "100"
HKR,NDI\params\RxBufferCount, min, 0, "10"
HKR,NDI\params\RxBufferCount, max, 0, "100000"
HKR,NDI\params\RxBufferCount, step, 0, "10"
HKR,,RxBufferSize,,"256"
HKR,,TxDescCount,,"128"
HKR,,RxDescCount,,"128"
HKR,,gNwDensity,,"Medium"
HKR,NDI\params\gNwDensity, ParamDesc, 0, "Network Density"
HKR,NDI\params\gNwDensity, type, 0, "enum"
HKR,NDI\params\gNwDensity, default, 0, "Medium"
HKR,NDI\params\gNwDensity\enum, "High", 0, "High"
HKR,NDI\params\gNwDensity\enum, "Medium", 0, "Medium"
HKR,NDI\params\gNwDensity\enum, "Low", 0, "Low"
HKR,,gTxPwrLevel,,"High"
HKR,NDI\params\gTxPwrLevel, ParamDesc, 0, "Tx Power"
HKR,NDI\params\gTxPwrLevel, type, 0, "enum"
HKR,NDI\params\gTxPwrLevel, default, 0, "High"
HKR,NDI\params\gTxPwrLevel\enum, "High", 0, "High"
HKR,NDI\params\gTxPwrLevel\enum, "Low", 0, "Low"
HKR,,gNumTxAntenna,,"2"
HKR,NDI\params\gNumTxAntenna, ParamDesc, 0, "Num Tx Antennas"
HKR,NDI\params\gNumTxAntenna, type, 0, "int"
HKR,NDI\params\gNumTxAntenna, default, 0, "2"
HKR,NDI\params\gNumTxAntenna, min, 0, "1"
HKR,NDI\params\gNumTxAntenna, max, 0, "2"
HKR,NDI\params\gNumTxAntenna, step, 0, "1"
HKR,,gNumRxAntenna,,"3"
HKR,NDI\params\gNumRxAntenna, ParamDesc, 0, "Num Rx Antennas"
HKR,NDI\params\gNumRxAntenna, type, 0, "int"
HKR,NDI\params\gNumRxAntenna, default, 0, "3"
HKR,NDI\params\gNumRxAntenna, min, 0, "1"
HKR,NDI\params\gNumRxAntenna, max, 0, "3"
HKR,NDI\params\gNumRxAntenna, step, 0, "1"
HKR,,gAckTimeout11A,,"25"
HKR,NDI\params\gAckTimeout11A, ParamDesc, 0, "AckTimeout11A"
HKR,NDI\params\gAckTimeout11A, type, 0, "int"
HKR,NDI\params\gAckTimeout11A, default, 0, "25"
HKR,NDI\params\gAckTimeout11A, min, 0, "0"
HKR,NDI\params\gAckTimeout11A, max, 0, "100"
HKR,NDI\params\gAckTimeout11A, step, 0, "1"
HKR,,gAckTimeout11BG,,"30"
HKR,NDI\params\gAckTimeout11BG, ParamDesc, 0, "AckTimeout11BG"
HKR,NDI\params\gAckTimeout11BG, type, 0, "int"
HKR,NDI\params\gAckTimeout11BG, default, 0, "30"
HKR,NDI\params\gAckTimeout11BG, min, 0, "0"
HKR,NDI\params\gAckTimeout11BG, max, 0, "100"
HKR,NDI\params\gAckTimeout11BG, step, 0, "1"
HKR,,gShortRetryLimit,,"0"
HKR,NDI\params\gShortRetryLimit, ParamDesc, 0, "ShortRetryLimit"
HKR,NDI\params\gShortRetryLimit, type, 0, "int"
HKR,NDI\params\gShortRetryLimit, default, 0, "0"
HKR,NDI\params\gShortRetryLimit, min, 0, "0"
HKR,NDI\params\gShortRetryLimit, max, 0, "255"
HKR,NDI\params\gShortRetryLimit, step, 0, "1"
HKR,,gLongRetryLimit,,"0"
HKR,NDI\params\gLongRetryLimit, ParamDesc, 0, "LongRetryLimit"
HKR,NDI\params\gLongRetryLimit, type, 0, "int"
HKR,NDI\params\gLongRetryLimit, default, 0, "0"
HKR,NDI\params\gLongRetryLimit, min, 0, "0"
HKR,NDI\params\gLongRetryLimit, max, 0, "255"
HKR,NDI\params\gLongRetryLimit, step, 0, "1"
HKR,,gFragmentationThreshold,,"2000"
HKR,NDI\params\gFragmentationThreshold, ParamDesc, 0, "Fragmentation Threshold"
HKR,NDI\params\gFragmentationThreshold, type, 0, "int"
HKR,NDI\params\gFragmentationThreshold, default, 0, "2000"
HKR,NDI\params\gFragmentationThreshold, min, 0, "256"
HKR,NDI\params\gFragmentationThreshold, max, 0, "2346"
HKR,NDI\params\gFragmentationThreshold, step, 0, "1"
HKR,,gRTSThreshold,,"2347"
HKR,NDI\params\gRTSThreshold, ParamDesc, 0, "RTS Threshold"
HKR,NDI\params\gRTSThreshold, type, 0, "int"
HKR,NDI\params\gRTSThreshold, default, 0, "2347"
HKR,NDI\params\gRTSThreshold, min, 0, "0"
HKR,NDI\params\gRTSThreshold, max, 0, "2347"
HKR,NDI\params\gRTSThreshold, step, 0, "1"
HKR,,gMaxAckRate11A,,"5"
HKR,NDI\params\gMaxAckRate11A, ParamDesc, 0, "Max Ack Rate (11A)"
HKR,NDI\params\gMaxAckRate11A, type, 0, "int"
HKR,NDI\params\gMaxAckRate11A, default, 0, "5"
HKR,NDI\params\gMaxAckRate11A, min, 0, "1"
HKR,NDI\params\gMaxAckRate11A, max, 0, "108"
HKR,NDI\params\gMaxAckRate11A, step, 0, "1"
HKR,,gMaxAckRate11B,,"22"
HKR,NDI\params\gMaxAckRate11B, ParamDesc, 0, "Max Ack Rate (11B)"
HKR,NDI\params\gMaxAckRate11B, type, 0, "int"
HKR,NDI\params\gMaxAckRate11B, default, 0, "22"
HKR,NDI\params\gMaxAckRate11B, min, 0, "2"
HKR,NDI\params\gMaxAckRate11B, max, 0, "22"
HKR,NDI\params\gMaxAckRate11B, step, 0, "1"
HKR,,gCalibration,,"1"
HKR,NDI\params\gCalibration, ParamDesc, 0, "Calibration (on/off)"
HKR,NDI\params\gCalibration, type, 0, "enum"
HKR,NDI\params\gCalibration, default, 0, "1"
HKR,NDI\params\gCalibration\enum, "0", 0, "OFF"
HKR,NDI\params\gCalibration\enum, "1", 0, "ON"
HKR,,gCalibrationPeriod,,"5"
HKR,NDI\params\gCalibrationPeriod, ParamDesc, 0, "Calibration period (minutes)"
HKR,NDI\params\gCalibrationPeriod, type, 0, "int"
HKR,NDI\params\gCalibrationPeriod, default, 0, "5"
HKR,NDI\params\gCalibrationPeriod, min, 0, "2"
HKR,NDI\params\gCalibrationPeriod, max, 0, "10"
HKR,NDI\params\gCalibrationPeriod, step, 0, "1"
HKR,,gBgScanPeriod,,"5000"
HKR,NDI\params\gBgScanPeriod, ParamDesc, 0, "Background Scan period (milliseconds)"
HKR,NDI\params\gBgScanPeriod, type, 0, "dword"
HKR,NDI\params\gBgScanPeriod, default, 0, "5000"
HKR,NDI\params\gBgScanPeriod, min, 0, "0"
HKR,NDI\params\gBgScanPeriod, max, 0, "180000"
HKR,NDI\params\gBgScanPeriod, step, 0, "1"
HKR,,gBgScanMinChannelTime,,"20"
HKR,NDI\params\gBgScanMinChannelTime, ParamDesc, 0, "Background Min Channel Time (milliseconds)"
HKR,NDI\params\gBgScanMinChannelTime, type, 0, "dword"
HKR,NDI\params\gBgScanMinChannelTime, default, 0, "20"
HKR,NDI\params\gBgScanMinChannelTime, min, 0, "1"
HKR,NDI\params\gBgScanMinChannelTime, max, 0, "65535"
HKR,NDI\params\gBgScanMinChannelTime, step, 0, "1"
HKR,,gBgScanMaxChannelTime,,"40"
HKR,NDI\params\gBgScanMaxChannelTime, ParamDesc, 0, "Background Max Channel Time (milliseconds)"
HKR,NDI\params\gBgScanMaxChannelTime, type, 0, "dword"
HKR,NDI\params\gBgScanMaxChannelTime, default, 0, "40"
HKR,NDI\params\gBgScanMaxChannelTime, min, 0, "1"
HKR,NDI\params\gBgScanMaxChannelTime, max, 0, "65535"
HKR,NDI\params\gBgScanMaxChannelTime, step, 0, "1"
HKR,,gAdaptiveThresholdAlgo,,"D0"
HKR,NDI\params\gAdaptiveThresholdAlgo, ParamDesc, 0, "Adaptive Threshold Algo Selection"
HKR,NDI\params\gAdaptiveThresholdAlgo, type, 0, "enum"
HKR,NDI\params\gAdaptiveThresholdAlgo, default, 0, "D0"
HKR,NDI\params\gAdaptiveThresholdAlgo\enum, "Disabled",0, "Disabled"
HKR,NDI\params\gAdaptiveThresholdAlgo\enum, "CD", 0, "CD"
HKR,NDI\params\gAdaptiveThresholdAlgo\enum, "D0", 0, "D0"
HKR,,gCCAMode,,"7"
HKR,NDI\params\gCCAMode, ParamDesc, 0, "CCA Mode"
HKR,NDI\params\gCCAMode, type, 0, "enum"
HKR,NDI\params\gCCAMode, default, 0, "7"
HKR,NDI\params\gCCAMode\enum, "0", 0, "None"
HKR,NDI\params\gCCAMode\enum, "1", 0, "ED"
HKR,NDI\params\gCCAMode\enum, "2", 0, "CD"
HKR,NDI\params\gCCAMode\enum, "3", 0, "CD and CS"
HKR,NDI\params\gCCAMode\enum, "4", 0, "ED and CD"
HKR,NDI\params\gCCAMode\enum, "5", 0, "ED or CD"
HKR,NDI\params\gCCAMode\enum, "6", 0, "ED and CS and CD"
HKR,NDI\params\gCCAMode\enum, "7", 0, "ED or CS and CD"
HKR,,gEDThreshold,,"60"
HKR,NDI\params\gEDThreshold, ParamDesc, 0, "ED Threshold"
HKR,NDI\params\gEDThreshold, type, 0, "dword"
HKR,NDI\params\gEDThreshold, default, 0, "60"
HKR,NDI\params\gEDThreshold, min, 0, "0"
HKR,NDI\params\gEDThreshold, max, 0, "114"
HKR,NDI\params\gEDThreshold, step, 0, "1"
HKR,,gAckPolicy,,"0"
HKR,NDI\params\gAckPolicy, ParamDesc, 0, "Ack Policy"
HKR,NDI\params\gAckPolicy, type, 0, "enum"
HKR,NDI\params\gAckPolicy, default, 0, "0"
HKR,NDI\params\gAckPolicy\enum, "0", 0, "Immediate"
HKR,NDI\params\gAckPolicy\enum, "1", 0, "No Ack"
HKR,NDI\params\gAckPolicy\enum, "2", 0, "Automatic"
HKR,NDI\params\gAckPolicy\enum, "3", 0, "Burst"
HKR,,gOperatingChannel,,"00000000"
HKR,NDI\params\gOperatingChannel, ParamDesc, 0, "Operating Channel or Band"
HKR,NDI\params\gOperatingChannel, type, 0, "enum"
HKR,NDI\params\gOperatingChannel, default, 0, "0"
HKR,NDI\params\gOperatingChannel\enum, "00000000", 0, "Any channel / Any band"
HKR,NDI\params\gOperatingChannel\enum, "00000001", 0, "Channel 1 only"
HKR,NDI\params\gOperatingChannel\enum, "00000002", 0, "Channel 2 only"
HKR,NDI\params\gOperatingChannel\enum, "00000003", 0, "Channel 3 only"
HKR,NDI\params\gOperatingChannel\enum, "00000004", 0, "Channel 4 only"
HKR,NDI\params\gOperatingChannel\enum, "00000005", 0, "Channel 5 only"
HKR,NDI\params\gOperatingChannel\enum, "00000006", 0, "Channel 6 only"
HKR,NDI\params\gOperatingChannel\enum, "00000007", 0, "Channel 7 only"
HKR,NDI\params\gOperatingChannel\enum, "00000008", 0, "Channel 8 only"
HKR,NDI\params\gOperatingChannel\enum, "00000009", 0, "Channel 9 only"
HKR,NDI\params\gOperatingChannel\enum, "0000000A", 0, "Channel 10 only"
HKR,NDI\params\gOperatingChannel\enum, "0000000B", 0, "Channel 11 only"
HKR,NDI\params\gOperatingChannel\enum, "0000000C", 0, "Channel 12 only"
HKR,NDI\params\gOperatingChannel\enum, "0000000D", 0, "Channel 13 only"
HKR,NDI\params\gOperatingChannel\enum, "0000000E", 0, "Channel 14 only"
HKR,NDI\params\gOperatingChannel\enum, "00000022", 0, "Channel 34 only"
HKR,NDI\params\gOperatingChannel\enum, "00000024", 0, "Channel 36 only"
HKR,NDI\params\gOperatingChannel\enum, "00000026", 0, "Channel 38 only"
HKR,NDI\params\gOperatingChannel\enum, "00000028", 0, "Channel 40 only"
HKR,NDI\params\gOperatingChannel\enum, "0000002A", 0, "Channel 42 only"
HKR,NDI\params\gOperatingChannel\enum, "0000002C", 0, "Channel 44 only"
HKR,NDI\params\gOperatingChannel\enum, "0000002E", 0, "Channel 46 only"
HKR,NDI\params\gOperatingChannel\enum, "00000030", 0, "Channel 48 only"
HKR,NDI\params\gOperatingChannel\enum, "00000034", 0, "Channel 52 only"
HKR,NDI\params\gOperatingChannel\enum, "00000038", 0, "Channel 56 only"
HKR,NDI\params\gOperatingChannel\enum, "0000003C", 0, "Channel 60 only"
HKR,NDI\params\gOperatingChannel\enum, "00000040", 0, "Channel 64 only"
HKR,NDI\params\gOperatingChannel\enum, "00000095", 0, "Channel 149 only"
HKR,NDI\params\gOperatingChannel\enum, "00000099", 0, "Channel 153 only"
HKR,NDI\params\gOperatingChannel\enum, "0000009D", 0, "Channel 157 only"
HKR,NDI\params\gOperatingChannel\enum, "000000A1", 0, "Channel 161 only"
HKR,NDI\params\gOperatingChannel\enum, "80000001", 0, "Band 11A only"
HKR,NDI\params\gOperatingChannel\enum, "80000002", 0, "Band 11B only"
HKR,NDI\params\gOperatingChannel\enum, "80000003", 0, "Band 11A or 11B"
HKR,NDI\params\gOperatingChannel\enum, "80000004", 0, "Band 11G only"
HKR,NDI\params\gOperatingChannel\enum, "80000005", 0, "Band 11A or 11G"
HKR,NDI\params\gOperatingChannel\enum, "80000006", 0, "Band 11B or 11G"
HKR,,gMediumAccess,,"0"
HKR,NDI\params\gMediumAccess, ParamDesc, 0, "Medium Access (QoS)"
HKR,NDI\params\gMediumAccess, type, 0, "enum"
HKR,NDI\params\gMediumAccess, default, 0, "0"
HKR,NDI\params\gMediumAccess\enum, "0", 0, "Automatic"
HKR,NDI\params\gMediumAccess\enum, "1", 0, "DCF"
HKR,NDI\params\gMediumAccess\enum, "2", 0, "eDCF"
HKR,NDI\params\gMediumAccess\enum, "3", 0, "HCF"
HKR,,gCfg1Id,,"0"
HKR,NDI\params\gCfg1Id, ParamDesc, 0, "Generic Cfg 1 Id (decimal; 0 == N/A)"
HKR,NDI\params\gCfg1Id, type, 0, "dword"
HKR,NDI\params\gCfg1Id, default, 0, "0"
HKR,,gCfg1Value,,"0"
HKR,NDI\params\gCfg1Value, ParamDesc, 0, "Generic Cfg 1 Value (decimal)"
HKR,NDI\params\gCfg1Value, type, 0, "dword"
HKR,NDI\params\gCfg1Value, default, 0, "0"
HKR,,gCfg2Id,,"0"
HKR,NDI\params\gCfg2Id, ParamDesc, 0, "Generic Cfg 2 Id (decimal; 0 == N/A)"
HKR,NDI\params\gCfg2Id, type, 0, "dword"
HKR,NDI\params\gCfg2Id, default, 0, "0"
HKR,,gCfg2Value,,"0"
HKR,NDI\params\gCfg2Value, ParamDesc, 0, "Generic Cfg 2 Value (decimal)"
HKR,NDI\params\gCfg2Value, type, 0, "dword"
HKR,NDI\params\gCfg2Value, default, 0, "0"
HKR,,gCfg3Id,,"0"
HKR,NDI\params\gCfg3Id, ParamDesc, 0, "Generic Cfg 3 Id (decimal; 0 == N/A)"
HKR,NDI\params\gCfg3Id, type, 0, "dword"
HKR,NDI\params\gCfg3Id, default, 0, "0"
HKR,,gCfg3Value,,"0"
HKR,NDI\params\gCfg3Value, ParamDesc, 0, "Generic Cfg 3 Value (decimal)"
HKR,NDI\params\gCfg3Value, type, 0, "dword"
HKR,NDI\params\gCfg3Value, default, 0, "0"
HKR,,gCfg4Id,,"0"
HKR,NDI\params\gCfg4Id, ParamDesc, 0, "Generic Cfg 4 Id (decimal; 0 == N/A)"
HKR,NDI\params\gCfg4Id, type, 0, "dword"
HKR,NDI\params\gCfg4Id, default, 0, "0"
HKR,,gCfg4Value,,"0"
HKR,NDI\params\gCfg4Value, ParamDesc, 0, "Generic Cfg 4 Value (decimal)"
HKR,NDI\params\gCfg4Value, type, 0, "dword"
HKR,NDI\params\gCfg4Value, default, 0, "0"
HKR,,gCfg5Id,,"0"
HKR,NDI\params\gCfg5Id, ParamDesc, 0, "Generic Cfg 5 Id (decimal; 0 == N/A)"
HKR,NDI\params\gCfg5Id, type, 0, "dword"
HKR,NDI\params\gCfg5Id, default, 0, "0"
HKR,,gCfg5Value,,"0"
HKR,NDI\params\gCfg5Value, ParamDesc, 0, "Generic Cfg 5 Value (decimal)"
HKR,NDI\params\gCfg5Value, type, 0, "dword"
HKR,NDI\params\gCfg5Value, default, 0, "0"
HKR,,gShortSlotTimeEnabled,,"1"
HKR,NDI\params\gShortSlotTimeEnabled, ParamDesc, 0, ".11g Short Slot Time"
HKR,NDI\params\gShortSlotTimeEnabled, type, 0, "dword"
HKR,NDI\params\gShortSlotTimeEnabled, default, 0, "1"
HKR,NDI\params\gShortSlotTimeEnabled, min, 0, "0"
HKR,NDI\params\gShortSlotTimeEnabled, max, 0, "1"
HKR,NDI\params\gShortSlotTimeEnabled, step, 0, "1"
HKR,,g11dSupportEnabled,,"0"
HKR,NDI\params\g11dSupportEnabled, ParamDesc, 0, ".11d Support"
HKR,NDI\params\g11dSupportEnabled, type, 0, "dword"
HKR,NDI\params\g11dSupportEnabled, default, 0, "0"
HKR,NDI\params\g11dSupportEnabled, min, 0, "0"
HKR,NDI\params\g11dSupportEnabled, max, 0, "1"
HKR,NDI\params\g11dSupportEnabled, step, 0, "1"
HKR,,gHeartbeat24,,"10"
HKR,NDI\params\gHeartbeat24, ParamDesc, 0, "Heartbeat Thresh (2.4)"
HKR,NDI\params\gHeartbeat24, type, 0, "dword"
HKR,NDI\params\gHeartbeat24, default, 0, "10"
HKR,NDI\params\gHeartbeat24, min, 0, "1"
HKR,NDI\params\gHeartbeat24, max, 0, "50"
HKR,NDI\params\gHeartbeat24, step, 0, "1"
HKR,,gHeartbeat50,,"6"
HKR,NDI\params\gHeartbeat50, ParamDesc, 0, "Heartbeat Thresh (5.0)"
HKR,NDI\params\gHeartbeat50, type, 0, "dword"
HKR,NDI\params\gHeartbeat50, default, 0, "6"
HKR,NDI\params\gHeartbeat50, min, 0, "1"
HKR,NDI\params\gHeartbeat50, max, 0, "50"
HKR,NDI\params\gHeartbeat50, step, 0, "1"
HKR,,gAgingTimerInBKScanUnits,,"3"
HKR,NDI\params\gAgingTimerInBKScanUnits, ParamDesc, 0, "Scan Results Age"
HKR,NDI\params\gAgingTimerInBKScanUnits, type, 0, "dword"
HKR,NDI\params\gAgingTimerInBKScanUnits, default, 0, "3"
HKR,NDI\params\gAgingTimerInBKScanUnits, min, 0, "2"
HKR,NDI\params\gAgingTimerInBKScanUnits, max, 0, "10"
HKR,NDI\params\gAgingTimerInBKScanUnits, step, 0, "1"
[StaticParms]
HKR, ,HardwareID, ,"WNI0000"
HKR,,RoamingFeatures,,"0"
HKR,,RoamingSignalDegradedThresh,,"10"
HKR,,RoamingSignalDegradedBeaconsPerPeriod,,"10"
HKR,,RoamingSignalDegradedPeriods,,"10"
[Strings]
Airgo="Belkin"
AirgoNet="Belkin Corporation"
Disk_1="Belkin WLAN Installation Disk #1"
Airgo.Service.DispName="Belkin Wireless Pre-N Notebook Network Driver"
Belkin.DeviceDesc="Belkin Wireless Pre-N Notebook Network Card"

