
[Version]
DriverVer=09/19/2003, 1.09.01.0000
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
[ControlFlags]
ExcludeFromSelect=PCI\VEN_1814&DEV_0101&SUBSYS_00081371
ExcludeFromSelect=PCI\VEN_1814&DEV_0101&SUBSYS_000A1371
ExcludeFromSelect=PCI\VEN_1814&DEV_0101&SUBSYS_00101371
[Manufacturer]
%V_Provider%=Adapters
[Adapters]
%RT2400.DeviceDesc% =RT2400.ndi, PCI\VEN_1814&DEV_0101&SUBSYS_00081371
%RT2400PCI.DeviceDesc% =RT2400PCI.ndi, PCI\VEN_1814&DEV_0101&SUBSYS_00101371
%RT2400MINIPCI.DeviceDesc% =RT2400MINIPCI.ndi, PCI\VEN_1814&DEV_0101&SUBSYS_000A1371
[RT2400.ndi]
AddReg=Common.reg, RT2400.ndi.reg
;CpyFiles=win9x.CopyFiles
[RT2400.ndi.NT]
AddReg=Common.reg, RT2400.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
[RT2400.ndi.NT.Services]
AddService=RT2400, 2, RT2400.Service, common.EventLog
[RT2400.ndi.reg]
HKR, , NTMPDriver, 0, RT2400.sys
HKR, Ndi, DeviceID, 0, "PCI\VEN_1814&DEV_0101&SUBSYS_00081371"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, RT2400.sys
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, 0, "RT2400"
HKR, NDIS, MajorNdisVersion,1, 03
HKR, NDIS, MinorNdisVersion,1, 0A
HKR, , BusType, 0, 5
HKR, NDI, CardType, 0, "PCI"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[win9x.CopyFiles]
RT2400.sys ; Win9x Installation
[RT2400MINIPCI.ndi]
AddReg=Common.reg, RT2400MINIPCI.ndi.reg
;CpyFiles=win9x.CopyFiles
[RT2400MINIPCI.ndi.NT]
AddReg=Common.reg, RT2400MINIPCI.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
[RT2400MINIPCI.ndi.NT.Services]
AddService=RT2400MINIPCI, 2, RT2400MINIPCI.Service, common.EventLog
[RT2400MINIPCI.ndi.reg]
HKR, , NTMPDriver, 0, RT2400.sys
HKR, Ndi, DeviceID, 0, "PCI\VEN_1814&DEV_0101&SUBSYS_000A1371"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, RT2400.sys
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, 0, "RT2400"
HKR, NDIS, MajorNdisVersion,1, 03
HKR, NDIS, MinorNdisVersion,1, 0A
HKR, , BusType, 0, 5
HKR, NDI, CardType, 0, "PCI"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[win9x.CopyFiles]
RT2400.sys ; Win9x Installation
[RT2400PCI.ndi]
AddReg=Common.reg, RT2400PCI.ndi.reg
;CpyFiles=win9x.CopyFiles
[RT2400PCI.ndi.NT]
AddReg=Common.reg, RT2400PCI.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
[RT2400PCI.ndi.NT.Services]
AddService=RT2400PCI, 2, RT2400PCI.Service, common.EventLog
[RT2400PCI.ndi.reg]
HKR, , NTMPDriver, 0, RT2400.sys
HKR, Ndi, DeviceID, 0, "PCI\VEN_1814&DEV_0101&SUBSYS_00101371"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, RT2400.sys
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, 0, "RT2400"
HKR, NDIS, MajorNdisVersion,1, 03
HKR, NDIS, MinorNdisVersion,1, 0A
HKR, , BusType, 0, 5
HKR, NDI, CardType, 0, "PCI"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[win9x.CopyFiles]
RT2400.sys ; Win9x Installation
[Common.reg]
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, Default, SSID, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, ParamDesc, 0, "SSID"
HKR, NDI\params\SSID, type, 0, "edit"
HKR, NDI\params\SSID, limitText, 0, "32"
HKR, NDI\params\SSID, default, 0, %SSID_DEF_STR%
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, Default, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0, 0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, NDI\params\Channel, ParamDesc, 0, "Channel"
HKR, NDI\params\Channel, type, 0, "enum"
HKR, NDI\params\Channel, default, 0, %CHANNEL%
HKR, NDI\params\Channel\enum, 1, 0, "01"
HKR, NDI\params\Channel\enum, 2, 0, "02"
HKR, NDI\params\Channel\enum, 3, 0, "03"
HKR, NDI\params\Channel\enum, 4, 0, "04"
HKR, NDI\params\Channel\enum, 5, 0, "05"
HKR, NDI\params\Channel\enum, 6, 0, "06"
HKR, NDI\params\Channel\enum, 7, 0, "07"
HKR, NDI\params\Channel\enum, 8, 0, "08"
HKR, NDI\params\Channel\enum, 9, 0, "09"
HKR, NDI\params\Channel\enum, 10, 0, "10"
HKR, NDI\params\Channel\enum, 11, 0, "11"
HKR, , NetworkAddress, 0, ""
HKR, Default, NetworkAddress, 0, ""
HKR, NDI\params\NetworkAddress, ParamDesc, 0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, limitText, 0, "12"
HKR, NDI\params\NetworkAddress, default, 0, ""
HKR, , FirstRun, 0, "0"
HKR, , ConfigSelect, 0, "0" ;0=RaConfig, 1=ZeroConfig
HKR, , CountryRegion, 0, "0"
HKR, NDI\params\CountryRegion, ParamDesc, 0, "Country Region"
HKR, NDI\params\CountryRegion, type, 0, "enum"
HKR, NDI\params\CountryRegion, default, 0, "0"
HKR, NDI\params\CountryRegion\enum, 0, 0, "USA (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum, 1, 0, "CANADA(Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum, 2, 0, "EUROPE(Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum, 3, 0, "SPAIN (Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum, 4, 0, "FRANCE(Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum, 5, 0, "JAPAN (Channel 14)"
HKR, NDI\params\CountryRegion\enum, 6, 0, "JAPAN (Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum, 7, 0, "ISRAEL(Channel 3 - 9)"
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Saving Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum, 1, 0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum, 2, 0, "Fast_PSP (Power Save Mode)"
HKR, , ACPowerCam, 0, "0"
HKR, Default, ACPowerCam, 0, "0"
HKR, NDI\params\ACPowerCam, ParamDesc, 0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam, type, 0, "enum"
HKR, NDI\params\ACPowerCam, default, 0, "0"
HKR, NDI\params\ACPowerCam\enum, 0, 0, "Disable"
HKR, NDI\params\ACPowerCam\enum, 1, 0, "Enable"
HKR, , AntennaTx, 0, "0"
HKR, Default, AntennaTx, 0, "0"
HKR, NDI\params\AntennaTx, ParamDesc, 0, "Antenna Tx Diversity"
HKR, NDI\params\AntennaTx, type, 0, "enum"
HKR, NDI\params\AntennaTx, default, 0, "0"
HKR, NDI\params\AntennaTx\enum, 0, 0, "Diversity"
HKR, NDI\params\AntennaTx\enum, 1, 0, "Antenna A Only"
HKR, NDI\params\AntennaTx\enum, 2, 0, "Antenna B Only"
HKR, , AntennaRx, 0, "0"
HKR, Default, AntennaRx, 0, "0"
HKR, NDI\params\AntennaRx, ParamDesc, 0, "Antenna Rx Diversity"
HKR, NDI\params\AntennaRx, type, 0, "enum"
HKR, NDI\params\AntennaRx, default, 0, "0"
HKR, NDI\params\AntennaRx\enum, 0, 0, "Diversity"
HKR, NDI\params\AntennaRx\enum, 1, 0, "Antenna A Only"
HKR, NDI\params\AntennaRx\enum, 2, 0, "Antenna B Only"
HKR, , TransRate, 0, "0"
HKR, Default, TransRate, 0, "0"
HKR, NDI\params\TransRate, ParamDesc, 0, "Transmit Rate"
HKR, NDI\params\TransRate, type, 0, "enum"
HKR, NDI\params\TransRate, default, 0, "0"
HKR, NDI\params\TransRate\enum, 0, 0, "Auto"
HKR, NDI\params\TransRate\enum, 1, 0, "11 Mb/s"
HKR, NDI\params\TransRate\enum, 2, 0, "5.5 Mb/s"
HKR, NDI\params\TransRate\enum, 3, 0, "2 Mb/s"
HKR, NDI\params\TransRate\enum, 4, 0, "1 Mb/s"
HKR, , PreambleType, 0, "2"
HKR, Default, PreambleType, 0, "2"
HKR, NDI\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, NDI\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType, default, 0, "2"
HKR, NDI\params\PreambleType\enum,0, 0, "Long"
HKR, NDI\params\PreambleType\enum,1, 0, "Short"
HKR, NDI\params\PreambleType\enum,2, 0, "Auto"
HKR, NDI\params\PreambleType, optional, 0, "0"
HKR, , RTSThresh, 0, "2347"
HKR, Default, RTSThresh, 0, "2347"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2347"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2347"
HKR, NDI\params\RTSThresh, step, 0, "32"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2346"
HKR, Default, FragThresh, 0, "2346"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragment Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2346"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2346"
HKR, NDI\params\FragThresh, step, 0, "32"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , Radio, 0, "0"
HKR, NDI\params\Radio, ParamDesc, 0, "Radio Status"
HKR, NDI\params\Radio, type, 0, "enum"
HKR, NDI\params\Radio, default, 0, "0"
HKR, NDI\params\Radio\enum, 1, 0, "Disable"
HKR, NDI\params\Radio\enum, 0, 0, "Enable"
HKR, , AuthenType, 0, "0"
HKR, Default, AuthenType, 0, "0"
HKR, NDI\params\AuthenType, ParamDesc, 0, "Authentication Type"
HKR, NDI\params\AuthenType, type, 0, "enum"
HKR, NDI\params\AuthenType, default, 0, "0"
HKR, NDI\params\AuthenType\enum, 0, 0, "Open System"
HKR, NDI\params\AuthenType\enum, 1, 0, "Shared Key"
HKR, , Encryption, 0, "0"
HKR, Default, Encryption, 0, "0"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
win9x.CopyFiles=11 ; system32 subdirectory on win9x
[NT.CopyFiles]
RT2400.sys ; NT Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
Rt2400.sys=1
[RT2400.ndi.NT.reg]
HKR, Ndi, Service, 0, "RT2400"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[RT2400.Service]
DisplayName=%RT2400.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\RT2400.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT2400.sys"
HKR, , TypesSupported, 0x00010001, 7
[RT2400PCI.ndi.NT.reg]
HKR, Ndi, Service, 0, "RT2400"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[RT2400PCI.Service]
DisplayName=%RT2400PCI.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\RT2400.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT2400.sys"
HKR, , TypesSupported, 0x00010001, 7
[RT2400MINIPCI.ndi.NT.reg]
HKR, Ndi, Service, 0, "RT2400"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[RT2400MINIPCI.Service]
DisplayName=%RT2400MINIPCI.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\RT2400.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT2400.sys"
HKR, , TypesSupported, 0x00010001, 7
[strings]
Provider= "OEM"
V_Provider= "802.11b Technology Corp."
RT2400.DeviceDesc= "802.11b WLAN CardBus"
RT2400.Service.DispName= "802.11b WLAN CardBus"
RT2400PCI.DeviceDesc= "802.11b WLAN PCI"
RT2400PCI.Service.DispName= "802.11b WLAN PCI"
RT2400MINIPCI.DeviceDesc= "802.11b WLAN Mini-PCI"
RT2400MINIPCI.Service.DispName= "802.11b WLAN Mini-PCI"
INSTALL_DISK_STR= "802.11b WLAN Installation Disk"
SSID_DEF_STR=""
NETWORK_TYPE_DEF_STR="1"
CHANNEL="1"
