
[version]
Signature="$Chicago$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%V_INPROCOMM%
Compatible=1
MillenniumPreferred=.ME
CatalogFile=WLIPNDS.cat
DriverVer=01/05/2004,1.22.01.2004
[Manufacturer]
%V_INPROCOMM%=Linksys
[ControlFlags]
ExcludeFromSelect=PCI\VEN_17FE&DEV_2220&SUBSYS_00291737
[Linksys]
%IPN2220.DeviceDesc%=IPN2220.ndi, PCI\VEN_17FE&DEV_2220&SUBSYS_00291737
[IPN2220.ndi.NT]
Characteristics=0x84
BusType=5
AddReg=IPN2220.common.reg, IPN2220WinNT.reg
DelReg=IPN2220.common.DelReg
;CpyFiles=IPN2220WinNT.CopyFiles
[IPN2220.ndi.NT.Services]
AddService=IPN2220, 2, IPN2220WinNT.Service, common.EventLog
[IPN2220.ndi.ME]
Characteristics=0x84
BusType=5
AddReg=IPN2220.common.reg, IPN2220WinME.reg
DelReg=IPN2220.common.DelReg
;CpyFiles=IPN2220WinME.CopyFiles
[IPN2220.ndi.ME.Services]
AddService=IPN2220, 2, IPN2220WinME.Service, common.EventLog
[IPN2220.ndi]
DriverVer=01/05/2004,1.22.01.2004
AddReg=IPN2220Win9X.id.reg, IPN2220.common.reg, IPN2220Win9X.flags.reg, IPN2220Win9X.win.reg
DelReg=IPN2220.common.DelReg
;CpyFiles=IPN2220Win9X.CopyFiles
[IPN2220.common.reg]
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress, Type, 0, "edit"
HKR, Ndi\params\NetworkAddress, Default, 0, ""
HKR, Ndi\params\NetworkAddress, Optional, 0, "1"
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate%
HKR, Ndi\params\Rate, Type, 0, "enum"
HKR, Ndi\params\Rate, Default, 0, "65295"
HKR, Ndi\params\Rate\enum, "1", 0, %Rate1M%
HKR, Ndi\params\Rate\enum, "2", 0, %Rate2M%
HKR, Ndi\params\Rate\enum, "4", 0, %Rate5_5M%
HKR, Ndi\params\Rate\enum, "8", 0, %Rate11M%
HKR, Ndi\params\Rate\enum, "256", 0, %Rate6M%
HKR, Ndi\params\Rate\enum, "512", 0, %Rate9M%
HKR, Ndi\params\Rate\enum, "1024", 0, %Rate12M%
HKR, Ndi\params\Rate\enum, "2048", 0, %Rate18M%
HKR, Ndi\params\Rate\enum, "4096", 0, %Rate24M%
HKR, Ndi\params\Rate\enum, "8192", 0, %Rate36M%
HKR, Ndi\params\Rate\enum, "16384", 0, %Rate48M%
HKR, Ndi\params\Rate\enum, "32768", 0, %Rate54M%
HKR, Ndi\params\Rate\enum, "65295", 0, %RateAutomatic%
HKR, Ndi\params\Rate\enum, "15", 0, %RateAutomatic2%
HKR, Ndi\params\Ssid, ParamDesc, 0, %SSID%
HKR, Ndi\params\Ssid, Type, 0, "edit"
HKR, Ndi\params\Ssid, Default, 0, ""
HKR, Ndi\params\Ssid, Optional, 0, "1"
HKR, Ndi\params\Ssid, LimitText, 0, "32"
HKR, Ndi\params\BssType, ParamDesc, 0, %BSSType%
HKR, Ndi\params\BssType, Type, 0, "enum"
HKR, Ndi\params\BssType, Default, 0, "1"
HKR, Ndi\params\BssType\enum, "1", 0, %ESS%
HKR, Ndi\params\BssType\enum, "2", 0, %IBSS%
HKR, Ndi\params\AdHocMode, ParamDesc, 0, %AdHocMode%
HKR, Ndi\params\AdHocMode, Type, 0, "enum"
HKR, Ndi\params\AdHocMode, Default, 0, "0"
HKR, Ndi\params\AdHocMode\enum, "0", 0, %WiFiMode%
HKR, Ndi\params\AdHocMode\enum, "1", 0, %IEEEMode%
HKR, Ndi\params\Channel, ParamDesc, 0, %Channel%
HKR, Ndi\params\Channel, Type, 0, "int"
HKR, Ndi\params\Channel, Default, 0, "1"
HKR, Ndi\params\Channel, Min, 0, "1"
HKR, Ndi\params\Channel, Max, 0, "14"
HKR, Ndi\params\Channel, Step, 0, "1"
HKR, Ndi\params\Channel, Base, 0, "10"
HKR, Ndi\params\BasicRateSet, ParamDesc, 0, %BasicRateSet%
HKR, Ndi\params\BasicRateSet, Type, 0, "enum"
HKR, Ndi\params\BasicRateSet, Default, 0, "15"
HKR, Ndi\params\BasicRateSet\enum, "15", 0, %BasicRateSet1%
HKR, Ndi\params\BasicRateSet\enum, "5391", 0, %BasicRateSet2%
HKR, Ndi\params\BasicRateSet\enum, "3", 0, %BasicRateSet3%
HKR, Ndi\params\BasicRateSet\enum, "65295", 0, %BasicRateSet5%
HKR, Ndi\params\RtsThreshold, ParamDesc, 0, %RTSThreshold%
HKR, Ndi\params\RtsThreshold, Type, 0, "int"
HKR, Ndi\params\RtsThreshold, Default, 0, "2347"
HKR, Ndi\params\RtsThreshold, Min, 0, "0"
HKR, Ndi\params\RtsThreshold, Max, 0, "00002347"
HKR, Ndi\params\RtsThreshold, Step, 0, "1"
HKR, Ndi\params\RtsThreshold, Base, 0, "10"
HKR, Ndi\params\FragThreshold, ParamDesc, 0, %FragmentationThreshold%
HKR, Ndi\params\FragThreshold, Type, 0, "int"
HKR, Ndi\params\FragThreshold, Default, 0, "2346"
HKR, Ndi\params\FragThreshold, Min, 0, "256"
HKR, Ndi\params\FragThreshold, Max, 0, "00002346"
HKR, Ndi\params\FragThreshold, Step, 0, "1"
HKR, Ndi\params\FragThreshold, Base, 0, "10"
[IPN2220.common.DelReg]
HKR,,NumRfb
HKR, Ndi\params\NumRfb
HKR,,NumTfcb
HKR, Ndi\params\NumTfcb
HKR, Ndi\params\BssType\enum, 130
HKR, Ndi\params\BasicRateSet\enum, 5376
HKR,,ScanType
HKR, Ndi\params\ScanType
HKR, Ndi\params\AuthMode
[IPN2220WinNT.reg]
HKR, Ndi, Service, 0, "IPN2220"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[IPN2220WinME.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "i2220.sys"
HKR, Ndi, CardType, 0, "PCI"
HKR, Ndi, Service, 0, "IPN2220"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "IPN2220"
HKR, NDIS, MajorNdisVersion, 1, 05
HKR, NDIS, MinorNdisVersion, 1, 00
[IPN2220Win9X.id.reg]
HKR, Ndi, CardType, 0, "PCI"
HKR, Ndi, DeviceID, 0, "PCI\VEN_17FE&DEV_2220&SUBSYS_00291737"
[IPN2220Win9X.flags.reg]
HKR, Ndi\params\Channel, flag, 1, 20,00,00,00
HKR, Ndi\params\RtsThreshold, flag, 1, 20,00,00,00
HKR, Ndi\params\FragThreshold, flag, 1, 20,00,00,00
[IPN2220Win9X.win.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "i2220.sys"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "IPN2220"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, Ndi\Install, ndis3, 0, "IPN2220.Install"
[IPN2220WinNT.Service]
DisplayName=%IPN2220.Service.DispName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\i2220ntx.sys
LoadOrderGroup=NDIS
[IPN2220WinME.Service]
DisplayName=%IPN2220.Service.DispName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\i2220.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[IPN2220WinNT.CopyFiles]
i2220ntx.sys,,,2
[IPN2220WinME.CopyFiles]
i2220.sys,,,2
[IPN2220Win9X.CopyFiles]
i2220.sys,,,2
[SourceDisksNames]
1=%IPN2220.SourceDiskName%,,,
[SourceDisksFiles]
i2220.sys=1,,
i2220ntx.sys=1,,
[DestinationDirs]
IPN2220WinNT.CopyFiles=12
IPN2220WinME.CopyFiles=11
IPN2220Win9X.CopyFiles=11
DefaultDestDir=11
[Strings]
V_INPROCOMM="Cisco-Linksys, LLC."
NetworkAddress="Network Address"
DeviceType="Device Type"
DeviceSTA="Wireless Station"
DeviceAP="Access Point (AP)"
Rate="Transmission Rate"
Rate1M="1 Mbps"
Rate2M="2 Mbps"
Rate5_5M="5.5 Mbps"
Rate11M="11 Mbps"
Rate6M="6 Mbps"
Rate9M="9 Mbps"
Rate12M="12 Mbps"
Rate18M="18 Mbps"
Rate24M="24 Mbps"
Rate36M="36 Mbps"
Rate48M="48 Mbps"
Rate54M="54 Mbps"
RateAutomatic="Automatic (All)"
RateAutomatic2="Automatic (1/2/5.5/11)"
SSID="SSID"
BSSType="Network Type"
ESS="Infrastructure"
IBSS="Ad Hoc (IBSS)"
AdHocMode="Ad Hoc Operational Mode"
WiFiMode="Wi-Fi 802.11g Mode"
IEEEMode="IEEE 802.11g Mode"
Channel="Channel to Start Ad Hoc/AP"
BasicRateSet="Basic Rates to Start Ad Hoc/AP"
BasicRateSet1="1/2/5.5/11 Mbps"
BasicRateSet2="1/2/5.5/11/6/12/24 Mbps"
BasicRateSet3="1/2 Mbps"
BasicRateSet5="All"
RTSThreshold="RTS Threshold"
FragmentationThreshold="Fragmentation Threshold"
PowerMode="Power Mode"
PowerModeCAM="Continuous Access Mode (CAM)"
PowerModeMAX_PSP="Maximum (MAX) Power-Saving Mode"
PowerModeFast_PSP="Fast Power-Saving Mode"
IPN2220.DeviceDesc="Wireless-G Notebook Adapter ver.4.0"
IPN2220.Service.DispName="Wireless-G Notebook Adapter ver.4.0 Driver"
IPN2220.SourceDiskName="Wireless-G Notebook Adapter ver.4.0 Driver Disk"

