
[Version]
DriverVer=12/01/2004, 3.3.13.1
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=SMC2862W.cat
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList,NTx86.5.1
[DeviceList]
%A021_DESC_STR%=PRISM_A021, USB\VID_0707&PID_EE13
[DeviceList.NTx86.5.1]
%A021_DESC_STR%=PRISM_A021_XP, USB\VID_0707&PID_EE13
[PRISM_A021] ; Win9x
AddReg=PRISM_A021.reg, PRISM_DCB1.reg1, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_CCU.copy
[PRISM_A021.NT] ; Win2k
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_CCU.copy
BusType=15
Characteristics= 0x84
[PRISM_A021.NT.Services]
AddService= "SMC2862W", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog
[PRISM_A021.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_A021_XP] ; Winxp
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.XP, PRISM_CCU.copy
BusType=15
Characteristics= 0x84
[PRISM_A021_XP.Services]
AddService= "SMC2862W", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog
[PRISM_A021_XP.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_DCB1.reg1]
[PRISM_A021.reg]
HKR,Ndi,DeviceID,0,"USB\VID_0707&PID_EE13"
HKR,,PlatformID,0,14480
HKR,,UsbVariant,0,14471
HKR,,VendorDesc,0,%A021_DESC_STR%
HKR,,CountryName,0,"US "
HKR,,11dMode,0,0
HKR,,EnableRadio,0,1
HKR,,CCUEnable,0,1
[PRISM_COINSTALL.reg.NT]
[PRISM_DRIVER_A02.Service]
DisplayName=%A02_SERVICE_STR%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\2862WICB.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_A02.reg]
HKR,NDI ,Service ,0 ,"SMC2862W"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"2862WICB.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"2862WICB"
HKR,NDIS ,MajorNdisVersion ,1 ,04
HKR,NDIS ,MinorNdisVersion ,1 ,00
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis5"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"2862WICB"
HKR,NDIS ,MajorNdisVersion ,1 ,04
HKR,NDIS ,MinorNdisVersion ,1 ,00
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,SSID ,0 ,"ANY"
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR, ,NitroMode ,0 ,"1"
HKR, ,NitroTime ,0 ,"650"
HKR,Ndi\params\RTSThresh,default,0,"2347"
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,"int"
HKR,NDI\params\RTSThresh,flag,1,"20","00","00","00"
HKR,NDI\params\RTSThresh,min,0,"256"
HKR,NDI\params\RTSThresh,max,0,"2347"
HKR,NDI\params\RTSThresh,step,0,"1"
HKR,Ndi\params\FragThresh,default,0,"2346"
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,"int"
HKR,NDI\params\FragThresh,flag,1,"20","00","00","00"
HKR,NDI\params\FragThresh,min,0,"256"
HKR,NDI\params\FragThresh,max,0,"2346"
HKR,NDI\params\FragThresh,step,0,"2"
HKR,NDI\params\ShortRetryLimit,default,0,"7"
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,"int"
HKR,NDI\params\ShortRetryLimit,min,0,"1"
HKR,NDI\params\ShortRetryLimit,max,0,"255"
HKR,NDI\params\ShortRetryLimit,step,0,"1"
HKR,NDI\params\LongRetryLimit,default,0,"4"
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,"int"
HKR,NDI\params\LongRetryLimit,min,0,"1"
HKR,NDI\params\LongRetryLimit,max,0,"255"
HKR,NDI\params\LongRetryLimit,step,0,"1"
HKR,NDI\params\ConfigProfile,default,0,"1"
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,,"enum"
HKR,NDI\params\ConfigProfile,flag,1,"20","00","00","00"
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
HKR,Ndi\params\PSMode,default,0,"1"
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,"enum"
HKR,NDI\params\PSMode,flag,1,"20","00","00","00"
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.ME=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
PRISM_DRIVER.copy.XP=12 ; Win2k=%windir%\system32\drivers
PRISM_CCU.copy=11 ; Win9x=%windir%\system
[PRISM_CCU.copy]
[PRISM_DRIVER.copy]
2862WICB.sys
[PRISM_DRIVER.copy.ME]
2862WICB.sys
[PRISM_DRIVER.copy.NT]
2862WICB.sys
[PRISM_DRIVER.copy.XP]
2862WICB.sys,2862WC51.sys,,
[PRISM_COINSTALL.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
2862WICB.sys=1
[SourceDisksFiles.ME] ; WinMe
2862WICB.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
2862WICB.sys=1
2862WC51.sys=1
[Strings]
VER_VENDOR_STR="SMC"
VER_VENDOR_NAME_STR="SMC Networks, Inc."
INSTALL_DISK_STR="SMC2862W-G EZ Connect g 802.11g Wireless USB 2.0 Adapter Driver Install Disk"
A021_DESC_STR="SMC2862W-G EZ Connect g 802.11g Wireless USB 2.0 Adapter"
A02_SERVICE_STR="SMC2862W-G EZ Connect g 802.11g Wireless USB 2.0 Adapter Driver"
ON_STR="On"
OFF_STR="Off"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WiFi"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"
PPE_PDLP="Direct Link"
PPE_COMPRESS="Compression"
PPE_CONCAT="Concatenation"
PPE_PIGGYBACK="PiggyBack"

