
[Version]
DriverVer=Thu 03/14/2002, 1.32.0.0000
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=PCMCIA\SMC-SMC2632W-AF67
ExcludeFromSelect=PCMCIA\SMC-SMC2632W-1783
ExcludeFromSelect=PCI\VEN_1638&DEV_1100&SUBSYS_11001638
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_260210b8
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%PRISM_PCMCIA1_STR%=PRISM_PCMCIA1, PCMCIA\SMC-SMC2632W-AF67
%PRISM_PCMCIA2_STR%=PRISM_PCMCIA2, PCMCIA\SMC-SMC2632W-1783
%PRISM_PCI1_STR%=PRISM_PCI1, PCI\VEN_1638&DEV_1100&SUBSYS_11001638
%PRISM_PCI2_STR%=PRISM_PCI2, PCI\VEN_1260&DEV_3873&SUBSYS_260210b8
[PRISM_PCMCIA1] ; Win9x
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCMCIA1.ME] ; WinMe
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA1.NT] ; Win2k
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA1.NT.Services]
AddService="SMC", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA1.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\SMC-SMC2632W-AF67"
[PRISM_PCMCIA2] ; Win9x
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCMCIA2.ME] ; WinMe
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA2.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA2.NT] ; Win2k
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA2.NT.Services]
AddService="SMC", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA2.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA2.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\SMC-SMC2632W-1783"
[PRISM_PCI1] ; Win9x
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCI1.ME] ; WinMe
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI1.NT] ; Win2k
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI1.NT.Services]
AddService="SMC", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCI1.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1638&DEV_1100&SUBSYS_11001638"
[PRISM_PCI2] ; Win9x
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCI2.ME] ; WinMe
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI2.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI2.NT] ; Win2k
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI2.NT.Services]
AddService="SMC", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI2.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCI2.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_260210b8"
[PRISM_COINSTALL.reg.NT]
[PRISM_DRIVER.Service]
DisplayName=%PRISM_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\SMCNDS.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_PCMCIA.reg]
HKR,NDI ,Service ,0 ,"SMC"
HKR,NDI ,CardType ,0 ,"PCMCIA"
HKR, ,BusType ,0 ,"8"
HKR, ,DeviceVxDs ,0 ,"SMCNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_PCI.reg]
HKR,NDI ,Service ,0 ,"SMC"
HKR,NDI ,CardType ,0 ,"PCI"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"SMCNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"SMCCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"SMC"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"SMCCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"SMC"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON.reg]
HKR, ,SMCIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,3
HKR,NDI\params\ListenInterval,,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,1
HKR,defaults,RTSThresh,0,2432
HKR,NDI\params\RTSThresh,,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,NDI\params\RTSThresh,optional,0,1
HKR,defaults,FragThresh,0,2432
HKR,NDI\params\FragThresh,,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,NDI\params\FragThresh,optional,0,1
HKR,defaults,PreambleMode,0,1
HKR,NDI\params\PreambleMode,,0,1
HKR,Ndi\params\PreambleMode,default,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,1
HKR,defaults,AuthentAlg,0,65535
HKR,NDI\params\AuthentAlg,,0,65535
HKR,NDI\params\AuthentAlg,default,0,65535
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,1
HKR,defaults,AdhocDemoMode,0,0
HKR,NDI\params\AdhocDemoMode,,0,0
HKR,Ndi\params\AdhocDemoMode,default,0,0
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,enum
HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
HKR,NDI\params\AdhocDemoMode,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.ME=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_NDI.copy]
SMCR16.dll ; Win9x NDI
SMCCFG.dll ; Win9x NDI
[PRISM_NDI.copy.ME]
SMCR16.dll ; Win9x NDI
SMCCFG.dll ; Win9x NDI
[PRISM_COINSTALL.copy.NT]
[PRISM_DRIVER.copy]
SMCNDS.sys
SMCIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.ME]
SMCNDS.sys
SMCIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.NT]
SMCNDS.sys
[PRISM_APPLET.copy]
[PRISM_APPLET.copy.ME]
[PRISM_APPLET.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
SMCR16.dll=1,win9x
SMCCFG.dll=1,win9x
SMCIOC.vxd=1,win9x
SMCNDS.sys=1
[SourceDisksFiles.ME] ; WinMe
SMCR16.dll=1,win9x
SMCCFG.dll=1,win9x
SMCIOC.vxd=1,win9x
SMCNDS.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
SMCNDS.sys=1
[Strings]
VER_VENDOR_STR="SMC"
VER_VENDOR_NAME_STR="SMC Networks, Inc"
PRISM_PCMCIA1_STR="SMC SMC2632W EZ Connect Wireless PC Card_5V"
PRISM_PCMCIA2_STR="SMC SMC2632W EZ Connect Wireless PC Card"
PRISM_PCI1_STR="SMC SMC2602W EZ Connect Wireless PCI Adapter"
PRISM_PCI2_STR="SMC SMC2602W V.2 EZ Connect Wireless MiniPCI Adapter"
PRISM_SERVICE_DISPLAY="SMC EZ Connect Wireless LAN Driver"
INSTALL_DISK_STR="SMC EZ Connect Wireless LAN Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"

