[Version]
Signature= "$Chicago$"
Compatible= 1
Class= Net
ClassGUID= {4d36e972-e325-11ce-bfc1-08002be10318}
MillenniumPreferred= .ME
Provider= %VENDOR%
DriverVer= 06/10/2003, 4.3.3.64
[Manufacturer]
%VENDOR%= VENDOR, NT.5.1
[ControlFlags]
ExcludeFromSelect=OEM-11Mbps_Wireless_LAN_PC_Card_V-5-EC99
[VENDOR]
%PCMCIAOEM5V.DeviceDesc%=DrvInst.Ndi, PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-5-EC99
[VENDOR.NT.5.1]
%PCMCIAOEM5V.DeviceDesc%=DrvInstXP.Ndi, PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-5-EC99
[DrvInst.Ndi]
AddReg=Win9x.Reg, Win9x2k.Params
;CpyFiles=CopyFile.Sys
DriverVer=06/10/2003, 4.3.3.64
[Win9x.Reg]
HKR,Ndi,DeviceID,0,"PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-5-EC99"
HKR,Ndi,CardType,,"PNP"
HKR,,BusType,0,"8"
HKR,,EnableIRQSharing,1,01,00,00,00
HKR,,IOBaseAddress,1,02,00,00,00
HKR,,InterruptNumber,1,04,00,00,00
HKR,,DevLoader,0,"*ndis"
HKR,,DeviceVxDs,0, "fvnete.sys"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,, "fvnete"
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi,HelpText,,%Help_Text%
[CopyFile.Sys]
[DrvInst.ndi.ME]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=WinMe.Reg, Win9x2k.Params
;CpyFiles=CopyFile.Me.Sys
[DrvInst.ndi.ME.Services]
AddService= "PCMCIAFVNETE", 2, PCMCIAFVNETEMe.Service, PCMCIAFVNETE.EventLog
[WinMe.Reg]
HKR,Ndi,DeviceID,0, "PCMCIA\CNet-CNWLC_11Mbps_Wireless_PC_Card_V-5-6643"
HKR,Ndi,Service,0, "PCMCIAFVNETE"
HKR,,DevLoader,0,*ndis
HKR,,DeviceVxDs,0, fvnete.sys
HKR,,EnumPropPages,0,"netdi.dll,EnumPropPages"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,, "fvnete"
HKR,Ndi\Interfaces,DefUpper,0,"ndis5"
HKR,Ndi\Interfaces,DefLower,0,"ethernet"
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet"
HKR, Ndi\Install, ndis3, 0, "PCMCIAFVNETR.ndis5me"
[PCMCIAFVNETR.ndis5me]
;CpyFiles=CopyFile.Me.Sys
[CopyFile.Me.Sys]
[PCMCIAFVNETRMe.Service]
DisplayName=%PCMCIAFVNETE.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%11%\fvnete.sys
LoadOrderGroup=NDIS
[DrvInst.Ndi.NTx86]
Characteristics=0x84 ;; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ;; PCMCIA
AddReg=Win2k.Reg, Win9x2k.Params
;CpyFiles=CopyFile.2k.Sys
[DrvInst.Ndi.NTx86.Services]
AddService="PCMCIAFVNETE", 2, PCMCIAFVNETE50.Service, PCMCIAFVNETE.EventLog
[Win2k.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "PCMCIAFVNETE"
[CopyFile.2k.Sys]
[PCMCIAFVNETE50.Service]
DisplayName=%PCMCIAFVNETE.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\fvnete.sys
LoadOrderGroup=NDIS
[DrvInstXP.Ndi.NTx86]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=WinXP.Reg, WinXP.Params
;CpyFiles=CopyFile.XP.Sys
[DrvInstXP.Ndi.NTx86.Services]
AddService="PCMCIAFVNETE", 2, PCMCIAFVNETE51.Service, PCMCIAFVNETE.EventLog
[WinXP.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "PCMCIAFVNETE"
[CopyFile.XP.Sys]
[PCMCIAFVNETE51.Service]
DisplayName=%PCMCIAFVNETE.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\fvnete.sys
LoadOrderGroup=NDIS
[PCMCIAFVNETE.EventLog]
AddReg=PCMCIAFVNETE.AddEventLog.Reg
[PCMCIAFVNETE.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR, , TypesSupported , 0x00010001, 7
[DestinationDirs]
DefaultDestDir=12 ;; Drivers directory
CopyFile.Sys=11
CopyFile.2k.Sys=12
CopyFile.Me.Sys=11
CopyFile.XP.Sys=12
[SourceDisksNames]
1= %DriverDisketteName%,,
[SourceDisksFiles]
fvnete.sys=1,,
fvnetexp.sys=1,,
[Win9x2k.Params]
HKR, Ndi\params\Channel, ParamDesc, 0, %ChannelStr%
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, default, 0, "3"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "3"
HKR, Ndi\params\Rate, ParamDesc, 0, %RateStr%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate, default, 0, "3"
HKR, Ndi\params\Rate\enum, 0, 0, %Fixed1Str%
HKR, Ndi\params\Rate\enum, 1, 0, %Fixed2Str%
HKR, Ndi\params\Rate\enum, 2, 0, %Fixed55Str%
HKR, Ndi\params\Rate\enum, 3, 0, %Fixed11Str%
HKR, Ndi\params\Rate\enum, 4, 0, %AutoStr%
HKR, , Rate, 0, "3"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, %RTS_Str%
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, %FragmentationStr%
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, %OperatingModeStr%
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, %AdHocStr%
HKR, Ndi\params\Operating_Mode\enum, 1, 0, %InfrastructureStr%
HKR, , Operating_Mode, 0, "1"
HKR, Ndi\params\ESSID, ParamDesc, 0, %ESSID_Str%
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, default, 0, ""
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, ""
HKR,Ndi\params\WEP_KEY_INDEX, ParamDesc, 0,%WEP_Key_Str%
HKR,Ndi\params\WEP_KEY_INDEX, type, 0,"enum"
HKR,Ndi\params\WEP_KEY_INDEX, default, 0,"0"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 0, 0,%Key1Str%
HKR,Ndi\params\WEP_KEY_INDEX\enum, 1, 0,%Key2Str%
HKR,Ndi\params\WEP_KEY_INDEX\enum, 2, 0,%Key3Str%
HKR,Ndi\params\WEP_KEY_INDEX\enum, 3, 0,%Key4Str%
HKR,, WEP_KEY_INDEX, 0,"0"
HKR,Ndi\params\EncryptionLevel, ParamDesc, 0,"Encryption Level"
HKR,Ndi\params\EncryptionLevel, type, 0,"enum"
HKR,Ndi\params\EncryptionLevel, default, 0,"0"
HKR,Ndi\params\EncryptionLevel\enum, 0, 0,%DisabledStr%
HKR,Ndi\params\EncryptionLevel\enum, 1, 0,%64bit%
HKR,Ndi\params\EncryptionLevel\enum, 2, 0,%128bit%
HKR,, EncryptionLevel,0,"0"
HKR,Ndi\params\WEP_KEY_1, ParamDesc, 0,%KEY1_Str%
HKR,Ndi\params\WEP_KEY_1, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_1, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_1, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_1, UpperCase, 0,"1"
HKR,, WEP_KEY_1, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_2, ParamDesc, 0,%KEY2_Str%
HKR,Ndi\params\WEP_KEY_2, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_2, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_2, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_2, UpperCase, 0,"1"
HKR,, WEP_KEY_2, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_3, ParamDesc, 0,%KEY3_Str%
HKR,Ndi\params\WEP_KEY_3, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_3, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_3, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_3, UpperCase, 0,"1"
HKR,, WEP_KEY_3, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_4, ParamDesc, 0,%KEY4_Str%
HKR,Ndi\params\WEP_KEY_4, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_4, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_4, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_4, UpperCase, 0,"1"
HKR,, WEP_KEY_4, 0,"0000000000"
HKR,Ndi\params\WEP_Mode, ParamDesc, 0,%WEP_Mode_Str%
HKR,Ndi\params\WEP_Mode, type, 0,"enum"
HKR,Ndi\params\WEP_Mode, default, 0,"0"
HKR,Ndi\params\WEP_Mode\enum, 0, 0,%WepMandatoryStr%
HKR,Ndi\params\WEP_Mode\enum, 1, 0,%WepOptionalStr%
HKR,, WEP_Mode, 0,"0"
HKR,Ndi\params\AuthenticationType, ParamDesc, 0,%AuthTypeStr%
HKR,Ndi\params\AuthenticationType, type, 0,"enum"
HKR,Ndi\params\AuthenticationType, default, 0,"2"
HKR,Ndi\params\AuthenticationType\enum, 0, 0,%OpenSystemStr%
HKR,Ndi\params\AuthenticationType\enum, 1, 0,%SharedKeyStr%
HKR,Ndi\params\AuthenticationType\enum, 2, 0,%AutoAuthStr%
HKR,, AuthenticationType, 0,"2"
HKR,Ndi\params\PreambleType, ParamDesc, 0,%PreambleStr%
HKR,Ndi\params\PreambleType, type, 0,"enum"
HKR,Ndi\params\PreambleType, default, 0,"2"
HKR,Ndi\params\PreambleType\enum, 0, 0,%LongPreambleStr%
HKR,Ndi\params\PreambleType\enum, 1, 0,%ShortPreambleStr%
HKR,Ndi\params\PreambleType\enum, 2, 0,%AutoPreambleStr%
HKR,, PreambleType, 0,"2"
HKR,Ndi\params\PowerMgmtMode, ParamDesc, 0,%PowerMgmtStr%
HKR,Ndi\params\PowerMgmtMode, type, 0,"enum"
HKR,Ndi\params\PowerMgmtMode, default, 0,"0"
HKR,Ndi\params\PowerMgmtMode\enum, 0, 0,%ActiveStr%
HKR,Ndi\params\PowerMgmtMode\enum, 1, 0,%PSStr%
HKR,, PowerMgmtMode, 0,"0"
HKR,Ndi\params\BasicRates, ParamDesc, 0,%BasicRatesStr%
HKR,Ndi\params\BasicRates, type, 0,"enum"
HKR,Ndi\params\BasicRates, default, 0,"1"
HKR,Ndi\params\BasicRates\enum, 0, 0,%BR1Str%
HKR,Ndi\params\BasicRates\enum, 1, 0,%BR2Str%
HKR,, BasicRates, 0,"1"
HKR, Ndi\params\BeaconPeriod, ParamDesc, 0, %BeaconPeriodStr%
HKR, Ndi\params\BeaconPeriod, type, 0, "int"
HKR, Ndi\params\BeaconPeriod, default, 0, "100"
HKR, Ndi\params\BeaconPeriod, min, 0, "20"
HKR, Ndi\params\BeaconPeriod, max, 0, "1000"
HKR, Ndi\params\BeaconPeriod, step, 0, "1"
HKR, , BeaconPeriod, 0, "100"
HKR,Ndi\params\RadioOnOff, ParamDesc, 0,%RadioOnOffStr%
HKR,Ndi\params\RadioOnOff, type, 0,"enum"
HKR,Ndi\params\RadioOnOff, default, 0,"1"
HKR,Ndi\params\RadioOnOff\enum, 0, 0,%RadioOffStr%
HKR,Ndi\params\RadioOnOff\enum, 1, 0,%RadioOnStr%
HKR,, RadioOnOff, 0,"1"
[WinXP.Params]
HKR, Ndi\params\Rate, ParamDesc, 0, %RateStr%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate, default, 0, "3"
HKR, Ndi\params\Rate\enum, 0, 0, %Fixed1Str%
HKR, Ndi\params\Rate\enum, 1, 0, %Fixed2Str%
HKR, Ndi\params\Rate\enum, 2, 0, %Fixed55Str%
HKR, Ndi\params\Rate\enum, 3, 0, %Fixed11Str%
HKR, Ndi\params\Rate\enum, 4, 0, %AutoStr%
HKR, , Rate, 0, "3"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, %RTS_Str%
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, %FragmentationStr%
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR,Ndi\params\PreambleType, ParamDesc, 0,%PreambleStr%
HKR,Ndi\params\PreambleType, type, 0,"enum"
HKR,Ndi\params\PreambleType, default, 0,"2"
HKR,Ndi\params\PreambleType\enum, 0, 0,%LongPreambleStr%
HKR,Ndi\params\PreambleType\enum, 1, 0,%ShortPreambleStr%
HKR,Ndi\params\PreambleType\enum, 2, 0,%AutoPreambleStr%
HKR,, PreambleType, 0,"2"
HKR,Ndi\params\RadioOnOff, ParamDesc, 0,%RadioOnOffStr%
HKR,Ndi\params\RadioOnOff, type, 0,"enum"
HKR,Ndi\params\RadioOnOff, default, 0,"1"
HKR,Ndi\params\RadioOnOff\enum, 0, 0,%RadioOffStr%
HKR,Ndi\params\RadioOnOff\enum, 1, 0,%RadioOnStr%
HKR,, RadioOnOff, 0,"1"
[Strings]
VENDOR= " "
PCMCIAOEM5V.DeviceDesc= "WLAN 11Mbps PCMCIA ADAPTER-E(5V)"
PCMCIAFVNETE.DisplayName= "WLAN 11Mbps PCMCIA ADAPTER-E"
DriverDisketteName= "WLAN 11Mbps PCMCIA ADAPTER-E Drivers Diskette/CD"
Help_Text="VirtualNET lets you set up easily and operate a Wireless LAN compliant with 802.11 Standard. It operates in the license free 2.4 GHz ISM band and achieves a peak data rate of 11 Mbs."
ChannelStr="Channel"
RateStr="Rate"
Fixed1Str="Fixed 1 Mbps"
Fixed2Str="Fixed 2 Mbps"
Fixed55Str="Fixed 5.5 Mbps"
Fixed11Str="Fixed 11 Mbps"
AutoStr="Auto"
RTS_Str="RTS Threshold"
FragmentationStr="Fragmentation Threshold"
OperatingModeStr="Operating Mode"
AdHocStr="Ad-Hoc"
InfrastructureStr="Infrastructure"
ESSID_Str="ESSID"
WEP_Key_Str="WEP Key To Use"
KEY1_Str="WEP Key 1"
KEY2_Str="WEP Key 2"
KEY3_Str="WEP Key 3"
KEY4_Str="WEP Key 4"
WEP_Mode_Str="WEP Mode"
Key1Str="Key 1"
Key2Str="Key 2"
Key3Str="Key 3"
Key4Str="Key 4"
DisabledStr="Disabled"
64bit="64-bit"
128bit="128-bit"
WepMandatoryStr="Mandatory"
WepOptionalStr="Optional"
AuthTypeStr="Authentication Type"
OpenSystemStr="Open System"
SharedKeyStr="Shared Key"
AutoAuthStr="Auto"
PreambleStr="Preamble Type"
LongPreambleStr="Long"
ShortPreambleStr="Short"
AutoPreambleStr="Auto"
PowerMgmtStr="Power Mgmt Mode"
ActiveStr="Active"
PSStr="Power Save"
BasicRatesStr="Basic Rates"
BR1Str="1, 2 Mbps"
BR2Str="1, 2, 5.5, 11 Mbps"
BeaconPeriodStr="Beacon Period"
RadioOnOffStr="Radio"
RadioOffStr="Off"
RadioOnStr="On"

