
[Version]
Signature="$CHICAGO$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%V_3COM%
CatalogFile=netwp92b.cat
DriverVer=08/04/2003,2.1.1.3005
[Manufacturer]
%V_3COM%=3COM,NTx86,NTx86.5.1
[ControlFlags]
ExcludeFromSelect.NTx86=*
[3COM]
%WLP92B.DeviceDesc%=WLP92B.Ndi,PCMCIA\3COM-3CRWE62092B_Wireless_LAN_PC_Card-9978
[3COM.NTx86]
%WLP92B.DeviceDesc%=WLP92B.Ndi.NT,PCMCIA\3COM-3CRWE62092B_Wireless_LAN_PC_Card-9978
[3COM.NTx86.5.1]
%WLP92B.DeviceDesc%=WLP92B.Ndi.NT.5.1,PCMCIA\3COM-3CRWE62092B_Wireless_LAN_PC_Card-9978
[WLP92B.Ndi]
AddReg=WLP92B.Reg, WLP92B.Params, WLP92B.ExtParams
;CpyFiles=CopyDriver.Sys
[WLP92B.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=WLP92B.NT.Reg, WLP92B.Params, WLP92B.ExtParams
;CpyFiles=CopyDriver.NT.Sys
[WLP92B.Ndi.NT.Services]
AddService=WLP92B, 2, WLP92B.NT.Service, Common.NT.EventLog
[WLP92B.Ndi.NT.5.1]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=WLP92B.NT.5.1.Reg, WLP92B.Params, WLP92B.ExtParams
;CpyFiles=CopyDriver.NT.5.1.Sys
[WLP92B.Ndi.NT.5.1.Services]
AddService=WLP92B, 2, WLP92B.NT.5.1.Service, Common.NT.EventLog
[WLP92B.Reg]
HKR,Ndi,DeviceID,,PCMCIA\3COM-3CRWE62092B_Wireless_LAN_PC_Card-9978
HKR,Ndi,CardType,,"PNP"
HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,wlp92be.sys
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,WLP92BE
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
[WLP92B.Params]
HKR, Ndi\params\Rate, ParamDesc, 0, %RateStr%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate, default, 0, "4"
HKR, Ndi\params\Rate\enum, 0, 0, %Fixed1Str%
HKR, Ndi\params\Rate\enum, 1, 0, %Fixed2Str%
HKR, Ndi\params\Rate\enum, 2, 0, %Fixed55Str%
HKR, Ndi\params\Rate\enum, 3, 0, %Fixed11Str%
HKR, Ndi\params\Rate\enum, 4, 0, %AutoStr%
HKR, , Rate, 0, "4"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, %RTS_Str%
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, %FragmentationStr%
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR,Ndi\params\PreambleType, ParamDesc, 0,%PreambleStr%
HKR,Ndi\params\PreambleType, type, 0,"enum"
HKR,Ndi\params\PreambleType, default, 0,"2"
HKR,Ndi\params\PreambleType\enum, 0, 0,%LongPreambleStr%
HKR,Ndi\params\PreambleType\enum, 1, 0,%ShortPreambleStr%
HKR,Ndi\params\PreambleType\enum, 2, 0,%AutoPreambleStr%
HKR,, PreambleType, 0,"2"
[WLP92B.ExtParams]
HKR,Ndi\params\ALBMode, ParamDesc, 0,%ALBModeStr%
HKR,Ndi\params\ALBMode, type, 0,"enum"
HKR,Ndi\params\ALBMode, default, 0,"1"
HKR,Ndi\params\ALBMode\enum, 0, 0,%DisabledStr%
HKR,Ndi\params\ALBMode\enum, 1, 0,%EnabledStr%
HKR,, ALBMode, 0,"1"
HKR,Ndi\params\AuthenticationType, ParamDesc, 0,%AuthTypeStr%
HKR,Ndi\params\AuthenticationType, type, 0,"enum"
HKR,Ndi\params\AuthenticationType, default, 0,"255"
HKR,Ndi\params\AuthenticationType\enum, 0, 0,%OpenSystemStr%
HKR,Ndi\params\AuthenticationType\enum, 1, 0,%SharedKeyStr%
HKR,Ndi\params\AuthenticationType\enum, 255, 0,%AutoAuthStr%
HKR,, AuthenticationType, 0,"255"
HKR,Ndi\params\BasicRates, ParamDesc, 0,%BasicRatesStr%
HKR,Ndi\params\BasicRates, type, 0,"enum"
HKR,Ndi\params\BasicRates, default, 0,"0"
HKR,Ndi\params\BasicRates\enum, 0, 0,%BR1Str%
HKR,Ndi\params\BasicRates\enum, 1, 0,%BR2Str%
HKR,, BasicRates, 0,"0"
HKR,Ndi\params\BeaconPeriod, ParamDesc, 0,%BeaconPeriodStr%
HKR,Ndi\params\BeaconPeriod, type, 0,"int"
HKR,Ndi\params\BeaconPeriod, default, 0,"100"
HKR,Ndi\params\BeaconPeriod, min, 0,"20"
HKR,Ndi\params\BeaconPeriod, max, 0,"1000"
HKR,Ndi\params\BeaconPeriod, step, 0,"1"
HKR,, BeaconPeriod, 0,"100"
HKR, Ndi\params\Channel, ParamDesc, 0, %ChannelStr%
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, default, 0, "3"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "11"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "3"
HKR, Ndi\params\ESSID, ParamDesc, 0, %ESSID_Str%
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, default, 0, ""
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, ""
HKR,Ndi\params\EncryptionLevel, ParamDesc, 0,"Encryption Level"
HKR,Ndi\params\EncryptionLevel, type, 0,"enum"
HKR,Ndi\params\EncryptionLevel, default, 0,"0"
HKR,Ndi\params\EncryptionLevel\enum, 0, 0,%DisabledStr%
HKR,Ndi\params\EncryptionLevel\enum, 1, 0,%64bit%
HKR,Ndi\params\EncryptionLevel\enum, 2, 0,%128bit%
HKR,Ndi\params\EncryptionLevel\enum, 3, 0,%3ComDSL%
HKR,, EncryptionLevel,0,"0"
HKR,Ndi\params\InternationalRoaming, ParamDesc, 0,%IntRoamingStr%
HKR,Ndi\params\InternationalRoaming, type, 0,"enum"
HKR,Ndi\params\InternationalRoaming, default, 0,"0"
HKR,Ndi\params\InternationalRoaming\enum, 0, 0,%DisabledStr%
HKR,Ndi\params\InternationalRoaming\enum, 1, 0,%EnabledStr%
HKR,, InternationalRoaming,0,"0"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, %OperatingModeStr%
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, %AdHocStr%
HKR, Ndi\params\Operating_Mode\enum, 1, 0, %InfrastructureStr%
HKR, , Operating_Mode, 0, "1"
HKR,Ndi\params\PowerMgmtMode, ParamDesc, 0,%PowerMgmtStr%
HKR,Ndi\params\PowerMgmtMode, type, 0,"enum"
HKR,Ndi\params\PowerMgmtMode, default, 0,"0"
HKR,Ndi\params\PowerMgmtMode\enum, 0, 0,%ActiveStr%
HKR,Ndi\params\PowerMgmtMode\enum, 1, 0,%PSStr%
HKR,, PowerMgmtMode, 0,"0"
HKR,Ndi\params\RadioMode, ParamDesc, 0,%RadioModeStr%
HKR,Ndi\params\RadioMode, type, 0,"enum"
HKR,Ndi\params\RadioMode, default, 0,"2"
HKR,Ndi\params\RadioMode\enum, 0, 0,%RadioOffStr%
HKR,Ndi\params\RadioMode\enum, 1, 0,%RadioOnStr%
HKR,Ndi\params\RadioMode\enum, 2, 0,%RadioAntennaStr%
HKR,, RadioMode, 0,"2"
HKR,Ndi\params\WEP_Mode, ParamDesc, 0,%WEP_Mode_Str%
HKR,Ndi\params\WEP_Mode, type, 0,"enum"
HKR,Ndi\params\WEP_Mode, default, 0,"0"
HKR,Ndi\params\WEP_Mode\enum, 0, 0,%WepMandatoryStr%
HKR,Ndi\params\WEP_Mode\enum, 1, 0,%WepOptionalStr%
HKR,, WEP_Mode, 0,"0"
[WLP92B.NT.5.1.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "wlp92b"
[WLP92B.NT.5.1.Service]
DisplayName=%WLP92B.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\wlp92bf.sys
LoadOrderGroup=NDIS
[WLP92B.NT.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "wlp92b"
[WLP92B.NT.Service]
DisplayName=%WLP92B.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\wlp92be.sys
LoadOrderGroup=NDIS
[Common.NT.EventLog]
AddReg=Common.AddEventLog.Reg
[Common.AddEventLog.Reg]
HKR,,EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR,,TypesSupported , 0x00010001, 7
[CopyDriver.NT.5.1.Sys]
wlp92bf.sys,,,2
[CopyDriver.NT.Sys]
wlp92be.sys,,,2
[CopyDriver.Sys]
wlp92be.sys,,,2
[DestinationDirs]
DefaultDestDir=11 ; System directory
CopyDriver.Sys=11 ; System Directory
CopyDriver.NT.5.1.Sys=12 ; Drivers directory
CopyDriver.NT.Sys=12 ; Drivers directory
[SourceDisksNames]
50=%DriverDisketteName%,,,
[SourceDisksFiles]
wlp92be.sys=50
wlp92bf.sys=50
[Strings]
V_3COM="3COM"
WLP92B.DeviceDesc="3Com 3CRWE62092B Wireless LAN PC Card"
WLP92B.DisplayName="3Com 3CRWE62092B Wireless LAN PC Card"
DriverDisketteName="3Com 3CRWE62092B Drivers Disk"
RateStr="Tx Rate"
Fixed1Str="Fixed 1 Mbps"
Fixed2Str="Fixed 2 Mbps"
Fixed55Str="Fixed 5.5 Mbps"
Fixed11Str="Fixed 11 Mbps"
AutoStr="Auto"
RTS_Str="RTS Threshold"
FragmentationStr="Fragmentation Threshold"
PreambleStr="Preamble Type"
LongPreambleStr="Long"
ShortPreambleStr="Short"
AutoPreambleStr="Auto"
ChannelStr="Channel"
OperatingModeStr="Operating Mode"
AdHocStr="Ad-Hoc"
InfrastructureStr="Infrastructure"
ESSID_Str="ESSID"
WEP_Key_Str="WEP Key To Use"
KEY1_Str="WEP Key 1"
KEY2_Str="WEP Key 2"
KEY3_Str="WEP Key 3"
KEY4_Str="WEP Key 4"
WEP_Mode_Str="WEP Mode"
Key1Str="Key 1"
Key2Str="Key 2"
Key3Str="Key 3"
Key4Str="Key 4"
DisabledStr="Disabled"
EnabledStr="Enabled"
64bit="64-bit"
128bit="128-bit"
3ComDSL="128-bit 3Com DSL"
WepMandatoryStr="Mandatory"
WepOptionalStr="Optional"
AuthTypeStr="Authentication Type"
OpenSystemStr="Open System"
SharedKeyStr="Shared Key"
AutoAuthStr="Auto"
PowerMgmtStr="Power Mgmt Mode"
ActiveStr="Active"
PSStr="Power Save"
BasicRatesStr="Basic Rates"
BR1Str="1, 2 Mbps"
BR2Str="1, 2, 5.5, 11 Mbps"
BeaconPeriodStr="Beacon Period"
IntRoamingStr="International Roaming"
ALBModeStr="ALB Mode"
RadioModeStr="Radio Mode"
RadioOnStr="Always ON"
RadioOffStr="Always OFF"
RadioAntennaStr="By Antenna Position"
