
[Version]
Signature="$CHICAGO$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%ATHEROS%
Compatible=1
DriverVer=07/14/2002,2.0.1.254
Catalogfile=net5211.cat
[Manufacturer]
%ATHEROS%=Atheros
[ControlFlags]
ExcludeFromSelect=*
[Atheros]
%ATHER.DeviceDesc.1022%=ATHER_DEV_1022.ndi, PCI\VEN_168C&DEV_0012&SUBSYS_10221154&REV_01
%ATHER.DeviceDesc.1022%=ATHER_DEV_1022.ndi, PCI\VEN_168C&DEV_0007&SUBSYS_000717F9&REV_01
%ATHER.DeviceDesc.1022%=ATHER_DEV_1022.ndi, PCI\VEN_168C&DEV_0007&SUBSYS_00071737&REV_01
%ATHER.DeviceDesc.1022%=ATHER_DEV_1022.ndi, PCI\VEN_168C&DEV_0012&SUBSYS_2022168C&REV_01
%ATHER.DeviceDesc.1022%=ATHER_DEV_1022.ndi, PCI\VEN_168C&DEV_0012&SUBSYS_00081737&REV_01
%ATHER.DeviceDesc.2022%=ATHER_DEV_2022.ndi, PCI\VEN_168C&DEV_0012&SUBSYS_00111737&REV_01 ;MiniPCI
[ATHER_DEV_1022.ndi]
AddReg=ATHER_DEV_1022.id.reg, 5211.reg, ATHER.win.reg, 5211.abcb.reg
;CpyFiles=ATHER.win.CopyFiles, DEFAULTDESTDIRS
[ATHER_DEV_2022.ndi]
AddReg=ATHER_DEV_2022.id.reg, 5211.reg, ATHER.win.reg, 5211.abmp.reg
;CpyFiles=ATHER.win.CopyFiles, DEFAULTDESTDIRS
[ATHER_DEV_1022.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
AddReg=5211.reg, ATHER.reg, 5211.reg, 5211.abcb.reg
;CpyFiles=ATHER.CopyFiles, DEFAULTDESTDIRS
[ATHER_DEV_2022.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
AddReg=5211.reg, ATHER.reg, 5211.reg, 5211.abmp.reg
;CpyFiles=ATHER.CopyFiles, DEFAULTDESTDIRS
[ATHER_DEV_1022.ndi.NT.Services]
AddService=AR5211, 2, ATHER.Service, common.EventLog
[ATHER_DEV_2022.ndi.NT.Services]
AddService=AR5211, 2, ATHER.Service, common.EventLog
[ATHER_DEV_1022.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0012&SUBSYS_10221154&REV_01"
[ATHER_DEV_2022.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0012&SUBSYS_00111737&REV_01"
[5211.abcb.reg]
HKR, , NetBand, 0x00002, "7"
HKR, CustomParams\Configurations, NicType, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, NetBand, 0x10003, 2
[5211.abmp.reg]
HKR, , NetBand, 0x00002, "7"
HKR, CustomParams\Configurations, NicType, 0x10003, 2
HKR, CustomParams\Configurations\Cfg0, NetBand, 0x10003, 2
[5211.reg]
HKR, Ndi\params\MapRegisters, ParamDesc, 0, %MapRegisters%
HKR, Ndi\params\MapRegisters, default, 0, "256"
HKR, Ndi\params\MapRegisters, min, 0, "32"
HKR, Ndi\params\MapRegisters, max, 0, "512"
HKR, Ndi\params\MapRegisters, step, 0, "8"
HKR, Ndi\params\MapRegisters, base, 0, "10"
HKR, Ndi\params\MapRegisters, type, 0, "int"
HKR, Ndi\params\roamRssiA, ParamDesc, 0, %roamRssiA%
HKR, Ndi\params\roamRssiA, default, 0, "24"
HKR, Ndi\params\roamRssiA, min, 0, "0"
HKR, Ndi\params\roamRssiA, max, 0, "100"
HKR, Ndi\params\roamRssiA, step, 0, "1"
HKR, Ndi\params\roamRssiA, base, 0, "10"
HKR, Ndi\params\roamRssiA, type, 0, "int"
HKR, Ndi\params\roamRssiB, ParamDesc, 0, %roamRssiB%
HKR, Ndi\params\roamRssiB, default, 0, "24"
HKR, Ndi\params\roamRssiB, min, 0, "0"
HKR, Ndi\params\roamRssiB, max, 0, "100"
HKR, Ndi\params\roamRssiB, step, 0, "1"
HKR, Ndi\params\roamRssiB, base, 0, "10"
HKR, Ndi\params\roamRssiB, type, 0, "int"
HKR, Ndi\params\roamRateA, ParamDesc, 0, %roamRateA%
HKR, Ndi\params\roamRateA, Base, 0, "10"
HKR, Ndi\params\roamRateA, default, 0, "4"
HKR, Ndi\params\roamRateA, type, 0, "enum"
HKR, Ndi\params\roamRateA\enum, "0", 0, "6 Mbps"
HKR, Ndi\params\roamRateA\enum, "1", 0, "9 Mbps"
HKR, Ndi\params\roamRateA\enum, "2", 0, "12 Mbps"
HKR, Ndi\params\roamRateA\enum, "3", 0, "18 Mbps"
HKR, Ndi\params\roamRateA\enum, "4", 0, "24 Mbps"
HKR, Ndi\params\roamRateA\enum, "5", 0, "36 Mbps"
HKR, Ndi\params\roamRateA\enum, "6", 0, "48 Mbps"
HKR, Ndi\params\roamRateA\enum, "7", 0, "54 Mbps"
HKR, Ndi\params\roamRateB, ParamDesc, 0, %roamRateB%
HKR, Ndi\params\roamRateB, Base, 0, "10"
HKR, Ndi\params\roamRateB, default, 0, "1"
HKR, Ndi\params\roamRateB, type, 0, "enum"
HKR, Ndi\params\roamRateB\enum, "0", 0, "1 Mbps"
HKR, Ndi\params\roamRateB\enum, "1", 0, "2 Mbps / short preamble"
HKR, Ndi\params\roamRateB\enum, "2", 0, "5.5 Mbps / short preamble"
HKR, Ndi\params\roamRateB\enum, "3", 0, "11 Mbps / short preamble"
HKR, Ndi\params\shortPreamble, ParamDesc, 0, "Preamble Mode"
HKR, Ndi\params\shortPreamble, Base, 0, "10"
HKR, Ndi\params\shortPreamble, default, 0, "1"
HKR, Ndi\params\shortPreamble, type, 0, "enum"
HKR, Ndi\params\shortPreamble\enum, "0", 0, "0"
HKR, Ndi\params\shortPreamble\enum, "1", 0, "1"
HKR, Ndi\params\Qos, ParamDesc, 0, "Qos"
HKR, Ndi\params\Qos, Base, 0, "10"
HKR, Ndi\params\Qos, default, 0, "0"
HKR, Ndi\params\Qos, type, 0, "enum"
HKR, Ndi\params\Qos\enum, "0", 0, "0"
HKR, Ndi\params\Qos\enum, "1", 0, "1"
HKR, Ndi\params\FragThreshold, ParamDesc, 0, "Fragmentation"
HKR, Ndi\params\FragThreshold, default, 0, "2346"
HKR, Ndi\params\FragThreshold, min, 0, "256"
HKR, Ndi\params\FragThreshold, max, 0, "32767"
HKR, Ndi\params\FragThreshold, step, 0, "128"
HKR, Ndi\params\FragThreshold, base, 0, "10"
HKR, Ndi\params\FragThreshold, type, 0, "int"
HKR, , AdHocBand, 0x00002, "1"
HKR, , AwakeTimePerf, 0x00002, "200"
HKR, , beaconInterval, 0x00002, "100"
HKR, , bkScanEnable, 0x00002, "1"
HKR, , bssType, 0x00002, "1"
HKR, , ccode, 0x00002, "US"
HKR, , clist, 0x00002, ""
HKR, , defaultKey, 0x00002, "0"
HKR, , EncryptionAlg, 0x00002, "2"
HKR, , FragThreshold, 0x00002, "2346"
HKR, , HwTxRetries, 0x00002, "5"
HKR, , privacyInvoked, 0x00002, "0"
HKR, , QoS, 0x00002, "0"
HKR, , rateCtrlEnable, 0x00002, "1"
HKR, , RTSThreshold, 0x00002, "2346"
HKR, , scanType, 0x00002, "2"
HKR, , sleepMode, 0x00002, "2"
HKR, , SwTxRetryScale, 0x00002, "1"
HKR, , SmeEnable, 0x00002, "1"
HKR, , tpc, 0x00002, "0"
HKR, , TransmitRate11a, 0x00002, "5" ; 36 Mbps
HKR, , TransmitRate11b, 0x00002, "1" ; 2 Mbps
HKR, , Ssid, 0, "Linksys" ;
HKR, CustomParams\Configurations, MajorVersion, 0x10003, 2
HKR, CustomParams\Configurations, MinorVersion, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
HKR, CustomParams\Configurations\Cfg0, AdHocBand, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, ConfigurationName, 0x00002, "Default"
HKR, CustomParams\Configurations\Cfg0, DefaultKey, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, Enable11g, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, EnableMacAddress, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, EnableRange, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, EnableSecurity, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, EnableTurbo, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, EncryptionAlg, 0x10003, 2
HKR, CustomParams\Configurations\Cfg0, MacAddress, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, NetworkConnectionType, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, NetworkName, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, PowerManagement, 0x10003, 1
HKR, CustomParams\Configurations\Cfgo, Preamble, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, QoS, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, scanType, 0x10003, 2
HKR, CustomParams\Configurations\Cfg0, tpc, 0x10003, 0
[ATHER.reg]
HKR, Ndi, Service, 0, "AR5211"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, , InitFile, 0, %InitFile%
HKR, , aifs, 0, "2"
HKR, , cwmin, 0, "15"
[ATHER.Service]
DisplayName=%ATHER.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\ar5211.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[ATHER.win.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "ar5211.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "AR5211"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, , InitFile, 0, %InitFile%
HKR, , aifs, 0, 2
HKR, , cwmin, 0, 15
HKR, Ndi\Install, ndis3, 0, "ATHER.install"
[ATHER.win.CopyFiles]
ar5211.sys
[ATHER.CopyFiles]
ar5211.sys
[SourceDisksNames]
1=%Atheros_Disk%,,,
[SourceDisksFiles]
ar5211.sys=1,, ; on distribution disk 1
[DestinationDirs]
ATHER.CopyFiles=12
ATHER.win.CopyFiles=11
DefaultDestDir=11
[DEFAULTDESTDIRS]
[Strings]
Atheros="Linksys"
MapRegisters="Map Registers"
InitFile="Athnic.ini"
Atheros_Disk="Dual Band Wireless A+B Notebook Adapter Disk"
ATHER.DeviceDesc.1022="Dual Band Wireless A+B Notebook Adapter"
ATHER.DeviceDesc.2022="Dual Band Wireless A+B Notebook Adapter"
ATHER.Service.DispName="Dual Band Wireless A+B Notebook Adapter Service"
roamRssiA="11a Network Rssi Threshold for Roaming"
roamRssiB="11b Network Rssi Threshold for Roaming"
roamRateA="11a Network Rate Threshold for Roaming"
roamRateB="11b Network Rate Threshold for Roaming"
