
[version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Realtek% ;;
CatalogFile.NT=net8192de.cat ;; for WHQL certified
DriverVer=08/30/2011,1002.03.0830.2011
[Manufacturer]
%Realtek%=Realtek,NTx86
[ControlFlags]
ExcludeFromSelect=*
[Realtek.NTx86]
%RTL8192de0.DeviceDesc%=RTL8192de.ndi, PCI\VEN_10EC&DEV_8193&SUBSYS_819310EC&REV_00
%RTL8192de1.DeviceDesc%=RTL8192de1.ndi, PCI\VEN_10EC&DEV_8193&SUBSYS_819310EC&REV_01
%RTL8192de0.DeviceDesc%=RTL8192de.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC&REV_00
%RTL8192de1.DeviceDesc%=RTL8192de1.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC&REV_01
%RTL8192de0.DeviceDesc%=RTL8192de.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA&REV_00
%RTL8192de1.DeviceDesc%=RTL8192de1.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA&REV_01
%RTL8192de0.DeviceDesc%=RTL8192de.ndi, PCI\VEN_10EC&DEV_8193&SUBSYS_01861025&REV_00
%RTL8192de1.DeviceDesc%=RTL8192de1.ndi, PCI\VEN_10EC&DEV_8193&SUBSYS_01861025&REV_01
[Realtek.NTamd64]
%RTL8192de0.DeviceDesc%=RTL8192de.ndi, PCI\VEN_10EC&DEV_8193&SUBSYS_819310EC&REV_00
%RTL8192de1.DeviceDesc%=RTL8192de1.ndi, PCI\VEN_10EC&DEV_8193&SUBSYS_819310EC&REV_01
%RTL8192de0.DeviceDesc%=RTL8192de.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC&REV_00
%RTL8192de1.DeviceDesc%=RTL8192de1.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC&REV_01
%RTL8192de0.DeviceDesc%=RTL8192de.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC&REV_00
%RTL8192de1.DeviceDesc%=RTL8192de1.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC&REV_01
%RTL8192de0.DeviceDesc%=RTL8192de.ndi, PCI\VEN_10EC&DEV_8193&SUBSYS_01861025&REV_00
%RTL8192de1.DeviceDesc%=RTL8192de1.ndi, PCI\VEN_10EC&DEV_8193&SUBSYS_01861025&REV_01
[RTL8192de.ndi.NT]
AddReg=RTL8192de.reg, 11nWirelessMode.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192de.CopyFiles
[RTL8192de.ndi.NT.Services]
AddService=RTL8192de, 2, RTL8192de.Service, RTL8192de.EventLog
[RTL8192de1.ndi.NT]
AddReg=RTL8192de.reg, 11nWirelessMode.reg, ConcurrentMode.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192de.CopyFiles
[RTL8192de1.ndi.NT.Services]
AddService=RTL8192de, 2, RTL8192de.Service, RTL8192de.EventLog
[RTLG8192de.ndi.NT]
AddReg=RTL8192de.reg, 11gWirelessMode.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192de.CopyFiles
[RTLG8192de.ndi.NT.Services]
AddService=RTL8192de, 2, RTL8192de.Service, RTL8192de.EventLog
[SS8192de.ndi.NT]
AddReg=RTL8192de.reg, 11nWirelessMode.reg, SS.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192de.CopyFiles
[SS8192de.ndi.NT.Services]
AddService=RTL8192de, 2, RTL8192de.Service, RTL8192de.EventLog
[SSG8192de.ndi.NT]
AddReg=RTL8192de.reg, 11gWirelessMode.reg, SS.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192de.CopyFiles
[SSG8192de.ndi.NT.Services]
AddService=RTL8192de, 2, RTL8192de.Service, RTL8192de.EventLog
[RTL8192de.reg]
HKR, Ndi, Service, 0, "RTL8192de"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR,defaults, AH_BcnIntv, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, default, 0, "100"
HKR,Ndi\params\AH_BcnIntv, ParamDesc, 0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, type, 0, "int"
HKR,Ndi\params\AH_BcnIntv, min, 0, "20"
HKR,Ndi\params\AH_BcnIntv, max, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, step, 0, "1"
HKR,Ndi\params\Dot11dEnable, ParamDesc, 0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable, type, 0, "enum"
HKR,Ndi\params\Dot11dEnable, default, 0, "0"
HKR,Ndi\params\Dot11dEnable\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum, "1", 0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, %ROAMING_SENSITIVITY_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel, Type, 0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default, 0, "80"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127", 0, %DISABLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "65", 0, %HIGH_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70", 0, %MIDDLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80", 0, %LOW_STR%
HKR,Ndi\params\PreambleMode, ParamDesc, 0, %PREAMBLE_MODE_STR%
HKR,Ndi\params\PreambleMode, type, 0, "enum"
HKR,Ndi\params\PreambleMode, default, 0, "2"
HKR,Ndi\params\PreambleMode\enum, "1", 0, %LONG_PREAMBLE_STR%
HKR,Ndi\params\PreambleMode\enum, "2", 0, %LONG_SHORT_PREAMBLE_STR%
HKR,defaults,PreambleMode,0,"2"
HKR,,PreambleMode,0,"2"
HKR,Ndi\params\TxPowerLevel, ParamDesc, 0, %TX_POWER_LEVEL_STR%
HKR,Ndi\params\TxPowerLevel, type, 0, "enum"
HKR,Ndi\params\TxPowerLevel, default, 0, "0"
HKR,Ndi\params\TxPowerLevel\enum, "0", 0, %AUTO_STR%
HKR,Ndi\params\TxPowerLevel\enum, "1", 0, %HIGH_TX_POWER_STR%
HKR,Ndi\params\TxPowerLevel\enum, "2", 0, %MIDDLE_TX_POWER_STR%
HKR,Ndi\params\TxPowerLevel\enum, "3", 0, %LOW_TX_POWER_STR%
HKR,Ndi\params\TxPowerLevel\enum, "4", 0, %VERY_LOW_TX_POWER_STR%
HKR,defaults,TxPowerLevel,0,"0"
HKR,,TxPowerLevel,0,"0"
HKR,,Channel,0,"10"
HKR,,Channel5G,0,"36"
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"
HKR,defaults,bFwCtrlLPS,0,"3"
HKR,,bFwCtrlLPS,0,"3"
HKR,,HwSwRfOffD3,0,"0"
HKR,defaults,PciASPM,0,"0"
HKR,,PciASPM,0,"0"
HKR,,LPS2RDisable,0,"1"
HKR,,UseRxInterruptWorkItem,0,"0"
HKR,,LPSIntvl,0,"5"
HKR,,GPIORFSW,0,"1"
HKR,,KeepAliveLevel,0,"1"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
HKR,,WiFiConfg,,"0"
HKR,,bEarlymodeEnable,,"1"
[11nAdhoc.reg]
HKR,Ndi\params\11nAdhoc, ParamDesc, 0, %11NADHOC_ENABLE_STR%
HKR,Ndi\params\11nAdhoc, type, 0, "enum"
HKR,Ndi\params\11nAdhoc, default, 0, "0"
HKR,Ndi\params\11nAdhoc\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\11nAdhoc\enum, "1", 0, %ENABLE_STR%
HKR,defaults,11nAdhoc,0,"0"
HKR,,11nAdhoc,0,"0"
[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, type, 0, "enum"
HKR,Ndi\params\WirelessMode, default, 0, "8"
HKR,Ndi\params\WirelessMode\enum, "2", 0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, "4", 0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"
[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, type, 0, "enum"
HKR,Ndi\params\WirelessMode, default, 0, "8"
HKR,Ndi\params\WirelessMode\enum, "8", 0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"
[SS.reg]
HKR,,PciASPM,0,"4"
HKR,,DevicePciASPMSetting,0,"2"
[ConcurrentMode.reg]
HKR,Ndi\params\TwoStaConcurrentMode, ParamDesc, 0, %TWO_STA_CONCURRENT_MODE%
HKR,Ndi\params\TwoStaConcurrentMode, type, 0, "enum"
HKR,Ndi\params\TwoStaConcurrentMode, default, 0, "1"
HKR,Ndi\params\TwoStaConcurrentMode\enum, "0", 0, %SECONDARY_DISABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum, "1", 0, %SECONDARY_ENABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum, "2", 0, %SECONDARY_AUTO%
HKR,defaults,TwoStaConcurrentMode,0,"0"
HKR,,TwoStaConcurrentMode,0,"0"
[RTL8192de.Service]
DisplayName=%Realtek.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rtl8192de.sys
LoadOrderGroup=NDIS
[RTL8192de.EventLog]
AddReg=RTL8192de.AddEventLog.reg
[RTL8192de.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[RTL8192de.CopyFiles]
rtl8192de.sys,,,2
[DestinationDirs]
RTL8192de.CopyFiles=12
DefaultDestDir=11 ; LDID_SYS
[SourceDisksNames]
1=%DISKNAME%,,,
[SourceDisksFiles]
rtl8192de.sys=1
[Strings]
Realtek="Realtek Semiconductor Corp."
SSID_STR="SSID"
CHANNEL_STR="Channel"
NETWORK_TYPE_STR="Network Type"
LED_CONTROL_STR="LED Control"
POWER_SAVE_STR="Power Save Mode"
WIFI_IBSS_STR="IBSS Default 11b Mode"
RATE_ADAPTIVE_STR="Rate Adaptive"
QOS_STR="QoS"
WMM_APSD="WMM APSD"
CCX_RM_STR="CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR="CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR="Forced Priority"
HW_PARA_STR="Init from HwParaFile"
THREE_WIRE_MODE_STR="Three Wire Programming Mode"
BOARD_TYPE_STR="Board Type"
PROTECTION_MODE_STR="Protection Mode"
TPC_STR="Transmit Power Control"
TPC_POLARITY_STR="TPC Polarity Select"
HIGH_POWER_STR="High Power Mechanism"
INIT_GAIN_STR="Initial Gain State"
CW_MAX_MIN_STR="Contention Window"
PSP_XLINK_STR="PSP XLink Mode"
CHANNEL_PLAN_STR="Channel Plan"
WL_MODE_STR="Wireless Mode"
PREAMBLE_MODE_STR="Preamble Mode"
FRAGTHRESH_STR="Fragmentation Threshold"
RTSTHRESH_STR="RTS Threshold"
DOT11_ENABLE_STR="802.11d"
11NADHOC_ENABLE_STR="11n AdHoc"
DISABLE_STR="Disable"
ENABLE_STR="Enable"
CAM_STR="CAM"
MAX_PSP_STR="MAX_PSP"
FAST_PSP_STR="Fast_PSP"
AD_HOC_STR="Ad Hoc"
INFRASTRUCTURE_STR="Infrastructure"
AUTO_SELECT_STR="Auto select"
DOMAIN_FROM_EEPROM_STR="DOMAIN_FROM_EEPROM"
AUTO_STR="Auto"
LONG_PREAMBLE_STR="Long only"
LONG_SHORT_PREAMBLE_STR="Short & long"
SHORT_PREAMBLE_STR="Short Preamble"
FCC_STR="FCC"
IC_STR="IC"
ETSI_STR="ETSI"
SPAIN_STR="Spain"
FRANCE_STR="France"
MKK_STR="MKK"
MKK1_STR="MKK1"
ISRAEL_STR="Israel"
TELEC_STR="TELEC"
IEEE_802_11A_STR="IEEE 802.11a"
IEEE_802_11B_STR="IEEE 802.11b"
IEEE_802_11BG_STR="IEEE 802.11b/g"
IEEE_802_11BGN_STR="IEEE 802.11b/g/n"
Roam_Retry_Limit_STR="Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR="Leisure Power Save"
AH_BCNINTV_STR="Beacon Interval"
ROAMING_SENSITIVITY_STR="Roaming Sensitivity Level"
HIGH_STR="High"
MIDDLE_STR="Middle"
LOW_STR="Low"
TX_POWER_LEVEL_STR="TX Power Level"
HIGH_TX_POWER_STR="100 %"
MIDDLE_TX_POWER_STR="75 %"
LOW_TX_POWER_STR="50 %"
VERY_LOW_TX_POWER_STR="20 %"
TWO_STA_CONCURRENT_MODE="Two STA Concurrent Mode"
SECONDARY_DISABLE="Secondary client Disable"
SECONDARY_ENABLE="Secondary Client Enable"
SECONDARY_AUTO="Secondary Client Auto Select"
DISKNAME=" Realtek Wireless LAN PCI-E Driver Disk "
Realtek.Service.DispName ="Realtek RTL8192DE Wireless LAN 802.11n PCI-E NIC Driver"
RTL8192de0.DeviceDesc ="Realtek RTL8192DE Wireless LAN 802.11n PCI-E NIC MAC0"
RTL8192de0.DeviceDesc.DispName ="Realtek RTL8192DE Wireless LAN 802.11n PCI-E NIC MAC0"
RTL8192de1.DeviceDesc ="Realtek RTL8192DE Wireless LAN 802.11n PCI-E NIC MAC1"
RTL8192de1.DeviceDesc.DispName ="Realtek RTL8192DE Wireless LAN 802.11n PCI-E NIC MAC1"

