
[version]
Signature="$Chicago$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%AirgoNet%
Compatible=1
DriverVer=02/04/2005, 1.4.4.183
MillenniumPreferred=.ME
CatalogFile=AniNet.cat
[SourceDisksNames]
1= %Disk_1%,,,
[SourceDisksFiles]
WNIhdd51.sys=1
WNIhdd50.sys=1
[DestinationDirs]
DefaultDestDir=11
Airgo_Driver.Copyfiles=12
Airgo_Driver.NT.5.1.Copyfiles=12
[Manufacturer]
%Airgo%=Airgo,NT.5.1
[ControlFlags]
ExcludeFromSelect=PCI\VEN_17CB&DEV_0001&SUBSYS_00371737
[Airgo]
%Linksys.DeviceDesc%=Airgo.ndi, PCI\VEN_17CB&DEV_0001&SUBSYS_00371737
[Airgo.NT.5.1]
%Linksys.DeviceDesc%=Airgo.ndi.NT.5.1, PCI\VEN_17CB&DEV_0001&SUBSYS_00371737
[Airgo.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8
AddReg=Airgo.NT.reg, AdvancedParms, StaticParms
;CpyFiles=Airgo_Driver.CopyFiles
[Airgo.ndi.NT.Services]
AddService=Airgo, 2, Airgo.Service, Airgo.EventLog
[Airgo.Service]
DisplayName=%Airgo.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\wnihdd50.sys
LoadOrderGroup=NDIS
[Airgo.EventLog]
AddReg=Airgo.AddEventLog.reg
[Airgo.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\wnihdd50.sys"
HKR, , TypesSupported, 0x00010001, 7
[Airgo.ndi.NT.5.1]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8
AddReg=Airgo.NT.reg, AdvancedParms, StaticParms
;CpyFiles=Airgo_Driver.NT.5.1.CopyFiles
[Airgo.ndi.NT.5.1.Services]
AddService=Airgo, 2, Airgo.NT.5.1.Service, Airgo.EventLog
[Airgo.NT.5.1.Service]
DisplayName=%Airgo.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\wnihdd51.sys
LoadOrderGroup=NDIS
[Airgo.EventLog]
AddReg=Airgo.NT.5.1.AddEventLog.reg
[Airgo.NT.5.1.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\wnihdd51.sys"
HKR, , TypesSupported, 0x00010001, 7
[Airgo.NT.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis5"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi, Service, 0, %Airgo.Service.Name%
[Airgo_Driver.Copyfiles]
wnihdd50.sys,,,2
[Airgo_Driver.NT.5.1.CopyFiles]
wnihdd51.sys,,,2
[AdvancedParms]
HKR,,MonBufSize,,"2600"
HKR,,MonBufCount,,"12"
HKR,,MBMsgBufSize,,"4096"
HKR,,MBMsgBufCount,,"6"
HKR,,RxBufferCount,,"100"
HKR,,RxBufferSize,,"256"
HKR,,TxDescCount,,"128"
HKR,,RxDescCount,,"128"
HKR,,gNwDensity,,"Auto"
HKR,NDI\params\gNwDensity, ParamDesc, 0, "Network Density"
HKR,NDI\params\gNwDensity, type, 0, "enum"
HKR,NDI\params\gNwDensity, default, 0, "Medium"
HKR,NDI\params\gNwDensity\enum, "Auto", 0, "Adaptive"
HKR,NDI\params\gNwDensity\enum, "High", 0, "High"
HKR,NDI\params\gNwDensity\enum, "Medium", 0, "Medium"
HKR,NDI\params\gNwDensity\enum, "Low", 0, "Low"
HKR,,gTxPwrLevel,,"High"
HKR,NDI\params\gTxPwrLevel, ParamDesc, 0, "Tx Power"
HKR,NDI\params\gTxPwrLevel, type, 0, "enum"
HKR,NDI\params\gTxPwrLevel, default, 0, "High"
HKR,NDI\params\gTxPwrLevel\enum, "High", 0, "High"
HKR,NDI\params\gTxPwrLevel\enum, "Low", 0, "Low"
HKR,,gNumTxAntenna,,"0"
HKR,,gNumRxAntenna,,"0"
HKR,,gAckTimeout11A,,"25"
HKR,,gAckTimeout11BG,,"30"
HKR,,gShortRetryLimit,,"0"
HKR,NDI\params\gShortRetryLimit, ParamDesc, 0, "ShortRetryLimit"
HKR,NDI\params\gShortRetryLimit, type, 0, "int"
HKR,NDI\params\gShortRetryLimit, default, 0, "0"
HKR,NDI\params\gShortRetryLimit, min, 0, "0"
HKR,NDI\params\gShortRetryLimit, max, 0, "255"
HKR,NDI\params\gShortRetryLimit, step, 0, "1"
HKR,,gLongRetryLimit,,"0"
HKR,NDI\params\gLongRetryLimit, ParamDesc, 0, "LongRetryLimit"
HKR,NDI\params\gLongRetryLimit, type, 0, "int"
HKR,NDI\params\gLongRetryLimit, default, 0, "0"
HKR,NDI\params\gLongRetryLimit, min, 0, "0"
HKR,NDI\params\gLongRetryLimit, max, 0, "255"
HKR,NDI\params\gLongRetryLimit, step, 0, "1"
HKR,,gFragmentationThreshold,,"2000"
HKR,NDI\params\gFragmentationThreshold, ParamDesc, 0, "Fragmentation Threshold"
HKR,NDI\params\gFragmentationThreshold, type, 0, "int"
HKR,NDI\params\gFragmentationThreshold, default, 0, "2000"
HKR,NDI\params\gFragmentationThreshold, min, 0, "256"
HKR,NDI\params\gFragmentationThreshold, max, 0, "2346"
HKR,NDI\params\gFragmentationThreshold, step, 0, "1"
HKR,,gRTSThreshold,,"2347"
HKR,NDI\params\gRTSThreshold, ParamDesc, 0, "RTS Threshold"
HKR,NDI\params\gRTSThreshold, type, 0, "int"
HKR,NDI\params\gRTSThreshold, default, 0, "2347"
HKR,NDI\params\gRTSThreshold, min, 0, "0"
HKR,NDI\params\gRTSThreshold, max, 0, "2347"
HKR,NDI\params\gRTSThreshold, step, 0, "1"
HKR,,gMaxAckRate11A,,"5"
HKR,,gMaxAckRate11B,,"22"
HKR,,gCalibration,,"1"
HKR,,gCalibrationPeriod,,"5"
HKR,,gBgScanPeriod,,"5000"
HKR,NDI\params\gBgScanPeriod, ParamDesc, 0, "Background Scan period (milliseconds)"
HKR,NDI\params\gBgScanPeriod, type, 0, "dword"
HKR,NDI\params\gBgScanPeriod, default, 0, "5000"
HKR,NDI\params\gBgScanPeriod, min, 0, "0"
HKR,NDI\params\gBgScanPeriod, max, 0, "180000"
HKR,NDI\params\gBgScanPeriod, step, 0, "1"
HKR,,gBgScanMinChannelTime,,"20"
HKR,,gBgScanMaxChannelTime,,"40"
HKR,,gCCAMode,,"7"
HKR,,gEDThreshold,,"60"
HKR,,gAckPolicy,,"0"
HKR,NDI\params\gAckPolicy, ParamDesc, 0, "Ack Policy"
HKR,NDI\params\gAckPolicy, type, 0, "enum"
HKR,NDI\params\gAckPolicy, default, 0, "0"
HKR,NDI\params\gAckPolicy\enum, "0", 0, "Immediate"
HKR,NDI\params\gAckPolicy\enum, "3", 0, "Burst"
HKR,,gDot11Mode,,"0"
HKR,NDI\params\gDot11Mode, ParamDesc, 0, "802.11 Mode"
HKR,NDI\params\gDot11Mode, type, 0, "enum"
HKR,NDI\params\gDot11Mode, default, 0, "0"
HKR,NDI\params\gDot11Mode\enum, "0", 0, "All"
HKR,NDI\params\gDot11Mode\enum, "1", 0, "802.11a"
HKR,NDI\params\gDot11Mode\enum, "2", 0, "802.11b"
HKR,NDI\params\gDot11Mode\enum, "3", 0, "802.11g"
HKR,,gEnhancedRatesEnabled,,"1"
HKR,NDI\params\gEnhancedRatesEnabled, ParamDesc, 0, "Enhanced Rates"
HKR,NDI\params\gEnhancedRatesEnabled, type, 0, "enum"
HKR,NDI\params\gEnhancedRatesEnabled, default, 0, "1"
HKR,NDI\params\gEnhancedRatesEnabled\enum, "0", 0, "Off"
HKR,NDI\params\gEnhancedRatesEnabled\enum, "1", 0, "On"
HKR,,gCfg1Id,,"0"
HKR,,gCfg1Value,,"0"
HKR,,gCfg2Id,,"0"
HKR,,gCfg2Value,,"0"
HKR,,gCfg3Id,,"0"
HKR,,gCfg3Value,,"0"
HKR,,gCfg4Id,,"0"
HKR,,gCfg4Value,,"0"
HKR,,gCfg5Id,,"0"
HKR,,gCfg5Value,,"0"
HKR,,gShortSlotTimeEnabled,,"1"
HKR,,g11dSupportEnabled,,"1"
HKR,NDI\params\g11dSupportEnabled, ParamDesc, 0, "802.11d Support"
HKR,NDI\params\g11dSupportEnabled, type, 0, "enum"
HKR,NDI\params\g11dSupportEnabled, default, 0, "1"
HKR,NDI\params\g11dSupportEnabled\enum, "0", 0, "Off"
HKR,NDI\params\g11dSupportEnabled\enum, "1", 0, "On"
HKR,,gWMMSupportEnabled,,"1"
HKR,NDI\params\gWMMSupportEnabled, ParamDesc, 0, "Wi-Fi Multimedia (WMM) Support"
HKR,NDI\params\gWMMSupportEnabled, type, 0, "enum"
HKR,NDI\params\gWMMSupportEnabled, default, 0, "1"
HKR,NDI\params\gWMMSupportEnabled\enum, "0", 0, "Off"
HKR,NDI\params\gWMMSupportEnabled\enum, "1", 0, "eDCA"
HKR,,g11eSupportEnabled,,"1"
HKR,NDI\params\g11eSupportEnabled, ParamDesc, 0, "802.11e Support"
HKR,NDI\params\g11eSupportEnabled, type, 0, "enum"
HKR,NDI\params\g11eSupportEnabled, default, 0, "1"
HKR,NDI\params\g11eSupportEnabled\enum, "0", 0, "Off"
HKR,NDI\params\g11eSupportEnabled\enum, "1", 0, "eDCA"
HKR,,gHeartbeat24,,"10"
HKR,,gHeartbeat50,,"6"
HKR,,gAgingTimerInBKScanUnits,,"3"
HKR,,gCountryCode,,"AGN"
[StaticParms]
HKR, ,HardwareID, ,"WNI0000"
HKR,,RoamingFeatures,,"3"
HKR,,RoamingSignalDegradedThresh,,"30"
HKR,,RoamingSignalDegradedBeaconsPerPeriod,,"10"
HKR,,RoamingSignalDegradedPeriods,,"10"
HKR,,RoamingSignalDegradedNewRssiThreshold,,"27"
HKR,,RoamingScanOnSignalDegradation,,"0"
[Strings]
Airgo="Linksys"
AirgoNet="Linksys"
Disk_1="Installation Disk"
Airgo.Service.DispName="Wireless-G Notebook Adapter with SRX"
Airgo.Service.Name="Linksys"
Linksys.DeviceDesc="Wireless-G Notebook Adapter with SRX"
