
[Version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
MillenniumPreferred=.ME
Provider=%VENDOR%
CatalogFile=smcusb.cat
DriverVer=08/31/2002,2.6.5.193
[Manufacturer]
%VENDOR%=SMC, NT.5.1
[ControlFlags]
ExcludeFromSelect=*
[SMC]
%DeviceDesc%=DrvInst.Ndi1,USB\VID_0D5C&PID_A002
%DeviceDesc%=DrvInst.Ndi2,USB\VID_083A&PID_3501
[SMC.NT.5.1]
%DeviceDesc%=DrvInstXP.Ndi1,USB\VID_0D5C&PID_A002
%DeviceDesc%=DrvInstXP.Ndi2,USB\VID_083A&PID_3501
[DrvInst.Ndi1]
AddReg=Win9x.Reg1, Win9x2k.Params
;CpyFiles=CopyFile.Sys
DriverVer=08/31/2002,2.6.5.193
[Win9x.Reg1]
HKR,Ndi,DeviceID,0,"USB\VID_0D5C&PID_A002"
HKR,Ndi,CardType,,"PNP"
HKR,,DevLoader,0,"*ndis"
HKR,,DeviceVxDs,0,"smcusb98.sys"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,%ServiceName%(R)
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi,HelpText,,%Help_Text%
[DrvInst.Ndi2]
AddReg=Win9x.Reg2, Win9x2k.Params
;CpyFiles=CopyFile.Sys
DriverVer=08/31/2002,2.6.5.193
[Win9x.Reg2]
HKR,Ndi,DeviceID,0,"USB\VID_083A&PID_3501"
HKR,Ndi,CardType,,"PNP"
HKR,,DevLoader,0,"*ndis"
HKR,,DeviceVxDs,0,"smcusb98.sys"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,%ServiceName%(R)
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi,HelpText,,%Help_Text%
[CopyFile.Sys]
smcusb98.sys,,,2
[DrvInst.ndi1.ME]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=WinMe.Reg, Win9x2k.Params
;CpyFiles=CopyFile.Me.Sys
[DrvInst.ndi2.ME]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=WinMe.Reg, Win9x2k.Params
;CpyFiles=CopyFile.Me.Sys
[DrvInst.ndi1.ME.Services]
AddService=%VENDOR% %ServiceName%(R), 2, FVNETusbMe.Service, FVNETusb.EventLog
[DrvInst.ndi2.ME.Services]
AddService=%VENDOR% %ServiceName%(R), 2, FVNETusbMe.Service, FVNETusb.EventLog
[WinMe.Reg]
HKR,Ndi,Service,0,%VENDOR% %ServiceName%(R)
HKR,,DevLoader,0,*ndis
HKR,,DeviceVxDs,0,smcusb98.sys
HKR,,EnumPropPages,0,"netdi.dll,EnumPropPages"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,%ServiceName%(R)
HKR,Ndi\Interfaces,DefUpper,0,"ndis5"
HKR,Ndi\Interfaces,DefLower,0,"ethernet"
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet"
HKR, Ndi\Install, ndis3, 0, "FVNETusb.ndis5me"
[FVNETusb.ndis5me]
;CpyFiles=CopyFile.Me.Sys
[CopyFile.Me.Sys]
smcusb98.sys
[FVNETusbMe.Service]
DisplayName=%VENDOR% %ServiceName%(R) Service for %DeviceDesc%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%11%\smcusb98.sys
LoadOrderGroup=NDIS
[DrvInst.Ndi1.NTx86]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=Win2k.Reg, Win9x2k.Params
;CpyFiles=CopyFile.2k.Sys
[DrvInst.Ndi1.NTx86.Services]
AddService=%VENDOR% %ServiceName%(R), 2, FVNETusb2k.Service, FVNETusb.EventLog
[DrvInst.Ndi2.NTx86]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=Win2k.Reg, Win9x2k.Params
;CpyFiles=CopyFile.2k.Sys
[DrvInst.Ndi2.NTx86.Services]
AddService=%VENDOR% %ServiceName%(R), 2, FVNETusb2k.Service, FVNETusb.EventLog
[Win2k.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "%VENDOR% %ServiceName%(R)"
[CopyFile.2k.Sys]
smcusb98.sys,,,2
[DrvInstXP.Ndi1.NTx86]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=WinXP.Reg, WinXP.Params
;CpyFiles=CopyFile.XP.Sys
[DrvInstXP.Ndi1.NTx86.Services]
AddService=%VENDOR% %ServiceName%(R), 2, FVNETusbXP.Service, FVNETusb.EventLog
[DrvInstXP.Ndi2.NTx86]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=WinXP.Reg, WinXP.Params
;CpyFiles=CopyFile.XP.Sys
[DrvInstXP.Ndi2.NTx86.Services]
AddService=%VENDOR% %ServiceName%(R), 2, FVNETusbXP.Service, FVNETusb.EventLog
[WinXP.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "%VENDOR% %ServiceName%(R)"
[CopyFile.XP.Sys]
smcusbxp.sys,,,2
[FVNETusb2k.Service]
DisplayName=%VENDOR% %ServiceName%(R) Service for %DeviceDesc%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\smcusb98.sys
LoadOrderGroup=NDIS
[FVNETusbXP.Service]
DisplayName=%VENDOR% %ServiceName%(R) Service for %DeviceDesc%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\smcusbxp.sys
LoadOrderGroup=NDIS
[FVNETusb.EventLog]
AddReg=FVNETusb.AddEventLog.Reg
[FVNETusb.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR, , TypesSupported , 0x00010001, 7
[DestinationDirs]
DefaultDestDir=12 ; Drivers directory
CopyFile.Sys=11
CopyFile.2k.Sys=12
CopyFile.Me.Sys=11
CopyFile.XP.Sys=12
[SourceDisksNames]
1=%DriverDiskName%,,
[SourceDisksFiles]
smcusbxp.sys=1
smcusb98.sys=1
[Win9x2k.Params]
HKR,, UseWZCS, 0,"1"
HKR, Ndi\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, Ndi\params\PreambleType, default, 0, "2"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, "Long"
HKR, Ndi\params\PreambleType\enum, 1, 0, "Short"
HKR, Ndi\params\PreambleType\enum, 2, 0, "Auto"
HKR, , PreambleType, 0, "2"
HKR, Ndi\params\Channel, ParamDesc, 0, "Channel"
HKR, Ndi\params\Channel, default, 0, "10"
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "10"
HKR, Ndi\params\Rate, ParamDesc, 0, "TX Rate (Mbps)"
HKR, Ndi\params\Rate, default, 0, "4"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, 0, 0, "1 Mbps"
HKR, Ndi\params\Rate\enum, 1, 0, "2 Mbps"
HKR, Ndi\params\Rate\enum, 2, 0, "5.5 Mbps"
HKR, Ndi\params\Rate\enum, 3, 0, "11 Mbps"
HKR, Ndi\params\Rate\enum, 4, 0, "Auto"
HKR, , Rate, 0, "4"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, "Operating Mode"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, "Ad-Hoc"
HKR, Ndi\params\Operating_Mode\enum, 1, 0, "Infrastructure"
HKR, , Operating_Mode, 0, "1"
HKR, Ndi\params\InternationalRoaming, ParamDesc, 0, "International Roaming"
HKR, Ndi\params\InternationalRoaming, default, 0, "0"
HKR, Ndi\params\InternationalRoaming, type, 0, "enum"
HKR, Ndi\params\InternationalRoaming\enum, 0, 0, "Disabled (Reg. Domain)"
HKR, Ndi\params\InternationalRoaming\enum, 1, 0, "Enabled (Int. Roaming)"
HKR, , InternationalRoaming,0, "0"
HKR, Ndi\params\ESSID, ParamDesc, 0, "ESSID"
HKR, Ndi\params\ESSID, default, 0, ""
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, ""
HKR, Ndi\params\AuthenticationType, ParamDesc, 0, "Authentication Type"
HKR, Ndi\params\AuthenticationType, default, 0, "2"
HKR, Ndi\params\AuthenticationType, type, 0, "enum"
HKR, Ndi\params\AuthenticationType\enum, 0, 0, "Open System"
HKR, Ndi\params\AuthenticationType\enum, 1, 0, "Shared Key"
HKR, Ndi\params\AuthenticationType\enum, 2, 0, "Auto"
HKR, , AuthenticationType, 0, "2"
HKR, Ndi\params\PowerMgmtMode, ParamDesc, 0, "802.11 Power Save"
HKR, Ndi\params\PowerMgmtMode, type, 0, "enum"
HKR, Ndi\params\PowerMgmtMode, default, 0, "0"
HKR, Ndi\params\PowerMgmtMode\enum, 0, 0, "Disabled"
HKR, Ndi\params\PowerMgmtMode\enum, 1, 0, "Enabled"
HKR, , PowerMgmtMode, 0, "0"
HKR, Ndi\params\WEP_Mode, ParamDesc, 0, "Encrypted Data Mode"
HKR, Ndi\params\WEP_Mode, default, 0, "0"
HKR, Ndi\params\WEP_Mode, type, 0, "enum"
HKR, Ndi\params\WEP_Mode\enum, 0, 0, "Mandatory"
HKR, Ndi\params\WEP_Mode\enum, 1, 0, "Optional"
HKR, , WEP_Mode, 0, "0"
HKR, Ndi\params\EncryptionLevel, ParamDesc, 0, "Encryption Level"
HKR, Ndi\params\EncryptionLevel, type, 0, "enum"
HKR, Ndi\params\EncryptionLevel, default, 0, "0"
HKR, Ndi\params\EncryptionLevel\enum, 0, 0, "None"
HKR, Ndi\params\EncryptionLevel\enum, 1, 0, "64-bit encryption"
HKR, Ndi\params\EncryptionLevel\enum, 2, 0, "128-bit encryption"
HKR, , EncryptionLevel, 0, "0"
HKR, Ndi\params\WEP_KEY_INDEX, ParamDesc, 0, "WEP Key to use"
HKR, Ndi\params\WEP_KEY_INDEX, type, 0, "enum"
HKR, Ndi\params\WEP_KEY_INDEX, default, 0, "0"
HKR, Ndi\params\WEP_KEY_INDEX\enum, 0, 0, "Key #1"
HKR, Ndi\params\WEP_KEY_INDEX\enum, 1, 0, "Key #2"
HKR, Ndi\params\WEP_KEY_INDEX\enum, 2, 0, "Key #3"
HKR, Ndi\params\WEP_KEY_INDEX\enum, 3, 0, "Key #4"
HKR, , WEP_KEY_INDEX, 0, "0"
HKR, Ndi\params\WEP_KEY_1, ParamDesc, 0, "WEP Key #1"
HKR, Ndi\params\WEP_KEY_1, default, 0, "00000000000000000000000000"
HKR, Ndi\params\WEP_KEY_1, type, 0, "edit"
HKR, Ndi\params\WEP_KEY_1, LimitText, 0, "26"
HKR, Ndi\params\WEP_KEY_1, UpperCase, 0, "1"
HKR, , WEP_KEY_1, 0, "00000000000000000000000000"
HKR, Ndi\params\WEP_KEY_2, ParamDesc, 0, "WEP Key #2"
HKR, Ndi\params\WEP_KEY_2, default, 0, "00000000000000000000000000"
HKR, Ndi\params\WEP_KEY_2, type, 0, "edit"
HKR, Ndi\params\WEP_KEY_2, LimitText, 0, "26"
HKR, Ndi\params\WEP_KEY_2, UpperCase, 0, "1"
HKR, , WEP_KEY_2, 0, "00000000000000000000000000"
HKR, Ndi\params\WEP_KEY_3, ParamDesc, 0, "WEP Key #3"
HKR, Ndi\params\WEP_KEY_3, default, 0, "00000000000000000000000000"
HKR, Ndi\params\WEP_KEY_3, type, 0, "edit"
HKR, Ndi\params\WEP_KEY_3, LimitText, 0, "26"
HKR, Ndi\params\WEP_KEY_3, UpperCase, 0, "1"
HKR, , WEP_KEY_3, 0, "00000000000000000000000000"
HKR, Ndi\params\WEP_KEY_4, ParamDesc, 0, "WEP Key #4"
HKR, Ndi\params\WEP_KEY_4, default, 0, "00000000000000000000000000"
HKR, Ndi\params\WEP_KEY_4, type, 0, "edit"
HKR, Ndi\params\WEP_KEY_4, LimitText, 0, "26"
HKR, Ndi\params\WEP_KEY_4, UpperCase, 0, "1"
HKR, , WEP_KEY_4, 0, "00000000000000000000000000"
HKR, Ndi\params\BasicRates, ParamDesc, 0, "Basic Rates"
HKR, Ndi\params\BasicRates, type, 0, "enum"
HKR, Ndi\params\BasicRates, default, 0, "1"
HKR, Ndi\params\BasicRates\enum, 0, 0, "1,2 Mbps"
HKR, Ndi\params\BasicRates\enum, 1, 0, "1,2,5.5,11 Mbps"
HKR, , BasicRates, 0, "1"
HKR, Ndi\params\BeaconPeriod, ParamDesc, 0, "Beacon Period"
HKR, Ndi\params\BeaconPeriod, type, 0, "int"
HKR, Ndi\params\BeaconPeriod, default, 0, "100"
HKR, Ndi\params\BeaconPeriod, min, 0, "20"
HKR, Ndi\params\BeaconPeriod, max, 0, "1000"
HKR, Ndi\params\BeaconPeriod, step, 0, "1"
HKR,, BeaconPeriod, 0, "100"
HKR, Ndi\params\UseWZCS, ParamDesc, 0, "API to use"
HKR, Ndi\params\UseWZCS, type, 0, "enum"
HKR, Ndi\params\UseWZCS, default, 0, "1"
HKR, Ndi\params\UseWZCS\enum, 0, 0, "Custom API"
HKR, Ndi\params\UseWZCS\enum, 1, 0, "WZCS API"
HKR, , UseWZCS, 0, "1"
HKR,Ndi\params\RadioOnOff, ParamDesc, 0, "Radio On/Off"
HKR,Ndi\params\RadioOnOff, type, 0, "enum"
HKR,Ndi\params\RadioOnOff, default, 0, "1"
HKR,Ndi\params\RadioOnOff\enum, 0, 0, "OFF"
HKR,Ndi\params\RadioOnOff\enum, 1, 0, "ON"
HKR,, RadioOnOff, 0, "1"
[WinXP.Params]
HKR,, UseWZCS, 0,"1"
HKR, , Operating_Mode, 0, "1"
HKR, , ESSID, 0, ""
HKR, , EncryptionLevel, 0, "0"
HKR, Ndi\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, Ndi\params\PreambleType, default, 0, "2"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, "Long"
HKR, Ndi\params\PreambleType\enum, 1, 0, "Short"
HKR, Ndi\params\PreambleType\enum, 2, 0, "Auto"
HKR, , PreambleType, 0, "2"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate (Mbps)"
HKR, Ndi\params\Rate, default, 0, "4"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, 0, 0, "1"
HKR, Ndi\params\Rate\enum, 1, 0, "2"
HKR, Ndi\params\Rate\enum, 2, 0, "5.5"
HKR, Ndi\params\Rate\enum, 3, 0, "11"
HKR, Ndi\params\Rate\enum, 4, 0, "Auto"
HKR, , Rate, 0, "4"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\PowerMgmtMode, ParamDesc, 0, "802.11 Power Save"
HKR, Ndi\params\PowerMgmtMode, type, 0, "enum"
HKR, Ndi\params\PowerMgmtMode, default, 0, "0"
HKR, Ndi\params\PowerMgmtMode\enum, 0, 0, "Disabled"
HKR, Ndi\params\PowerMgmtMode\enum, 1, 0, "Enabled"
HKR, , PowerMgmtMode, 0, "0"
HKR, Ndi\params\UseWZCS, ParamDesc, 0, "API to use"
HKR, Ndi\params\UseWZCS, type, 0, "enum"
HKR, Ndi\params\UseWZCS, default, 0, "1"
HKR, Ndi\params\UseWZCS\enum, 0, 0, "Custom API"
HKR, Ndi\params\UseWZCS\enum, 1, 0, "WZCS API"
HKR, , UseWZCS, 0, "1"
[Strings]
VENDOR="SMC"
DeviceDesc="SMC2662W V.2 EZ Connect 11 Mbps Wireless USB Adapter"
ServiceName="SMC2662W V.2 EZ Connect 11 Mbps Wireless USB Adapter"
DriverDiskName="SMC2662W V.2 EZ Connect 11 Mbps Wireless USB Adapter Installation Disk"
Help_Text="SMC2662W V.2 EZ Connect 11 Mbps Wireless USB Adapter lets you set up easily and operate a Wireless LAN compliant with 802.11 Standard. It operates in the license free 2.4 GHz ISM band and achieves a peak data rate of 11Mbps."
