
[Version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Realtek% ;;
CatalogFile.NT=net8192du.cat ;; for WHQL certified
DriverVer=08/16/2011,1002.01.0816.2011
[Manufacturer]
%Realtek%=Realtek,NTx86
%PCI%=PCI,NTx86
%TRENDnet%=TRENDnet,NTx86
%Abocom%=Abocom,NTx86
[ControlFlags]
ExcludeFromSelect=*
[Realtek.NTx86]
%RTL8192du.DeviceDesc%=RTL8192du.ndi, USB\VID_0BDA&PID_8194
%RTL8192du.DeviceDesc%=RTL8192du.ndi, USB\VID_0BDA&PID_8111
%RTL8192du0.DeviceDesc%=RTL8192du.ndi, USB\VID_0BDA&PID_8193&MI_00
%RTL8192du1.DeviceDesc%=RTL8192du1.ndi, USB\VID_0BDA&PID_8193&MI_01
%RTL8192du2.DeviceDesc%=RTL8192du.ndi, USB\VID_0BDA&PID_0193&MI_00
%RTL8192du3.DeviceDesc%=RTL8192du1.ndi, USB\VID_0BDA&PID_0193&MI_01
[PCI.NTx86]
%PCI_Abocom_du0.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_AB2C&MI_00
%PCI_Abocom_du1.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_AB2C&MI_01
%PCI_3_du0.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_4903&MI_00
%PCI_3_du1.DeviceDesc%=RTL8192du1.ndi, USB\VID_2019&PID_4903&MI_01
%PCI_4_du0.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_4904&MI_00
%PCI_4_du1.DeviceDesc%=RTL8192du1.ndi, USB\VID_2019&PID_4904&MI_01
%PCIWIDI.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_AB2D
[TRENDnet.NTx86]
%TRENDnet_du.DeviceDesc%=RTL8192du.ndi, USB\VID_20F4&PID_664B
[Abocom.NTx86]
%Abocom0.DeviceDesc%=RTL8192du.ndi, USB\VID_07B8&PID_8193&MI_00
%Abocom1.DeviceDesc%=RTL8192du1.ndi, USB\VID_07B8&PID_8193&MI_01
[Realtek.NTamd64]
%RTL8192du.DeviceDesc%=RTL8192du.ndi, USB\VID_0BDA&PID_8194
%RTL8192du.DeviceDesc%=RTL8192du.ndi, USB\VID_0BDA&PID_8111
%RTL8192du0.DeviceDesc%=RTL8192du.ndi, USB\VID_0BDA&PID_8193&MI_00
%RTL8192du1.DeviceDesc%=RTL8192du1.ndi, USB\VID_0BDA&PID_8193&MI_01
[PCI.NTamd64]
%PCI_Abocom_du0.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_AB2C&MI_00
%PCI_Abocom_du1.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_AB2C&MI_01
%PCI_3_du0.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_4903&MI_00
%PCI_3_du1.DeviceDesc%=RTL8192du1.ndi, USB\VID_2019&PID_4903&MI_01
%PCI_4_du0.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_4904&MI_00
%PCI_4_du1.DeviceDesc%=RTL8192du1.ndi, USB\VID_2019&PID_4904&MI_01
%PCIWIDI.DeviceDesc%=RTL8192du.ndi, USB\VID_2019&PID_AB2D
[TRENDnet.NTamd64]
%TRENDnet_du.DeviceDesc%=RTL8192du.ndi, USB\VID_20F4&PID_664B
[Abocom.NTamd64]
%Abocom0.DeviceDesc%=RTL8192du.ndi, USB\VID_07B8&PID_8193&MI_00
%Abocom1.DeviceDesc%=RTL8192du1.ndi, USB\VID_07B8&PID_8193&MI_01
[RTL8192du.ndi.NT]
AddReg=RTL8192du.nt5.reg, RTL8192du.common.reg, RTLWLAN.reg, RxReorder_MAC0.reg
Characteristics=0x84
BusType=15
;CpyFiles=RTL8192du.CopyFiles
[RTL8192du.ndi.NT.Services]
AddService=RTL8192du, 2, RTL8192du.nt5.Service, RTL8192du.nt5.EventLog
[RTL8192du1.ndi.NT]
AddReg=RTL8192du.nt5.reg, RTL8192du.common.reg, RTLWLAN.reg, ConcurrentMode.reg, RxReorder_MAC1.reg
Characteristics=0x84
BusType=15
;CpyFiles=RTL8192du.CopyFiles
[RTL8192du1.ndi.NT.Services]
AddService=RTL8192du, 2, RTL8192du.nt5.Service, RTL8192du.nt5.EventLog
[RTL8192du.nt5.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, Service, 0, "RTL8192du"
[RTL8192du.nt5.Service]
DisplayName=%RTL8192du.DeviceDesc%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERRVICE_DEMAND_START%
ErrorControl=1 ; %SERRVICE_ERROR_NORMAL%
ServiceBinary=%12%\RTL8192du.sys
LoadOrderGroup=NDIS
[RTL8192du.nt5.EventLog]
AddReg=RTL8192du.nt5.AddEventLog.reg
[RTL8192du.nt5.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported , 0x00010001, 7
[RTL8192du.common.reg]
HKR,Ndi\params\LedCtrl, ParamDesc, 0, %LED_CONTROL_STR%
HKR,Ndi\params\LedCtrl, type, 0, "enum"
HKR,Ndi\params\LedCtrl, default, 0, "1"
HKR,Ndi\params\LedCtrl\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\LedCtrl\enum, "1", 0, %ENABLE_STR%
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"
HKR,Ndi\params\WiFi11bIbss, ParamDesc, 0, %WIFI_IBSS_STR%
HKR,Ndi\params\WiFi11bIbss, type, 0, "enum"
HKR,Ndi\params\WiFi11bIbss, default, 0, "0"
HKR,Ndi\params\WiFi11bIbss\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\WiFi11bIbss\enum, "1", 0, %ENABLE_STR%
HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"
HKR,Ndi\params\bRateAdaptive, ParamDesc, 0, %RATE_ADAPTIVE_STR%
HKR,Ndi\params\bRateAdaptive, type, 0, "enum"
HKR,Ndi\params\bRateAdaptive, default, 0, "1"
HKR,Ndi\params\bRateAdaptive\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\bRateAdaptive\enum, "1", 0, %ENABLE_STR%
HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"
HKR,Ndi\params\QoS, ParamDesc, 0, %QOS_STR%
HKR,Ndi\params\QoS, type, 0, "enum"
HKR,Ndi\params\QoS, default, 0, "1"
HKR,Ndi\params\QoS\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\QoS\enum, "1", 0, %ENABLE_STR%
HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"
HKR,Ndi\params\WiFiConfg, ParamDesc, 0, %WiFiConfg_STR%
HKR,Ndi\params\WiFiConfg, type, 0, "enum"
HKR,Ndi\params\WiFiConfg, default, 0, "0"
HKR,Ndi\params\WiFiConfg\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\WiFiConfg\enum, "1", 0, %ENABLE_STR%
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"
HKR,Ndi\params\CcxRm, ParamDesc, 0, %CCX_RM_STR%
HKR,Ndi\params\CcxRm, type, 0, "enum"
HKR,Ndi\params\CcxRm, default, 0, "1"
HKR,Ndi\params\CcxRm\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\CcxRm\enum, "1", 0, %ENABLE_STR%
HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"
HKR,Ndi\params\CcxOffLineDurUpLimit, ParamDesc, 0, %CCX_OFF_LINE_DUR_UP_LIMIT_STR%
HKR,Ndi\params\CcxOffLineDurUpLimit, type, 0, "word"
HKR,Ndi\params\CcxOffLineDurUpLimit, default, 0, "0"
HKR,Ndi\params\CcxOffLineDurUpLimit, min, 0, "0"
HKR,Ndi\params\CcxOffLineDurUpLimit, max, 0, "65535"
HKR,Ndi\params\CcxOffLineDurUpLimit, step, 0, "1"
HKR,Ndi\params\CcxOffLineDurUpLimit, base, 0, "10"
HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"
[RTLWLAN.reg]
HKR,Ndi\params\SSID, ParamDesc, 0, %SSID_STR%
HKR,Ndi\params\SSID, type, 0, "edit"
HKR,Ndi\params\SSID, default, 0, "ANY"
HKR,Ndi\params\SSID, LimitText, 0, "32"
HKR,defaults,SSID,0,"ANY"
HKR,,SSID,0,"ANY"
HKR,Ndi\params\Channel, ParamDesc, 0, %CHANNEL_STR%
HKR,Ndi\params\Channel, type, 0, "int"
HKR,Ndi\params\Channel, default, 0, "1"
HKR,Ndi\params\Channel, Min, 0, "1"
HKR,Ndi\params\Channel, Max, 0, "14"
HKR,Ndi\params\Channel, Step, 0, "1"
HKR,Ndi\params\Channel, Base, 0, "10"
HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"
HKR,,Channel5G,0,"36"
HKR,Ndi\params\NetworkType, ParamDesc, 0, %NETWORK_TYPE_STR%
HKR,Ndi\params\NetworkType, type, 0, "enum"
HKR,Ndi\params\NetworkType, default, 0, "1"
HKR,Ndi\params\NetworkType\enum, "0", 0, %AD_HOC_STR%
HKR,Ndi\params\NetworkType\enum, "1", 0, %INFRASTRUCTURE_STR%
HKR,Ndi\params\NetworkType\enum, "2", 0, %AUTO_SELECT%
HKR,defaults,NetworkType,0,"1"
HKR,,NetworkType,0,"1"
HKR,NDI\params\PowerSaveMode, ParamDesc, 0, %POWER_SAVE_STR%
HKR,NDI\params\PowerSaveMode, type, 0, "enum"
HKR,Ndi\params\PowerSaveMode, default, 0, "0"
HKR,NDI\params\PowerSaveMode\enum, "0", 0, %CAM_STR%
HKR,NDI\params\PowerSaveMode\enum, "1", 0, %MAX_PSP_STR%
HKR,NDI\params\PowerSaveMode\enum, "2", 0, %Fast_PSP_STR%
HKR,defaults,PowerSaveMode,0,"0"
HKR,,PowerSaveMode,0,"0"
HKR,Ndi\params\StaUapsd, ParamDesc, 0, %WMM_APSD%
HKR,Ndi\params\StaUapsd, type, 0, "enum"
HKR,Ndi\params\StaUapsd, default, 0, "0"
HKR,Ndi\params\StaUapsd\enum, "0", 0, %No_AC_STR%
HKR,Ndi\params\StaUapsd\enum, "15", 0, %ALL_AC_STR%
HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"
HKR,Ndi\params\PSPXlinkMode, ParamDesc, 0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode, type, 0, "enum"
HKR,Ndi\params\PSPXlinkMode, default, 0, "0"
HKR,Ndi\params\PSPXlinkMode\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum, "1", 0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"
HKR,defaults,bWiDiPairingEnable,0,"0"
HKR,,bWiDiPairingEnable,0,"0"
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"
HKR,defaults,bFwCtrlLPS,0,"3"
HKR,,bFwCtrlLPS,0,"3"
HKR,,LPSIntvl,0,"5"
HKR,,bEarlymodeEnable,,"1"
HKR,Ndi\params\UsbRxAggMode, ParamDesc, 0, %RX_AGG_MODE_STR%
HKR,Ndi\params\UsbRxAggMode, type, 0, "enum"
HKR,Ndi\params\UsbRxAggMode, default, 0, "0"
HKR,Ndi\params\UsbRxAggMode\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\UsbRxAggMode\enum, "1", 0, %RX_AGG_MODE_PAGE_STR%
HKR,Ndi\params\UsbRxAggMode\enum, "2", 0, %RX_AGG_MODE_BLOCK_STR%
HKR,Ndi\params\UsbRxAggMode\enum, "3", 0, %RX_AGG_MODE_MIXED_STR%
HKR,defaults,UsbRxAggMode,0,"2"
HKR,,UsbRxAggMode,0,"2"
HKR,Ndi\params\UsbRxAggBlockCount, ParamDesc, 0, %RX_AGG_USB_BLOCK_STR%
HKR,Ndi\params\UsbRxAggBlockCount, type, 0, "int"
HKR,Ndi\params\UsbRxAggBlockCount, default, 0, "1"
HKR,Ndi\params\UsbRxAggBlockCount, Min, 0, "0"
HKR,Ndi\params\UsbRxAggBlockCount, Max, 0, "255"
HKR,Ndi\params\UsbRxAggBlockCount, Step, 0, "1"
HKR,Ndi\params\UsbRxAggBlockCount, Base, 0, "10"
HKR,defaults,UsbRxAggBlockCount,0,"18"
HKR,,UsbRxAggBlockCount,0,"18"
HKR,Ndi\params\UsbRxAggBlockTimeout, ParamDesc, 0, %RX_AGG_USB_TIMEOUT_STR%
HKR,Ndi\params\UsbRxAggBlockTimeout, type, 0, "int"
HKR,Ndi\params\UsbRxAggBlockTimeout, default, 0, "1"
HKR,Ndi\params\UsbRxAggBlockTimeout, Min, 0, "1"
HKR,Ndi\params\UsbRxAggBlockTimeout, Max, 0, "15"
HKR,Ndi\params\UsbRxAggBlockTimeout, Step, 0, "1"
HKR,Ndi\params\UsbRxAggBlockTimeout, Base, 0, "10"
HKR,defaults,UsbRxAggBlockTimeout,0,"7"
HKR,,UsbRxAggBlockTimeout,0,"7"
HKR,Ndi\params\UsbRxAggPageCount, ParamDesc, 0, %RX_AGG_DMA_PAGE_STR%
HKR,Ndi\params\UsbRxAggPageCount, type, 0, "int"
HKR,Ndi\params\UsbRxAggPageCount, default, 0, "1"
HKR,Ndi\params\UsbRxAggPageCount, Min, 0, "0"
HKR,Ndi\params\UsbRxAggPageCount, Max, 0, "255"
HKR,Ndi\params\UsbRxAggPageCount, Step, 0, "1"
HKR,Ndi\params\UsbRxAggPageCount, Base, 0, "10"
HKR,defaults,UsbRxAggPageCount,0,"1"
HKR,,UsbRxAggPageCount,0,"1"
HKR,Ndi\params\UsbRxAggPageTimeout, ParamDesc, 0, %RX_AGG_DMA_TIMEOUT_STR%
HKR,Ndi\params\UsbRxAggPageTimeout, type, 0, "int"
HKR,Ndi\params\UsbRxAggPageTimeout, default, 0, "1"
HKR,Ndi\params\UsbRxAggPageTimeout, Min, 0, "1"
HKR,Ndi\params\UsbRxAggPageTimeout, Max, 0, "15"
HKR,Ndi\params\UsbRxAggPageTimeout, Step, 0, "1"
HKR,Ndi\params\UsbRxAggPageTimeout, Base, 0, "10"
HKR,defaults,UsbRxAggPageTimeout,0,"5"
HKR,,UsbRxAggPageTimeout,0,"5"
HKR,Ndi\params\UsbTxAggMode, ParamDesc, 0, %TX_AGG_MODE_STR%
HKR,Ndi\params\UsbTxAggMode, type, 0, "enum"
HKR,Ndi\params\UsbTxAggMode, default, 0, "0"
HKR,Ndi\params\UsbTxAggMode\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\UsbTxAggMode\enum, "1", 0, %ENABLE_STR%
HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"
HKR,Ndi\params\UsbTxAggDescNum, ParamDesc, 0, %TX_AGG_DESC_PER_OUT_STR%
HKR,Ndi\params\UsbTxAggDescNum, type, 0, "int"
HKR,Ndi\params\UsbTxAggDescNum, default, 0, "0"
HKR,Ndi\params\UsbTxAggDescNum, Min, 0, "0"
HKR,Ndi\params\UsbTxAggDescNum, Max, 0, "15"
HKR,Ndi\params\UsbTxAggDescNum, Step, 0, "1"
HKR,Ndi\params\UsbTxAggDescNum, Base, 0, "10"
HKR,defaults,UsbTxAggDescNum,0,"4"
HKR,,UsbTxAggDescNum,0,"4"
[ConcurrentMode.reg]
HKR,Ndi\params\TwoStaConcurrentMode, ParamDesc, 0, %TWO_STA_CONCURRENT_MODE%
HKR,Ndi\params\TwoStaConcurrentMode, type, 0, "enum"
HKR,Ndi\params\TwoStaConcurrentMode, default, 0, "1"
HKR,Ndi\params\TwoStaConcurrentMode\enum, "0", 0, %SECONDARY_DISABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum, "1", 0, %SECONDARY_ENABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum, "2", 0, %SECONDARY_AUTO%
HKR,defaults,TwoStaConcurrentMode,0,"0"
HKR,,TwoStaConcurrentMode,0,"0"
[RxReorder_MAC0.reg]
HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"
[RxReorder_MAC1.reg]
HKR,defaults,RxReorder,0,"0"
HKR,,RxReorder,0,"0"
[RTL8192du.CopyFiles]
RTL8192du.sys,,,2
[DestinationDirs]
RTL8192du.CopyFiles=12
[SourceDisksFiles]
RTL8192du.sys=1
[SourceDisksNames]
1=%DISKNAME%,,,
[Strings]
SSID_STR="SSID"
CHANNEL_STR="Channel"
NETWORK_TYPE_STR="Network Type"
LED_CONTROL_STR="LED Control"
POWER_SAVE_STR="Power Save Mode"
WIFI_IBSS_STR="IBSS Default 11b Mode"
RATE_ADAPTIVE_STR="Rate Adaptive"
QOS_STR="QoS"
WiFiConfg_STR="WiFiConfg"
WMM_APSD="WMM APSD"
CCX_RM_STR="CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR="CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR="Forced Priority"
HW_PARA_STR="Init from HwParaFile"
THREE_WIRE_MODE_STR="Three Wire Programming Mode"
BOARD_TYPE_STR="Board Type"
PROTECTION_MODE_STR="Protection Mode"
TPC_STR="Transmit Power Control"
TPC_POLARITY_STR="TPC Polarity Select"
HIGH_POWER_STR="High Power Mechanism"
INIT_GAIN_STR="Initial Gain State"
CW_MAX_MIN_STR="Contention Window"
PSP_XLINK_STR="PSP XLink Mode"
DISABLE_STR="Disable"
ENABLE_STR="Enable"
AD_HOC_STR="Ad Hoc"
INFRASTRUCTURE_STR="Infrastructure"
AUTO_SELECT="Auto select"
RX_REORDER_STR="Rx Reorder"
CAM_STR="CAM"
MAX_PSP_STR="MAX_PSP"
Fast_PSP_STR="Fast_PSP"
NO_AC_STR="No AC (Disable)"
ALL_AC_STR="ALL AC"
RX_AGG_MODE_STR="Rx Aggregation Mode"
RX_AGG_MODE_BLOCK_STR="Rx Agg USB Block Mode"
RX_AGG_MODE_PAGE_STR="Rx Agg DMA Page Mode"
RX_AGG_MODE_MIXED_STR="Rx Agg USB and Page Mixed Mode"
RX_AGG_USB_BLOCK_STR="Rx Agg USB Block Threshold"
RX_AGG_USB_TIMEOUT_STR="Rx Agg USB Timeout"
RX_AGG_DMA_PAGE_STR="Rx Agg DMA Page Threshold"
RX_AGG_DMA_TIMEOUT_STR="Rx Agg DMA Timeout"
TX_AGG_MODE_STR="Tx Aggregation Mode"
TX_AGG_DESC_PER_OUT_STR="Tx Agg Number of descriptor per bulk out"
TWO_STA_CONCURRENT_MODE="Two STA Concurrent Mode"
SECONDARY_DISABLE="Secondary client Disable"
SECONDARY_ENABLE="Secondary Client Enable"
SECONDARY_AUTO="Secondary Client Auto Select"
Realtek="Realtek Semiconductor Corp."
PCI="PLANEX COMMUNICATIONS INC"
TRENDnet="TRENDnet"
Abocom="AboCom System, Inc"
DISKNAME="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
RTL8192du.DeviceDesc="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du.DeviceDesc.DispName="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du0.DeviceDesc="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du0.DeviceDesc.DispName="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du1.DeviceDesc="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du1.DeviceDesc.DispName="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du2.DeviceDesc="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du2.DeviceDesc.DispName="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du3.DeviceDesc="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du3.DeviceDesc.DispName="Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
PCIWIDI.DeviceDesc="MZK-WD300DH"
PCIWIDI.DeviceDesc.DispName="MZK-WD300DH"
PCI_Abocom_du0.DeviceDesc="GW-USDual300 MAC0"
PCI_Abocom_du0.DeviceDesc.DispName="GW-USDual300 MAC0"
PCI_Abocom_du1.DeviceDesc="GW-USDual300 MAC1"
PCI_Abocom_du1.DeviceDesc.DispName="GW-USDual300 MAC1"
PCI_3_du0.DeviceDesc="GW-USFang300 MAC0"
PCI_3_du0.DeviceDesc.DispName="GW-USFang300 MAC0"
PCI_3_du1.DeviceDesc="GW-USFang300 MAC1"
PCI_3_du1.DeviceDesc.DispName="GW-USFang300 MAC1"
PCI_4_du0.DeviceDesc="GW-USUltra300 MAC0"
PCI_4_du0.DeviceDesc.DispName="GW-USUltra300 MAC0"
PCI_4_du1.DeviceDesc="GW-USUltra300 MAC1"
PCI_4_du1.DeviceDesc.DispName="GW-USUltra300 MAC1"
TRENDnet_du.DeviceDesc="TRENDnet 300Mbps Dual Band Wireless USB Adapter"
TRENDnet_du.DeviceDesc.DispName="TRENDnet 300Mbps Dual Band Wireless USB Adapter"
Abocom0.DeviceDesc="802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom0.DeviceDesc.DispName="802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom1.DeviceDesc="802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
Abocom1.DeviceDesc.DispName="802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
