
[Version]
DriverVer=03/29/2004, 1.0.14
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%DRV_PROVIDER_STR%
CatalogFile.NT=WlanUIG.cat
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%MANUFACTURER_STR%=DeviceList
[DeviceList]
%WLAN_USB_DESC_STR%=WLAN_USB1, USB\VID_0707&PID_EE06
[WLAN_USB1] ; Win9x
AddReg=WLAN_USB1_REG, COMMON_USB_REG, COMMON_NDIS_REG_9x, COMMON_REG
;CpyFiles=WLAN_USB_DRIVER_COPY
[WLAN_USB1.NT] ; Win2k
AddReg=WLAN_USB1_REG, COMMON_USB_REG, COMMON_NDIS_REG_NT, COMMON_REG
;CpyFiles=WLAN_USB_DRIVER_COPY_NT
BusType=15 ;USB
Characteristics= 0x84
[WLAN_USB1.NT.Services]
AddService= "WlanUIG", 2, WLAN_DRIVER_USB_SERVICE, WLAN_USB_DRIVER_EVENTLOG
[WLAN_USB1_REG]
HKR,Ndi,DeviceID,0,"USB\VID_0707&PID_EE06"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%WLAN_USB_DESC_STR%
[WLAN_DRIVER_USB_SERVICE]
DisplayName=%WLAN_USB_SERVICE_STR%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\2862w.sys
LoadOrderGroup=NDIS
[WLAN_USB_DRIVER_EVENTLOG]
AddReg=WLAN_USB_DRIVER_EVENTLOG_REG
[WLAN_USB_DRIVER_EVENTLOG_REG]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_USB_REG]
HKR, ,WLANIOC ,0 ,"XG-300"
HKR,NDI ,Service ,0 ,"WlanUIG"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"15"
HKR, ,DeviceVxDs ,0 ,"2862w.sys"
[COMMON_NDIS_REG_NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON_NDIS_REG_9x]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"WlanUIG"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_REG]
HKR, ,RTSThresh,0,2347
HKR,defaults ,RTSThresh,0,2347
HKR,Ndi\params\RTSThresh,default,0,2347
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2347
HKR,NDI\params\RTSThresh,step,0,1
HKR, ,FragThresh,0,2346
HKR,defaults ,FragThresh,0,2346
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
HKR, ,ShortRetryLimit,0,7
HKR,defaults ,ShortRetryLimit,0,7
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR, ,LongRetryLimit,0,4
HKR,defaults ,LongRetryLimit,0,4
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR, ,ConfigProfile,0,256
HKR,defaults ,ConfigProfile,0,256
HKR,NDI\params\ConfigProfile,default,0,256
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,,enum
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
HKR, ,NitroMode,0,1
HKR,defaults ,NitroMode,0,1
HKR,NDI\params\NitroMode,default,0,1
HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
HKR,NDI\params\NitroMode,type,,enum
HKR,NDI\params\NitroMode,flag,1,30,00,00,00
HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
HKR, ,PSMode,0,1
HKR,defaults ,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR, ,SSID,0,"ANY"
HKR,defaults ,SSID,0,"ANY" ;Default value is "any"
HKR, ,NetworkType,0,1
HKR,defaults ,NetworkType,0,1 ;Infrasturcture
HKR, ,NitroTime,0,1400
HKR, defaults,NitroTime,0,1400
HKR, NDI\params\NitroTime,default,0,1400
HKR, NDI\params\NitroTime,ParamDesc,0,"NitroTime"
HKR, NDI\params\NitroTime,type ,0,int
HKR, NDI\params\NitroTime,min ,0,0
HKR, NDI\params\NitroTime,max ,0,5000
HKR, NDI\params\NitroTime,step ,0,10
HKR,NDI\params\PpePdlpEnable,default,0,1
HKR,NDI\params\PpePdlpEnable,ParamDesc,,%PPE_PDLP%
HKR,NDI\params\PpePdlpEnable,type,,enum
HKR,NDI\params\PpePdlpEnable,flag,1,30,00,00,00
HKR,NDI\params\PpePdlpEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpePdlpEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpeCompressEnable,default,0,1
HKR,NDI\params\PpeCompressEnable,ParamDesc,,%PPE_COMPRESS%
HKR,NDI\params\PpeCompressEnable,type,,enum
HKR,NDI\params\PpeCompressEnable,flag,1,30,00,00,00
HKR,NDI\params\PpeCompressEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpeCompressEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpeConcatEnable,default,0,1
HKR,NDI\params\PpeConcatEnable,ParamDesc,,%PPE_CONCAT%
HKR,NDI\params\PpeConcatEnable,type,,enum
HKR,NDI\params\PpeConcatEnable,flag,1,30,00,00,00
HKR,NDI\params\PpeConcatEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpeConcatEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpePiggyBackEnable,default,0,1
HKR,NDI\params\PpePiggyBackEnable,ParamDesc,,%PPE_PIGGYBACK%
HKR,NDI\params\PpePiggyBackEnable,type,,enum
HKR,NDI\params\PpePiggyBackEnable,flag,1,30,00,00,00
HKR,NDI\params\PpePiggyBackEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpePiggyBackEnable\enum,1,,%ON_STR%
[DestinationDirs]
WLAN_USB_DRIVER_COPY_NT=12 ; Win2k=%windir%\system32\drivers
WLAN_USB_DRIVER_COPY=11 ; Win9x=%windir%\system
[WLAN_USB_DRIVER_COPY]
2862w.sys
[WLAN_USB_DRIVER_COPY_NT]
2862w.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
W2862w.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
2862w.sys=1
[Strings]
DRV_PROVIDER_STR="SMC"
MANUFACTURER_STR="SMC Networks, Inc."
WLAN_USB_SERVICE_STR="SMC 802.11g 2862W-G Driver"
INSTALL_DISK_STR="54Mbps WLAN Driver & Utility disk"
WLAN_USB_DESC_STR="SMC2862W-G 54Mbps Wireless USB 2.0 Adapter"
ON_STR="On"
OFF_STR="Off"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WiFi"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"
NITRO_MODE="Nitro Mode"
PPE_PDLP="Direct Link"
PPE_COMPRESS="Compression"
PPE_CONCAT="Concatenation"
PPE_PIGGYBACK="PiggyBack"
