
[Version]
DriverVer=08/07/2003, 2.1.5.0
Signature="$Windows NT$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=PRISMA00.cat
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%A001_DESC_STR%=PRISM_A001, PCI\VEN_1260&DEV_3890&SUBSYS_200416BE
[PRISM_A001.NT] ; Win2k
AddReg=PRISM_A001.reg, COMMON_A00.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT, PRISM_DOM.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_A001.NT.Services]
AddService="PRISM_A00", 2, PRISM_DRIVER_A00.Service, PRISM_DRIVER.EventLog
[PRISM_A001.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_A001.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_200416BE"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%A001_DESC_STR%
[PRISM_COINSTALL.reg.NT]
[PRISM_DRIVER_A00.Service]
DisplayName=%A00_SERVICE_STR%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\PRISMA00.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_A00.reg]
HKR,NDI ,Service ,0 ,"PRISM_A00"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"PRISMA00.sys"
HKR, ,CardBusBridgeLatencyTimer ,0 ,"32"
HKR, ,CardBusBridgeCacheLineSize ,0 ,"8"
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,NDI\params\RTSThresh,0,2347
HKR,Ndi\params\RTSThresh,default,0,2347
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2347
HKR,NDI\params\RTSThresh,step,0,1
HKR,NDI\params\RTSThresh,optional,0,1
HKR,defaults,NDI\params\FragThresh,0,2346
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
HKR,NDI\params\FragThresh,optional,0,1
HKR,defaults,NDI\params\ShortRetryLimit,0,7
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR,NDI\params\ShortRetryLimit,optional,0,1
HKR,defaults,NDI\params\LongRetryLimit,0,4
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR,NDI\params\LongRetryLimit,optional,0,1
HKR,,ConfigProfile,0,2 ; Mixed Long
HKR,defaults,NDI\params\ConfigProfile,0,2 ; Mixed Long
HKR,NDI\params\ConfigProfile,default,0,2 ; Mixed long
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,,enum
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
HKR,NDI\params\ConfigProfile,optional,0,1
HKR,,NitroMode,0,"1"
HKR,defaults,NDI\params\NitroMode,0,1
HKR,NDI\params\NitroMode,default,0,1
HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
HKR,NDI\params\NitroMode,type,,enum
HKR,NDI\params\NitroMode,flag,1,30,00,00,00
HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
HKR,NDI\params\NitroMode,optional,0,1
HKR,,PSMode,0,1
HKR,defaults,NDI\params\PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode,optional,0,1
HKR,,DSFreq,0,"2462000"
[DestinationDirs]
DefaultDestDir=11 ; %windir%\system32
PRISM_DRIVER.copy.NT=12 ; %windir%\system32\drivers
PRISM_DOM.copy=10 ; %windir% all OS
[PRISM_COINSTALL.copy.NT]
[PRISM_DRIVER.copy.NT]
PRISMA00.sys
[PRISM_APPLET.copy.NT]
[PRISM_DOM.copy]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles.X86] ; XP
PRISMA00.sys=1
[Strings]
VER_VENDOR_STR="CREATIX"
VER_VENDOR_NAME_STR="CREATIX"
INSTALL_DISK_STR ="CREATIX Wireless LAN Install Disk"
A001_DESC_STR="CREATIX 802.11g Adapter"
A00_SERVICE_STR="CREATIX 802.11g Driver"
ON_STR="On"
OFF_STR="Off"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WiFi"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"
NITRO_MODE="Nitro Mode"

