
[Version]
DriverVer=03/12/2005, 2.00.01.0000
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
CatalogFile=NetRTUSB.CAT ;for WHQL certified
[ControlFlags]
ExcludeFromSelect=VID_2001&PID_3C00
[Manufacturer]
%V_Provider%=Adapters
[Adapters]
%NetRTUSB.DeviceDesc%=NetRTUSB.ndi, USB\VID_2001&PID_3C00
[NetRTUSB.ndi]
AddReg=Common.reg, NetRTUSB.ndi.reg
;CpyFiles=win9x.CopyFiles
[NetRTUSB.ndi.NT]
AddReg=Common.reg, NetRTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15;USB
;CpyFiles=NT.CopyFiles
[NetRTUSB.ndi.NT.Services]
AddService=rt2500usb, 2, NetRTUSB.Service, common.EventLog
[Common.reg]
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
HKR, , Radio, 0, "0"
HKR, NDI\params\Radio, ParamDesc, 0, "Radio On/Off"
HKR, NDI\params\Radio, type, 0, "enum"
HKR, NDI\params\Radio, default, 0, "0"
HKR, NDI\params\Radio\enum, 1, 0, "Disable"
HKR, NDI\params\Radio\enum, 0, 0, "Enable"
HKR, , AutoReconnect, 0, "1"
HKR, NDI\params\AutoReconnect, ParamDesc, 0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect, type, 0, "enum"
HKR, NDI\params\AutoReconnect, default, 0, "1"
HKR, NDI\params\AutoReconnect\enum, 0, 0, "Disable"
HKR, NDI\params\AutoReconnect\enum, 1, 0, "Enable"
HKR, , ShowHiddenSSID, 0, "1" ; 0=disable(default), 1=enable
HKR, , ConfigSelect, 0, "0" ;0=RaConfig, 1=ZeroConfig
HKR, , CountryRegion, 0, "0"
HKR, , WirelessMode, 0, "0"
HKR, , TXBurst, 0, "0"
HKR, , ShortSlot, 0, "0"
HKR, , TurboRate, 0, "0"
HKR, , AdhocOfdm, 0, "0"
HKR, , BGProtection, 0, "0"
HKR, , VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, Default, VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, Default, SSID, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, ParamDesc, 0, "SSID"
HKR, NDI\params\SSID, type, 0, "edit"
HKR, NDI\params\SSID, limitText, 0, "32"
HKR, NDI\params\SSID, default, 0, %SSID_DEF_STR%
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, Default, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0, 0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, , NetworkAddress, 0, ""
HKR, Default, NetworkAddress, 0, ""
HKR, NDI\params\NetworkAddress, ParamDesc, 0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, limitText, 0, "12"
HKR, NDI\params\NetworkAddress, default, 0, ""
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Saving Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum, 1, 0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum, 2, 0, "Fast_PSP (Power Save Mode)"
HKR, , ACPowerCam, 0, "0"
HKR, Default, ACPowerCam, 0, "0"
HKR, NDI\params\ACPowerCam, ParamDesc, 0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam, type, 0, "enum"
HKR, NDI\params\ACPowerCam, default, 0, "0"
HKR, NDI\params\ACPowerCam\enum, 0, 0, "Disable"
HKR, NDI\params\ACPowerCam\enum, 1, 0, "Enable"
HKR, , PreambleType, 0, "2"
HKR, Default, PreambleType, 0, "2"
HKR, , RTSThresh, 0, "2347"
HKR, Default, RTSThresh, 0, "2347"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2347"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2347"
HKR, NDI\params\RTSThresh, step, 0, "32"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2346"
HKR, Default, FragThresh, 0, "2346"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragment Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2346"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2346"
HKR, NDI\params\FragThresh, step, 0, "32"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , AuthenType, 0, "0" ; Open System
HKR, Default, AuthenType, 0, "0"
HKR, , Encryption, 0, "1" ; Disable
HKR, Default, Encryption, 0, "1"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
[NetRTUSB.ndi.reg]
HKR, , NTMPDriver, 0, rt25u98.sys
HKR, Ndi, DeviceID, 0, "USB\VID_2001&PID_3C00"
HKR, , BusType, 0, 15
HKR, NDI, CardType, 0, "PNP"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, rt25u98.sys
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "rt25u98"
HKR, NDIS, MajorNdisVersion,1, 03
HKR, NDIS, MinorNdisVersion,1, 0A
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
win9x.CopyFiles=11 ; system32 subdirectory on win9x
[NT.CopyFiles]
rt2500usb.sys ; NT Installation
[win9x.CopyFiles]
rt25u98.sys ; Win9x Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
rt2500usb.sys=1
rt25u98.sys=1
[NetRTUSB.ndi.NT.reg]
HKR, Ndi, Service, 0, "rt2500usb"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[NetRTUSB.Service]
DisplayName=%NetRTUSB.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2500usb.sys"
HKR, , TypesSupported, 0x00010001, 7
[strings]
Provider= "D-Link"
V_Provider= "D-Link"
NetRTUSB.DeviceDesc= "D-Link AirPlus G DWL-G122 Wireless USB Adapter(rev.B)"
NetRTUSB.Service.DispName= "DWL-G122(rev.B) USB Wireless LAN Driver"
INSTALL_DISK_STR= "D-Link Wireless LAN Installation Disk"
SSID_DEF_STR="default"
VENDOR_DESC_DEF_STR=""
NETWORK_TYPE_DEF_STR="1"
CHANNEL="6"
