
[Version]
DriverVer=09/01/2003, 3.1.3
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%USB_DESC_STR%=WLAN_USB1, USB\VID_0CDE&PID_0005
%USB_DESC_STR%=WLAN_USB2, USB\VID_0CDE&PID_0004
%USB_DESC_STR%=WLAN_USB3, USB\VID_0CDE&PID_0003
%USB_DESC_STR%=WLAN_USB4, USB\VID_09AA&PID_3642
%USB_DESC_STR%=WLAN_USB5, USB\VID_9016&PID_182D
[WLAN_USB1.NT] ; Win2k
AddReg=WLAN_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=WLAN_DRIVER.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[WLAN_USB1.NT.Services]
AddService="WlanUIB", 2, WLAN_DRIVER_USB.Service, WLAN_DRIVER.EventLog
[WLAN_USB1.reg]
HKR,Ndi ,DeviceID,0,"USB\Vid_0cde&Pid_0005"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%USB_DESC_STR%
[WLAN_USB2.NT] ; Win2k
AddReg=WLAN_USB2.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=WLAN_DRIVER.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[WLAN_USB2.NT.Services]
AddService="WlanUIB", 2, WLAN_DRIVER_USB.Service, WLAN_DRIVER.EventLog
[WLAN_USB2.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_0CDE&PID_0004"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%USB_DESC_STR%
[WLAN_USB3.NT] ; Win2k
AddReg=WLAN_USB3.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=WLAN_DRIVER.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[WLAN_USB3.NT.Services]
AddService="WlanUIB", 2, WLAN_DRIVER_USB.Service, WLAN_DRIVER.EventLog
[WLAN_USB3.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_0CDE&PID_0003"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%USB_DESC_STR%
[WLAN_USB4.NT] ; Win2k
AddReg=WLAN_USB4.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=WLAN_DRIVER.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[WLAN_USB4.NT.Services]
AddService="WlanUIB", 2, WLAN_DRIVER_USB.Service, WLAN_DRIVER.EventLog
[WLAN_USB4.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_09AA&PID_3642"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%USB_DESC_STR%
[WLAN_USB5.NT] ; Win2k
AddReg=WLAN_USB5.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=WLAN_DRIVER.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[WLAN_USB5.NT.Services]
AddService="WlanUIB", 2, WLAN_DRIVER_USB.Service, WLAN_DRIVER.EventLog
[WLAN_USB5.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_9016&PID_182D"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%USB_DESC_STR%
[WLAN_DRIVER_USB.Service]
DisplayName=%WLAN_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\WlanUIB.sys
LoadOrderGroup=NDIS
[WLAN_DRIVER.EventLog]
AddReg=WLAN_DRIVER.EventLog.reg
[WLAN_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_USB.reg]
HKR, ,WLANIOC ,0 ,"XI-735"
HKR,NDI ,Service ,0 ,"WlanUIB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"15"
HKR, ,DeviceVxDs ,0 ,"WlanUIB.sys"
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,PSMode,0,1
HKR, defaults,PSMode,0,1
HKR, Ndi\params\PSMode,default,0,1
HKR, NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR, NDI\params\PSMode,type,,enum
HKR, NDI\params\PSMode,flag,1,30,00,00,00
HKR, NDI\params\PSMode\enum,1,,"Disable"
HKR, NDI\params\PSMode\enum,2,,"Always Enable"
HKR, NDI\params\PSMode\enum,3,,"Auto Enable"
HKR, NDI\params\PSMode,optional,0,1
HKR, ,ListenInterval,0,3
HKR, defaults,ListenInterval,0,3
HKR, Ndi\params\ListenInterval,default,0,3
HKR, NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR, NDI\params\ListenInterval,type,,int
HKR, NDI\params\ListenInterval,flag,1,30,00,00,00
HKR, NDI\params\ListenInterval,min,0,0
HKR, NDI\params\ListenInterval,max,0,77
HKR, NDI\params\ListenInterval,step,0,1
HKR, NDI\params\ListenInterval,optional,0,1
HKR, ,RTSThresh,0,2432
HKR, defaults,RTSThresh,0,2432
HKR, Ndi\params\RTSThresh,default,0,2432
HKR, NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR, NDI\params\RTSThresh,type,0,int
HKR, NDI\params\RTSThresh,flag,1,20,00,00,00
HKR, NDI\params\RTSThresh,min,0,0
HKR, NDI\params\RTSThresh,max,0,2432
HKR, NDI\params\RTSThresh,step,0,64
HKR, NDI\params\RTSThresh,optional,0,1
HKR, ,FragThresh,0,2346
HKR,defaults,FragThresh,0,2346
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,30,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
HKR,NDI\params\FragThresh,optional,0,1
HKR, ,PreambleMode,0,1
HKR, defaults,PreambleMode,0,1
HKR, Ndi\params\PreambleMode,default,0,1
HKR, NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR, NDI\params\PreambleMode,type,,enum
HKR, NDI\params\PreambleMode,flag,1,30,00,00,00
HKR, NDI\params\PreambleMode\enum,1,,"Long"
HKR, NDI\params\PreambleMode\enum,2,,"Short"
HKR, NDI\params\PreambleMode,optional,0,1
HKR, ,AuthentAlg,0,65535
HKR, defaults,AuthentAlg,0,65535
HKR, NDI\params\AuthentAlg,default,0,65535
HKR, NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR, NDI\params\AuthentAlg,type,,enum
HKR, NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR, NDI\params\AuthentAlg\enum,1,,"Open"
HKR, NDI\params\AuthentAlg\enum,2,,"Share Key"
HKR, NDI\params\AuthentAlg\enum,65535,,"Auto"
HKR, NDI\params\AuthentAlg,optional,0,1
HKR, ,DSChannel,0,6
HKR, defaults,DSChannel,0,6 ;Default as 6
HKR, Ndi\params\DSChannel,default, 0, "6"
HKR, Ndi\params\DSChannel,ParamDesc,0, %CHANNEL_STR%
HKR, Ndi\params\DSChannel,type,0, "int"
HKR, Ndi\params\DSChannel,min,0, "1"
HKR, Ndi\params\DSChannel,max,0, "14"
HKR, Ndi\params\DSChannel,step,0, "1"
HKR, NDI\params\DSChannel,optional,0,1
HKR, ,SSID,0,"Sitecom"
HKR, defaults,SSID,0,"Sitecom" ;Default value is "Sitecom"
HKR, Ndi\params\SSID,default, 0, "Sitecom"
HKR, Ndi\params\SSID,ParamDesc,0, %ESSID_Str%
HKR, Ndi\params\SSID,type,0, "edit"
HKR, Ndi\params\SSID,default,0, "Sitecom"
HKR, Ndi\params\SSID,LimitText,0, "32"
HKR, Ndi\params\SSID,UpperCase,0, "0"
HKR, NDI\params\SSID,optional,0,1
HKR, ,TxRate,0,15
HKR, defaults,TxRate,0,15 ;Auto.
HKR, Ndi\params\TxRate,default,0,15
HKR, NDI\params\TxRate,ParamDesc,,%TX_RATE%
HKR, NDI\params\TxRate,type,,enum
HKR, NDI\params\TxRate\enum,1,0,"1Mbps"
HKR, NDI\params\TxRate\enum,2,0,"2Mbps"
HKR, NDI\params\TxRate\enum,4,0,"5Mbps"
HKR, NDI\params\TxRate\enum,8,0,"11Mbps"
HKR, NDI\params\TxRate\enum,15,0,"Auto"
HKR, NDI\params\TxRate,optional,0,1
HKR, ,WepReq,0,0
HKR, defaults,WepReq,0,0 ;Disable
HKR, Ndi\params\WepReq,default,0,0
HKR, Ndi\params\WepReq,ParamDesc,0,%ENCRYPTION_LEVEL%
HKR, Ndi\params\WepReq,type,0,"enum"
HKR, Ndi\params\WepReq,default, 0,"0"
HKR, Ndi\params\WepReq\enum,0,0,"Disable"
HKR, Ndi\params\WepReq\enum,2,0,"64(40) Bit"
HKR, Ndi\params\WepReq\enum,6,0,"128(104) Bit"
HKR, NDI\params\WepReq,optional,0,1
HKR, ,NetworkType,0,1
HKR, defaults,NetworkType,0,1 ;Infrasturcture
HKR, Ndi\params\NetworkType,default,0,1
HKR, Ndi\params\NetworkType,ParamDesc,0, %NET_WORK_TYPE%
HKR, Ndi\params\NetworkType,type,0, "enum"
HKR, Ndi\params\NetworkType,default,0, "1"
HKR, Ndi\params\NetworkType\enum,1,0, "Infrastructure"
HKR, Ndi\params\NetworkType\enum,2,0, "802.11 AdHoc"
HKR, Ndi\params\NetworkType\enum,3,0, "AdHoc"
HKR, NDI\params\NetworkType,optional,0,1
HKR, ,LoadFirmware,0,1
HKR, defaults,LoadFirmware,0,1
HKR, Ndi\params\LoadFirmware,default,0,1
HKR, NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
HKR, NDI\params\LoadFirmware,type,,enum
HKR, NDI\params\LoadFirmware,flag,1,30,00,00,00
HKR, NDI\params\LoadFirmware\enum,0,,"Disable"
HKR, NDI\params\LoadFirmware\enum,1,,"Enable"
HKR, NDI\params\LoadFirmware,optional,0,1
HKR, ,11dMode,0,0
HKR, defaults,11dMode,0,0 ;Disalbed
HKR, Ndi\params\11dMode,default,0,0
HKR, Ndi\params\11dMode,ParamDesc,0, %11D_MODE%
HKR, Ndi\params\11dMode,type,0, "enum"
HKR, Ndi\params\11dMode,default,0, "0"
HKR, Ndi\params\11dMode\enum,0,0, "Disabled"
HKR, Ndi\params\11dMode\enum,1,0, "Strict"
HKR, Ndi\params\11dMode\enum,2,0, "Flexible"
HKR, NDI\params\11dMode,optional,0,1
HKR,,DefaultKeyId,0,0
HKR,,EncryptInDriver,0,1
HKR,,DecryptInDriver,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
WLAN_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[WLAN_DRIVER.copy.NT]
WlanUIB.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles.X86] ; Win2k/Xp
WlanUIB.sys=1
[Strings]
VER_VENDOR_STR="Sitecom Europe BV"
VER_VENDOR_NAME_STR="Sitecom Europe BV"
WLAN_SERVICE_DISPLAY="Sitecom 802.11b USB Driver"
INSTALL_DISK_STR="WL-022"
USB_DESC_STR="Sitecom Wireless USB adapter 11M WL-022"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication"
LISTENINTERVAL_STR="Listen Interval"
CHANNEL_STR="AdHoc Channel"
ESSID_Str="ssid"
TX_RATE="TxRate"
ENCRYPTION_LEVEL="Encryption"
NET_WORK_TYPE="Network Type"
LOAD_FIRMWARE_STR="Firmware Download"
POWER_SAVE_STR="Power Save Mode"
11D_MODE="11D Mode"
