
[Version]
DriverVer=09/06/2004, 2.1.25
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%DCB_DESC_STR%=PRISM_DCB2, PCI\VEN_1260&DEV_3890&SUBSYS_00001260
%DCB_DESC_STR%=PRISM_DCB1, PCI\VEN_1260&DEV_3890&SUBSYS_48001385
[PRISM_DCB1] ; Win9x
DelReg=COMMON_A00_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
;DlFiles=PRISM_FW.del
[PRISM_DCB1.ME] ; WinMe
DelReg=COMMON_A00_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME
;DlFiles=PRISM_FW.del.ME
[PRISM_DCB1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
DelReg=COMMON_A00_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME
;DlFiles=PRISM_FW.del.ME
[PRISM_DCB1.NT] ; Win2k
DelReg=COMMON_A00_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
;DlFiles=PRISM_FW.del.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_DCB1.NT.Services]
AddService="PRISM_ICB", 2, PRISM_DRIVER_DCB.Service, PRISM_DRIVER.EventLog
[PRISM_DCB1.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_48001385"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB_DESC_STR%
[PRISM_DCB2] ; Win9x
DelReg=COMMON_A00_DEL.reg
AddReg=PRISM_DCB2.reg, COMMON_ICB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
;DlFiles=PRISM_FW.del
[PRISM_DCB2.ME] ; WinMe
DelReg=COMMON_A00_DEL.reg
AddReg=PRISM_DCB2.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME
;DlFiles=PRISM_FW.del.ME
[PRISM_DCB2.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
DelReg=COMMON_A00_DEL.reg
AddReg=PRISM_DCB2.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME
;DlFiles=PRISM_FW.del.ME
[PRISM_DCB2.NT] ; Win2k
DelReg=COMMON_A00_DEL.reg
AddReg=PRISM_DCB2.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
;DlFiles=PRISM_FW.del.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_DCB2.NT.Services]
AddService="PRISM_ICB", 2, PRISM_DRIVER_DCB.Service, PRISM_DRIVER.EventLog
[PRISM_DCB2.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_00001260"
HKR,,PlatformID,0,0
HKR,,VendorDesc,0,%DCB_DESC_STR%
[PRISM_DRIVER_DCB.Service]
DisplayName=%PRISM_SERVICE_DISPLAY_DCB%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\WG511ICB.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_ICB.reg]
HKR,NDI ,Service ,0 ,"PRISM_ICB"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"WG511ICB.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
HKR, ,CardBusBridgeLatencyTimer ,0 ,"32"
HKR, ,CardBusBridgeCacheLineSize ,0 ,"8"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,04
HKR,NDIS ,MinorNdisVersion ,1 ,00
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis5"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,04
HKR,NDIS ,MinorNdisVersion ,1 ,00
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON_A00_DEL.reg]
HKR,,FWFileName
[COMMON.reg]
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR, ,SSID ,0 ,%SSID_DEF_STR%
HKR, ,DefaultSSID ,0 ,%UI_SSID_DEF_STR%
HKR, ,LanExpress ,0 ,%LanExpress_STR%
HKR, ,11dMode ,0 ,"0"
HKR, ,Band ,0 ,"1"
HKR, ,BandPreference ,0 ,"0"
HKR, ,DSFreq ,0 ,"2457000"
HKR, ,RTSThresh ,0 ,"2347"
HKR, ,FragThresh ,0 ,"2346"
HKR,,CountryCode,0,%CCode_DEFAULT%
HKR,NDI\params\CountryCode,default,0,%CCode_DEFAULT%
HKR,NDI\params\CountryCode,ParamDesc,0,%CCode_Description%
HKR,NDI\params\CountryCode,type,0,enum
HKR,NDI\params\CountryCode,flag,1,30,00,00,00
HKR,NDI\params\CountryCode\enum,"DK",0,%CCode_Africa%
HKR,NDI\params\CountryCode\enum,"CH",0,%CCode_Asia%
HKR,NDI\params\CountryCode\enum,"AT",0,%CCode_Australia%
HKR,NDI\params\CountryCode\enum,"CA",0,%CCode_Canada%
HKR,NDI\params\CountryCode\enum,"GB",0,%CCode_Europe%
HKR,NDI\params\CountryCode\enum,"FR",0,%CCode_France%
HKR,NDI\params\CountryCode\enum,"JP",0,%CCode_Japan%
HKR,NDI\params\CountryCode\enum,"BR",0,%CCode_SourthAmerica%
HKR,NDI\params\CountryCode\enum,"US",0,%CCode_UnitedStates%
HKR,NDI\params\CountryCode,optional,0,0
HKR,,ConfigProfile,0,256
HKR,NDI\params\ConfigProfile,default,0,256
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,,enum
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
HKR,NDI\params\ConfigProfile,optional,0,0
HKR,,NitroMode,0,"1"
HKR,defaults,PSMode,0,1
HKR,,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode,optional,0,0
[COMMON.reg.security]
"D:ARAI(A;;GA;;;BA)(A;;GA;;;SY)(A;CI;GA;;;IU)"
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.ME=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
PRISM_FW.del=11 ; Win9x=%windir%\system
PRISM_FW.del.ME=11 ; Win9x=%windir%\system
PRISM_FW.del.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_DRIVER.copy]
WG511ICB.sys
[PRISM_DRIVER.copy.ME]
WG511ICB.sys
[PRISM_DRIVER.copy.NT]
WG511ICB.sys
[PRISM_FW.del]
WG511DCB.arm
[PRISM_FW.del.ME]
WG511DCB.arm
[PRISM_FW.del.NT]
WG511DCB.arm
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
WG511ICB.sys=1
[SourceDisksFiles.ME] ; WinMe
WG511ICB.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
WG511ICB.sys=1
[Strings]
VER_VENDOR_STR="NETGEAR"
VER_VENDOR_NAME_STR="NETGEAR"
PRISM_SERVICE_DISPLAY_DCB="NETGEAR WG511 Wireless LAN Driver"
INSTALL_DISK_STR="NETGEAR WG511 Wireless LAN Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
POWER_SAVE_AUTO_DYN_STR="Auto Dynamic"
POWER_SAVE_AUTO_MAX_STR="Auto Maximum"
LOAD_FIRMWARE_STR="Firmware Download"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CHANNEL_STR="Channel"
DATARATES_STR="Data Rate"
DATARATES_AUTO="Fully Automatic"
ALSR_STR="Auto Long Slot Reassociation"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="11b only"
CONFIG_PROF_MIXED="Auto(11g+11b)"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="11g only"
CONFIG_PROF_TEST="Test Mode"
CONFIG_PROF_B_WIFI="B WIFI"
CONFIG_PROF_WIFI_SPEC="WIFI Spec"
NITRO_MODE="Nitro Mode"
NITRO_DISABLED="Disabled"
NITRO_ENABLED="Enabled"
SSID_DEF_STR="NETGEAR"
UI_SSID_DEF_STR="NETGEAR"
LanExpress_STR="IL00"
CCode_DEFAULT="US"
CCode_Description="Country/Domain"
CCode_Africa="Africa"
CCode_Asia="Asia"
CCode_Australia="Australia"
CCode_Canada="Canada"
CCode_Europe="Europe"
CCode_France="France"
CCode_Israel="Israel"
CCode_Mexico="Mexico"
CCode_Japan="Japan"
CCode_Taiwan="Taiwan"
CCode_SourthAmerica="Sourth America"
CCode_UnitedStates="United States"
DCB_DESC_STR="NETGEAR WG511 54 Mbps Wireless PC Card"

