
[version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Realtek%
CatalogFile.NT=net8187Se.cat ;; for WHQL certified
DriverVer=04/01/2010,5.9110.0401.2010
[Manufacturer]
%Realtek%=Realtek,NTx86
[ControlFlags]
ExcludeFromSelect=PCI\VEN_10EC&DEV_8185&REV_22
[Realtek.NTamd64]
%RTL8187Se.DeviceDesc.ASUS%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_831F1043&REV_22
%RTL8187Se.DeviceDesc.MSI%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_68941462&REV_22
%RTL8187Se.DeviceDesc.WL194G%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_83411043&REV_22
%RTL8187Se.DeviceDesc.WL174GH%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_00661B0A&REV_22
%RTL8187Se.DeviceDesc.WL174%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_00351B0A&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_0CD6105B&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_819910EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_818110EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_818210EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_815010EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_815110EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_815210EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8185&REV_22
[Realtek.NTx86]
%RTL8187Se.DeviceDesc.ASUS%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_831F1043&REV_22
%RTL8187Se.DeviceDesc.MSI%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_68941462&REV_22
%RTL8187Se.DeviceDesc.WL194G%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_83411043&REV_22
%RTL8187Se.DeviceDesc.WL174GH%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_00661B0A&REV_22
%RTL8187Se.DeviceDesc.WL174%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_00351B0A&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_0CD6105B&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_819910EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_818110EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_818210EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_815010EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_815110EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_815210EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8185&REV_22
[Realtek]
%RTL8187Se.DeviceDesc.ASUS%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_831F1043&REV_22
%RTL8187Se.DeviceDesc.MSI%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_68941462&REV_22
%RTL8187Se.DeviceDesc.WL194G%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_83411043&REV_22
%RTL8187Se.DeviceDesc.WL174GH%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_00661B0A&REV_22
%RTL8187Se.DeviceDesc.WL174%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_00351B0A&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_0CD6105B&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_819910EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_818110EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_818210EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_815010EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_815110EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&SUBSYS_815210EC&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8199&REV_22
%RTL8187Se.DeviceDesc%=RTL8187Se.ndi, PCI\VEN_10EC&DEV_8185&REV_22
[RTL8187Se.ndi]
DriverVer=04/01/2010,9110
AddReg=RTL8187Se.win.reg, RTL8187Se.common.reg, RTLWLAN.reg
;CpyFiles=RTL8187Se.CopyFiles98
[RTL8187Se.ndi.NT]
AddReg=RTL8187Se.nt5.reg, RTL8187Se.common.reg, RTLWLAN.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8187Se.CopyFiles
[RTL8187Se.ndi.NT.Services]
AddService=rtl8187Se, 2, RTL8187Se.nt5.Service, RTL8187Se.nt5.EventLog
[RTL8187Se.win.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_10EC&DEV_8185&REV_22"
HKR, Ndi\Install, , 0, rtsnt.install
HKR, NDI\Params\NetworkAddress, flag, 1, 30, 00, 00, 00
HKR, , DriverDesc, 0, "Realtek RTL8187S Wireless LAN PCIE Network Adapter"
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, rtl8187Se.sys
HKR, , EnumPropPages, 0, netdi.dll, EnumPropPages
HKR, , MediaType, 0, 1
HKR, , AdapterType, 0, 5
HKR, , BusType, 0, 5
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0a
HKR, NDIS, LogDriverName, 0, "RTL8187Se"
HKR, Ndi\Interfaces, DefLower, , "ethernet"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
HKR, Ndi\Interfaces, DefUpper, , "ndis3"
HKR, Ndi\Interfaces, UpperRange, , "ndis3"
HKR, Ndi\Install, ndis3, 0, "rtl8187Se.ndis5"
[RTL8187Se.nt5.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, Service, 0, "RTL8187Se"
[RTL8187Se.nt5.Service]
DisplayName=%RTL8187Se.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rtl8187Se.sys
LoadOrderGroup=NDIS
[RTL8187Se.nt5.EventLog]
Addreg=RTL8187Se.nt5.AddEventLog.reg
[RTL8187Se.nt5.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[RTL8187Se.common.reg]
HKR,Ndi\params\QoS, ParamDesc, 0, %QOS_STR%
HKR,Ndi\params\QoS, type, 0, "enum"
HKR,Ndi\params\QoS, default, 0, "0"
HKR,Ndi\params\QoS\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\QoS\enum, "1", 0, %ENABLE_STR%
HKR,defaults,QoS,0,"0"
HKR,,QoS,0,"0"
HKR,,CcxRm,0,"1"
[RTLWLAN.reg]
HKR,,Channel,0,"10"
HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, type, 0, "enum"
HKR,Ndi\params\WirelessMode, default, 0, "4"
HKR,Ndi\params\WirelessMode\enum, "2", 0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, "4", 0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"
HKR,Ndi\params\Dot11dEnable, ParamDesc, 0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable, type, 0, "enum"
HKR,Ndi\params\Dot11dEnable, default, 0, "0"
HKR,Ndi\params\Dot11dEnable\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum, "1", 0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"
HKR,Ndi\params\PSPXlinkMode, ParamDesc, 0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode, type, 0, "enum"
HKR,Ndi\params\PSPXlinkMode, default, 0, "0"
HKR,Ndi\params\PSPXlinkMode\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum, "1", 0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"
HKR,,LeisurePsMode,0,"2"
HKR,,bInactivePs,0,"1"
HKR,,KeepAliveLevel,0,"1"
HKR,,RoamRetryLimit, 0, "24"
HKR,,HwSwRfOffD3,0,"2"
HKR,,RegROAMSensitiveLevel,0,"0"
HKR,,bEnableL0s,0,"0"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
[RTL8187Se.CopyFiles]
rtl8187Se.sys,,,2
[RTL8187Se.CopyFiles98]
rtl8187Se.sys,,,2
[DestinationDirs]
RTL8187Se.CopyFiles=12
RTL8187Se.CopyFiles98=11
DefaultDestDir=11 ; LDID_SYS
[SourceDisksNames]
1=%DISKNAME%,,,
[SourceDisksFiles]
rtl8187Se.sys=1
[Strings]
Realtek="Realtek Semiconductor Corp."
SSID_STR="SSID"
CHANNEL_STR="Channel"
NETWORK_TYPE_STR="Network Type"
LED_CONTROL_STR="LED Control"
POWER_SAVE_STR="Power Save Mode"
WIFI_IBSS_STR="IBSS Default 11b Mode"
RATE_ADAPTIVE_STR="Rate Adaptive"
QOS_STR="QoS"
WMM_APSD="WMM APSD"
CCX_RM_STR="CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR="CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR="Forced Priority"
HW_PARA_STR="Init from HwParaFile"
THREE_WIRE_MODE_STR="Three Wire Programming Mode"
BOARD_TYPE_STR="Board Type"
PROTECTION_MODE_STR="Protection Mode"
TPC_STR="Transmit Power Control"
TPC_POLARITY_STR="TPC Polarity Select"
PSP_XLINK_STR="PSP XLink Mode"
CHANNEL_PLAN_STR="Channel Plan"
HIGH_POWER_STR="High Power Mechanism"
INIT_GAIN_STR="Initial Gain State"
CW_MAX_MIN_STR="Contention Window"
WL_MODE_STR="Wireless Mode"
PREAMBLE_MODE_STR="Preamble Mode"
FRAGTHRESH_STR="Fragmentation Threshold"
RTSTHRESH_STR="RTS Threshold"
DOT11_ENABLE_STR="802.11d"
DISABLE_STR="Disable"
ENABLE_STR="Enable"
CAM_STR="CAM"
MAX_PSP_STR="MAX_PSP"
FAST_PSP_STR="Fast_PSP"
AD_HOC_STR="Ad Hoc"
INFRASTRUCTURE_STR="Infrastructure"
AUTO_SELECT_STR="Auto select"
DOMAIN_FROM_EEPROM_STR="DOMAIN_FROM_EEPROM"
AUTO_STR="Auto"
LONG_PREAMBLE_STR="Long Preamble"
SHORT_PREAMBLE_STR="Short Preamble"
FCC_STR="FCC"
IC_STR="IC"
ETSI_STR="ETSI"
SPAIN_STR="Spain"
FRANCE_STR="France"
MKK_STR="MKK"
MKK1_STR="MKK1"
ISRAEL_STR="Israel"
TELEC_STR="TELEC"
IEEE_802_11A_STR="IEEE 802.11a"
IEEE_802_11B_STR="IEEE 802.11b"
IEEE_802_11BG_STR="IEEE 802.11 b/g"
Roam_Retry_Limit_STR="Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR="Leisure Power Save"
DISKNAME="Realtek RTL8187SE Wireless LAN PCIE Network Driver Disk"
RTL8187Se.DeviceDesc.ASUS="Realtek RTL8187SE 802.11b/g Wireless LAN PCIE Network"
RTL8187Se.DeviceDesc.MSI="802.11b/g Mini Card Wireless Adapter"
RTL8187Se.DeviceDesc.WL194G="Realtek RTL8187SE 802.11b/g Wireless LAN PCIE Network"
RTL8187Se.DeviceDesc.WL174GH="Realtek RTL8187SE 802.11b/g Wireless LAN HMC Network"
RTL8187Se.DeviceDesc.WL174="Realtek RTL8187SE 802.11b/g Wireless LAN mini-PCIE Network"
RTL8187Se.DeviceDesc="Realtek RTL8187SE Wireless LAN PCIE Network Adapter"
RTL8187Se.Service.DispName="Realtek RTL8187SE Wireless LAN PCIE Network Adapter"

