
[Version]
Signature="$Chicago$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
Compatible=1
DriverVer=06/12/2009, 1.02.08.0000
CatalogFile=NetRT61G.CAT
[ControlFlags]
ExcludeFromSelect=VEN_1814&DEV_0301&SUBSYS_3C081186
ExcludeFromSelect=VEN_1814&DEV_0301&SUBSYS_3C091186
ExcludeFromSelect=VEN_1814&DEV_0302&SUBSYS_3C081186
ExcludeFromSelect=VEN_1814&DEV_0302&SUBSYS_3C091186
ExcludeFromSelect=VEN_1814&DEV_0302&SUBSYS_3C101186
ExcludeFromSelect=VEN_1814&DEV_0302&SUBSYS_3C111186
ExcludeFromSelect=VEN_1814&DEV_0302&SUBSYS_3C121186
ExcludeFromSelect=VEN_1814&DEV_0302&SUBSYS_3C131186
ExcludeFromSelect=VEN_1814&DEV_0302&SUBSYS_3A711186
ExcludeFromSelect=VEN_1814&DEV_0302&SUBSYS_3A721186
[Manufacturer]
%Provider%=D-Link
[D-Link]
%G630.DeviceDesc%=NetRT61G_0302.ndi, PCI\VEN_1814&DEV_0301&SUBSYS_3C081186
%G510.DeviceDesc%=NetRT61G_0302.ndi, PCI\VEN_1814&DEV_0301&SUBSYS_3C091186
%G630B.DeviceDesc%=NetRT61G_0302.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_3C081186
%G510B.DeviceDesc%=NetRT61G_0302.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_3C091186
%G650A.DeviceDesc%=NetRT61G_0302.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_3C101186
%G520A.DeviceDesc%=NetRT61G_0302.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_3C111186
%G630M.DeviceDesc%=NetRT61G_0401.ndi, PCI\VEN_1814&DEV_0401&SUBSYS_3C121186
%G510M.DeviceDesc%=NetRT61G_0401.ndi, PCI\VEN_1814&DEV_0401&SUBSYS_3C131186
%DWA510.DeviceDesc%=NetRT61G_0302.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_3A711186
%DWA610.DeviceDesc%=NetRT61G_0302.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_3A721186
[NetRT61G_0301.ndi]
AddReg=PCI0301.ndi.reg, RT619X.ndi.reg, Common.reg
;CpyFiles=win9x.CopyFiles
[NetRT61G_0302.ndi]
AddReg=PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
;CpyFiles=win9x.CopyFiles
[NetRT61G_0401.ndi]
AddReg=PCI0401.ndi.reg, RT619X.ndi.reg, Common.reg
;CpyFiles=win9x.CopyFiles
[NetRT61G_0301.ndi.NT]
AddReg=Common.reg, RT61.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
[NetRT61G_0302.ndi.NT]
AddReg=Common.reg, RT61.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
[NetRT61G_0401.ndi.NT]
AddReg=Common.reg, RT61.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
[NetRT61G_0301.ndi.NT.Services]
AddService=RT61, 2, DLink.Service, common.EventLog
[NetRT61G_0302.ndi.NT.Services]
AddService=RT61, 2, DLink.Service, common.EventLog
[NetRT61G_0401.ndi.NT.Services]
AddService=RT61, 2, DLink.Service, common.EventLog
[Common.reg]
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
HKR, , Radio, 0, "0" ; 0=Enable(default), 1=Disable
HKR, , AutoReconnect, 0, "1" ; 0=disable(default), 1=enable
HKR, , ShowHiddenSSID, 0, "1" ; 0=disable(default), 1=enable
HKR, , CountryRegion, 0, "0"
HKR, , CountryRegionABand, 0, "0"
HKR, , OpMode, 0, "0"
HKR, , WirelessMode, 0, "3"
HKR, , TXBurst, 0, "1"
HKR, , ShortSlot, 0, "1"
HKR, , TurboRate, 0, "0"
HKR, , AdhocOfdm, 0, "0"
HKR, , BGProtection, 0, "0"
HKR, , FrameAggregation,0, "1"
HKR, , IEEE80211H, 0, "0"
HKR, , AutoChannelSelect, 0, "0"
HKR, , WMMCapable, 0, "1"
HKR, NDI\params\WMMCapable, ParamDesc, 0, %WMMCapable%
HKR, NDI\params\WMMCapable, type, 0, "enum"
HKR, NDI\params\WMMCapable, default, 0, "1"
HKR, NDI\params\WMMCapable\enum, 0, 0, %Disable%
HKR, NDI\params\WMMCapable\enum, 1, 0, %Enable%
HKR, , APSDCapable, 0, "0"
HKR, NDI\params\APSDCapable, ParamDesc, 0, %APSDCapable%
HKR, NDI\params\APSDCapable, type, 0, "enum"
HKR, NDI\params\APSDCapable, default, 0, "1"
HKR, NDI\params\APSDCapable\enum, 0, 0, %Disable%
HKR, NDI\params\APSDCapable\enum, 1, 0, %Enable%
HKR, , APSDAC_BE, 0, "0"
HKR, NDI\params\APSDAC_BE, ParamDesc, 0, %APSDAC_BE%
HKR, NDI\params\APSDAC_BE, type, 0, "enum"
HKR, NDI\params\APSDAC_BE, default, 0, "1"
HKR, NDI\params\APSDAC_BE\enum, 0, 0, %Disable%
HKR, NDI\params\APSDAC_BE\enum, 1, 0, %Enable%
HKR, , APSDAC_BK, 0, "0"
HKR, NDI\params\APSDAC_BK, ParamDesc, 0, %APSDAC_BK%
HKR, NDI\params\APSDAC_BK, type, 0, "enum"
HKR, NDI\params\APSDAC_BK, default, 0, "1"
HKR, NDI\params\APSDAC_BK\enum, 0, 0, %Disable%
HKR, NDI\params\APSDAC_BK\enum, 1, 0, %Enable%
HKR, , APSDAC_VI, 0, "0"
HKR, NDI\params\APSDAC_VI, ParamDesc, 0, %APSDAC_VI%
HKR, NDI\params\APSDAC_VI, type, 0, "enum"
HKR, NDI\params\APSDAC_VI, default, 0, "1"
HKR, NDI\params\APSDAC_VI\enum, 0, 0, %Disable%
HKR, NDI\params\APSDAC_VI\enum, 1, 0, %Enable%
HKR, , APSDAC_VO, 0, "0"
HKR, NDI\params\APSDAC_VO, ParamDesc, 0, %APSDAC_VO%
HKR, NDI\params\APSDAC_VO, type, 0, "enum"
HKR, NDI\params\APSDAC_VO, default, 0, "1"
HKR, NDI\params\APSDAC_VO\enum, 0, 0, %Disable%
HKR, NDI\params\APSDAC_VO\enum, 1, 0, %Enable%
HKR, , MaxSPLength, 0, "0"
HKR, , DLSCapable, 0, "1"
HKR, , SmartScan, 0, "1"
HKR, NDI\params\SmartScan, ParamDesc, 0, %SmartScan%
HKR, NDI\params\SmartScan, type, 0, "enum"
HKR, NDI\params\SmartScan, default, 0, "0"
HKR, NDI\params\SmartScan\enum, 0, 0, %Disable%
HKR, NDI\params\SmartScan\enum, 1, 0, %Enable%
HKR, , CarrierDetect, 0, "0"
HKR, , PSPXlink, 0, "0"
HKR, NDI\params\PSPXlink, ParamDesc, 0, %PSPXlink%
HKR, NDI\params\PSPXlink, type, 0, "enum"
HKR, NDI\params\PSPXlink, default, 0, "0"
HKR, NDI\params\PSPXlink\enum, 0, 0, %Disable%
HKR, NDI\params\PSPXlink\enum, 1, 0, %Enable%
HKR, , CCX2Control, 0x00010001, 0x00fa4600
HKR, , VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, Default, VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, , WPSDevName, 0, %WPS_DEVNAME_DEF_STR%
HKR, Default, WPSDevName, 0, %WPS_DEVNAME_DEF_STR%
HKR, , W53Control, 0, "0"
HKR, , FstRoam, 0, "0"
HKR, NDI\params\FstRoam, ParamDesc, 0, %Aggressive_Roaming_Condition%
HKR, NDI\params\FstRoam, type, 0, "enum"
HKR, NDI\params\FstRoam, default, 0, "Disabled"
HKR, NDI\params\FstRoam\enum, 0, 0, %Disable%
HKR, NDI\params\FstRoam\enum, 1, 0, %60dbm%
HKR, NDI\params\FstRoam\enum, 2, 0, %70dbm%
HKR, NDI\params\FstRoam\enum, 3, 0, %80dbm%
HKR, NDI\params\FstRoam\enum, 4, 0, %90dbm%
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR% ;1=Infrastructure , 0=adhoc
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, , NetworkAddress, 0, ""
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, %PSMode%
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, %CAM%
HKR, NDI\params\PSMode\enum, 1, 0, %MAXPSP%
HKR, , PreambleType, 0, "0"
HKR, Default, PreambleType, 0, "0"
HKR, , RTSThresh, 0, "2347"
HKR, , FragThresh, 0, "2346"
HKR, , AuthenType, 0, "0" ; Open System
HKR, Default, AuthenType, 0, "0"
HKR, , Encryption, 0, "1" ; Disable
HKR, Default, Encryption, 0, "1"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
[PCI0301.ndi.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_1814&DEV_0301"
[PCI0302.ndi.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_1814&DEV_0302"
[PCI0401.ndi.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_1814&DEV_0401"
[RT619X.ndi.reg]
HKR, , NTMPDriver, 0, RT619x.sys
HKR, , BusType, 0, 5
HKR, NDI, CardType, 0, "PCI"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "RT619x.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "RT619X"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
XP.CopyFiles=12 ; system32\drivers subdirectory on Windows XP
win9x.CopyFiles=11 ; system subdirectory on win9x
[NT.CopyFiles]
rt61.sys ; NT Installation
[XP.CopyFiles]
rt61.sys
[win9x.CopyFiles]
rt619x.sys ; Win9x Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
rt61.sys=1
rt619x.sys=1
[RT61.ndi.NT.reg]
HKR, Ndi, Service, 0, "RT61"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[DLink.Service]
DisplayName=%DLink.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\RT61.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT61.sys"
HKR, , TypesSupported, 0x00010001, 7
[Strings]
Provider="D-Link"
G630.DeviceDesc="D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter(rev.E)"
G510.DeviceDesc="D-Link AirPlus G DWL-G510 Wireless PCI Adapter(rev.C)"
G630B.DeviceDesc="D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter(rev.E)"
G510B.DeviceDesc="D-Link AirPlus G DWL-G510 Wireless PCI Adapter(rev.C)"
G650A.DeviceDesc="D-Link AirPlus G DWL-G650+A Wireless Cardbus Adapter(rev.E)"
G520A.DeviceDesc="D-Link AirPlus G DWL-G520+A Wireless PCI Adapter(rev.C)"
G630M.DeviceDesc="D-Link AirPlus G DWL-G630M Wireless Cardbus Adapter(rev.A)"
G510M.DeviceDesc="D-Link AirPlus G DWL-G510M Wireless PCI Adapter(rev.A)"
DWA610.DeviceDesc="D-Link Wireless G DWA-610 Notebook Adapter"
DWA510.DeviceDesc="D-Link Wireless G DWA-510 Desktop Adapter"
INSTALL_DISK_STR="D-Link AirPlus G Installation Disk"
DLink.Service.DispName="D-Link RT61g Wireless Driver"
SSID_DEF_STR="dlink"
VENDOR_DESC_DEF_STR="D-Link 802.11g Wireless LAN Card."
NETWORK_TYPE_DEF_STR="1"
CHANNEL="6"
WPS_DEVNAME_DEF_STR="D-Link Client"
RadioOnOff="Radio On/Off"
Disable="Disable"
Enable="Enable"
AutoReconnectMode="Auto Reconnect Mode"
CountryRegion24G="Country Region 11G"
CountryRegion24G_0="#0 (Channel 1 - 11)"
CountryRegion24G_1="#1 (Channel 1 - 13)"
CountryRegion24G_2="#2 (Channel 10 - 11)"
CountryRegion24G_3="#3 (Channel 10 - 13)"
CountryRegion24G_4="#4 (Channel 14)"
CountryRegion24G_5="#5 (Channel 1 - 14)"
CountryRegion24G_6="#6 (Channel 3 - 9)"
CountryRegion24G_7="#7 (Channel 5 - 13)"
CountryRegion5G="Country Region 11A"
CountryRegion5G_0="#0 Ch(36 - 64,149 - 165)"
CountryRegion5G_1="#1 Ch(36 - 140)"
CountryRegion5G_2="#2 Ch(36 - 64)"
CountryRegion5G_3="#3 Ch(52 - 64,149 - 161)"
CountryRegion5G_4="#4 Ch(149 - 165)"
CountryRegion5G_5="#5 Ch(149 - 161)"
CountryRegion5G_6="#6 Ch(36 - 48)"
CountryRegion5G_7="#7 Ch(36 - 165)"
CountryRegion5G_8="#8 Ch(52 - 64)"
CountryRegion5G_9="#9 Ch(34 - 46)"
CountryRegion5G_10="#10 Ch(34 - 64)"
BGProtection="B/G Protection"
Auto="Auto"
On="On"
Off="Off"
FrameAggregation="Frame Aggregation"
IEEE802_11h="IEEE802.11h"
AutoChannelSelect="Auto Channel Select"
WMMCapable="WMM Capable"
APSDCapable="APSD Capable"
APSDAC_BE="AC_BE support APSD"
APSDAC_BK="AC_BK support APSD"
APSDAC_VI="AC_VI support APSD"
APSDAC_VO="AC_VO support APSD"
DLSCapable="DLS Capable"
MaxSPLength="Max Service Period Length"
SmartScan="SmartScan"
CarrierDetect="Carrier Detect"
PSPXlink="PSP Xlink Mode"
NetworkType="Network Type"
AdHoc="802.11 Ad Hoc"
Infrastructure="Infrastructure"
LocalNetworkAddress="Local Administration MAC Network Address"
PSMode="Power Saving Mode"
CAM="CAM (Constantly Awake Mode)"
MAXPSP="Max_PSP (Max Power Savings)"
RTSThresh="RTS Threshold"
FragThresh="Fragment Threshold"
Aggressive_Roaming_Condition= "Aggressive Roaming Condition"
60dbm="-60dbm"
70dbm="-70dbm"
80dbm="-80dbm"
90dbm="-90dbm"
Adhoc_Wireless_Mode="Adhoc Wireless Mode"
802_11_B_Only="802.11 B Only"
802_11_BG_Mix="802.11 B/G Mix"
802_11_G_Only="802.11 G Only"
SSID="SSID"
