
[version]
DriverVer=12/06/2000, 0.30.0
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
[Manufacturer]
%Provider%=Adapters
[ControlFlags]
ExcludeFromSelect=PCMCIA\INTERSIL-HFA384X/IEEE-CA62
ExcludeFromSelect=PCMCIA\CHOICE_MICROSYSTEMS-CW10/IEEE-4AE8
ExcludeFromSelect=PCMCIA\INTERSIL-PRISM2_MINI-PCI_ADAPTER-B537
ExcludeFromSelect=PCI\VEN_1260&DEV_3873
[Adapters]
%CW10.DeviceDescMiniPCIA%=CW10_MINIPCMA.ndi, PCMCIA\INTERSIL-PRISM2_MINI-PCI_ADAPTER-0EE7
%CW10.DeviceDescMiniPCIB%=CW10_MINIPCMB.ndi, PCMCIA\INTERSIL-PRISM2_MINI-PCI_ADAPTER-B537
%CW10.DeviceDescMiniPCI25%=CW10_MINIPCM25.ndi, PCMCIA\INTERSIL-PRISM2_5_MINI-PCI_ADAPTER-7759
%CW10.DeviceDescPRISM1%=CW10_PRISM1.ndi, PCMCIA\INTERSIL-HFA384X/IEEE-CA62
%CW10.DeviceDescPRISM2%=CW10_PRISM2.ndi, PCMCIA\INTERSIL-HFA384x/IEEE-CC3C
%CW10.DeviceDescEVB1%=CW10_EVB2.ndi, PCMCIA\CHOICE_Microsystems-CW10/IEEE-5F95
%CW10.DeviceDescEVB2%=CW10_EVB1.ndi, PCMCIA\CHOICE_Microsystems-CW10/IEEE-4AE8
%CW10.DeviceDescUSB%=CW10_USB_1.ndi, USB\VID_2474&PID_3642
%CW10.DeviceDescUSB%=CW10_USB.ndi, USB\VID_09AA&PID_3642
%CW10.DeviceDescFreedom%=CW10_FREEDOM.ndi, PCMCIA\INTERSIL-PRISM_FREEDOM_PCMCIA_ADAPTER-40CB
%CW10.DeviceDescPCM25%=CW10_PCMCIA25.ndi, PCMCIA\INTERSIL-PRISM_2_5_PCMCIA_ADAPTER-F429
%CW10.DeviceDescPCI%=CW10_PCI.ndi, PCI\VEN_1260&DEV_3873
[CW10_PRISM1.ndi]
AddReg=PRISM1_ID.reg, Common.reg, win9x.reg, Pcmcia9x.reg, Pcmcia.reg
;CpyFiles=win9x.CopyFiles
[CW10_PRISM2.ndi]
AddReg=PRISM2_ID.reg, Common.reg, win9x.reg, Pcmcia9x.reg, Pcmcia.reg
;CpyFiles=win9x.CopyFiles
[CW10_EVB1.ndi]
AddReg=EVB1_ID.reg, Common.reg, win9x.reg, Pcmcia9x.reg, Pcmcia.reg
;CpyFiles=win9x.CopyFiles
[CW10_EVB2.ndi]
AddReg=EVB2_ID.reg, Common.reg, win9x.reg, Pcmcia9x.reg, Pcmcia.reg
;CpyFiles=win9x.CopyFiles
[CW10_MINIPCMA.ndi]
AddReg=MINIPCMA_ID.reg, Common.reg, win9x.reg, Pcmcia9x.reg, Pcmcia.reg
;CpyFiles=win9x.CopyFiles
[CW10_MINIPCMB.ndi]
AddReg=MINIPCMB_ID.reg, Common.reg, win9x.reg, Pcmcia9x.reg, Pcmcia.reg
;CpyFiles=win9x.CopyFiles
[CW10_MINIPCM25.ndi]
AddReg=MINIPCM25_ID.reg, Common.reg, win9x.reg, Pcmcia9x.reg, Pcmcia.reg
;CpyFiles=win9x.CopyFiles
[CW10_USB_1.ndi]
AddReg=USB_ID_1.reg, Common.reg, win9x.reg, USB.reg
;CpyFiles=win9x.USBCopyFiles
[CW10_USB.ndi]
AddReg=USB_ID.reg, Common.reg, win9x.reg, USB.reg
;CpyFiles=win9x.USBCopyFiles
[CW10_FREEDOM.ndi]
AddReg=FREEDOM_ID.reg, Common.reg, win9x.reg, Pcmcia9x.reg, Pcmcia.reg
;CpyFiles=win9x.CopyFiles
[CW10_PCMCIA25.ndi]
AddReg=PCMCIA25_ID.reg, Common.reg, win9x.reg, Pcmcia9x.reg, Pcmcia.reg
;CpyFiles=win9x.CopyFiles
[CW10_PCI.ndi]
AddReg=PCI_ID.reg, Common.reg, win9x.reg, PCI.reg
;CpyFiles=win9x.PCICopyFiles
[CW10_PRISM1.ndi.NT]
AddReg=Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
[CW10_PRISM2.ndi.NT]
AddReg=Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
[CW10_EVB1.ndi.NT]
AddReg=Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
[CW10_EVB2.ndi.NT]
AddReg=Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
[CW10_MINIPCMA.ndi.NT]
AddReg=Common.reg, nt.reg, MiniPCM2k.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
[CW10_MINIPCMB.ndi.NT]
AddReg=Common.reg, nt.reg, MiniPCM2k.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
[CW10_MINIPCM25.ndi.NT]
AddReg=Common.reg, nt.reg, MiniPCM2k.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
[CW10_USB_1.ndi.NT]
DriverVer=03/13/2001, 0.31.7.5
AddReg=Common.reg, nt.reg, USB.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=0 ; USB
;CpyFiles=NT.USBCopyFiles
[CW10_USB.ndi.NT]
DriverVer=03/13/2001, 0.31.7.5
AddReg=Common.reg, nt.reg, USB.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=0 ; USB
;CpyFiles=NT.USBCopyFiles
[CW10_FREEDOM.ndi.NT]
AddReg=Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
[CW10_PCMCIA25.ndi.NT]
AddReg=Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
[CW10_PCI.ndi.NT]
AddReg=Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
[CW10_PRISM1.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_PRISM2.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_EVB1.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_EVB2.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_MINIPCMA.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_MINIPCMB.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_MINIPCM25.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_USB_1.ndi.NT.Services]
AddService=CW10, 2, CW10_USB.Service, common.EventLog
[CW10_USB.ndi.NT.Services]
AddService=CW10, 2, CW10_USB.Service, common.EventLog
[CW10_FREEDOM.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_PCMCIA25.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[CW10_PCI.ndi.NT.Services]
AddService=CW10, 2, CW10.Service, common.EventLog
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
NT.PCICopyFiles=12 ; system32\drivers subdirectory on NT
NT.USBCopyFiles=12 ; system32\drivers subdirectory on NT
win9x.CopyFiles=11 ; system32 subdirectory on win9x
win9x.PCICopyFiles=11 ; system32 subdirectory on win9x
win9x.USBCopyFiles=11 ; system32 subdirectory on win9x
[NT.CopyFiles]
cw10.sys ; NT Installation
[NT.PCICopyFiles]
cw10.sys ; NT Installation
[NT.USBCopyFiles]
cw10usb.sys ; NT Installation
[win9x.CopyFiles]
cw10.sys ; win9x Installation
[win9x.PCICopyFiles]
cw10.sys ; win9x Installation
[win9x.USBCopyFiles]
cw10usb.sys ; win9x Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
cw10.sys=1
cw10usb.sys=1
cw10pci.sys=1
[Common.reg]
HKR, , VendorDesc, 0, "PRISM IEEE 802.11 Adapter"
HKR, , APDensity, 0, 1
HKR, defaults, APDensity, 0, 1
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, defaults, SSID, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, ParamDesc, 0, "SSID"
HKR, NDI\params\SSID, type, 0, edit
HKR, NDI\params\SSID, limitText, 0, 32
HKR, NDI\params\SSID, default, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, flag, 1, 30,00,00,00
HKR, , StationName, 0, "Client"
HKR, defaults, StationName, 0, "Client"
HKR, , ListenInterval, 0, 3
HKR, defaults, ListenInterval, 0, 3
HKR, NDI\params\ListenInterval, , 0, 3
HKR, NDI\params\ListenInterval, ParamDesc, 0, "Maximum Listen Interval"
HKR, NDI\params\ListenInterval, flag, 1, 30,00,00,00
HKR, NDI\params\ListenInterval, type, 0, int
HKR, Ndi\params\ListenInterval, default, 0, 3
HKR, NDI\params\ListenInterval, min, 0, 0
HKR, NDI\params\ListenInterval, max, 0, 77
HKR, NDI\params\ListenInterval, step, 0, 1
HKR, NDI\params\ListenInterval, optional, 0, 0
HKR, , DSChannel, 0, 10
HKR, defaults, DSChannel, 0, 10
HKR, , Encapsulation, 0, 1
HKR, defaults, Encapsulation, 0, 1
HKR, , TxRate, 0, 15
HKR, defaults, TxRate, 0, 15
HKR, NDI\params\TxRate, ParamDesc, 0, "Transmit Rate"
HKR, NDI\params\TxRate, type, 0, enum
HKR, NDI\params\TxRate, default, 0, 15
HKR, NDI\params\TxRate, flag, 1, 30,00,00,00
HKR, NDI\params\TxRate\enum, 1, 0, "Fixed 1 Mb/s"
HKR, NDI\params\TxRate\enum, 2, 0, "Fixed 2 Mb/s"
HKR, NDI\params\TxRate\enum, 3, 0, "Auto Select 1 or 2"
HKR, NDI\params\TxRate\enum, 4, 0, "Fixed 5.5 Mb/s"
HKR, NDI\params\TxRate\enum, 8, 0, "Fixed 11 Mb/s"
HKR, NDI\params\TxRate\enum, 15, 0, "Fully Auto"
HKR, , RTSThresh, 0, 2432
HKR, defaults, RTSThresh, 0, 2432
HKR, NDI\params\RTSThresh, ParamDesc, 0, "Medium Reservation"
HKR, NDI\params\RTSThresh, type, 0, enum
HKR, NDI\params\RTSThresh, default, 0, 2432
HKR, NDI\params\RTSThresh, flag, 1, 30, 00, 00, 00
HKR, NDI\params\RTSThresh\enum, 2432, 0, "Off"
HKR, NDI\params\RTSThresh\enum, 500, 0, "Hidden Stations"
HKR, , FragThresh, 0, 2432
HKR, defaults, FragThresh, 0, 2432
HKR, NDI\params\FragThresh, , 0, 2432
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragmentation Threshold"
HKR, NDI\params\FragThresh, type, 0, int
HKR, Ndi\params\FragThresh, default, 0, 2432
HKR, NDI\params\FragThresh, min, 0, 256
HKR, NDI\params\FragThresh, max, 0, 2432
HKR, NDI\params\FragThresh, step, 0, 128
HKR, NDI\params\FragThresh, flag, 1, 20,00,00,00
HKR, NDI\params\FragThresh, optional, 0, 0
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, defaults, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, enum
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, flag, 1, 30,00,00,00
HKR, NDI\params\NetworkType\enum, 0, 0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, NDI\params\NetworkType\enum, 3, 0, "Ad Hoc"
HKR, , PSMode, 0, 1
HKR, defaults, PSMode, 0, 1
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Save Mode"
HKR, NDI\params\PSMode, type, 0, enum
HKR, NDI\params\PSMode, default, 0, 1
HKR, NDI\params\PSMode, flag, 1, 30,00,00,00
HKR, NDI\params\PSMode\enum, 1, 0, "Disabled"
HKR, NDI\params\PSMode\enum, 2, 0, "Enabled"
HKR, , WepReq, 0, %WEP_REQUIRED_DEF_STR%
HKR, defaults, WepReq, 0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq, , 0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq, ParamDesc, 0, "Encryption"
HKR, NDI\params\WepReq, flag, 1, 30,00,00,00
HKR, NDI\params\WepReq, type, 0, enum
HKR, Ndi\params\WepReq, default, 0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq\enum, 0, 0, "Disabled"
HKR, NDI\params\WepReq\enum, 2, 0, "64 bit"
HKR, NDI\params\WepReq\enum, 6, 0, "128 bit"
HKR, NDI\params\WepReq, optional, 0, 0
HKR, , EncryptInDriver, 0, 1
HKR, defaults, EncryptInDriver, 0, 1
HKR, , DecryptInDriver, 0, 1
HKR, defaults, DecryptInDriver, 0, 1
HKR, , WEPFactor, 0, 3
HKR, defaults, WEPFactor, 0, 3
HKR, , Esarhpssap, 0, %PASSPHRASE_DEF_STR%
HKR, defaults, Esarhpssap, 0, %PASSPHRASE_DEF_STR%
HKR, NDI\params\Esarhpssap, ParamDesc, 0, "WEP Passphrase"
HKR, NDI\params\Esarhpssap, type, 0, edit
HKR, NDI\params\Esarhpssap, limitText, 0, 64
HKR, NDI\params\Esarhpssap, default, 0, %PASSPHRASE_DEF_STR%
HKR, NDI\params\Esarhpssap, flag, 1, 30,00,00,00
HKR, , PreambleMode, 0, 1
HKR, defaults, PreambleMode, 0, 1
HKR, NDI\params\PreambleMode, , 0, 1
HKR, NDI\params\PreambleMode, ParamDesc, 0, %SHORT_PREAM_STR%
HKR, NDI\params\PreambleMode, flag, 1, 30,00,00,00
HKR, NDI\params\PreambleMode, type, 0, enum
HKR, Ndi\params\PreambleMode, default, 0, 1
HKR, NDI\params\PreambleMode\enum,1, 0, "Long Tx Preamble"
HKR, NDI\params\PreambleMode\enum,2, 0, "Short Tx Preamble"
HKR, NDI\params\PreambleMode\enum,3, 0, "Auto"
HKR, NDI\params\PreambleMode, optional, 0, 0
HKR, , AuthentAlg, 0, %AUTHENT_TYPE_DEF_STR%
HKR, defaults, AuthentAlg, 0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg, ParamDesc, 0, "Authentication Algorithm"
HKR, NDI\params\AuthentAlg, type, 0, enum
HKR, NDI\params\AuthentAlg, default, 0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg, flag, 1, 30,00,00,00
HKR, NDI\params\AuthentAlg\enum, 1, 0, "WECA Compliant (always use Open)"
HKR, NDI\params\AuthentAlg\enum, 2, 0, "Must use Shared with WEP"
HKR, , IBSSInDriver, 0, 1
HKR, defaults, IBSSInDriver, 0, 1
HKR, NDI\params\IBSSInDriver, , 0, 1
HKR, NDI\params\IBSSInDriver, ParamDesc, 0, "Driver based IBSS"
HKR, NDI\params\IBSSInDriver, type, 0, enum
HKR, NDI\params\IBSSInDriver, default, 0, 1
HKR, NDI\params\IBSSInDriver, flag, 1, 30,00,00,00
HKR, NDI\params\IBSSInDriver\enum,0, 0, "Disabled"
HKR, NDI\params\IBSSInDriver\enum,1, 0, "Enabled"
[Pcmcia9x.reg]
HKR, , IOBaseAddress, 1, 02,00,00,00
HKR, , InterruptNumber, 1, 04,00,00,00
HKR, , EnableIRQSharing,1, 01,00,00,00
[Pcmcia.reg]
HKR, , BusType, 0, 8
HKR, NDI, CardType, 0, "PCMCIA"
[MiniPCM2k.reg]
HKLM, System\CurrentControlSet\Services\Pcmcia\Parameters, DisableIsaToPciRouting, 0x00010001, 0
[PCI.reg]
HKR, , BusType, 0, 5
HKR, NDI, CardType, 0, "PCI"
HKR, , IOBaseAddress, 1, 02,00,00,00
HKR, , InterruptNumber, 1, 04,00,00,00
[USB.reg]
HKR, , BusType, 0, 0
HKR, NDI, CardType, 0, "PNP"
[win9x.reg]
HKR, , DevLoader, 0, "*ndis,*ntkern,*ndis"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, 0, "cw10"
HKR, NDIS, MajorNdisVersion,1, 03
HKR, NDIS, MinorNdisVersion,1, 0A
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[PRISM1_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCMCIA\INTERSIL-HFA384X/IEEE-CA62"
[PRISM2_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCMCIA\INTERSIL-HFA384x/IEEE-CC3C"
[EVB1_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCMCIA\CHOICE_MICROSYSTEMS-CW10/IEEE-5F95"
[EVB2_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCMCIA\CHOICE_MICROSYSTEMS-CW10/IEEE-4AE8"
[MINIPCMA_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCMCIA\INTERSIL-PRISM2_MINI-PCI_ADAPTER-0EE7"
[MINIPCMB_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCMCIA\INTERSIL-PRISM2_MINI-PCI_ADAPTER-B537"
[MINIPCM25_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCMCIA\INTERSIL-PRISM2_5_MINI-PCI_ADAPTER-7759
[USB_ID_1.reg]
HKR, , DeviceVxDs, 0, cw10usb.sys
HKR, , NTMPDriver, 0, cw10usb.sys
HKR, Ndi, DeviceID, 0, "USB\VID_2474&PID_3642"
[USB_ID.reg]
HKR, , DeviceVxDs, 0, cw10usb.sys
HKR, , NTMPDriver, 0, cw10usb.sys
HKR, Ndi, DeviceID, 0, "USB\VID_09AA&PID_3642"
[FREEDOM_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCMCIA\INTERSIL-PRISM_FREEDOM_PCMCIA_ADAPTER-40CB"
[PCMCIA25_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCMCIA\INTERSIL-PRISM_2_5_PCMCIA_ADAPTER-F429"
[PCI_ID.reg]
HKR, , DeviceVxDs, 0, cw10.sys
HKR, , NTMPDriver, 0, cw10.sys
HKR, Ndi, DeviceID, 0, "PCI\VEN_1260&DEV_3873"
[nt.reg]
HKR, Ndi, Service, 0, "CW10"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis4"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[CW10.Service]
DisplayName=%CW10.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\CW10.sys
LoadOrderGroup=NDIS
[CW10_USB.Service]
DisplayName=%CW10_USB.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\CW10Usb.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\CW10.sys"
HKR, , TypesSupported, 0x00010001, 7
[Strings]
Provider="Intersil Corporation"
CW10="CW10"
CW10.DeviceDescPRISM1="PRISM1 IEEE 802.11 PC CARD Adapter"
CW10.DeviceDescPRISM2="PRISM2 IEEE 802.11 PC CARD Adapter"
CW10.DeviceDescEVB1="PRISM1 IEEE 802.11 PC CARD Adapter/EVB"
CW10.DeviceDescEVB2="PRISM2 IEEE 802.11 PC CARD Adapter/EVB"
CW10.DeviceDescMiniPCIA="Intersil PRISM2 Mini-PCI Adapter"
CW10.DeviceDescMiniPCIB="Intersil PRISM2 Mini-PCI Adapter"
CW10.DeviceDescMiniPCI25="Intersil PRISM2.5 Mini-PCI Adapter"
CW10.DeviceDescUSB="Intersil IEEE 802.11 LAN USB Adapter"
CW10.DeviceDescFreedom="Intersil PRISM Freedom PCMCIA Adapter"
CW10.DeviceDescPCM25="Intersil PRISM2.5 PCMCIA Adapter"
CW10.DeviceDescPCI="Intersil PRISM2 11Mbps Wireless LAN PCI Card"
CW10.Service.DispName="Prism PCMCIA Wireless LAN Driver"
CW10_USB.Service.DispName="Prism USB Wireless LAN Driver"
SHORT_PREAM_STR="Preamble Mode"
INSTALL_DISK_STR="Wireless LAN Installation Disk"
SSID_DEF_STR="IEEE 802.11 LAN"
NETWORK_TYPE_DEF_STR="1"
AUTHENT_TYPE_DEF_STR="2"
PASSPHRASE_DEF_STR="INTERSIL"
WEP_REQUIRED_DEF_STR="0"
