
[Version]
Signature="$Chicago$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
Compatible=1
DriverVer=07/17/2009, 1.03.05.0000
[ControlFlags]
[Manufacturer]
%Belkin%=Belkin
[Belkin]
%Belkin.DeviceDesc%=Belkin1.ndi, USB\VID_050D&PID_905C
%Belkin.DeviceDesc%=Belkin2.ndi, USB\VID_050D&PID_905B
%Belkin705B.DeviceDesc%=Belkin3.ndi, USB\VID_050D&PID_705B
[Belkin1.ndi]
AddReg=USB_050D_905C.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[Belkin2.ndi]
AddReg=USB_050D_905B.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[Belkin3.ndi]
AddReg=USB_050D_705B.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[Belkin1.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[Belkin2.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[Belkin3.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[Belkin1.ndi.NT.Services]
AddService=RT73, 2, Belkin.Service, common.EventLog
[Belkin2.ndi.NT.Services]
AddService=RT73, 2, Belkin.Service, common.EventLog
[Belkin3.ndi.NT.Services]
AddService=RT73, 2, Belkin.Service, common.EventLog
[Common.reg]
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
HKR, , Radio, 0, "0"
HKR, NDI\params\Radio, ParamDesc, 0, "Radio On/Off"
HKR, NDI\params\Radio, type, 0, "enum"
HKR, NDI\params\Radio, default, 0, "0"
HKR, NDI\params\Radio\enum, 1, 0, "Disable"
HKR, NDI\params\Radio\enum, 0, 0, "Enable"
HKR, , AutoReconnect, 0, "1"
HKR, NDI\params\AutoReconnect, ParamDesc, 0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect, type, 0, "enum"
HKR, NDI\params\AutoReconnect, default, 0, "1"
HKR, NDI\params\AutoReconnect\enum, 0, 0, "Disable"
HKR, NDI\params\AutoReconnect\enum, 1, 0, "Enable"
HKR, , ShowHiddenSSID, 0, "0" ; 0=disable(default), 1=enable
HKR, , CountryRegion, 0, "0"
HKR, NDI\params\CountryRegion, ParamDesc, 0, "Country Region 11G"
HKR, NDI\params\CountryRegion, type, 0, "enum"
HKR, NDI\params\CountryRegion, default, 0, "0"
HKR, NDI\params\CountryRegion\enum, 0, 0, "(Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum, 1, 0, "(Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum, 2, 0, "(Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum, 3, 0, "(Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum, 4, 0, "(Channel 14)"
HKR, NDI\params\CountryRegion\enum, 5, 0, "(Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum, 6, 0, "(Channel 3 - 9)"
HKR, NDI\params\CountryRegion\enum, 7, 0, "(Channel 5 - 13)"
HKR, , CountryRegionABand, 0, "7"
HKR, NDI\params\CountryRegionABand, ParamDesc, 0, "Country Region 11A"
HKR, NDI\params\CountryRegionABand, type, 0, "enum"
HKR, NDI\params\CountryRegionABand, default, 0, "7"
HKR, NDI\params\CountryRegionABand\enum,0, 0, "Ch(36 - 64,149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,1, 0, "Ch(36 - 140)"
HKR, NDI\params\CountryRegionABand\enum,2, 0, "Ch(36 - 64)"
HKR, NDI\params\CountryRegionABand\enum,3, 0, "Ch(52 - 64,149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,4, 0, "Ch(149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,5, 0, "Ch(149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,6, 0, "Ch(36 - 48)"
HKR, NDI\params\CountryRegionABand\enum,7, 0, "Ch(36 - 165)"
HKR, NDI\params\CountryRegionABand\enum,8, 0, "Ch(52 - 64)"
HKR, NDI\params\CountryRegionABand\enum,9, 0, "Ch(34 - 46)"
HKR, NDI\params\CountryRegionABand\enum,10, 0, "Ch(34 - 64)"
HKR, , OpMode, 0, "0"
HKR, , WirelessMode, 0, "3"
HKR, , TXBurst, 0, "0"
HKR, , ShortSlot, 0, "1"
HKR, , TurboRate, 0, "0"
HKR, , AdhocOfdm, 0, "0"
HKR, NDI\params\AdhocOfdm, ParamDesc, 0, "Adhoc Wireless Mode"
HKR, NDI\params\AdhocOfdm, type, 0, "enum"
HKR, NDI\params\AdhocOfdm, default, 0, "0"
HKR, NDI\params\AdhocOfdm\enum, 0, 0, "802.11 B Only"
HKR, NDI\params\AdhocOfdm\enum, 1, 0, "802.11 B/G Mix"
HKR, NDI\params\AdhocOfdm\enum, 2, 0, "802.11 G Only"
HKR, NDI\params\AdhocOfdm\enum, 3, 0, "802.11 A Only"
HKR, NDI\params\AdhocOfdm\enum, 4, 0, "802.11 A/B/G Mix"
HKR, , BGProtection, 0, "0"
HKR, NDI\params\BGProtection, ParamDesc, 0, "B/G Protection"
HKR, NDI\params\BGProtection, type, 0, "enum"
HKR, NDI\params\BGProtection, default, 0, "0"
HKR, NDI\params\BGProtection\enum, 0, 0, "Auto"
HKR, NDI\params\BGProtection\enum, 1, 0, "On"
HKR, NDI\params\BGProtection\enum, 2, 0, "Off"
HKR, , FrameAggregation,0, "1"
HKR, NDI\params\FrameAggregation, ParamDesc, 0, "Frame Aggregation"
HKR, NDI\params\FrameAggregation, type, 0, "enum"
HKR, NDI\params\FrameAggregation, default, 0, "1"
HKR, NDI\params\FrameAggregation\enum, 0, 0, "Disable"
HKR, NDI\params\FrameAggregation\enum, 1, 0, "Enable"
HKR, , IEEE80211H, 0, "0"
HKR, NDI\params\IEEE80211H, ParamDesc, 0, "IEEE802.11h"
HKR, NDI\params\IEEE80211H, type, 0, "enum"
HKR, NDI\params\IEEE80211H, default, 0, "0"
HKR, NDI\params\IEEE80211H\enum, 0, 0, "Disable"
HKR, NDI\params\IEEE80211H\enum, 1, 0, "Enable"
HKR, , AutoChannelSelect, 0, "0"
HKR, NDI\params\AutoChannelSelect, ParamDesc,0, "Auto Channel Select"
HKR, NDI\params\AutoChannelSelect, type, 0, "enum"
HKR, NDI\params\AutoChannelSelect, default, 0, "0"
HKR, NDI\params\AutoChannelSelect\enum, 0, 0, "Disable"
HKR, NDI\params\AutoChannelSelect\enum, 1, 0, "Enable"
HKR, , WMMCapable, 0, "0"
HKR, NDI\params\WMMCapable, ParamDesc, 0, "WMM Capable"
HKR, NDI\params\WMMCapable, type, 0, "enum"
HKR, NDI\params\WMMCapable, default, 0, "0"
HKR, NDI\params\WMMCapable\enum, 0, 0, "Disable"
HKR, NDI\params\WMMCapable\enum, 1, 0, "Enable"
HKR, , APSDCapable, 0, "0"
HKR, NDI\params\APSDCapable, ParamDesc, 0, "APSD Capable"
HKR, NDI\params\APSDCapable, type, 0, "enum"
HKR, NDI\params\APSDCapable, default, 0, "0"
HKR, NDI\params\APSDCapable\enum, 0, 0, "Disable"
HKR, NDI\params\APSDCapable\enum, 1, 0, "Enable"
HKR, , APSDAC_BE, 0, "0"
HKR, NDI\params\APSDAC_BE, ParamDesc, 0, "AC_BE support APSD"
HKR, NDI\params\APSDAC_BE, type, 0, "enum"
HKR, NDI\params\APSDAC_BE, default, 0, "0"
HKR, NDI\params\APSDAC_BE\enum, 0, 0, "Disable"
HKR, NDI\params\APSDAC_BE\enum, 1, 0, "Enable"
HKR, , APSDAC_BK, 0, "0"
HKR, NDI\params\APSDAC_BK, ParamDesc, 0, "AC_BK support APSD"
HKR, NDI\params\APSDAC_BK, type, 0, "enum"
HKR, NDI\params\APSDAC_BK, default, 0, "0"
HKR, NDI\params\APSDAC_BK\enum, 0, 0, "Disable"
HKR, NDI\params\APSDAC_BK\enum, 1, 0, "Enable"
HKR, , APSDAC_VI, 0, "0"
HKR, NDI\params\APSDAC_VI, ParamDesc, 0, "AC_VI support APSD"
HKR, NDI\params\APSDAC_VI, type, 0, "enum"
HKR, NDI\params\APSDAC_VI, default, 0, "0"
HKR, NDI\params\APSDAC_VI\enum, 0, 0, "Disable"
HKR, NDI\params\APSDAC_VI\enum, 1, 0, "Enable"
HKR, , APSDAC_VO, 0, "0"
HKR, NDI\params\APSDAC_VO, ParamDesc, 0, "AC_VO support APSD"
HKR, NDI\params\APSDAC_VO, type, 0, "enum"
HKR, NDI\params\APSDAC_VO, default, 0, "0"
HKR, NDI\params\APSDAC_VO\enum, 0, 0, "Disable"
HKR, NDI\params\APSDAC_VO\enum, 1, 0, "Enable"
HKR, , MaxSPLength, 0, "0"
HKR, Default, MaxSPLength, 0, "0"
HKR, NDI\params\MaxSPLength, ParamDesc, 0, "Max Service Period Length"
HKR, NDI\params\MaxSPLength, type, 0, "int"
HKR, Ndi\params\MaxSPLength, default, 0, "0"
HKR, NDI\params\MaxSPLength, min, 0, "0"
HKR, NDI\params\MaxSPLength, max, 0, "3"
HKR, NDI\params\MaxSPLength, step, 0, "1"
HKR, NDI\params\MaxSPLength, optional, 0, "0"
HKR, , DLSCapable, 0, "0"
HKR, NDI\params\DLSCapable, ParamDesc, 0, "DLS Capable"
HKR, NDI\params\DLSCapable, type, 0, "enum"
HKR, NDI\params\DLSCapable, default, 0, "0"
HKR, NDI\params\DLSCapable\enum, 0, 0, "Disable"
HKR, NDI\params\DLSCapable\enum, 1, 0, "Enable"
HKR, , PSPXlink, 0, "0"
HKR, NDI\params\PSPXlink, ParamDesc, 0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink, type, 0, "enum"
HKR, NDI\params\PSPXlink, default, 0, "0"
HKR, NDI\params\PSPXlink\enum, 0, 0, "Disable"
HKR, NDI\params\PSPXlink\enum, 1, 0, "Enable"
HKR, , CCX2Control, 0x00010001, 0x00fa4600
HKR, , VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, Default, VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, , WPSDevName, 0, %WPS_DEVNAME_DEF_STR%
HKR, Default, WPSDevName, 0, %WPS_DEVNAME_DEF_STR%
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, Default, SSID, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, ParamDesc, 0, "SSID"
HKR, NDI\params\SSID, type, 0, "edit"
HKR, NDI\params\SSID, limitText, 0, "32"
HKR, NDI\params\SSID, default, 0, %SSID_DEF_STR%
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, Default, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0, 0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, , NetworkAddress, 0, ""
HKR, Default, NetworkAddress, 0, ""
HKR, NDI\params\NetworkAddress, ParamDesc, 0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, limitText, 0, "12"
HKR, NDI\params\NetworkAddress, default, 0, ""
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Saving Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum, 2, 0, "Fast_PSP (Power Save Mode)"
HKR, , PreambleType, 0, "0"
HKR, Default, PreambleType, 0, "0"
HKR, , RTSThresh, 0, "2347"
HKR, Default, RTSThresh, 0, "2347"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2347"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2347"
HKR, NDI\params\RTSThresh, step, 0, "32"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2346"
HKR, Default, FragThresh, 0, "2346"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragment Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2346"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2346"
HKR, NDI\params\FragThresh, step, 0, "32"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , AuthenType, 0, "0" ; Open System
HKR, Default, AuthenType, 0, "0"
HKR, , Encryption, 0, "1" ; Disable
HKR, Default, Encryption, 0, "1"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
[USB_050D_905C.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_050D&PID_905C"
[USB_050D_905B.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_050D&PID_905B"
[USB_050D_705B.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_050D&PID_705B"
[USB9X.ndi.reg]
HKR, , NTMPDriver, 0, rt73u98.sys
HKR, , BusType, 0, 15
HKR, NDI, CardType, 0, "PNP"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "rt73u98.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "rt73u98"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
win9x.CopyFiles=11 ; system32 subdirectory on win9x
[NT.CopyFiles]
rt73.sys ; NT Installation
[win9x.CopyFiles]
rt73u98.sys ; Win9x Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
rt73.sys=1
rt73u98.sys=1
[RTUSB.ndi.NT.reg]
HKR, Ndi, Service, 0, "rt73"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[Ralink.Service]
DisplayName=%Ralink.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt73.sys
LoadOrderGroup=NDIS
[Belkin.Service]
DisplayName=%Belkin.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt73.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt73.sys"
HKR, , TypesSupported, 0x00010001, 7
[strings]
Provider="Ralink"
Ralink="Ralink Technology Corp."
Qcom="Qcom Technology Inc."
Gigabyte="Gigabyte Technology Corp."
Conceptronic="2L (Conceptronic)"
Surecom="SURECOM Technology Corp."
Asus="ASUSTeK Computer Inc."
Amit="AMIT Technology, Inc."
CNet="CNet Technology Inc."
Huawei-3Com="Huawei-3Com Technology Co., Ltd."
Askey="WLAN"
Amigo="Amigo Technology Inc."
HP="Gemtek"
Belkin="Belkin Components"
Buffalo="Buffalo Technology Inc."
Ralink.DeviceDesc="RT73 USB Wireless LAN Card"
Qcom.DeviceDesc="RT73 USB Wireless LAN Card"
Gigabyte.DeviceDesc="Gigabyte GN-WB01GS USB WLAN Card"
Gigabyte2.DeviceDesc="Gigabyte GN-WI05GS mini WLAN Card"
Conceptronic.DeviceDesc="Conceptronic 54Mbps USB adapter"
M6877.DeviceDesc="802.11g Mini Card Wireless Adapter"
MA874.DeviceDesc="802.11g MiniUSB 2.0 Wireless Bluetooth Combo"
M6874.DeviceDesc="802.11g MiniUSB 2.0 Wireless Bluetooth Combo"
MA861.DeviceDesc="802.11g USB 2.0 Stick"
GMEWLGRL.DeviceDesc="RT73 USB Wireless LAN Card"
Surecom.DeviceDesc="802.11g 54M Wireless LAN USB Adapter"
ASUS.DeviceDesc="ASUS USB Wireless Network Adapter"
ASUSGEN.DeviceDesc="802.11b/g USB Wireless Network Adapter"
AMIT.DeviceDesc="CG-WLUSB2GO, corega Wireless USB Adapter"
CNet.DeviceDesc="CNet Wireless USB dongle"
Huawei-3Com.DeviceDesc="Aolynk WUB320g USB Wireless LAN Card"
Askey.DeviceDesc="WLAN USB Wireless LAN Stick"
Amigo1.DeviceDesc="Wireless USB Card"
Amigo2.DeviceDesc="Wireless USB Card"
HP.DeviceDesc="USB Wireless 802.11 b/g Adaptor"
Belkin.DeviceDesc="Belkin Wireless G Plus MIMO USB Network Adapter"
Belkin705B.DeviceDesc="Belkin Wireless G USB Adapter"
Buffalo.DeviceDesc="BUFFALO WLI-U2-SG54HP"
INSTALL_DISK_STR="Wireless 11g USB Installation Disk"
Ralink.Service.DispName="RT73 USB Wireless LAN Card Driver"
Qcom.Service.DispName="RT73 USB Wireless LAN Card Driver"
Gigabyte.Service.DispName="Gigabyte RT73 Wireless Driver"
Conceptronic.Service.DispName="Conceptronic RT73 Wireles Driver"
Surecom.Service.DispName="Surecom RT73 Wireles Driver"
ASUS.Service.DispName="ASUS USB Wireless LAN Card Driver"
AMIT.Service.DispName="CG-WLUSB2GO RT73 Wireles Driver"
CNET.Service.DispName="CNet RT73 Wireless Driver"
HUAWEI.Service.DispName="Huawei-3Com RT73 Wireless Driver"
Askey.Service.DispName="Askey RT73 Wireless Driver"
Amigo.Service.DispName="Amigo RT73 Wireless Driver"
HP.Service.DispName="USB Wireless 802.11 b/g Adaptor Driver"
Belkin.Service.DispName="Belkin Wireless G Plus MIMO USB Network Adapter Driver"
Buffalo.Service.DispName="BUFFALO WLI-U2-SG54HP Wireless Driver"
SSID_DEF_STR=""
VENDOR_DESC_DEF_STR="IEEE 802.11g Wireless Card."
NETWORK_TYPE_DEF_STR="1"
CHANNEL="1"
WPS_DEVNAME_DEF_STR="Ralink Client"

