
[Version]
DriverVer=06/23/2004, 3.0.11.1
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=O4I01A.cat
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList,NTx86.5.1
[DeviceList.NTx86.5.1]
%DCB1_DESC_STR%=NIC_DCB1_XP, PCI\VEN_1FCA&DEV_0110&SUBSYS_01100000
[DeviceList]
%DCB1_DESC_STR%=NIC_DCB1, PCI\VEN_1FCA&DEV_0110&SUBSYS_01100000
[NIC_DCB1] ; Win9x
DelReg=COMMON_AMAC_DEL.reg
AddReg=NIC_DCB1.reg, NIC_DCB1.reg1, COMMON_ICB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
;CpyFiles=NIC_DRIVER.copy, NIC_CCU.copy
[NIC_DCB1.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=NIC_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=NIC_DRIVER.copy.NT, NIC_CCU.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[NIC_DCB1.NT.Services]
AddService="O4I01A", 2, NIC_DRIVER_DCB1.Service, NIC_DRIVER.EventLog
[NIC_DCB1.NT.CoInstallers]
;CpyFiles=NIC_COINSTALL.copy.NT
AddReg=NIC_COINSTALL.reg.NT
[NIC_DCB1_XP] ; Winxp
DelReg=COMMON_AMAC_DEL.reg
AddReg=NIC_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=NIC_DRIVER.copy.XP, NIC_CCU.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[NIC_DCB1_XP.Services]
AddService="O4I01A", 2, NIC_DRIVER_DCB1.Service, NIC_DRIVER.EventLog
[NIC_DCB1_XP.CoInstallers]
;CpyFiles=NIC_COINSTALL.copy.NT
AddReg=NIC_COINSTALL.reg.NT
[NIC_DCB1.reg1]
[NIC_DCB1.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1FCA&DEV_0110&SUBSYS_01100000"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB1_DESC_STR%
HKR,,11dMode,0,0
HKR,,CountryName,0,"US "
HKR,,EnableRadio,0,1
[NIC_COINSTALL.reg.NT]
[NIC_DRIVER_DCB1.Service]
DisplayName=%NIC_SERVICE_DISPLAY_DCB%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\O4I01A.sys
LoadOrderGroup=NDIS
[NIC_DRIVER.EventLog]
AddReg=NIC_DRIVER.EventLog.reg
[NIC_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_ICB.reg]
HKR,NDI ,Service ,0 ,"O4I01A"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"O4I01A.sys"
HKR, ,CardBusBridgeLatencyTimer ,0 ,"0"
HKR, ,CardBusBridgeCacheLineSize ,0 ,"0"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"O4I01A"
HKR,NDIS ,MajorNdisVersion ,1 ,04
HKR,NDIS ,MinorNdisVersion ,1 ,00
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,SSID ,0 ,"speedtouch"
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR, ,NitroMode ,0 ,"0"
HKR,Ndi\params\RTSThresh,default,0,"2347"
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,"int"
HKR,NDI\params\RTSThresh,flag,1,"20","00","00","00"
HKR,NDI\params\RTSThresh,min,0,"0"
HKR,NDI\params\RTSThresh,max,0,"2347"
HKR,NDI\params\RTSThresh,step,0,"1"
HKR,Ndi\params\FragThresh,default,0,"2346"
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,"int"
HKR,NDI\params\FragThresh,flag,1,"20","00","00","00"
HKR,NDI\params\FragThresh,min,0,"256"
HKR,NDI\params\FragThresh,max,0,"2346"
HKR,NDI\params\FragThresh,step,0,"2"
[COMMON_AMAC_DEL.reg]
HKR,defaults,DataRates
HKR,NDI\params\DataRates
HKR,NDI\params\DataRate
HKR,DSChannel
HKR,defaults,DSChannel
HKR,NDI\params\DSChannel
[COMMON_AMAC.reg]
HKR,NDI\params\ShortRetryLimit,default,0,"7"
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,"int"
HKR,NDI\params\ShortRetryLimit,min,0,"1"
HKR,NDI\params\ShortRetryLimit,max,0,"255"
HKR,NDI\params\ShortRetryLimit,step,0,"1"
HKR,NDI\params\LongRetryLimit,default,0,"4"
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,"int"
HKR,NDI\params\LongRetryLimit,min,0,"1"
HKR,NDI\params\LongRetryLimit,max,0,"255"
HKR,NDI\params\LongRetryLimit,step,0,"1"
HKR,NDI\params\ConfigProfile,default,0,"1"
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,,"enum"
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
HKR,NDI\params\PpePdlpEnable,default,0,0
HKR,NDI\params\PpePdlpEnable,ParamDesc,,%PPE_PDLP%
HKR,NDI\params\PpePdlpEnable,type,,enum
HKR,NDI\params\PpePdlpEnable,flag,1,30,00,00,00
HKR,NDI\params\PpePdlpEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpePdlpEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpeCompressEnable,default,0,0
HKR,NDI\params\PpeCompressEnable,ParamDesc,,%PPE_COMPRESS%
HKR,NDI\params\PpeCompressEnable,type,,enum
HKR,NDI\params\PpeCompressEnable,flag,1,30,00,00,00
HKR,NDI\params\PpeCompressEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpeCompressEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpeConcatEnable,default,0,0
HKR,NDI\params\PpeConcatEnable,ParamDesc,,%PPE_CONCAT%
HKR,NDI\params\PpeConcatEnable,type,,enum
HKR,NDI\params\PpeConcatEnable,flag,1,30,00,00,00
HKR,NDI\params\PpeConcatEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpeConcatEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpePiggyBackEnable,default,0,0
HKR,NDI\params\PpePiggyBackEnable,ParamDesc,,%PPE_PIGGYBACK%
HKR,NDI\params\PpePiggyBackEnable,type,,enum
HKR,NDI\params\PpePiggyBackEnable,flag,1,30,00,00,00
HKR,NDI\params\PpePiggyBackEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpePiggyBackEnable\enum,1,,%ON_STR%
[COMMON_PSMODE.reg]
HKR,Ndi\params\PSMode,default,0,"1"
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,"enum"
HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
[COMMON_PS_MODE_XP.reg]
HKR,Ndi\params\PSMode,default,0,"1"
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,"enum"
HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
NIC_DRIVER.copy=11 ; Win9x=%windir%\system
NIC_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
NIC_DRIVER.copy.XP=12 ; Winxp=%windir%\system32\drivers
NIC_CCU.copy=11 ; Win9x=%windir%\system
[NIC_CCU.copy]
[NIC_DRIVER.copy]
O4I01A.sys
[NIC_DRIVER.copy.NT]
O4I01A.sys
[NIC_DRIVER.copy.XP]
O4I01A.sys,O4I01A51.sys
[NIC_COINSTALL.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
O4I01A.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
O4I01A.sys=1
O4I01A51.sys=1
[Strings]
VER_VENDOR_STR="THOMSON"
VER_VENDOR_NAME_STR="THOMSON"
NIC_SERVICE_DISPLAY_DCB="ST110 54Mbps 2.4GHz Wireless Adapter Driver"
INSTALL_DISK_STR="ST110 54Mbps 2.4GHz Wireless Adapter Install Disk"
ON_STR="On"
OFF_STR="Off"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
LOAD_FIRMWARE_STR="Firmware Download"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
ANTENNA_TX_STR="Antenna Tx"
ANTENNA_RX_STR="Antenna Rx"
ANTENNA_DIVERSITY_STR="Antenna Diversity"
CHANNEL_STR="Channel"
DATARATES_STR="Data Rate"
DATARATES_AUTO="Fully Automatic"
ALSR_STR="Auto Long Slot Reassociation"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WIFI"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"
PPE_PDLP="Direct Link"
PPE_COMPRESS="Compression"
PPE_CONCAT="Concatenation"
PPE_PIGGYBACK="PiggyBack"
DCB1_DESC_STR="SpeedTouch 110g Wireless PC Card"

