
[Version]
Signature="$CHICAGO$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%ATHEROS%
Compatible=1
DriverVer=07/28/2011,7.7.0.102
Catalogfile.nt=netathuw.cat
[Manufacturer]
%ATHEROS%=Atheros
%NETGEAR%=NETGEAR
%DLINK%=DLINK
%AZUREWAVE%=AZUREWAVE
%LITEON%=LITEON
%SMC%=SMC
%VIA%=VIA
%VERIZON%=Verizon
[ControlFlags]
ExcludeFromSelect=*
[Atheros]
%ATHER.DeviceDesc.9271%=ATHER_DEV_9271.ndi, USB\VID_0CF3&PID_9271
%ATHER.DeviceDesc.7010%=ATHER_DEV_7010.ndi, USB\VID_0CF3&PID_7010
%ATHER.DeviceDesc.7015%=ATHER_DEV_7015.ndi, USB\VID_0CF3&PID_7015
%ATHER.DeviceDesc.1006%=ATHER_DEV_1006.ndi, USB\VID_0CF3&PID_1006
[NETGEAR]
%NTGR.DeviceDesc.9030%=NTGR_DEV_9030.ndi, USB\VID_0846&PID_9030
%NTGR.DeviceDesc.9018%=NTGR_DEV_9018.ndi, USB\VID_0846&PID_9018
[DLINK]
%DLINK.DeviceDesc.3A10%=DLINK_DEV_3A10.ndi, USB\VID_07D1&PID_3A10
[AZUREWAVE]
%AZWV.DeviceDesc.3327%=AZWV_DEV_3327.ndi, USB\VID_13D3&PID_3327
%AZWV.DeviceDesc.3328%=AZWV_DEV_3328.ndi, USB\VID_13D3&PID_3328
%AZWV.DeviceDesc.3346%=AZWV_DEV_3346.ndi, USB\VID_13D3&PID_3346
%AZWV.DeviceDesc.3348%=AZWV_DEV_3348.ndi, USB\VID_13D3&PID_3348
%AZWV.DeviceDesc.3349%=AZWV_DEV_3349.ndi, USB\VID_13D3&PID_3349
%AZWV.DeviceDesc.3350%=AZWV_DEV_3350.ndi, USB\VID_13D3&PID_3350
[LITEON]
%ATHER.DeviceDesc.9271%=ATHER_DEV_9271.ndi, USB\VID_04CA&PID_4605
[SMC]
%SMC.DeviceDesc.A704%=SMC_DEV_A704.ndi, USB\VID_083A&PID_A704
[VIA]
%VIA.DeviceDesc.3801%=ATHER_DEV_9271.ndi, USB\VID_040D&PID_3801
[VERIZON]
%VRZN.DeviceDesc.1200%=ATHER_DEV_7015.ndi, USB\VID_1668&PID_1200
[ATHER_DEV_9271.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_9271.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[ATHER_DEV_7010.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.abgnub.reg, uapsd.reg, 7010.reg, htDisableWepTkip.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_7010.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[ATHER_DEV_7015.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg, 7015.reg, htDisableWepTkip.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_7015.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[ATHER_DEV_1006.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, customer1.SCAN.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_1006.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[NTGR_DEV_9030.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, NTGR.reg, scanReduce.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[NTGR_DEV_9030.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[NTGR_DEV_9018.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.abgnub.reg, uapsd_VO.reg, NTGR_9018.reg, htDisableWepTkip.reg, scanReduce.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[NTGR_DEV_9018.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[DLINK_DEV_3A10.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, DLINK.reg, htDisableWepTkip.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[DLINK_DEV_3A10.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[AZWV_DEV_3327.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[AZWV_DEV_3327.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[AZWV_DEV_3328.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[AZWV_DEV_3328.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[AZWV_DEV_3346.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[AZWV_DEV_3346.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[AZWV_DEV_3348.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[AZWV_DEV_3348.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[AZWV_DEV_3349.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[AZWV_DEV_3349.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[AZWV_DEV_3350.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, sys.TcpParams.reg, uapsd.reg, ATHR_9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[AZWV_DEV_3350.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[SMC_DEV_A704.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, 5416.bgnub.reg, uapsd.reg, 7015.reg, htDisableWepTkip.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[SMC_DEV_A704.ndi.NT.Services]
AddService=AR9271, 2, ATHER.Service, common.EventLog
[5416.bgub.reg]
HKR, , NetBand, 0x00002, "12"
HKR, , wModeSelect, 0x00002, "40972"
HKR, CustomParams\Configurations, NicType, 0x10003, 1
HKR, , abolt, 0x00002, "0"
HKR, , rateCtrlEnable, 0x00002, "1"
HKR, , rmEnable, 0x00002, "1"
[5416.bgnub.reg]
HKR, , NetBand, 0x00002, "40972"
HKR, , wModeSelect, 0x00002, "40972"
HKR, CustomParams\Configurations, NicType, 0x10003, 1
HKR, , abolt, 0x00002, "0"
HKR, , rateCtrlEnable, 0x00002, "1"
HKR, , rmEnable, 0x00002, "1"
[5416.abgnub.reg]
HKR, CustomParams\Configurations, NicType, 0x10003, 1
HKR, , abolt, 0x00002, "0"
HKR, , rateCtrlEnable, 0x00002, "1"
HKR, , rmEnable, 0x00002, "1"
HKR, Ndi\params\NetBand, ParamDesc, 0, %WirelessMode%
HKR, Ndi\params\NetBand, Base, 0, "10"
HKR, Ndi\params\NetBand, default, 0, "61455"
HKR, Ndi\params\NetBand, type, 0, "enum"
HKR, Ndi\params\NetBand\enum, "61455", 0, %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum, "20481", 0, %WirelessMode5GHzOnly%
HKR, Ndi\params\NetBand\enum, "40972", 0, %WirelessMode2GHzOnly%
[5416.antennacontrols.reg]
HKR, , rxChainSelect, 0x00002, "7"
HKR, , rxChainSelectLegacy, 0x00002, "7"
HKR, , forceBias, 0x00002, "2"
HKR, , rxChainDetect, 0x00002, "1"
HKR, , rxChainDetectRef, 0x00002, "0"
HKR, , rxChainDetectThreshA, 0x00002, "0"
HKR, , rxChainDetectThreshG, 0x00002, "0"
HKR, , rxChainDetectDeltaA, 0x00002, "20"
HKR, , rxChainDetectDeltaG, 0x00002, "20"
[pushbutton.reg]
HKR, , wpsButtonGpio, 0x00002, "9"
[bandselect.reg]
HKR, Ndi\params\NetBand, ParamDesc, 0, %WirelessMode%
HKR, Ndi\params\NetBand, Base, 0, "10"
HKR, Ndi\params\NetBand, default, 0, "1823"
HKR, Ndi\params\NetBand, type, 0, "enum"
HKR, Ndi\params\NetBand\enum, "1823", 0, %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum, "1795", 0, %WirelessMode5GHzOnly%
HKR, Ndi\params\NetBand\enum, "28", 0, %WirelessMode2GHzOnly%
[pcibusconfig.reg]
HKR, , BusConfig, 0x00002, "0"
[d3hot.reg]
HKR, , pciePowerReset, 0x00002, "0"
HKR, , pcieRestore, 0x00002, "1"
[expresscardaspmoff.reg]
HKR, , pciDetectEnable, 0x00002, "2"
HKR, , pciePowerSaveEnable, 0x00002, "1"
HKR, , pcieAspm, 0x00002, "0"
[gpioled.reg]
HKR,, linkLEDFunc, 0, "49"
HKR,, activityLEDFunc, 0, "51"
HKR,, connectionLEDFunc, 0, "55"
[uapsd.reg]
HKR, Ndi\params\uapsdEnabledBE, ParamDesc, 0, %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledBE, default, 0, "0"
HKR, Ndi\params\uapsdEnabledBE, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledBE\enum, "1", 0, %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum, "0", 0, %uapsdEnabledBEOff%
HKR, Ndi\params\uapsdEnabledBK, ParamDesc, 0, %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledBK, default, 0, "0"
HKR, Ndi\params\uapsdEnabledBK, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledBK\enum, "1", 0, %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum, "0", 0, %uapsdEnabledBKOff%
HKR, Ndi\params\uapsdEnabledVI, ParamDesc, 0, %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledVI, default, 0, "0"
HKR, Ndi\params\uapsdEnabledVI, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledVI\enum, "1", 0, %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum, "0", 0, %uapsdEnabledVIOff%
HKR, Ndi\params\uapsdEnabledVO, ParamDesc, 0, %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledVO, default, 0, "0"
HKR, Ndi\params\uapsdEnabledVO, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledVO\enum, "1", 0, %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum, "0", 0, %uapsdEnabledVOOff%
HKR, Ndi\params\psPollEnable, ParamDesc, 0, %psPoll%
HKR, Ndi\params\psPollEnable, Base, 0, "10"
HKR, Ndi\params\psPollEnable, default, 0, "0"
HKR, Ndi\params\psPollEnable, type, 0, "enum"
HKR, Ndi\params\psPollEnable\enum, "1", 0, %psPollEnable%
HKR, Ndi\params\psPollEnable\enum, "0", 0, %psPollDisable%
[uapsd_VO.reg]
HKR, Ndi\params\uapsdEnabledBE, ParamDesc, 0, %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledBE, default, 0, "0"
HKR, Ndi\params\uapsdEnabledBE, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledBE\enum, "1", 0, %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum, "0", 0, %uapsdEnabledBEOff%
HKR, Ndi\params\uapsdEnabledBK, ParamDesc, 0, %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledBK, default, 0, "0"
HKR, Ndi\params\uapsdEnabledBK, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledBK\enum, "1", 0, %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum, "0", 0, %uapsdEnabledBKOff%
HKR, Ndi\params\uapsdEnabledVI, ParamDesc, 0, %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledVI, default, 0, "0"
HKR, Ndi\params\uapsdEnabledVI, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledVI\enum, "1", 0, %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum, "0", 0, %uapsdEnabledVIOff%
HKR, Ndi\params\uapsdEnabledVO, ParamDesc, 0, %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledVO, default, 0, "1"
HKR, Ndi\params\uapsdEnabledVO, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledVO\enum, "1", 0, %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum, "0", 0, %uapsdEnabledVOOff%
HKR, Ndi\params\psPollEnable, ParamDesc, 0, %psPoll%
HKR, Ndi\params\psPollEnable, Base, 0, "10"
HKR, Ndi\params\psPollEnable, default, 0, "1"
HKR, Ndi\params\psPollEnable, type, 0, "enum"
HKR, Ndi\params\psPollEnable\enum, "1", 0, %psPollEnable%
HKR, Ndi\params\psPollEnable\enum, "0", 0, %psPollDisable%
[5416.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,pcieClockReq
HKR,,rmEnable
HKR,,overrideACstatus
HKR, Ndi\params\NetBand
HKR,,rxChainSelect
HKR,,txChainSelectLegacy
HKR,,rxChainSelectLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR,,pciePowerSaveEnable
HKR,,pcieAspm
HKR,,scanReduceLevel
HKR,,scanTimePreSleep
[5416.reg]
HKR, Ndi\params\MapRegisters, ParamDesc, 0, %MapRegisters%
HKR, Ndi\params\MapRegisters, default, 0, "256"
HKR, Ndi\params\MapRegisters, min, 0, "32"
HKR, Ndi\params\MapRegisters, max, 0, "512"
HKR, Ndi\params\MapRegisters, step, 0, "8"
HKR, Ndi\params\MapRegisters, base, 0, "10"
HKR, Ndi\params\MapRegisters, type, 0, "int"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\sleepMode, ParamDesc, 0, %sleepMode%
HKR, Ndi\params\sleepMode, Base, 0, "10"
HKR, Ndi\params\sleepMode, default, 0, "0"
HKR, Ndi\params\sleepMode, type, 0, "enum"
HKR, Ndi\params\sleepMode\enum, "0", 0, %sleepModeOff%
HKR, Ndi\params\sleepMode\enum, "2", 0, %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum, "1", 0, %sleepModeMax%
HKR, Ndi\params\shortPreamble, ParamDesc, 0, %shortPreamble%
HKR, Ndi\params\shortPreamble, Base, 0, "10"
HKR, Ndi\params\shortPreamble, default, 0, "1"
HKR, Ndi\params\shortPreamble, type, 0, "enum"
HKR, Ndi\params\shortPreamble\enum, "1", 0, %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0", 0, %shortPreambleDisable%
HKR, Ndi\params\radioEnable, ParamDesc, 0, %radioEnable%
HKR, Ndi\params\radioEnable, Base, 0, "10"
HKR, Ndi\params\radioEnable, default, 0, "1"
HKR, Ndi\params\radioEnable, type, 0, "enum"
HKR, Ndi\params\radioEnable\enum, "1", 0, %radioEnableOn%
HKR, Ndi\params\radioEnable\enum, "0", 0, %radioEnableOff%
HKR, Ndi\params\scanTimeValid, ParamDesc, 0, %scanTimeValid%
HKR, Ndi\params\scanTimeValid, default, 0, "60"
HKR, Ndi\params\scanTimeValid, min, 0, "20"
HKR, Ndi\params\scanTimeValid, max, 0, "120"
HKR, Ndi\params\scanTimeValid, step, 0, "5"
HKR, Ndi\params\scanTimeValid, base, 0, "10"
HKR, Ndi\params\scanTimeValid, type, 0, "int"
HKR, Ndi\params\ccx5FeatureEnable, ParamDesc, 0, %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable, Base, 0, "10"
HKR, Ndi\params\ccx5FeatureEnable, default, 0, "0"
HKR, Ndi\params\ccx5FeatureEnable, type, 0, "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1", 0, %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0", 0, %ccx5FeatureEnableMfpDisable%
HKR, Ndi\params\PSPXLinkMode, ParamDesc, 0, %PSPXLinkMode%
HKR, Ndi\params\PSPXLinkMode, Base, 0, "10"
HKR, Ndi\params\PSPXLinkMode, default, 0, "0"
HKR, Ndi\params\PSPXLinkMode, type, 0, "enum"
HKR, Ndi\params\PSPXLinkMode\enum, "1", 0, %PSPXLinkModeEnable%
HKR, Ndi\params\PSPXLinkMode\enum, "0", 0, %PSPXLinkModeDisable%
HKR, CustomParams\Configurations, MajorVersion, 0x10003, 2
HKR, CustomParams\Configurations, MinorVersion, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
[7010.reg]
HKR, , forceNormalSlotMrvl, 0x00002, "1"
HKR, , htAdhocEnable, 0x00002, "0"
HKR, , isMagpie, 0x00002, "1"
HKR, , gpioLedCustom, 0x00002, "1"
HKR, , gpioPinFunc0, 0x00002, "12"
HKR, , gpioPinFunc1, 0x00002, "10"
HKR, , stbcEnable, 0x00002, "1"
HKR, , wpsButtonGpio, 0x00002, "13"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program, USBVIDPID, 0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%;%AZWV_VID_13D3%;%LION_VID_04CA%"
[7015.reg]
HKR, , forceNormalSlotMrvl, 0x00002, "1"
HKR, , htAdhocEnable, 0x00002, "0"
HKR, , isMagpie, 0x00002, "1"
HKR, , gpioLedCustom, 0x00002, "1"
HKR, , gpioPinFunc0, 0x00002, "12"
HKR, , gpioPinFunc1, 0x00002, "10"
HKR, , stbcEnable, 0x00002, "1"
HKR, , wpsButtonGpio, 0x00002, "4"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program, USBVIDPID, 0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%;%AZWV_VID_13D3%;%LION_VID_04CA%"
[htDisableWepTkip.reg]
HKR, , htEnableWepTkip, 0x00002, "0"
[surpriseRemovalOk.reg]
HKR, , surpriseRemovalOk, 0x10003, 1
[scanReduce.reg]
HKR, , scanReduceLevel, 0x00002, "1"
HKR, , scanTimePreSleep, 0x00002, "10"
[NTGR.reg]
HKR, , ignore11dBeacon, 0, 1
HKR, , gpioLedCustom, 0, 8
HKR, , gpioPinFunc0, 0, 15
HKR, , swapDefaultLED, 0, 1
HKR, , GreenTx, 0, 15
HKR, , htEnableWepTkip, 0x00002, "3"
HKR, , htEnableWepTkipAgg, 0x00002, "0"
[NTGR_9018.reg]
HKR, , forceNormalSlotMrvl, 0x00002, "1"
HKR, , htAdhocEnable, 0x00002, "0"
HKR, , isMagpie, 0x00002, "1"
HKR, , gpioLedCustom, 0x00002, "9"
HKR, , gpioPinFunc0, 0x00002, "12"
HKR, , gpioPinFunc1, 0x00002, "10"
HKR, , GreenTx, 0, 0
HKR, , updatelinkspeed, 0, 1
HKR, , pciePowerSaveEnable, 0, 2
HKR, , stbcEnable, 0x00002, "1"
HKR, , wpsButtonGpio, 0x00002, "13"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program, USBVIDPID, 0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%;%AZWV_VID_13D3%;%LION_VID_04CA%"
[DLINK.reg]
HKR, , gpioLedCustom, 0, 1
HKR, , gpioPinFunc0, 0, 15
HKR, , swapDefaultLED, 0, 1
[customer0.reg]
HKR, , pcieAspm, 0x00002, "2"
HKR, , pciePowerSaveEnable, 0x00002, "1"
HKR, , overrideACstatus, 0x00002, "1"
HKR, , forceWake, 0x00002, "0"
HKR, , antennaSwitchSwap, 0x00002, "1"
HKR, , gpioPinFunc1, 0x00002, "1"
HKR, , ssid, 0x00002, "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,, %Mode11d%
HKR,NDI\params\ignore11dBeacon,type,, "enum"
HKR,NDI\params\ignore11dBeacon,Default,, "1"
HKR,NDI\params\ignore11dBeacon\enum,0,, %Mode11dEnable%
HKR,NDI\params\ignore11dBeacon\enum,1,, %Mode11dDisable%
HKR, Ndi\params\roamRssiA, ParamDesc, 0, %roamRssiA%
HKR, Ndi\params\roamRssiA, default, 0, "15"
HKR, Ndi\params\roamRssiA, min, 0, "1"
HKR, Ndi\params\roamRssiA, max, 0, "95"
HKR, Ndi\params\roamRssiA, step, 0, "1"
HKR, Ndi\params\roamRssiA, base, 0, "10"
HKR, Ndi\params\roamRssiA, type, 0, "int"
HKR, Ndi\params\sleepMode, ParamDesc, 0, %sleepMode%
HKR, Ndi\params\sleepMode, Base, 0, "10"
HKR, Ndi\params\sleepMode, default, 0, "1"
HKR, Ndi\params\sleepMode, type, 0, "enum"
HKR, Ndi\params\sleepMode\enum, "0", 0, %sleepModeOff%
HKR, Ndi\params\sleepMode\enum, "2", 0, %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum, "1", 0, %sleepModeMax%
HKR, Ndi\params\scanTimeValid, ParamDesc, 0, %scanTime%
HKR, Ndi\params\scanTimeValid, default, 0, "60"
HKR, Ndi\params\scanTimeValid, min, 0, "20"
HKR, Ndi\params\scanTimeValid, max, 0, "120"
HKR, Ndi\params\scanTimeValid, step, 0, "5"
HKR, Ndi\params\scanTimeValid, base, 0, "10"
HKR, Ndi\params\scanTimeValid, type, 0, "int"
HKR,, isMagpie, 0, 0
[customer0.LED.reg]
HKR, , gpioPinFunc1, 0x00002, "0"
[customer0.LED1.reg]
HKR, , gpioPinFunc1, 0x00002, "1"
HKR, , overrideACstatus, 0x00002, "1"
HKR, , pcieClockReq, 0x00002, "0"
HKR, , pciePowerSaveEnable, 0x00002, "1"
HKR, , pcieAspm, 0x00002, "2"
[customer1.SCAN.reg]
HKR, , bkPeriodicScanEnable, 0x00002, "0"
HKR, , scanPendingCriterion, 0x00002, "65"
[customer11_11nwmode.reg]
HKR, Ndi\params\wModeSelect, ParamDesc, 0, %wModeSelect%
HKR, Ndi\params\wModeSelect, Base, 0, "10"
HKR, Ndi\params\wModeSelect, default, 0, "49719"
HKR, Ndi\params\wModeSelect, type, 0, "enum"
HKR, Ndi\params\wModeSelect\enum, "32772", 0, %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum, "16387", 0, %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum, "32796", 0, %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum, "49719", 0, %wModeSelect11abgn%
[customer11_legacywmode.reg]
HKR, Ndi\params\wModeSelect, ParamDesc, 0, %wModeSelect%
HKR, Ndi\params\wModeSelect, Base, 0, "10"
HKR, Ndi\params\wModeSelect, default, 0, "2075"
HKR, Ndi\params\wModeSelect, type, 0, "enum"
HKR, Ndi\params\wModeSelect\enum, "4", 0, %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum, "3", 0, %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum, "28", 0, %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum, "2075", 0, %wModeLegacy11abg%
[customer11Ant.reg]
HKR, Ndi\params\antennaSwitch, ParamDesc, 0, %antennaSwitch%
HKR, Ndi\params\antennaSwitch, Base, 0, "10"
HKR, Ndi\params\antennaSwitch, default, 0, "0"
HKR, Ndi\params\antennaSwitch, type, 0, "enum"
HKR, Ndi\params\antennaSwitch\enum, "1", 0, %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum, "2", 0, %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum, "0", 0, %antennaSwitchAuto%
[rssiAdjust.reg]
HKR, , rssiAdjust, 0x00002, "7"
[cmdRegister.reg]
HKR, , cmdRegister, 0x00002, "838"
[ATHER.reg]
HKR, Ndi, Service, 0, "AR9271"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[ATHER.Service]
DisplayName=%ATHER.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\athuw.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[sys.TcpParams.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000001
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000
[sys.TcpParamslan.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000001
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000
[ATHR_9271.reg]
HKR, , forceNormalSlotMrvl, 0x00002, "1"
HKR, , htAdhocEnable, 0x00002, "0"
HKR, , wpsButtonGpio, 0x00002, "13"
HKLM,SOFTWARE\Atheros\Atheros Client Installation Program, USBVIDPID, 0, "%ATHR_VID_0CF3%;%NTGR_VID_0846%;%AZWV_VID_13D3%;%LION_VID_04CA%"
[ATHER.CopyFiles.nt]
athuw.sys,,,2
[ATHER.DelIniFiles]
Athnic.ini,,,1
[SourceDisksNames]
1=%Atheros_Disk%,,,
[SourceDisksFiles]
athuw.sys=1,, ; on distribution disk 1
[DestinationDirs]
ATHER.CopyFiles.nt=12
ATHER.DelIniFiles=10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir=11
[DEFAULTDESTDIRS]
[Strings]
Atheros="Atheros Communications Inc."
NETGEAR="Netgear Inc."
DLINK="D-Link"
AZUREWAVE="AzureWave Technologies, Inc."
LITEON="Lite-On"
SMC="SMC Networks, Inc."
VIA="VIA"
VERIZON="Verizon"
MapRegisters="Map Registers"
NetworkAddress="Network Address"
sleepMode="Power Save Mode"
scanTimeValid="Scan Valid Interval"
scanTime="Roam Time (sec)"
roamRssiA="Roam Time Threshold (db)"
sleepModeOff="Off"
sleepModeNormal="Normal"
sleepModeMax="Maximum"
tpc="Transmit Power"
tpcLowest="Lowest"
tpc12="12.5%"
tpc25="25%"
tpc50="50%"
tpc100="100%"
shortPreamble="802.11b Preamble"
shortPreambleEnable="Long and Short"
shortPreambleDisable="Long only"
radioEnable="Radio On/Off"
radioEnableOn="On"
radioEnableOff="Off"
WirelessMode="Wireless Mode Selection"
WirelessModeAuto="Auto"
WirelessMode5GHzOnly="5 GHz Only"
WirelessMode2GHzOnly="2.4 GHz Only"
rssiThrHigh="RSSI Threshold"
rssiThrHighNormal="Normal"
rssiThrHighMin="Min"
roamPolicy="Roaming Policy"
roamPolicyVeryLow="Very Low"
roamPolicyLow="Low"
roamPolicyNormal="Normal"
roamPolicyHigh="High"
roamPolicyVeryHigh="Very High"
scanTimeValidcust="Roam Time (sec)"
scanTimeValidcust120="120"
scanTimeValidcust60="60"
scanTimeValidcust45="45"
scanTimeValidcust30="30"
scanTimeValidcust20="20"
scanTimeValidcust10="10"
scanTimeValidcust5="5"
sleepMode_DEFAULT="2"
NetBand_DEF_STR_A="3" ; (A/T)
NetBand_DEF_STR_AB="7" ; (A/T/B)
NetBand_DEF_STR_G="12" ; (B/G)
NetBand_DEF_STR_AG="15" ; (A/T/B/G)
AdhocBand_DEF_STR_A="1" ; (A)
AdhocBand_DEF_STR_AB="1" ; (A)
AdhocBand_DEF_STR_G="0" ; (B)
AdhocBand_DEF_STR_AG="0" ; (B)
shortPreamble_DEFAULT="1"
authTypeUseOnly="802.11 Authentication Type"
authAuto="Auto"
authOpen="Open"
authShared="Shared"
bkScanEnable="BackgroundScan On/Off"
bkScanEnableOn="On"
bkScanEnableOff="Off"
roamRssi11A="roamRssiA"
roamRssi11B="roamRssiB"
roamRssi11BOnly="roamRssiBOnly"
roamRateA="roamRateA"
roamRateA6M=" 6Mbps"
roamRateA9M=" 9Mbps"
roamRateA12M="12Mbps"
roamRateA18M="18Mbps"
roamRateA24M="24Mbps"
roamRateA36M="36Mbps"
roamRateA48M="48Mbps"
roamRateA54M="54Mbps"
roamRateBOnly="roamRateBOnly"
roamRateBOnly1M=" 1Mbps"
roamRateBOnly2M=" 2Mbps"
roamRateBOnly5M=" 5Mbps"
roamRateBOnly11M="11Mbps"
roamRateB="roamRateB"
roamRateB1M=" 1Mbps"
roamRateB2M=" 2Mbps"
roamRateB5M=" 5Mbps"
roamRateB6M=" 6Mbps"
roamRateB9M=" 9Mbps"
roamRateB11M="11Mbps"
pcieAspm="pcieAspm"
pcieAspmOff="L0s Off, L1 Off"
pcieAspmL1On="L0s Off, L1 On"
wModeSelect="Wireless Mode"
wModeSelect11bonly="11b only"
wModeSelect11nbg="11n(2.4GHz) and g and b"
wModeSelect11na="11n(5GHz) and a"
wModeSelect11abgn="11abgn"
wModeLegacy11a="11a only"
wModeLegacy11bonly="11b only"
wModeLegacy11bg="11g and 11b"
wModeLegacy11abg="11abg"
antennaSwitch="AntennaSwitch"
antennaSwitchAuto="Auto"
antennaSwitchA="Antenna A"
antennaSwitchB="Antenna B"
uapsdEnabledBE="Power Save Policy (Best Effort)"
uapsdEnabledBEOn="WMM Power Save (UAPSD)"
uapsdEnabledBEOff="Legacy Power Save"
uapsdEnabledBK="Power Save Policy (Background)"
uapsdEnabledBKOn="WMM Power Save (UAPSD)"
uapsdEnabledBKOff="Legacy Power Save"
uapsdEnabledVI="Power Save Policy (Video)"
uapsdEnabledVIOn="WMM Power Save (UAPSD)"
uapsdEnabledVIOff="Legacy Power Save"
uapsdEnabledVO="Power Save Policy (Voice)"
uapsdEnabledVOOn="WMM Power Save (UAPSD)"
uapsdEnabledVOOff="Legacy Power Save"
psPoll="Power Save Legacy Algorithm"
psPollEnable="PS Poll"
psPollDisable="PS non Poll"
ccx5FeatureEnable="MFP"
ccx5FeatureEnableMfpEnable="Enable"
ccx5FeatureEnableMfpDisable="Disable"
Mode11d="11d Mode Switch"
Mode11dEnable="Enable"
Mode11dDisable="Disable"
RateCtrl="Auto Transmit Rate"
RateCtrlEnable="Enable"
RateCtrlDisable="Disable"
TxRate11b="11b Transmit Rates"
TxRate11b1M="1 Mbps"
TxRate11b2M="2 Mbps"
TxRate11b5M="5.5 Mbps"
TxRate11b11M="11 Mbps"
TxRate11g="11g Transmit Rates"
TxRate11g1M="1 Mbps"
TxRate11g2M="2 Mbps"
TxRate11g5M="5.5 Mbps"
TxRate11g11M="11 Mbps"
TxRate11g6M="6 Mbps"
TxRate11g9M="9 Mbps"
TxRate11g12M="12 Mbps"
TxRate11g18M="18 Mbps"
TxRate11g24M="24 Mbps"
TxRate11g36M="36 Mbps"
TxRate11g48M="48 Mbps"
TxRate11g54M="54 Mbps"
TxRate11a="11a Transmit Rates"
TxRate11a6M="6 Mbps"
TxRate11a9M="9 Mbps"
TxRate11a12M="12 Mbps"
TxRate11a18M="18 Mbps"
TxRate11a24M="24 Mbps"
TxRate11a36M="36 Mbps"
TxRate11a48M="48 Mbps"
TxRate11a54M="54 Mbps"
ATHR_VID_0CF3="VID_0CF3"
NTGR_VID_0846="VID_0846"
AZWV_VID_13D3="VID_13D3"
LION_VID_04CA="VID_04CA"
PSPXLinkMode="PSP XLink mode"
PSPXLinkModeEnable="Enable"
PSPXLinkModeDisable="Disable"
Atheros_Disk="Atheros Driver Disk 1"
ATHER.Service.DispName="Atheros AR9271 Wireless Network Adapter Service"
ATHER.DeviceDesc.9271="Atheros AR9271 Wireless Network Adapter"
ATHER.DeviceDesc.7010="Atheros AR7010 Wireless Network Adapter"
ATHER.DeviceDesc.7015="Atheros AR7015 Wireless Network Adapter"
ATHER.DeviceDesc.1006="Atheros 11G USB Wireless Network Adapter"
NTGR.DeviceDesc.9030="NETGEAR WNA1100 N150 Wireless USB Adapter"
NTGR.DeviceDesc.9018="NETGEAR WNDA3200 Wireless 11N Dual-band USB Adapter"
DLINK.DeviceDesc.3A10="High-Power Wireless 150 USB adapter"
AZWV.DeviceDesc.3327="Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3328="Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3346="Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3348="Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3349="Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3350="Atheros AR9271 Wireless Network Adapter"
SMC.DeviceDesc.A704="SMC Networks EZ Connect N 802.11n Wireless USB 2.0 Adapter"
VIA.DeviceDesc.3801="VIA 802.11b/g/n USB Wireless Network Adapter"
VRZN.DeviceDesc.1200="Verizon Wireless N 300 USB Adapter"
