
[Version]
Signature="$Windows NT$"
Compatible=1
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318}
Provider=%MRVL%
CatalogFile=WN121T.cat
DriverVer=12/07/2006,1.0.5.1
[SourceDisksNames]
1=%DriverDisk%,,,
[SourceDisksFiles]
WN121TXP.sys=1
WN121T2K.sys=1
[DestinationDirs]
W8360USB.XP.CopyFiles=12
W8360USB.2K.CopyFiles=12
DefaultDestDir=11
[Manufacturer]
%MRVL%=Marvell,NT.5.1
[Marvell]
%MRVL8360USB.DeviceDesc%=W8360USB.ndi.NT,USB\VID_1286&PID_2006
%BelkinN1USB.DeviceDesc%=W8360USB.ndi.NT,USB\VID_1799&PID_8051
%LinksysNUSB.DeviceDesc%=W8360USB.ndi.NT,USB\VID_13B1&PID_0029
%WN121TUSB.DeviceDesc%=W8360USB.ndi.NT,USB\VID_0846&PID_7100
%N650USB.DeviceDesc%=W8360USB.ndi.NT,USB\VID_07D1&PID_3B10
%AsusUSB1.DeviceDesc%=W8360USB.ndi.NT,USB\VID_0B05&PID_172A
%AsusUSB2.DeviceDesc%=W8360USB.ndi.NT,USB\VID_0B05&PID_172B
[Marvell.NT.5.1]
%MRVL8360USB.DeviceDesc%=W8360USBXP.ndi,USB\VID_1286&PID_2006
%BelkinN1USB.DeviceDesc%=W8360USBXP.ndi,USB\VID_1799&PID_8051
%LinksysNUSB.DeviceDesc%=W8360USBXP.ndi,USB\VID_13B1&PID_0029
%WN121TUSB.DeviceDesc%=W8360USBXP.ndi,USB\VID_0846&PID_7100
%N650USB.DeviceDesc%=W8360USBXP.ndi,USB\VID_07D1&PID_3B10
%AsusUSB1.DeviceDesc%=W8360USBXP.ndi,USB\VID_0B05&PID_172A
%AsusUSB2.DeviceDesc%=W8360USBXP.ndi,USB\VID_0B05&PID_172B
[ControlFlags]
ExcludeFromSelect=*
[W8360USBXP.ndi]
Characteristics=0x84
BusType=15 ;Is USB
AddReg=W8360USBWXP.reg, W8360USB.reg, W8360USBXP.reg
;CpyFiles=W8360USB.XP.CopyFiles
[W8360USBXP.ndi.Services]
AddService=MRVW245, 2, W8360USBXP.Service, CommonXP.EventLog
[W8360USBXP.reg]
HKR, Ndi, Service, 0, "MRVW245"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[W8360USB.XP.CopyFiles]
WN121TXP.sys,,,2
[W8360USBXP.Service]
DisplayName=%W8360USBXP.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\WN121TXP.sys
LoadOrderGroup=NDIS
[CommonXP.EventLog]
AddReg=CommonXP.AddEventLog.reg
[CommonXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[W8360USB.ndi.NT]
Characteristics=0x84
BusType=15; Is USB.
AddReg=W8360USBW2K.reg, W8360USB.reg, W8360USB2K.reg, W8360USB2K.devID.reg
;CpyFiles=W8360USB.2K.CopyFiles
[W8360USB.ndi.NT.Services]
AddService=MRVW243, 2, W8360USB2K.Service, Common.EventLog
[W8360USB2K.reg]
HKR, Ndi, Service, 0, "MRVW243"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[W8360USB2K.devID.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_1286&PID_2006"
[W8360USB.2K.CopyFiles]
WN121T2K.sys,,,2
[W8360USB2K.Service]
DisplayName=%W8360USB2K.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\WN121T2K.sys
LoadOrderGroup=NDIS
[Common.EventLog]
AddReg=Common.AddEventLog.reg
[Common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[W8360USB.reg]
HKR,, OpMode, 0x00002, 0 ;//STA Mode
HKR,, LED0PowerOn, 0x00002, "0100ff00"
HKR,, LED1PowerOn, 0x00002, "0101fe00"
HKR,, LED0PowerOff, 0x00002, "0100fe00"
HKR,, LED1PowerOff, 0x00002, "0101fe00"
HKR,, LED0Scan, 0x00002, "0100ff00"
HKR,, LED1Scan, 0x00002, "01010200"
HKR,, LED0Associated, 0x00002, "0100ff00"
HKR,, LED1Associated, 0x00002, "0101fe00"
HKR,, LED0Joined, 0x00002, "0100ff00"
HKR,, LED1Joined, 0x00002, "0101fe00"
HKR,, LED0Started, 0x00002, "0100ff00"
HKR,, LED1Started, 0x00002, "0101fe00"
HKR,, LED0Tx, 0x00002, "0100ff00"
HKR,, LED1Tx, 0x00002, "01010200"
HKR,, LED0Rx, 0x00002, "0100ff00"
HKR,, LED1Rx, 0x00002, "01010200"
HKR,, LED0TxHigh, 0x00002, "0100ff00"
HKR,, LED1TxHigh, 0x00002, "01010200"
HKR,, LED0RxHigh, 0x00002, "0100ff00"
HKR,, LED1RxHigh, 0x00002, "01010200"
HKR,, LEDOffAfterRadioOff, 0x00002, "1"
HKR, Ndi\params\AdhocMode,ParamDesc,,"%AdhocMode%"
HKR, Ndi\params\AdhocMode,default,,"1"
HKR, Ndi\params\AdhocMode,type,,enum
HKR, Ndi\params\AdhocMode\enum,"0",,"%AdhocMode_GMode%"
HKR, Ndi\params\AdhocMode\enum,"1",,"%AdhocMode_BMode%"
HKR, Ndi\params\AdhocMode\enum,"4",,"%AdhocMode_NMode%"
HKR, Ndi\xparams\DesiredSSID,ParamDesc,,"%SSID%"
HKR, Ndi\xparams\DesiredSSID,default,,""
HKR, Ndi\xparams\DesiredSSID,type,,"edit"
HKR, Ndi\xparams\DesiredSSID,LimitText,,"32"
HKR, Ndi\xparams\DesiredSSID,UpperCase,,"0"
HKR, Ndi\xparams\DesiredSSID,Optional,,"1"
HKR, Ndi\xparams\AuthMode,ParamDesc,,"%AuthMode%"
HKR, Ndi\xparams\AuthMode,default,,"0"
HKR, Ndi\xparams\AuthMode,type,,enum
HKR, Ndi\xparams\AuthMode\enum,"0",,"%AuthMode_Open%"
HKR, Ndi\xparams\AuthMode\enum,"1",,"%AuthMode_Shared%"
HKR, Ndi\xparams\NetworkMode,ParamDesc,,"%NetworkMode%"
HKR, Ndi\xparams\NetworkMode,default,,"1"
HKR, Ndi\xparams\NetworkMode,type,,enum
HKR, Ndi\xparams\NetworkMode\enum,"0",,"%NetworkMode_AdHoc%"
HKR, Ndi\xparams\NetworkMode\enum,"1",,"%NetworkMode_Infra%"
HKR, Ndi\params\FragThsd, ParamDesc,0 , "%FragThsds%"
HKR, Ndi\params\FragThsd, default, 0 , "2346"
HKR, Ndi\params\FragThsd, min, 0 , "256"
HKR, Ndi\params\FragThsd, max, 0 , "2346"
HKR, Ndi\params\FragThsd, step, 0 , "1"
HKR, Ndi\params\FragThsd, Base, 0 , "10"
HKR, Ndi\params\FragThsd, type, 0 ,"dword"
HKR, Ndi\xparams\Channel, ParamDesc,0 , "%Channel%"
HKR, Ndi\xparams\Channel, default, 0 , "36"
HKR, Ndi\xparams\Channel, min, 0 , "1"
HKR, Ndi\xparams\Channel, max, 0 , "165"
HKR, Ndi\xparams\Channel, step, 0 , "1"
HKR, Ndi\xparams\Channel, Base, 0 , "10"
HKR, Ndi\xparams\Channel, type, 0 ,"dword"
HKR, Ndi\xparams\TxAntenna, ParamDesc,0 , "%TxAntennaStr%"
HKR, Ndi\xparams\TxAntenna, default, 0 , "2"
HKR, Ndi\xparams\TxAntenna, min, 0 , "1"
HKR, Ndi\xparams\TxAntenna, max, 0 , "ffff"
HKR, Ndi\xparams\TxAntenna, step, 0 , "1"
HKR, Ndi\xparams\TxAntenna, Base, 0 , "16"
HKR, Ndi\xparams\TxAntenna, type, 0 ,"dword"
HKR, Ndi\xparams\RxAntenna, ParamDesc,0 , "%RxAntennaStr%"
HKR, Ndi\xparams\RxAntenna, default, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna, min, 0 , "1"
HKR, Ndi\xparams\RxAntenna, max, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna, step, 0 , "1"
HKR, Ndi\xparams\RxAntenna, Base, 0 , "16"
HKR, Ndi\xparams\RxAntenna, type, 0 ,"dword"
HKR, Ndi\params\RTSThsd, ParamDesc, 0, "%RTSThsds%"
HKR, Ndi\params\RTSThsd, default, 0, "2346"
HKR, Ndi\params\RTSThsd, min, 0, "0"
HKR, Ndi\params\RTSThsd, max, 0, "2346"
HKR, Ndi\params\RTSThsd, step, 0, "1"
HKR, Ndi\params\RTSThsd, Base, 0, "10"
HKR, Ndi\params\RTSThsd, type, 0, "dword"
HKR, Ndi\params\PowerMode,ParamDesc,,"%PowerMode%"
HKR, Ndi\params\PowerMode,default,,"0"
HKR, Ndi\params\PowerMode,type,,enum
HKR, Ndi\params\PowerMode\enum,"0",,"%PowerMode_CAM%"
HKR, Ndi\params\PowerMode\enum,"1",,"%PowerMode_Max%"
HKR, Ndi\xparams\DataRate,ParamDesc,,"%DataRate%"
HKR, Ndi\xparams\DataRate,default,,"FF"
HKR, Ndi\xparams\DataRate,type,,enum
HKR, Ndi\xparams\DataRate\enum,"FF",,"%DataRate_Auto%"
HKR, Ndi\xparams\DataRate\enum,"2",,"%DataRate_1Mbps%"
HKR, Ndi\xparams\DataRate\enum,"4",,"%DataRate_2Mbps%"
HKR, Ndi\xparams\DataRate\enum,"b",,"%DataRate_5_5Mbps%"
HKR, Ndi\xparams\DataRate\enum,"16",,"%DataRate_11Mbps%"
HKR, Ndi\xparams\DataRate\enum,"C",,"%DataRate_6Mbps%"
HKR, Ndi\xparams\DataRate\enum,"12",,"%DataRate_9Mbps%"
HKR, Ndi\xparams\DataRate\enum,"18",,"%DataRate_12Mbps%"
HKR, Ndi\xparams\DataRate\enum,"24",,"%DataRate_18Mbps%"
HKR, Ndi\xparams\DataRate\enum,"30",,"%DataRate_24Mbps%"
HKR, Ndi\xparams\DataRate\enum,"48",,"%DataRate_36Mbps%"
HKR, Ndi\xparams\DataRate\enum,"60",,"%DataRate_48Mbps%"
HKR, Ndi\xparams\DataRate\enum,"6C",,"%DataRate_54Mbps%"
HKR, Ndi\xparams\WepStatus,ParamDesc,,"%WepStatus%"
HKR, Ndi\xparams\WepStatus,default,,"1"
HKR, Ndi\xparams\WepStatus,type,,enum
HKR, Ndi\xparams\WepStatus\enum,"0",,"%Enabled%"
HKR, Ndi\xparams\WepStatus\enum,"1",,"%Disabled%"
HKR, Ndi\params\Preamble,ParamDesc,,"%PreambleStr%"
HKR, Ndi\params\Preamble,default,,"3"
HKR, Ndi\params\Preamble,type,,enum
HKR, Ndi\params\Preamble\enum,"1",,"%PreambleStr_Auto%"
HKR, Ndi\params\Preamble\enum,"2",,"%PreambleStr_Short%"
HKR, Ndi\params\Preamble\enum,"3",,"%PreambleStr_Long%"
HKR,, TxWepKey, 2, ""
HKR,, WepKey1, 2, ""
HKR,, WepKey2, 2, ""
HKR,, WepKey3, 2, ""
HKR,, WepKey4, 2, ""
HKR,, RadioOn,2, "1"
HKR,, DriverRel, 2, "12/07/2006"
HKR,, AMSDUCompatible,2, "1"
HKR,, AMPDUCompatible,2, "1"
HKR,, SSIDScanOnce,2, "0"
HKR, Ndi\params\BlockAckMode,ParamDesc,,"%AMPDUSettings%"
HKR, Ndi\params\BlockAckMode,default,,"2"
HKR, Ndi\params\BlockAckMode,type,,enum
HKR, Ndi\params\BlockAckMode\enum,"2",,"%Partial%"
HKR, Ndi\params\BlockAckMode\enum,"3",,"%Full%"
HKR, Ndi\params\EncryptionType,ParamDesc,,"%EncryptionType%"
HKR, Ndi\params\EncryptionType,default,,"0"
HKR, Ndi\params\EncryptionType,type,,enum
HKR, Ndi\params\EncryptionType\enum,"0",,"%HwEncryption%"
HKR, Ndi\params\EncryptionType\enum,"1",,"%SwEncryption%"
HKR, Ndi\params\EWCTurboMode,ParamDesc,,"%EWCTurboMode%"
HKR, Ndi\params\EWCTurboMode,default,,"1"
HKR, Ndi\params\EWCTurboMode,type,,enum
HKR, Ndi\params\EWCTurboMode\enum,"0",,"%Disabled%"
HKR, Ndi\params\EWCTurboMode\enum,"1",,"%Enabled%"
HKR, Ndi\params\HTModeEnabled
HKR, Ndi\params\HTModeEnabled, ParamDesc,,"%HTModeEnabled%"
HKR, Ndi\params\HTModeEnabled, default,,"1"
HKR, Ndi\params\HTModeEnabled, type,,enum
HKR, Ndi\params\HTModeEnabled\enum,"0",,"%Disabled%"
HKR, Ndi\params\HTModeEnabled\enum,"1",,"%Enabled%"
HKR, Ndi\params\ChannelWidth, ParamDesc,,"%ChannelWidth%"
HKR, Ndi\params\ChannelWidth, default,,"-1"
HKR, Ndi\params\ChannelWidth, type,,enum
HKR, Ndi\params\ChannelWidth\enum,"0",,"%20MHz%"
HKR, Ndi\params\ChannelWidth\enum,"1",,"%40MHz%"
HKR, Ndi\params\ChannelWidth\enum,"-1",,"%Auto%"
HKR, Ndi\params\ExtChannelOffset, ParamDesc,,"%ExtChannelOffset%"
HKR, Ndi\params\ExtChannelOffset, default,,"-1"
HKR, Ndi\params\ExtChannelOffset, type,,enum
HKR, Ndi\params\ExtChannelOffset\enum,"0",,"%Below%"
HKR, Ndi\params\ExtChannelOffset\enum,"1",,"%Above%"
HKR, Ndi\params\ExtChannelOffset\enum,"2",,"%None%"
HKR, Ndi\params\ExtChannelOffset\enum,"-1",,"%Auto%"
HKR, Ndi\params\GuardInterval, ParamDesc,,"%GuardInterval%"
HKR, Ndi\params\GuardInterval, default,,"-1"
HKR, Ndi\params\GuardInterval, type,,enum
HKR, Ndi\params\GuardInterval\enum,"0",,"%LongGI%"
HKR, Ndi\params\GuardInterval\enum,"1",,"%ShortGI%"
HKR, Ndi\params\GuardInterval\enum,"-1",,"%Auto%"
HKR, Ndi\params\RegistryMimoCfg, ParamDesc,,"%Antenna%"
HKR, Ndi\params\RegistryMimoCfg, default,,"-1"
HKR, Ndi\params\RegistryMimoCfg, type,,enum
HKR, Ndi\params\RegistryMimoCfg\enum,"0",,"%2by3%"
HKR, Ndi\params\RegistryMimoCfg\enum,"1",,"%Antenna_A%"
HKR, Ndi\params\RegistryMimoCfg\enum,"2",,"%Antenna_B%"
HKR, Ndi\params\RegistryMimoCfg\enum,"3",,"%2by2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"4",,"%Aby2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"5",,"%Bby2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"-1",,"%Auto%"
HKR, Ndi\params\RateAdaptMode, ParamDesc,,"%RateAdaptMode%"
HKR, Ndi\params\RateAdaptMode, default,,"0"
HKR, Ndi\params\RateAdaptMode, type,,enum
HKR, Ndi\params\RateAdaptMode\enum,"0",,"%In%"
HKR, Ndi\params\RateAdaptMode\enum,"1",,"%Out%"
HKR, Ndi\params\CSMode, ParamDesc,,"%LinkAdaptCSMode%"
HKR, Ndi\params\CSMode, default,,"0"
HKR, Ndi\params\CSMode, type,,enum
HKR, Ndi\params\CSMode\enum,"0",,"%Conservative%"
HKR, Ndi\params\CSMode\enum,"1",,"%Aggressive%"
HKR, Ndi\params\CSMode\enum,"2",,"%Auto%"
[W8360USBW2K.reg]
HKR, Ndi\params\AMSDUEnabled,ParamDesc,,"%AMSDUEnabled%"
HKR, Ndi\params\AMSDUEnabled,default,,"1"
HKR, Ndi\params\AMSDUEnabled,type,,enum
HKR, Ndi\params\AMSDUEnabled\enum,"0",,"%Disabled%"
HKR, Ndi\params\AMSDUEnabled\enum,"1",,"%AMSDUEnabled_3839Bytes%"
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters,TcpWindowSize,0x00010001,00065535
[W8360USBWXP.reg]
HKR, Ndi\params\AMSDUEnabled,ParamDesc,,"%AMSDUEnabled%"
HKR, Ndi\params\AMSDUEnabled,default,,"2"
HKR, Ndi\params\AMSDUEnabled,type,,enum
HKR, Ndi\params\AMSDUEnabled\enum,"0",,"%Disabled%"
HKR, Ndi\params\AMSDUEnabled\enum,"1",,"%AMSDUEnabled_3839Bytes%"
HKR, Ndi\params\AMSDUEnabled\enum,"2",,"%AMSDUEnabled_Max%"
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters,Tcp1323Opts,0x00010001,00000001
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters,TcpWindowSize,0x00010001,00262144
[Strings]
MRVL="Marvell"
Enabled="Enabled"
Disabled="Disabled"
Off="Off"
On="On"
TxAntennaStr="Tx Antenna Select"
RxAntennaStr="Rx Antenna Select"
Channel="Channel"
FragThsds="Fragmentation Threshold"
DataRate="Data Rate"
DataRate_Auto="Auto"
DataRate_1Mbps="1 Mbps"
DataRate_2Mbps="2 Mbps"
DataRate_5_5Mbps="5.5 Mbps"
DataRate_11Mbps="11 Mbps"
DataRate_6Mbps="6 Mbps"
DataRate_9Mbps="9 Mbps"
DataRate_12Mbps="12 Mbps"
DataRate_18Mbps="18 Mbps"
DataRate_24Mbps="24 Mbps"
DataRate_36Mbps="36 Mbps"
DataRate_48Mbps="48 Mbps"
DataRate_54Mbps="54 Mbps"
RTSThsds="RTS Threshold"
AuthMode="Authentication Mode"
AuthMode_Open="Open"
AuthMode_Shared="Shared"
NetworkMode="Operation Mode"
NetworkMode_AdHoc="Ad-Hoc"
NetworkMode_Infra="Infrastructure"
WepStatus="WEP Status"
SSID="SSID"
PreambleStr="Preamble Select"
PreambleStr_Auto="Auto"
PreambleStr_Short="Short Preamble"
PreambleStr_Long="Long Preamble"
PowerMode="Power Save Mode"
PowerMode_CAM="CAM-Constantly Awake Mode"
PowerMode_Max="MaxPSP-Max Power Savings"
PowerMode_Fast="FastPSP-Fast Power Savings"
AdhocMode="Ad-Hoc Mode"
AdhocMode_GMode="Ad-Hoc G Mode"
AdhocMode_BMode="Ad-Hoc B Mode only"
AdhocMode_NMode="Ad-Hoc N Mode"
DefaultAdhocMediaModeStr="Default Ad-Hoc Media Mode"
DefaultAdhocMediaModeStr_11b="11b"
DefaultAdhocMediaModeStr_11g="11g"
DefaultAdhocMediaModeStr_11a="11a"
AMSDUEnabled="MSDU Aggregation"
AMSDUEnabled_3839Bytes="Enabled (3839 Bytes)"
AMSDUEnabled_Max="Enabled (Device Max)"
EWCTurboMode="802.11n Turbo Mode"
AMPDUSettings= "Packet Aggregation (A-MPDU)"
HTModeEnabled="802.11n Network"
ChannelWidth="Channel Width"
20MHz="20 MHz"
40MHz="40 MHz"
Auto="Auto"
ExtChannelOffset="Extension Channel"
Below="Lower"
Above="Upper"
None="None"
GuardInterval="Guard Interval"
LongGI="Standard"
ShortGI="Short"
Antenna="Antenna"
2by3="2by3"
Antenna_A="Antenna A"
Antenna_B="Antenna B"
2by2="2by2"
Aby2="A by 2"
Bby2="B by 2"
RateAdaptMode= "Rate adapt mode"
In="Indoor"
Out="Outdoor"
LinkAdaptCSMode="Link Adapt CS Mode"
Conservative="Conservative"
Aggressive="Aggressive"
Full="Full"
Partial="Partial"
EncryptionType= "Encryption Type"
SwEncryption="Sw Encryption"
HwEncryption="Hw Encryption"
DriverDisk="Marvell installation disk 1"
MRVL8360USB.DeviceDesc="NETGEAR WN121T Wireless USB 2.0 Adapter"
BelkinN1USB.DeviceDesc="N1 Wireless USB Network Adapter"
LinksysNUSB.DeviceDesc="Wireless-N USB Network Adapter"
WN121TUSB.DeviceDesc="NETGEAR WN121T Wireless USB 2.0 Adapter"
N650USB.DeviceDesc="D-Link RangeBooster N USB adapter"
AsusUSB1.DeviceDesc="ASUS 802.11n Network Adapter"
AsusUSB2.DeviceDesc="802.11n Network Adapter"
W8360USBXP.Service.DispName="Marvell TOPDOG 802.11n WLAN Driver for Windows XP (USB8x)"
W8360USB2K.Service.DispName="Marvell TOPDOG 802.11n WLAN Driver for Windows 2K (USB8x)"

