
[Version]
DriverVer=12/05/2003, 1.00.6.0
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=VID_2001&PID_3762
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%A021_DESC_STR%=PRISM_A021, USB\VID_2001&PID_3762
[PRISM_A021] ; Win9x
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_A021.ME] ; WinMe
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_A021.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_A021.NT] ; Win2k
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=0
Characteristics= 0x84
[PRISM_A021.NT.Services]
AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog
[PRISM_A021.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_A021.reg]
HKR,Ndi,DeviceID,0,"USB\VID_2001&PID_3762"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%A021_DESC_STR%
[PRISM_COINSTALL.reg.NT]
[PRISM_DRIVER_A02.Service]
DisplayName=%A02_SERVICE_STR%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\PRISMA02.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_A02_DEL.reg]
HKR, ,FWFileName
[COMMON_A02.reg]
HKR,NDI ,Service ,0 ,"PRISM_A02"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"PRISMA02.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM_A02"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM_A02"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,NDI\params\RTSThresh,,0,2347
HKR,Ndi\params\RTSThresh,default,0,2347
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2347
HKR,NDI\params\RTSThresh,step,0,1
HKR,NDI\params\RTSThresh,optional,0,1
HKR,NDI\params\FragThresh,,0,2346
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
HKR,NDI\params\FragThresh,optional,0,1
HKR,NDI\params\ShortRetryLimit,,0,7
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR,NDI\params\ShortRetryLimit,optional,0,1
HKR,NDI\params\LongRetryLimit,,0,4
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR,NDI\params\LongRetryLimit,optional,0,1
HKR,,ConfigProfile,0,256
HKR,NDI\params\ConfigProfile,,0,256
HKR,NDI\params\ConfigProfile,default,0,256
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,,enum
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
HKR,NDI\params\ConfigProfile,optional,0,1
HKR,,NitroMode,0,"1"
HKR,NDI\params\NitroMode,,0,1
HKR,NDI\params\NitroMode,default,0,1
HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
HKR,NDI\params\NitroMode,type,,enum
HKR,NDI\params\NitroMode,flag,1,30,00,00,00
HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
HKR,NDI\params\NitroMode,optional,0,1
HKR,,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.ME=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_NDI.copy]
[PRISM_NDI.copy.ME]
[PRISM_COINSTALL.copy.NT]
[PRISM_DRIVER.copy]
PRISMA02.sys
[PRISM_DRIVER.copy.ME]
PRISMA02.sys
[PRISM_DRIVER.copy.NT]
PRISMA02.sys
[PRISM_APPLET.copy]
[PRISM_APPLET.copy.ME]
[PRISM_APPLET.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
PRISMA02.sys=1
[SourceDisksFiles.ME] ; WinMe
PRISMA02.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
PRISMA02.sys=1
[Strings]
VER_VENDOR_STR="Conceptronic"
VER_VENDOR_NAME_STR="Conceptronic"
INSTALL_DISK_STR="Wireless LAN Install Disk"
A021_DESC_STR="Conceptronic Wireless 54Mbps USB adapter"
A02_SERVICE_STR="IEEE802.11g Wireless USB2.0 Driver"
ON_STR="On"
OFF_STR="Off"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WiFi"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"
NITRO_MODE="Nitro Mode"

