
[Version]
Signature="$Windows NT$"
Provider=%Provider%
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=07/02/2003,4.0.40
[Manufacturer]
%Provider%=DeviceList
[ControlFlags]
ExcludeFromSelect=*
[DeviceList]
%TIACX.DeviceDesc_Cardbus%=TIACX_CardBus, PCI\VEN_104C&DEV_9066&SUBSYS_003217CF
%TIACX.DeviceDesc_PCI%=TIACX_PCI1, PCI\VEN_104C&DEV_9066&SUBSYS_003317CF
%TIACX.DeviceDesc_PCI%=TIACX_PCI2, PCI\VEN_104C&DEV_9066&SUBSYS_003417CF
[TIACX_CardBus.NT]
BusType=5
AddReg =TIACX.ndi.reg.NT, TI.Param.Reg,TIACX_Cardbus.ndi.reg
Characteristics=0x84
;CpyFiles =TIACX.CopyFiles.NT
[TIACX_CardBus.NT.Services]
AddService=XG350TI, 2, TNET1130.Service, TNET1130.EventLog
[TIACX_Cardbus.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_9066&SUBSYS_9066104C&REV_00"
[TIACX_PCI1.NT]
BusType=5
AddReg =TIACX.ndi.reg.NT, TI.Param.Reg,TIACX_PCI.ndi.reg
Characteristics=0x84
;CpyFiles =TIACX.CopyFiles.NT
[TIACX_PCI1.NT.Services]
AddService=XG350TI, 2, TNET1130.Service, TNET1130.EventLog
[TIACX_PCI1.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_9066&SUBSYS_003317CF"
[TIACX_PCI2.NT]
BusType=5
AddReg =TIACX.ndi.reg.NT, TI.Param.Reg,TIACX_PCI.ndi.reg
Characteristics=0x84
;CpyFiles =TIACX.CopyFiles.NT
[TIACX_PCI2.NT.Services]
AddService=XG350TI, 2, TNET1130.Service, TNET1130.EventLog
[TIACX_PCI2.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_9066&SUBSYS_003417CF"
[TIACX.CopyFiles.NT]
XG350TI.sys
[TIACX.ndi.reg.NT]
HKR, Ndi, Service, 0, "XG350TI"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[TNET1130.Service]
DisplayName=%TNET1130.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\XG350TI.sys
LoadOrderGroup=NDIS
[TNET1130.EventLog]
AddReg=TNET1130.AddEventLog.reg
[TNET1130.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[TI.Param.Reg]
HKR, ,WLANIOC,0,"XG-350"
HKR, ,DeviceVxDs,0,"XG350TI.sys"
HKR, ,FactorRSSI, , 88
HKR, ,RateAdaptationTable0,, "1 2 5 11"
HKR, ,RateAdaptationFBThd0,, "50 50 50 50"
HKR, ,RateAdaptationSUThd0,, "30 30 30 30"
HKR, ,RateAdaptationTable1,, "1 2 5 11 22"
HKR, ,RateAdaptationFBThd1,, "50 50 50 50 50"
HKR, ,RateAdaptationSUThd1,, "30 30 30 30 30"
HKR, ,RateAdaptationTable2,, "1 2 5 11 18 24 36 48 54"
HKR, ,RateAdaptationFBThd2,, "50 50 50 50 45 45 45 45 20"
HKR, ,RateAdaptationSUThd2,, "30 30 30 30 30 30 10 5 0"
HKR,,PermAddress,,112233
HKR, ,HardwareID, ,"TNET1130"
HKR, ,dot11DesiredChannel, ,6
HKR, ,NumACXRxDescriptors, ,32
HKR, ,NumACXTxDescriptors, ,32
HKR, ,CalibrationInterval, ,300
HKR, ,EnergyDetection, ,1
HKR, ,LeapUserPassword, ,""
HKR, ,DriverDescription, ,"IEEE 802.11g Wireless Network Cardbus Adapter"
HKR, ,TriggerRxMem, ,1
HKR, ,TriggerTx, ,5
HKR, ,TriggerFcs, ,0
HKR, ,ScrPad5, ,0
HKR, ,dot11ABAMode, ,2
HKR, ,ClockRate, ,80
HKR, ,ShortSlotTime, ,0
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x10001, 25200
HKR, ,RtsCtsProtection, ,1
HKR,NDI\params\RtsCtsProtection,ParamDesc,,"ERP Protection"
HKR,NDI\params\RtsCtsProtection,type,,"enum"
HKR,NDI\params\RtsCtsProtection,default,,"1"
HKR,NDI\params\RtsCtsProtection\enum,"1",,"Enabled"
HKR,NDI\params\RtsCtsProtection\enum,"0",,"Disabled"
HKR,NDI\params\dot11DesiredBSSType,ParamDesc,,"Desired BSS Type"
HKR,NDI\params\dot11DesiredBSSType,type,,"enum"
HKR,NDI\params\dot11DesiredBSSType,default,,"1"
HKR,NDI\params\dot11DesiredBSSType\enum,"0",,"802.11 Ad-hoc"
HKR,NDI\params\dot11DesiredBSSType\enum,"1",,"Infrastructure"
HKR, Ndi\Params\dot11DesiredSSID, ParamDesc, ,"Desired SSID"
HKR, Ndi\Params\dot11DesiredSSID, Type, ,"edit"
HKR, Ndi\Params\dot11DesiredSSID, LimitText, ,"32"
HKR, Ndi\Params\dot11DesiredSSID, Default,,""
HKR, Ndi\Params\dot11DesiredSSID, UpperCase,,"0"
HKR,NDI\params\dot11PowerMode,ParamDesc,,"Power Mode"
HKR,NDI\params\dot11PowerMode,type,,"enum"
HKR,NDI\params\dot11PowerMode,default,,"0"
HKR,NDI\params\dot11PowerMode\enum,"0",,"Continuous Access Mode"
HKR,NDI\params\dot11PowerMode\enum,"1",,"Maximum Power Save"
HKR,NDI\params\dot11PowerMode\enum,"2",,"Fast Power Save"
HKR,NDI\params\dot11DesiredTxRate,ParamDesc,, "Desired Tx Rate"
HKR,NDI\params\dot11DesiredTxRate,type,,"enum"
HKR,NDI\params\dot11DesiredTxRate,default,,"0"
HKR,NDI\params\dot11DesiredTxRate\enum,"0",,"Auto"
HKR,NDI\params\dot11DesiredTxRate\enum,"1",,"1 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"2",,"2 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"3",,"5.5 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"4",,"6 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"5",,"9 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"6",,"11 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"7",,"12 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"8",,"18 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"9",,"22 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"10",,"24 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"11",,"36 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"12",,"48 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"13",,"54 Mbps"
HKR,NDI\params\dot11SupportedRateMask,ParamDesc,, "Desired Supported Rate Set"
HKR,NDI\params\dot11SupportedRateMask,type,,"enum"
HKR,NDI\params\dot11SupportedRateMask,default,,"8"
HKR,NDI\params\dot11SupportedRateMask\enum,"0",,"1,2 Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"1",,"1,2,5.5,11 Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"2",,"1,2,5.5,11,22 Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"3",,"Up to 18Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"4",,"Up to 24Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"5",,"Up to 36Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"6",,"Up to 48Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"7",,"Up to 54Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"8",,"All"
HKR,NDI\params\dot11BasicRateMask,ParamDesc,, "Desired Basic Rate Set"
HKR,NDI\params\dot11BasicRateMask,type,,"enum"
HKR,NDI\params\dot11BasicRateMask,default,,"1"
HKR,NDI\params\dot11BasicRateMask\enum,"0",,"1,2 Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"1",,"1,2,5.5,11 Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"2",,"Up to 12Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"3",,"Up to 18Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"4",,"Up to 24Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"5",,"Up to 36Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"6",,"Up to 48Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"7",,"Up to 54Mbps"
HKR, Ndi\Params\dot11FragmentationThreshold, ParamDesc, ,"Fragmentation Threshold"
HKR, Ndi\Params\dot11FragmentationThreshold, Type, , "int"
HKR, Ndi\Params\dot11FragmentationThreshold, Default, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Min, , "256"
HKR, Ndi\Params\dot11FragmentationThreshold, Max, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Step, , "1"
HKR, Ndi\Params\dot11FragmentationThreshold, Base, , "10"
HKR, Ndi\Params\dot11RTSThreshold, ParamDesc, ,"RTS Threshold"
HKR, Ndi\Params\dot11RTSThreshold, Type, , "int"
HKR, Ndi\Params\dot11RTSThreshold, Default, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Min, , "0"
HKR, Ndi\Params\dot11RTSThreshold, Max, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Step, , "1"
HKR, Ndi\Params\dot11RTSThreshold, Base, , "10"
HKR,NDI\params\dot11WEPStatus,ParamDesc,,"WEP Option"
HKR,NDI\params\dot11WEPStatus,type,,"enum"
HKR,NDI\params\dot11WEPStatus,default,,"1"
HKR,NDI\params\dot11WEPStatus\enum,"0",,"WEP Enabled"
HKR,NDI\params\dot11WEPStatus\enum,"1",,"WEP Disabled"
HKR,NDI\params\dot11AuthenticationMode,ParamDesc,,"Authentication Mode"
HKR,NDI\params\dot11AuthenticationMode,type,,"enum"
HKR,NDI\params\dot11AuthenticationMode,default,,"0"
HKR,NDI\params\dot11AuthenticationMode\enum,"0",,"Open Authentication"
HKR,NDI\params\dot11AuthenticationMode\enum,"1",,"Shared Authentication"
HKR,NDI\params\dot11AuthenticationMode\enum,"2",,"Auto Switch"
HKR,NDI\params\dot11ShortPreambleInvoked,ParamDesc,,"Short Preamble"
HKR,NDI\params\dot11ShortPreambleInvoked,type,,"enum"
HKR,NDI\params\dot11ShortPreambleInvoked,default,,"0"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"0",,"Off"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"1",,"On"
HKR,NDI\params\Mode4x,ParamDesc,,"Mode4x"
HKR,NDI\params\Mode4x,type,,"enum"
HKR,NDI\params\Mode4x,default,,"1"
HKR,NDI\params\Mode4x\enum,"0",,"Off"
HKR,NDI\params\Mode4x\enum,"1",,"On"
HKR,NDI\params\Mode4xMixed,ParamDesc,,"Mode4xMixed"
HKR,NDI\params\Mode4xMixed,type,,"enum"
HKR,NDI\params\Mode4xMixed,default,,"0"
HKR,NDI\params\Mode4xMixed\enum,"0",,"Off"
HKR,NDI\params\Mode4xMixed\enum,"1",,"On"
[DestinationDirs]
DefaultDestDir=12 ; System Directory
[SourceDisksNames]
1=%DiskName%,,
[SourceDisksFiles]
XG350TI.sys=1
[Strings]
Provider=" "
TIACX.DeviceDesc_Cardbus="IEEE 802.11g Wireless Network Cardbus Adapter"
TIACX.DeviceDesc_PCI="IEEE 802.11g Wireless Network PCI Adapter"
WLANAdapterHelpText="A WLAN Adapter provides high speed connection to the Internet through 802.11g technology"
DiskName="IEEE 802.11g NIC Driver Disk"
