
[Version]
DriverVer=10/02/2003, 3.1.3
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=LSPMUSB.cat
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%USB_DESC_STR%=PRISM_USB, USB\VID_1915&PID_2236
%USB_DESC_STR%=PRISM_USB, USB\VID_066B&PID_2213
[PRISM_USB]
AddReg=PRISM_USB.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_USB.NT]
AddReg=PRISM_USB.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=15
Characteristics= 0x84
[PRISM_USB.NT.Services]
AddService= "PRISM_USB", 2, PRISM_DRIVER_USB.Service, PRISM_DRIVER.EventLog
[PRISM_USB.reg]
HKR,Ndi,DeviceID,0,"USB\VID_2474&PID_3642"
HKR,,PlatformId,0,"0"
HKR,,VendorDesc,0,%USB_DESC_STR%
HKR,,LoadFirmware,0,1
[PRISM_DRIVER_USB.Service]
DisplayName=%PRISM_SERVICE_DISPLAY_USB%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\LSPMUSB.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_USB.reg]
HKR,NDI ,Service ,0 ,"PRISM_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"LSPMUSB.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON.reg]
HKR,defaults,ListenInterval,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,1
HKR,defaults,RTSThresh,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,NDI\params\RTSThresh,optional,0,1
HKR,defaults,FragThresh,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,NDI\params\FragThresh,optional,0,1
HKR,defaults,PreambleMode,0,1
HKR,Ndi\params\PreambleMode,default,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,1
HKR,defaults,AuthentAlg,0,65535
HKR,NDI\params\AuthentAlg,default,0,65535
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,1
HKR,defaults,AdhocDemoMode,0,0
HKR,Ndi\params\AdhocDemoMode,default,0,0
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,enum
HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
HKR,NDI\params\AdhocDemoMode,optional,0,1
HKR,defaults,LoadFirmware,0,1
HKR,Ndi\params\LoadFirmware,default,0,1
HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
HKR,NDI\params\LoadFirmware,type,,enum
HKR,NDI\params\LoadFirmware,flag,1,30,00,00,00
HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
HKR,NDI\params\LoadFirmware,optional,0,1
HKR,defaults,PDwellTime,0,120
HKR,Ndi\params\PDwellTime,default,0,120
HKR,NDI\params\PDwellTime,ParamDesc,0,%PDWELL_STR%
HKR,NDI\params\PDwellTime,type,0,int
HKR,NDI\params\PDwellTime,flag,1,20,00,00,00
HKR,NDI\params\PDwellTime,min,0,0
HKR,NDI\params\PDwellTime,max,0,1000
HKR,NDI\params\PDwellTime,step,0,10
HKR,NDI\params\PDwellTime,optional,0,1
HKR,defaults,11dMode,0,0
HKR,Ndi\params\11dMode,default,0,0
HKR,NDI\params\11dMode,ParamDesc,,%MDC_CONTROL_STR%
HKR,NDI\params\11dMode,type,,enum
HKR,NDI\params\11dMode,flag,1,30,00,00,00
HKR,NDI\params\11dMode\enum,0,,"None"
HKR,NDI\params\11dMode\enum,1,,"Strict"
HKR,NDI\params\11dMode\enum,2,,"Flexible"
HKR,NDI\params\11dMode,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_DRIVER.copy]
LSPMUSB.sys
[PRISM_DRIVER.copy.NT]
LSPMUSB.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
LSPMUSB.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
LSPMUSB.sys=1
[Strings]
VER_VENDOR_STR="Cisco-Linksys, LLC."
VER_VENDOR_NAME_STR="Cisco-Linksys, LLC."
PRISM_SERVICE_DISPLAY="Linksys Wireless-B USB Network Adapter Driver"
PRISM_SERVICE_DISPLAY_USB="Linksys Wireless-B USB Network Adapter Driver"
INSTALL_DISK_STR="Linksys Wireless-B USB Network Adapter Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"
LOAD_FIRMWARE_STR="Firmware Download"
PDWELL_STR="Passive Scan Dwell Time"
MDC_CONTROL_STR="802.11D Control"
USB_DESC_STR="Linksys Wireless-B USB Network Adapter v3.0"

