
[Version]
CatalogFile=vntwnet.cat
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Prov%
DriverVer=03/31/2006,2.07.00.0222
[Manufacturer]
%Manuf%=MANUF
[MANUF]
%VT3253.DeviceDesc%=VT3253.ndi, PCI\VEN_1106&DEV_3253&SUBSYS_66551106
%VT3253.DeviceDesc%=VT3253.ndi, PCI\VEN_1106&DEV_3253&SUBSYS_66581106
%VT3253.DeviceDesc%=VT3253.ndi, PCI\VEN_1106&DEV_3253
[VT3253.ndi]
DelReg=WET.delreg, WET.SW.delreg
AddReg=VT3253.reg, WET.reg, WET.reg.win, WET.SW.win
;CpyFiles=WET.CopyFiles.Win, WET.SW.CopyFiles
[VT3253.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType=5
DelReg=WET.delreg, WET.SW.delreg
AddReg=VT3253.reg, WET.reg, WET.reg.NT, WET.SW.NT
;CpyFiles=WET.CopyFiles.NT, WET.SW.CopyFiles.NTx86
[VT3253.ndi.NT.Services]
AddService=VNWLNDIS, 2, WET.Service, WET.EventLog
[VT3253.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_1106&DEV_3253"
HKR, , AdapterCFID, 0, "844304646"
HKR, , AdapterType, 0, "5"
HKR, , MediaType, 0, "1"
HKR, , ReceiveBurstIndicate,0,"64"
HKR, , ReceiveThreshold, 0, "0"
HKR, , TransmitThreshold, 0, "0"
HKR, , BurstLength, 0, "2"
HKR, , MapRegisters, 0, "32"
HKR, , TransmitBuffers, 0, "64"
HKR, Ndi\params\TransmitBuffers, ParamDesc, 0, %TXBuffer%
HKR, Ndi\params\TransmitBuffers, default, 0, "64"
HKR, Ndi\params\TransmitBuffers, type, 0, "int"
HKR, Ndi\params\TransmitBuffers, Min, 0, "16"
HKR, Ndi\params\TransmitBuffers, Max, 0, "64"
HKR, Ndi\params\TransmitBuffers, Step, 0, "1"
HKR, Ndi\params\TransmitBuffers, Base, 0, "10"
HKR, Ndi\params\TransmitBuffers, flag, 1, "20","00","00","00"
HKR, , ReceiveBuffers, 0, "64"
HKR, Ndi\params\ReceiveBuffers, ParamDesc, 0, %RXBuffer%
HKR, Ndi\params\ReceiveBuffers, default, 0, "64"
HKR, Ndi\params\ReceiveBuffers, type, 0, "int"
HKR, Ndi\params\ReceiveBuffers, Min, 0, "16"
HKR, Ndi\params\ReceiveBuffers, Max, 0, "128"
HKR, Ndi\params\ReceiveBuffers, Step, 0, "1"
HKR, Ndi\params\ReceiveBuffers, Base, 0, "10"
HKR, Ndi\params\ReceiveBuffers, flag, 1, "20","00","00","00"
[WET.reg]
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %NetAddress%
HKR, Ndi\params\NetworkAddress, Default, 0, ""
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, LimitText, 0, "12"
HKR, NDI\params\NetworkAddress, UpperCase, 0, "1"
HKR, NDI\params\NetworkAddress, optional, 0, "1"
HKR, NDI\params\NetworkAddress, Base, 0, "16"
HKR, Ndi\params\NetworkAddress, flag, 1, "20","00","00","00"
HKR, , OperationMode, 0, "0"
HKR, Ndi\params\OperationMode, ParamDesc, 0, %OperationMode%
HKR, Ndi\params\OperationMode, default, 0, "0"
HKR, Ndi\params\OperationMode, type, 0, "enum"
HKR, Ndi\params\OperationMode\enum, 0, 0, "Infrastructure"
HKR, Ndi\params\OperationMode\enum, 1, 0, "Ad-Hoc"
HKR, , DesiredSSID, 0, ""
HKR, NDI\params\DesiredSSID, ParamDesc, 0, %DesiredSSID%
HKR, NDI\params\DesiredSSID, default, 0, ""
HKR, NDI\params\DesiredSSID, type, 0, "edit"
HKR, NDI\params\DesiredSSID, LimitText, 0, "32"
HKR, NDI\params\DesiredSSID, optional, 0, "1"
HKR, , RTSThreshold, 0, "2347"
HKR, Ndi\params\RTSThreshold, ParamDesc, 0, %RTSThreshold%
HKR, Ndi\params\RTSThreshold, default, 0, "2347"
HKR, Ndi\params\RTSThreshold, type, 0, "int"
HKR, Ndi\params\RTSThreshold, Min, 0, "256"
HKR, Ndi\params\RTSThreshold, Max, 0, "2347"
HKR, Ndi\params\RTSThreshold, Step, 0, "1"
HKR, Ndi\params\RTSThreshold, Base, 0, "10"
HKR, Ndi\params\RTSThreshold, flag, 1, "30","00","00","00"
HKR, , FragThreshold, 0, "2346"
HKR, Ndi\params\FragThreshold, ParamDesc, 0, %FragThreshold%
HKR, Ndi\params\FragThreshold, default, 0, "2346"
HKR, Ndi\params\FragThreshold, type, 0, "int"
HKR, Ndi\params\FragThreshold, Min, 0, "256"
HKR, Ndi\params\FragThreshold, Max, 0, "2346"
HKR, Ndi\params\FragThreshold, Step, 0, "1"
HKR, Ndi\params\FragThreshold, Base, 0, "10"
HKR, Ndi\params\FragThreshold, flag, 1, "30","00","00","00"
HKR, , BeaconInterval, 0, "100"
HKR, Ndi\params\BeaconInterval, ParamDesc, 0, %BeaconInterval%
HKR, Ndi\params\BeaconInterval, default, 0, "100"
HKR, Ndi\params\BeaconInterval, type, 0, "int"
HKR, Ndi\params\BeaconInterval, Min, 0, "1"
HKR, Ndi\params\BeaconInterval, Max, 0, "1000"
HKR, Ndi\params\BeaconInterval, Step, 0, "1"
HKR, Ndi\params\BeaconInterval, Base, 0, "10"
HKR, Ndi\params\BeaconInterval, flag, 1, "30","00","00","00"
HKR, , RadioControl, 0, "0"
HKR, Ndi\params\RadioControl, ParamDesc, 0, %RadioControl%
HKR, Ndi\params\RadioControl, default, 0, "0"
HKR, Ndi\params\RadioControl, type, 0, "enum"
HKR, Ndi\params\RadioControl\enum, 0, 0, "On"
HKR, Ndi\params\RadioControl\enum, 1, 0, "Off"
HKR, , AntennaDiversity, 0, "0"
HKR, Ndi\params\AntennaDiversity, ParamDesc, 0, %AntennaDiversity%
HKR, Ndi\params\AntennaDiversity, default, 0, "0"
HKR, Ndi\params\AntennaDiversity, type, 0, "enum"
HKR, Ndi\params\AntennaDiversity\enum, 0, 0, "Disable"
HKR, Ndi\params\AntennaDiversity\enum, 1, 0, "Enable"
HKR, , PowerSaveMode, 0, "0"
HKR, Ndi\params\PowerSaveMode, ParamDesc, 0, %PowerSaveMode%
HKR, Ndi\params\PowerSaveMode, default, 0, "0"
HKR, Ndi\params\PowerSaveMode, type, 0, "enum"
HKR, Ndi\params\PowerSaveMode\enum, 0, 0, %CAM%
HKR, Ndi\params\PowerSaveMode\enum, 1, 0, %FastPSP%
HKR, Ndi\params\PowerSaveMode\enum, 2, 0, %MaxPSP%
[WET.reg.win]
HKR, NDIS, MajorNdisVersion,1,03
HKR, NDIS, MinorNdisVersion,1,0A
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "VNWL5A.sys"
HKR, NDIS, LogDriverName, 0, "VNWLNDIS"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
[WET.SW.win]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_PCI_VNT, DisplayName, 0, %VT3253.DeviceDesc%
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_PCI_VNT, UninstallString, 0, "Rundll.exe vuins16.dll,vuins16Ex $PCI $VNT"
HKLM, Software\VN_VUIns\PCI\VNT\DeviceIdList, 3253, 0, "0"
[WET.reg.NT]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "VNWLNDIS"
HKR, , ScatterGather, 0, "1"
[WET.SW.NT]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_PCI_VNT, DisplayName, 0, %VT3253.DeviceDesc%
HKLM, Software\VN_VUIns\PCI\VNT\DeviceIdList, 3253, 0, "0"
[WET.CopyFiles.NT]
VNWL5B.sys,,,2
[WET.SW.CopyFiles.NTx86]
[WET.Service]
DisplayName=%WET.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\VNWL5B.sys
LoadOrderGroup=NDIS
[WET.EventLog]
AddReg=WET.AddEventLog.reg
[WET.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[WET.CopyFiles.Win]
VNWL5A.sys,,,2
[WET.SW.CopyFiles]
vuins16.dll,,,2
[DestinationDirs]
DefaultDestDir=11
WET.CopyFiles.Win=11
WET.CopyFiles.NT=12
WET.SW.CopyFiles.NTx86=11
WET.SW.CopyFiles=11
[SourceDisksFiles]
VNWL.inf=1
VNWL5B.sys=1
[SourceDisksNames]
1=%DiskName%,,,
[WET.delreg]
HKR,Ndi\Params\ReceiveBuffers
HKR,,ReceiveBuffers
HKR,Ndi\Params\TransmitBuffers
HKR,,TransmitBuffers
HKR,Ndi\Params\ConnectionRate
HKR,,ConnectionRate
HKR,,NetworkAddress
HKR,Ndi\Params\Channel
HKR,,Channel
HKR,Ndi\Params\PreambleType
HKR,,PreambleType
HKR,Ndi\Params\RTSThreshold
HKR,,RTSThreshold
HKR,Ndi\Params\FragThreshold
HKR,,FragThreshold
HKR,Ndi\Params\ShortRetryLimit
HKR,,ShortRetryLimit
HKR,Ndi\Params\LongRetryLimit
HKR,,LongRetryLimit
HKR,Ndi\Params\OperationMode
HKR,,OperationMode
HKR,Ndi\Params\PowerSaveMode
HKR,,PowerSaveMode
HKR,Ndi\Params\DesiredSSID
HKR,,DesiredSSID
HKR,Ndi\params\802_11_Mode
HKR,,802_11_Mode
HKR,Ndi\params\BeaconInterval
HKR,,BeaconInterval
HKR,Ndi\Params\RadioControl
HKR,,RadioControl
HKR,Ndi\Params\AntennaDiversity
HKR,,AntennaDiversity
HKR,Ndi\Params\IEEE802_11h
HKR,,IEEE802_11h
[WET.SW.delreg]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_PCI_VNT
HKLM, Software\VN_VUIns\PCI\VNT
[Strings]
Prov="VNT"
DiskName="VIA Networking Technologies PCI-Cardbus Wireless LAN Adapter source disk"
ConnectionRate="Connection Rate"
Channel="Default Channel"
autoR="Auto-Rate"
1M=" 1Mbps"
2M=" 2Mbps"
5M=" 5.5Mbps"
11M="11Mbps"
6M=" 6Mbps"
9M=" 9Mbps"
12M="12Mbps"
18M="18Mbps"
24M="24Mbps"
36M="36Mbps"
48M="48Mbps"
54M="54Mbps"
PreambleType="Preamble Type"
Long="Long"
Short="Short"
Disabled="Disabled"
Enabled="Enabled"
TXBuffer="Transmit Buffers"
RXBuffer="Receive Buffers"
NetAddress="Network Address"
HwDefault="Hardware Default"
OperationMode="Operation Mode"
DesiredSSID="Desired SSID"
802_11_Mode="802.11 Mode"
BeaconInterval="Adhoc Beacon Interval"
RTSThreshold="RTS Threshold"
FragThreshold="Fragment Threshold"
RadioControl="RadioControl"
AntennaDiversity="Antenna Diversity"
PowerSaveMode="Power Save Mode"
CAM="CAM(Continuous Access Mode)"
FastPSP="FastPSP(Fast Power Saving Mode)"
MaxPSP="MaxPSP(Max Power Saving Mode)"
IEEE802_11h="IEEE 802.11h"
Manuf="VIA Networking Technologies, Inc."
VT3253.DeviceDesc="VIA Networking Technologies PCI-Cardbus Wireless LAN Adapter"
WET.Service.DispName="VIA Networking Technologies PCI-Cardbus Wireless LAN Adapter NT Driver"
