[version]
Signature="$Windows NT$" ; Combined WinXP/Vista inf
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%V_BCM%
Compatible=1
DriverVer=08/25/2009, 5.60.18.9
CatalogFile=BCM43XX.CAT
CatalogFile.NTamd64=BCM43XX64.CAT
[Manufacturer]
%V_BCM%=BROADCOM, NTamd64
[ControlFlags]
ExcludeFromSelect=*
[BROADCOM.NTamd64.6.1]
%BCM430B_DeviceDesc%=BCM43XZ_NT61, PCI\VEN_14E4&DEV_4303
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&REV_03
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4318
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4311
%BCM430A_DeviceDesc%=BCM43XA_NT61, PCI\VEN_14E4&DEV_4321&REV_03
%BCM430A_DeviceDesc%=BCM43XA_NT61, PCI\VEN_14E4&DEV_431A
%BCM430M_DeviceDesc%=BCM43XM_NT61, PCI\VEN_14E4&DEV_4324&REV_03
%BCM430M_DeviceDesc%=BCM43XM_NT61, PCI\VEN_14E4&DEV_4319
%BCM430M_DeviceDesc%=BCM43XM_NT61, PCI\VEN_14E4&DEV_4312
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4313
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_432b
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_432c
%BCM430N_DeviceDesc%=BCM43XA_NT61, PCI\VEN_14E4&DEV_432A
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4716
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4722
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4340
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_4341
%BCM430M_DeviceDesc%=BCM43XM_NT61, PCI\VEN_14E4&DEV_4314
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4315
%BCM430A_DeviceDesc%=BCM43XA_NT61, PCI\VEN_14E4&DEV_4316
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4350
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_4351
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4353
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_4357
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4354
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_A8D6
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_A8D8
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_A8DA
[BROADCOM.NTx86.6.1]
%BCM430B_DeviceDesc%=BCM43XZ_NT61, PCI\VEN_14E4&DEV_4303
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&REV_03
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4318
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4311
%BCM430A_DeviceDesc%=BCM43XA_NT61, PCI\VEN_14E4&DEV_4321&REV_03
%BCM430A_DeviceDesc%=BCM43XA_NT61, PCI\VEN_14E4&DEV_431A
%BCM430M_DeviceDesc%=BCM43XM_NT61, PCI\VEN_14E4&DEV_4324&REV_03
%BCM430M_DeviceDesc%=BCM43XM_NT61, PCI\VEN_14E4&DEV_4319
%BCM430M_DeviceDesc%=BCM43XM_NT61, PCI\VEN_14E4&DEV_4312
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4313
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_432b
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_432c
%BCM430N_DeviceDesc%=BCM43XA_NT61, PCI\VEN_14E4&DEV_432A
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4716
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4722
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4340
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_4341
%BCM430M_DeviceDesc%=BCM43XM_NT61, PCI\VEN_14E4&DEV_4314
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4315
%BCM430A_DeviceDesc%=BCM43XA_NT61, PCI\VEN_14E4&DEV_4316
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4350
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_4351
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4353
%BCM430N_DeviceDesc%=BCM43XNG_NT61, PCI\VEN_14E4&DEV_4357
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_4354
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_A8D6
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_A8D8
%BCM430N_DeviceDesc%=BCM43XNM_NT61, PCI\VEN_14E4&DEV_A8DA
[BROADCOM.NTamd64.6.0]
%BCM430B_DeviceDesc%=BCM43XZ_NT60, PCI\VEN_14E4&DEV_4303
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4320&REV_03
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4318
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4311
%BCM430A_DeviceDesc%=BCM43XA_NT60, PCI\VEN_14E4&DEV_4321&REV_03
%BCM430A_DeviceDesc%=BCM43XA_NT60, PCI\VEN_14E4&DEV_431A
%BCM430M_DeviceDesc%=BCM43XM_NT60, PCI\VEN_14E4&DEV_4324&REV_03
%BCM430M_DeviceDesc%=BCM43XM_NT60, PCI\VEN_14E4&DEV_4319
%BCM430M_DeviceDesc%=BCM43XM_NT60, PCI\VEN_14E4&DEV_4312
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4313
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4328
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_4329
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4322
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_432b
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_432c
%BCM430N_DeviceDesc%=BCM43XA_NT60, PCI\VEN_14E4&DEV_432A
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4716
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4722
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4340
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_4341
%BCM430M_DeviceDesc%=BCM43XM_NT60, PCI\VEN_14E4&DEV_4314
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4315
%BCM430A_DeviceDesc%=BCM43XA_NT60, PCI\VEN_14E4&DEV_4316
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4350
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_4351
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4353
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_4357
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4354
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_A8D6
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_A8D8
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_A8DA
[BROADCOM.NTx86.6.0]
%BCM430B_DeviceDesc%=BCM43XZ_NT60, PCI\VEN_14E4&DEV_4303
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4320&REV_03
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4318
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4311
%BCM430A_DeviceDesc%=BCM43XA_NT60, PCI\VEN_14E4&DEV_4321&REV_03
%BCM430A_DeviceDesc%=BCM43XA_NT60, PCI\VEN_14E4&DEV_431A
%BCM430M_DeviceDesc%=BCM43XM_NT60, PCI\VEN_14E4&DEV_4324&REV_03
%BCM430M_DeviceDesc%=BCM43XM_NT60, PCI\VEN_14E4&DEV_4319
%BCM430M_DeviceDesc%=BCM43XM_NT60, PCI\VEN_14E4&DEV_4312
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4313
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4328
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_4329
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4322
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_432b
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_432c
%BCM430N_DeviceDesc%=BCM43XA_NT60, PCI\VEN_14E4&DEV_432A
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4716
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4722
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4340
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_4341
%BCM430M_DeviceDesc%=BCM43XM_NT60, PCI\VEN_14E4&DEV_4314
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4315
%BCM430A_DeviceDesc%=BCM43XA_NT60, PCI\VEN_14E4&DEV_4316
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4350
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_4351
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4353
%BCM430N_DeviceDesc%=BCM43XNG_NT60, PCI\VEN_14E4&DEV_4357
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_4354
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_A8D6
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_A8D8
%BCM430N_DeviceDesc%=BCM43XNM_NT60, PCI\VEN_14E4&DEV_A8DA
[BROADCOM.NTamd64]
%BCM430B_DeviceDesc%=BCM43XZ, PCI\VEN_14E4&DEV_4303
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4320&REV_03
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4318
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4311
%BCM430A_DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_4321&REV_03
%BCM430A_DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_431A
%BCM430M_DeviceDesc%=BCM43XM, PCI\VEN_14E4&DEV_4324&REV_03
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_1095&DEV_0670 ;Arasan SDIO HC
%BCM430M_DeviceDesc%=BCM43XM, PCI\VEN_14E4&DEV_4319
%BCM430M_DeviceDesc%=BCM43XM, PCI\VEN_14E4&DEV_4312
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4313
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4328
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_4329
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4322
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_432b
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_432c
%BCM430N_DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_432A
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4716
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4722
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4340
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_4341
%BCM430M_DeviceDesc%=BCM43XM, PCI\VEN_14E4&DEV_4314
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4315
%BCM430A_DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_4316
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4350
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_4351
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4353
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_4357
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4354
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_A8D6
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_A8D8
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_A8DA
[BROADCOM]
%BCM430B_DeviceDesc%=BCM43XZ, PCI\VEN_14E4&DEV_4303
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4320&REV_03
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4318
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4311
%BCM430A_DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_4321&REV_03
%BCM430A_DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_431A
%BCM430M_DeviceDesc%=BCM43XM, PCI\VEN_14E4&DEV_4324&REV_03
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_1095&DEV_0670 ;Arasan SDIO HC
%BCM430M_DeviceDesc%=BCM43XM, PCI\VEN_14E4&DEV_4319
%BCM430M_DeviceDesc%=BCM43XM, PCI\VEN_14E4&DEV_4312
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4313
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4328
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_4329
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4322
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_432b
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_432c
%BCM430N_DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_432A
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4716
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4722
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4340
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_4341
%BCM430M_DeviceDesc%=BCM43XM, PCI\VEN_14E4&DEV_4314
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4315
%BCM430A_DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_4316
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4350
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_4351
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4353
%BCM430N_DeviceDesc%=BCM43XNG, PCI\VEN_14E4&DEV_4357
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_4354
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_A8D6
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_A8D8
%BCM430N_DeviceDesc%=BCM43XNM, PCI\VEN_14E4&DEV_A8DA
[BCM43XZ_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, b.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43PCMG_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8 ; PCMCIA bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XA_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, a.options.reg, a.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.options.reg, a.channels.reg, bg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNG_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn.options.reg, bg.options.reg, nbg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNMD_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15 ; PNP bus
AddReg=BCM43XX_NT61.reg, BCMH43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XZ_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43PCMG_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XA_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNG_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNMD_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCMH43XX, 2, BCMH43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XZ_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43PCMG_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XA_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNG_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XND_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XZ_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43PCMG_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XA_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNG_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNMD_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64, BCM43XNMD_NT60.CoInstaller.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg, BCM43XNMD_NT60_CoInstaller_AddReg.NTamd64
[BCM43XZ_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, b.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43PCMG_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8 ; PCMCIA bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XA_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, a.options.reg, a.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.options.reg, a.channels.reg, bg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNG_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn.options.reg, bg.options.reg, nbg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNMD_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15 ; PNP bus
AddReg=BCM43XX_NT61.reg, BCMH43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XZ_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43PCMG_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XA_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNG_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNMD_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCMH43XX, 2, BCMH43XX_NT60.Service.NTx86, common.EventLog
[BCM43XZ_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43PCMG_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XA_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNG_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNMD_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XZ_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43PCMG_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XA_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNG_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNMD_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86, BCM43XNMD_NT60.CoInstaller.CopyFiles.NTx86
AddReg=CoInstallers.AddReg, BCM43XNMD_NT60_CoInstaller_AddReg.NTx86
[BCM43XZ_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, b.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43PCMG_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8 ; PCMCIA bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XA_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, a.options.reg, a.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.options.reg, a.channels.reg, bg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNG_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn.options.reg, bg.options.reg, nbg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNMD_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15 ; PNP bus
AddReg=BCM43XX_NT60.reg, BCMH43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XZ_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43PCMG_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XA_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNG_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNMD_NT60.NTamd64.Services]
AddService=BCMH43XX, 2, BCMH43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XZ_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43PCMG_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XA_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNG_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNMD_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64, BCM43XNMD_NT60.CoInstaller.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg, BCM43XNMD_NT60_CoInstaller_AddReg.NTamd64
[BCM43XNMD_NT60_CoInstaller_AddReg.NTamd64]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"
[BCM43XNMD_NT60.NTamd64.Wdf]
KmdfService=BCMH43XX, BCM43XNMD_NT60_wdfsect
[BCM43XNMD_NT60_wdfsect]
KmdfLibraryVersion=1.9
[BCM43XZ_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, b.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43PCMG_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8 ; PCMCIA bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XA_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, a.options.reg, a.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.options.reg, a.channels.reg, bg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNG_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn.options.reg, bg.options.reg, nbg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNMD_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15 ; PNP bus
AddReg=BCM43XX_NT60.reg, BCMH43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XZ_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43PCMG_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XA_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNG_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNMD_NT60.NTx86.Services]
AddService=BCMH43XX, 2, BCMH43XX_NT60.Service.NTx86, common.EventLog
[BCM43XZ_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43PCMG_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XA_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNG_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNMD_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86, BCM43XNMD_NT60.CoInstaller.CopyFiles.NTx86
AddReg=CoInstallers.AddReg, BCM43XNMD_NT60_CoInstaller_AddReg.NTx86
[BCM43XNMD_NT60_CoInstaller_AddReg.NTx86]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"
[BCM43XNMD_NT60.NTx86.Wdf]
KmdfService=BCMH43XX, BCM43XNMD_NT60_wdfsect
[BCM43XZ.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, b.options.reg, bg.options.reg, bg.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43PCMG.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8 ; PCMCIA bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, g.options.reg, bg.options.reg, bg.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XG.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, g.options.reg, bg.options.reg, bg.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XA.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, a.options.reg, a.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XM.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.options.reg, a.channels.reg, bg.channels.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNG.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, gn.options.reg, bg.options.reg, nbg.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNM.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNMD.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15 ; PNP bus
AddReg=BCM43XX.reg, BCMH43XX.brcm.reg, common.reg, common.prevista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XZ.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43PCMG.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XG.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XA.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XM.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNG.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNM.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNMD.NTamd64.Services]
AddService=BCMH43XX, 2, BCMH43XX.Service.NTamd64, common.EventLog
[BCM43XZ.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, b.options.reg, bg.options.reg, bg.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43PCMG.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8 ; PCMCIA bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, g.options.reg, bg.options.reg, bg.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XG.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, g.options.reg, bg.options.reg, bg.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XA.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, a.options.reg, a.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XM.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.options.reg, a.channels.reg, bg.channels.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNG.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, gn.options.reg, bg.options.reg, nbg.channels.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNM.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNMD.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15 ; PNP bus
AddReg=BCM43XX.reg, BCMH43XX.brcm.reg, common.reg, common.prevista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XZ.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43PCMG.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XG.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XA.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XM.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNG.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNM.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNMD.NT.Services]
AddService=BCMH43XX, 2, BCMH43XX.Service.NT, common.EventLog
[BCM43XX_NT61.reg]
HKR, Ndi\Interfaces, UpperRange, , "ndis5"
HKR, Ndi\Interfaces, LowerRange, , "ethernet,wlan,vwifi"
[BCM43XX_NT60.reg]
HKR, Ndi\Interfaces, UpperRange, , "ndis5"
HKR, Ndi\Interfaces, LowerRange, , "ethernet,wlan"
[BCM43XX.reg]
HKR, Ndi\Interfaces, UpperRange, , "ndis5"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
[BCM43XX.brcm.reg]
HKR, Ndi, HelpText, , %BCM43XX_HELP%
HKR, Ndi, Service, 0, "BCM43XX"
[BCMH43XX.brcm.reg]
HKR, Ndi, HelpText, , %BCM43XX_HELP%
HKR, Ndi, Service, 0, "BCMH43XX"
HKR, ,"featureflag", 65537, "0x00000004"
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[BCM43XZ]
[BCM43PCMG]
[BCM43XG]
[BCM43XA]
[BCM43XM]
[BCM43XNG]
[BCM43XNM]
[BCM43XNMD]
[BCM43XX_NT60.Service.NTamd64]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl664.sys
LoadOrderGroup=NDIS
[BCM43XX_NT60.Service.NTx86]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl6.sys
LoadOrderGroup=NDIS
[BCM43XX.Service.NTamd64]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl564.sys
LoadOrderGroup=NDIS
[BCM43XX.Service.NT]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl5.sys
LoadOrderGroup=NDIS
[BCM43XX.Service]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl5.sys
LoadOrderGroup=NDIS
[BCMH43XX_NT60.Service.NTamd64]
DisplayName=%BCMH43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwlhigh664.sys
LoadOrderGroup=NDIS
[BCMH43XX_NT60.Service.NTx86]
DisplayName=%BCMH43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwlhigh6.sys
LoadOrderGroup=NDIS
[BCMH43XX.Service.NTamd64]
DisplayName=%BCMH43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwlhigh564.sys
LoadOrderGroup=NDIS
[BCMH43XX.Service.NT]
DisplayName=%BCMH43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwlhigh5.sys
LoadOrderGroup=NDIS
[BCMH43XX.Service]
DisplayName=%BCMH43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwlhigh5.sys
LoadOrderGroup=NDIS
[BCM43XX_NT60.files.NTamd64]
BCMWL664.SYS,,,6
[BCM43XX_NT60.files.NTx86]
BCMWL6.SYS,,,6
[BCM43XX.files.NTamd64]
BCMWL564.SYS,,,6
[BCM43XX.files.NT]
BCMWL5.SYS,,,6
[BCM43XX.sys.files]
BCMWL5.SYS,,,6
[BCMIHV.files.NTamd64]
bcmihvsrv64.dll,,,6
bcmihvui64.dll,,,6
[BCMIHV.files.NTx86]
bcmihvsrv.dll,,,6
bcmihvui.dll,,,6
[BCMIHVUI.regsrv.NTamd64]
11,,bcmihvui64.dll,1
[BCMIHVUI.regsrv.NTx86]
11,,bcmihvui.dll,1
[CoInstall.CopyFiles.NTamd64]
bcmwlcoi.dll,bcmwlcoi64.dll,,6
[CoInstall.CopyFiles.NTx86]
bcmwlcoi.dll,bcmwlcoi.dll,,6
[CoInstallers.AddReg]
HKR,,CoInstallers32,0x00010000,"bcmwlcoi.dll, BCMWlanCoInstall"
[BCM43XNMD_NT60.CoInstaller.CopyFiles.NTx86]
WdfCoInstaller01009.dll
[BCM43XNMD_NT60.CoInstaller.CopyFiles.NTamd64]
WdfCoInstaller01009.dll,WdfCoInstaller0100964.dll,,6
[DestinationDirs]
DefaultDestDir=11
BCM43XX.sys.files=11
BCM43XX.files.NT=12
BCM43XX.files.NTamd64=12
BCM43XX_NT60.files.NTx86=12
BCM43XX_NT60.files.NTamd64=12
BCMIHV.files.NTx86=11
BCMIHV.files.NTamd64=11
CoInstall.CopyFiles.NTamd64=11
CoInstall.CopyFiles.NTx86=11
BCM43XNMD_NT60.CoInstaller.CopyFiles.NTamd64=11
BCM43XNMD_NT60.CoInstaller.CopyFiles.NTx86=11
[SourceDisksNames]
1=%BCM43XX_DiskName%,,
[SourceDisksFiles.amd64]
BCMWL564.SYS=1
[SourceDisksFiles.x86]
BCMWL5.SYS=1
[SourceDisksFiles]
BCMWL5.SYS=1
[Cleanup]
UnregisterDlls=BCMIHVUI.regsrv.NTamd64, BCMIHVUI.regsrv.NTx86
;DlFiles=BCMIHV.files.NTamd64, BCMIHV.files.NTx86
[common.vista.delreg]
HKR,,"MPC"
HKR, Ndi\params\vlan_mode
HKR,,vlan_mode
HKR, Ndi\params\PowerSaveMode
HKR, Ndi\params\Country
HKR,,Country
[common.delreg]
HKR,,"gpiotimerval"
HKR,,"gpio3"
HKR,,"gpio2"
HKR,,"gpio1"
HKR,,"gpio0"
HKR, Ndi\params\RoamPref
HKR, Ndi\params\AssocPref
HKR, Ndi\params\Locale
HKR,,Locale
HKR, Ndi\params\RoamTrigger
HKR, Ndi\params\WME
HKR, Ndi\params\MixedCell
HKR, Ndi\params\Channel
HKR,,Channel
HKR, Ndi\params\IBSSGMode
HKR,,IBSSGMode
HKR, Ndi\params\Intolerant
HKR,,Intolerant
HKLM,Software\Broadcom\802.11,SupportedApps
[rate.delreg]
HKR, Ndi\params\Rate
HKR, Ndi\params\RateA
[BCMIHV.reg.NTamd64]
HKR, Ndi\IHVExtensions, ExtensibilityDLL, 0, "%%SystemRoot%%\System32\bcmihvsrv64.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID, 0, "{AAA6DEE9-31B9-4f18-AB39-82EF9B06EB73}"
HKR, Ndi\IHVExtensions, AdapterOUI, 0x00010001, 0x001018
[BCMIHV.reg.NTx86]
HKR, Ndi\IHVExtensions, ExtensibilityDLL, 0, "%%SystemRoot%%\System32\bcmihvsrv.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID, 0, "{AAA6DEE9-31B9-4f18-AB39-82EF9B06EB73}"
HKR, Ndi\IHVExtensions, AdapterOUI, 0x00010001, 0x001018
[common.vista.reg]
HKR, Ndi\params\*PriorityVLANTag, ParamDesc, 0, %PriorityVLANTag%
HKR, Ndi\params\*PriorityVLANTag, type, 0, "enum"
HKR, Ndi\params\*PriorityVLANTag\enum, "0", 0, %PriorityAndVLANDisabled%
HKR, Ndi\params\*PriorityVLANTag\enum, "1", 0, %PriorityEnabled%
HKR, Ndi\params\*PriorityVLANTag\enum, "2", 0, %VLANEnabled%
HKR, Ndi\params\*PriorityVLANTag\enum, "3", 0, %PriorityAndVLANEnabled%
HKR, Ndi\params\*PriorityVLANTag,default,,"0"
HKR, Ndi\params\*PriorityVLANTag,optional,,"0"
HKR, ,"PowerSaveMode", 0, "2"
[common.prevista.reg]
HKR, ,"assoc_recreate", 0, "1"
HKR, Ndi\params\IBSSAllowed, ParamDesc, 0, %IbssAllowed%
HKR, Ndi\params\IBSSAllowed, type, 0, "enum"
HKR, Ndi\params\IBSSAllowed\enum, "0", 0, %Disabled%
HKR, Ndi\params\IBSSAllowed\enum, "1", 0, %Enabled%
HKR, Ndi\params\IBSSAllowed,default,,"1"
HKR, Ndi\params\ssid_auto_promote, ParamDesc, 0, %SSIDAutoPromote%
HKR, Ndi\params\ssid_auto_promote, type, 0, "enum"
HKR, Ndi\params\ssid_auto_promote\enum, "0", 0, %Disabled%
HKR, Ndi\params\ssid_auto_promote\enum, "1", 0, %Enabled%
HKR, Ndi\params\ssid_auto_promote,default,,"0"
HKR, Ndi\params\RadioState, ParamDesc, 0, %RadioEnableDisable%
HKR, Ndi\params\RadioState, type, 0, "enum"
HKR, Ndi\params\RadioState\enum, "1", 0, %Disabled%
HKR, Ndi\params\RadioState\enum, "0", 0, %Enabled%
HKR, Ndi\params\RadioState,default,,"0"
HKR, Ndi\params\WZCCoexist, ParamDesc,0, %WZC_Managed_Ethernet%
HKR, Ndi\params\WZCCoexist, type, 0, "enum"
HKR, Ndi\params\WZCCoexist\enum, "0", 0, %Disabled%
HKR, Ndi\params\WZCCoexist\enum, "1", 0, %Enabled%
HKR, Ndi\params\WZCCoexist,default,,"0"
HKR, Ndi\params\Managed, ParamDesc,0, %Manage_Wireless_Settings%
HKR, Ndi\params\Managed, type, 0, "enum"
HKR, Ndi\params\Managed\enum, "0", 0, %Disabled%
HKR, Ndi\params\Managed\enum, "1", 0, %Enabled%
HKR, Ndi\params\Managed,default,,"1"
HKR, Ndi\params\LockWlSettings, ParamDesc,0, %Lock_Wireless_Settings%
HKR, Ndi\params\LockWlSettings, type, 0, "enum"
HKR, Ndi\params\LockWlSettings\enum, "0", 0, %Disabled%
HKR, Ndi\params\LockWlSettings\enum, "1", 0, %Enabled%
HKR, Ndi\params\LockWlSettings,default,,"0"
HKR, Ndi\params\IBSSLink, ParamDesc, 0, %IBSS_Link_Indication%
HKR, Ndi\params\IBSSLink, type, 0, "enum"
HKR, Ndi\params\IBSSLink\enum, "0", 0, %Legacy%
HKR, Ndi\params\IBSSLink\enum, "1", 0, %Default%
HKR, Ndi\params\IBSSLink,default,,"1"
HKR, Ndi\params\vlan_mode, ParamDesc,0, %vlan_mode%
HKR, Ndi\params\vlan_mode, type, 0, "enum"
HKR, Ndi\params\vlan_mode\enum, "-1",0, %Auto%
HKR, Ndi\params\vlan_mode\enum, "1", 0, %Enabled%
HKR, Ndi\params\vlan_mode\enum, "0", 0, %Disabled%
HKR, Ndi\params\vlan_mode,default,,"-1"
HKR, Ndi\params\PowerSaveMode, ParamDesc, 0, %PowerSaveMode%
HKR, Ndi\params\PowerSaveMode, type, 0, "enum"
HKR, Ndi\params\PowerSaveMode\enum, "0", 0, %Disabled%
HKR, Ndi\params\PowerSaveMode\enum, "1", 0, %Enabled%
HKR, Ndi\params\PowerSaveMode\enum, "2", 0, %Fast%
HKR, Ndi\params\PowerSaveMode,default,,"2"
[common.reg]
HKR, ,"EnableSoftAP", 0, "0"
HKR, ,"EnableAutoConnect", 0, "0"
HKR, Ndi\params\LOM, ParamDesc, 0, %DisableRadioUponWiredConnection%
HKR, Ndi\params\LOM, type, 0, "enum"
HKR, Ndi\params\LOM\enum, "0", 0, %Disabled%
HKR, Ndi\params\LOM\enum, "1", 0, %Enabled%
HKR, Ndi\params\LOM,default,,"0"
HKR, Ndi\params\RoamDelta, ParamDesc, 0, %RoamingTendency%
HKR, Ndi\params\RoamDelta, type, 0, "enum"
HKR, Ndi\params\RoamDelta\enum, "0", 0, %Aggressive%
HKR, Ndi\params\RoamDelta\enum, "1", 0, %Moderate%
HKR, Ndi\params\RoamDelta\enum, "2", 0, %Conservative%
HKR, Ndi\params\RoamDelta\enum, "3", 0, %Auto%
HKR, Ndi\params\RoamDelta,default,,"3"
HKR, Ndi\params\MPC, ParamDesc, 0, %MinimumPowerConsumption%
HKR, Ndi\params\MPC, type, 0, "enum"
HKR, Ndi\params\MPC\enum, "0", 0, %Disabled%
HKR, Ndi\params\MPC\enum, "1", 0, %Enabled%
HKR, Ndi\params\MPC,default,,"1"
HKR, Ndi\params\frag, ParamDesc, 0, %FragmentationThreshold%
HKR, Ndi\params\frag,type,0,"dword"
HKR, Ndi\params\frag,min,,"256"
HKR, Ndi\params\frag,max,,"2346"
HKR, Ndi\params\frag,default,,"2346"
HKR, Ndi\params\rts, ParamDesc, 0, %RTSThreshold%
HKR, Ndi\params\rts,type,0,"dword"
HKR, Ndi\params\rts,min,,"0"
HKR, Ndi\params\rts,max,,"2347"
HKR, Ndi\params\rts,default,,"2347"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %LocallyAdministeredMACAddress%
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\PwrOut, ParamDesc, 0, %PowerOutput%
HKR, Ndi\params\PwrOut, type, 0, "enum"
HKR, Ndi\params\PwrOut\enum, "100", 0, "100%"
HKR, Ndi\params\PwrOut\enum, "75", 0, "75%"
HKR, Ndi\params\PwrOut\enum, "50", 0, "50%"
HKR, Ndi\params\PwrOut\enum, "25", 0, "25%"
HKR, Ndi\params\PwrOut,default,,"100"
HKR, Ndi\params\FrameBursting, ParamDesc, 0, %XPress_Technology%
HKR, Ndi\params\FrameBursting, type, 0, "enum"
HKR, Ndi\params\FrameBursting\enum, "0", 0, %Disabled%
HKR, Ndi\params\FrameBursting\enum, "1", 0, %Enabled%
HKR, Ndi\params\FrameBursting,default,,"0"
HKR, Ndi\params\BTCoexist, ParamDesc, 0, %BlueToothCollaboration%
HKR, Ndi\params\BTCoexist, type, 0, "enum"
HKR, Ndi\params\BTCoexist\enum, "0", 0, %Disable%
HKR, Ndi\params\BTCoexist\enum, "1", 0, %Enable%
HKR, Ndi\params\BTCoexist\enum, "3", 0, %Auto%
HKR, Ndi\params\BTCoexist,default,,"3"
HKR, Ndi\params\WakeUpCapabilities, ParamDesc, 0, %WakeUpCapabilities%
HKR, Ndi\params\WakeUpCapabilities, type, 0, "enum"
HKR, Ndi\params\WakeUpCapabilities\enum, "0", 0, %None%
HKR, Ndi\params\WakeUpCapabilities\enum, "1", 0, %MagicPacket%
HKR, Ndi\params\WakeUpCapabilities\enum, "2", 0, %NetPattern%
HKR, Ndi\params\WakeUpCapabilities\enum, "28", 0, %LossofAP%
HKR, Ndi\params\WakeUpCapabilities\enum, "3", 0, %MagicNet%
HKR, Ndi\params\WakeUpCapabilities\enum, "29", 0, %LossMagic%
HKR, Ndi\params\WakeUpCapabilities\enum, "30", 0, %LossNet%
HKR, Ndi\params\WakeUpCapabilities\enum, "31", 0, %All%
HKR, Ndi\params\WakeUpCapabilities,default,,"3"
HKR, ,"WowlKeyRot", 0, "1"
HKR, ,"WEP", 0, ""
HKR, ,"NetworkType", 0, "-1"
HKR, ,"SSID", 0, ""
HKR, ,"ledbh0", 0, "-1"
HKR, ,"ledbh1", 0, "-1"
HKR, ,"ledbh2", 0, "-1"
HKR, ,"ledbh3", 0, "-1"
HKR, ,"ledblinkslow", 0, "-1"
HKR, ,"ledblinkmed", 0, "-1"
HKR, ,"ledblinkfast", 0, "-1"
HKR, ,"leddc", 0, "0"
HKR, ,"scan_channel_time", 0, "-1"
HKR, ,"scan_unassoc_time", 0, "-1"
HKR, ,"scan_home_time", 0, "-1"
HKR, ,"scan_passes", 0, "-1"
HKR, ,"BadFramePreempt", 0, "0"
HKR, ,"Interference_Mode", 0, "-1"
HKR, ,"ccx_rm", 0, "1"
HKR, ,"ccx_rm_limit", 0, "300"
HKR, ,"EFCEnable", 0, "0"
HKR, Ndi\params\antdiv, ParamDesc, 0, %AntennaDiversity%
HKR, Ndi\params\antdiv, type, 0, "enum"
HKR, Ndi\params\antdiv\enum, "-1", 0, %Auto%
HKR, Ndi\params\antdiv,default,,"-1"
HKR, Ndi\params\WME, ParamDesc, 0, %WME%
HKR, Ndi\params\WME, type, 0, "enum"
HKR, Ndi\params\WME\enum, "-1", 0, %Auto%
HKR, Ndi\params\WME\enum, "1", 0, %Enabled%
HKR, Ndi\params\WME\enum, "0", 0, %Disabled%
HKR, Ndi\params\WME,default,,"-1"
HKR, ,"WME",0,"-1"
HKR, Ndi\params\MixedCell, ParamDesc,0, %MixedCell%
HKR, Ndi\params\MixedCell, type, 0, "enum"
HKR, Ndi\params\MixedCell\enum, "0", 0, %Disabled%
HKR, Ndi\params\MixedCell\enum, "1", 0, %Enabled%
HKR, Ndi\params\MixedCell,default,,"0"
[bg.channels.reg]
HKR, Ndi\params\Chanspec\enum, "1", 0, " 1"
HKR, Ndi\params\Chanspec\enum, "2", 0, " 2"
HKR, Ndi\params\Chanspec\enum, "3", 0, " 3"
HKR, Ndi\params\Chanspec\enum, "4", 0, " 4"
HKR, Ndi\params\Chanspec\enum, "5", 0, " 5"
HKR, Ndi\params\Chanspec\enum, "6", 0, " 6"
HKR, Ndi\params\Chanspec\enum, "7", 0, " 7"
HKR, Ndi\params\Chanspec\enum, "8", 0, " 8"
HKR, Ndi\params\Chanspec\enum, "9", 0, " 9"
HKR, Ndi\params\Chanspec\enum, "10", 0, " 10"
HKR, Ndi\params\Chanspec\enum, "11", 0, " 11"
HKR, Ndi\params\Chanspec\enum, "12", 0, " 12"
HKR, Ndi\params\Chanspec\enum, "13", 0, " 13"
HKR, Ndi\params\Chanspec\enum, "14", 0, " 14"
[nbg.channels.reg]
HKR, Ndi\params\Chanspec\enum, "1", 0, " 1(20MHz)"
HKR, Ndi\params\Chanspec\enum, "2", 0, " 2(20MHz)"
HKR, Ndi\params\Chanspec\enum, "3", 0, " 3(20MHz)"
HKR, Ndi\params\Chanspec\enum, "4", 0, " 4(20MHz)"
HKR, Ndi\params\Chanspec\enum, "5", 0, " 5(20MHz)"
HKR, Ndi\params\Chanspec\enum, "6", 0, " 6(20MHz)"
HKR, Ndi\params\Chanspec\enum, "7", 0, " 7(20MHz)"
HKR, Ndi\params\Chanspec\enum, "8", 0, " 8(20MHz)"
HKR, Ndi\params\Chanspec\enum, "9", 0, " 9(20MHz)"
HKR, Ndi\params\Chanspec\enum, "10", 0, " 10(20MHz)"
HKR, Ndi\params\Chanspec\enum, "11", 0, " 11(20MHz)"
HKR, Ndi\params\Chanspec\enum, "12", 0, " 12(20MHz)"
HKR, Ndi\params\Chanspec\enum, "13", 0, " 13(20MHz)"
HKR, Ndi\params\Chanspec\enum, "14", 0, " 14(20MHz)"
HKR, Ndi\params\Chanspec\enum, "1bl", 0, " 1(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "6bl", 0, " 6(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "6bu", 0, " 6(40MHz-U)"
HKR, Ndi\params\Chanspec\enum, "11bu", 0, " 11(40MHz-U)"
[a.channels.reg]
HKR, Ndi\params\Chanspec\enum, "36", 0, " 36"
HKR, Ndi\params\Chanspec\enum, "40", 0, " 40"
HKR, Ndi\params\Chanspec\enum, "44", 0, " 44"
HKR, Ndi\params\Chanspec\enum, "48", 0, " 48"
HKR, Ndi\params\Chanspec\enum, "52", 0, " 52"
HKR, Ndi\params\Chanspec\enum, "56", 0, " 56"
HKR, Ndi\params\Chanspec\enum, "60", 0, " 60"
HKR, Ndi\params\Chanspec\enum, "64", 0, " 64"
HKR, Ndi\params\Chanspec\enum, "100", 0, "100"
HKR, Ndi\params\Chanspec\enum, "104", 0, "104"
HKR, Ndi\params\Chanspec\enum, "108", 0, "108"
HKR, Ndi\params\Chanspec\enum, "112", 0, "112"
HKR, Ndi\params\Chanspec\enum, "116", 0, "116"
HKR, Ndi\params\Chanspec\enum, "120", 0, "120"
HKR, Ndi\params\Chanspec\enum, "124", 0, "124"
HKR, Ndi\params\Chanspec\enum, "128", 0, "128"
HKR, Ndi\params\Chanspec\enum, "132", 0, "132"
HKR, Ndi\params\Chanspec\enum, "136", 0, "136"
HKR, Ndi\params\Chanspec\enum, "140", 0, "140"
[na.channels.reg]
HKR, Ndi\params\Chanspec\enum, "36", 0, " 36(20MHz)"
HKR, Ndi\params\Chanspec\enum, "40", 0, " 40(20MHz)"
HKR, Ndi\params\Chanspec\enum, "44", 0, " 44(20MHz)"
HKR, Ndi\params\Chanspec\enum, "48", 0, " 48(20MHz)"
HKR, Ndi\params\Chanspec\enum, "52", 0, " 52(20MHz)"
HKR, Ndi\params\Chanspec\enum, "56", 0, " 56(20MHz)"
HKR, Ndi\params\Chanspec\enum, "60", 0, " 60(20MHz)"
HKR, Ndi\params\Chanspec\enum, "64", 0, " 64(20MHz)"
HKR, Ndi\params\Chanspec\enum, "100", 0, "100(20MHz)"
HKR, Ndi\params\Chanspec\enum, "104", 0, "104(20MHz)"
HKR, Ndi\params\Chanspec\enum, "108", 0, "108(20MHz)"
HKR, Ndi\params\Chanspec\enum, "112", 0, "112(20MHz)"
HKR, Ndi\params\Chanspec\enum, "116", 0, "116(20MHz)"
HKR, Ndi\params\Chanspec\enum, "120", 0, "120(20MHz)"
HKR, Ndi\params\Chanspec\enum, "124", 0, "124(20MHz)"
HKR, Ndi\params\Chanspec\enum, "128", 0, "128(20MHz)"
HKR, Ndi\params\Chanspec\enum, "132", 0, "132(20MHz)"
HKR, Ndi\params\Chanspec\enum, "136", 0, "136(20MHz)"
HKR, Ndi\params\Chanspec\enum, "140", 0, "140(20MHz)"
HKR, Ndi\params\Chanspec\enum, "149", 0, "149(20MHz)"
HKR, Ndi\params\Chanspec\enum, "153", 0, "153(20MHz)"
HKR, Ndi\params\Chanspec\enum, "157", 0, "157(20MHz)"
HKR, Ndi\params\Chanspec\enum, "161", 0, "161(20MHz)"
HKR, Ndi\params\Chanspec\enum, "165", 0, "165(20MHz)"
HKR, Ndi\params\Chanspec\enum, "36al", 0, " 36(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "44al", 0, " 44(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "52al", 0, " 52(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "60al", 0, " 60(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "100al", 0, "100(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "108al", 0, "108(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "116al", 0, "116(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "124al", 0, "124(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "132al", 0, "132(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "149al", 0, "149(40MHz-L)"
HKR, Ndi\params\Chanspec\enum, "157al", 0, "157(40MHz-L)"
[b.options.reg]
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %PLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate,default,,"0"
[g.options.reg]
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "3", 0, %Auto%
HKR, Ndi\params\RoamTrigger\enum, "1", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "0", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "2", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"3"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\IBSSMode, ParamDesc, 0, %IBSS54gtmMode%
HKR, Ndi\params\IBSSMode, type, 0, "enum"
HKR, Ndi\params\IBSSMode\enum, "0", 0, %80211bOnly%
HKR, Ndi\params\IBSSMode\enum, "2", 0, %54gAuto%
HKR, Ndi\params\IBSSMode\enum, "4", 0, %54gPerformance%
HKR, Ndi\params\IBSSMode,default,,"0"
HKR, Ndi\params\IBSSGProtection, ParamDesc, 0, %IBSS54gtmProtectionMode%
HKR, Ndi\params\IBSSGProtection, type, 0, "enum"
HKR, Ndi\params\IBSSGProtection\enum, "0", 0, %Disabled%
HKR, Ndi\params\IBSSGProtection\enum, "2", 0, %Auto%
HKR, Ndi\params\IBSSGProtection,default,,"2"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108",0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"0"
[gn.options.reg]
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "3", 0, %Auto%
HKR, Ndi\params\RoamTrigger\enum, "1", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "0", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "2", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"3"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\IBSSMode, ParamDesc, 0, %IBSSMode%
HKR, Ndi\params\IBSSMode, type, 0, "enum"
HKR, Ndi\params\IBSSMode\enum, "0", 0, %80211abOnly%
HKR, Ndi\params\IBSSMode\enum, "2", 0, %80211abgAuto%
HKR, Ndi\params\IBSSMode\enum, "4", 0, %80211abgPerf%
HKR, Ndi\params\IBSSMode\enum, "5", 0, %80211abgnAuto%
HKR, Ndi\params\IBSSMode,default,,"0"
HKR, Ndi\params\IBSSGProtection, ParamDesc, 0, %IBSS54gtmProtectionMode%
HKR, Ndi\params\IBSSGProtection, type, 0, "enum"
HKR, Ndi\params\IBSSGProtection\enum, "0", 0, %Disabled%
HKR, Ndi\params\IBSSGProtection\enum, "2", 0, %Auto%
HKR, Ndi\params\IBSSGProtection,default,,"2"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108",0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"0"
HKR, Ndi\params\Intolerant, ParamDesc, 0, %Intolerant%
HKR, Ndi\params\Intolerant, type, 0, "enum"
HKR, Ndi\params\Intolerant\enum, "0", 0, %Disabled%
HKR, Ndi\params\Intolerant\enum, "1", 0, %Enabled%
HKR, Ndi\params\Intolerant,default,,"0"
HKR, ,"mimo_antsel", 0, "-1"
[bg.options.reg]
HKR, Ndi\params\Chanspec, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Chanspec, type, 0, "enum"
HKR, Ndi\params\Chanspec, default, 0, "11"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
[a.options.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"0"
HKR, Ndi\params\RateA, ParamDesc, 0, %Rate_802_11a%
HKR, Ndi\params\RateA, type, 0, "enum"
HKR, Ndi\params\RateA\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\RateA\enum, "12", 0, " 6"
HKR, Ndi\params\RateA\enum, "18", 0, " 9"
HKR, Ndi\params\RateA\enum, "24", 0, "12"
HKR, Ndi\params\RateA\enum, "36", 0, "18"
HKR, Ndi\params\RateA\enum, "48", 0, "24"
HKR, Ndi\params\RateA\enum, "72", 0, "36"
HKR, Ndi\params\RateA\enum, "96", 0, "48"
HKR, Ndi\params\RateA\enum, "108",0, "54"
HKR, Ndi\params\RateA,default,,"0"
HKR, Ndi\params\Chanspec, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Chanspec, type, 0, "enum"
HKR, Ndi\params\Chanspec, default, 0, "36"
[bag.options.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"0"
HKR, Ndi\params\11HNetworks, ParamDesc, 0, "802.11h+d"
HKR, Ndi\params\11HNetworks, type, 0, "enum"
HKR, Ndi\params\11HNetworks\enum, "1", 0, %Loose_11h%
HKR, Ndi\params\11HNetworks\enum, "2", 0, %Strict_11h%
HKR, Ndi\params\11HNetworks\enum, "4", 0, %Loose_11h_and_11d%
HKR, Ndi\params\11HNetworks,default,,"1"
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "3", 0, %Auto%
HKR, Ndi\params\RoamTrigger\enum, "1", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "0", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "2", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"3"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\band, ParamDesc, 0, %DisableBands%
HKR, Ndi\params\band, type, 0, "enum"
HKR, Ndi\params\band\enum, "0", 0, %None%
HKR, Ndi\params\band\enum, "1", 0, %Disable80211gb%
HKR, Ndi\params\band\enum, "2", 0, %Disable80211a%
HKR, Ndi\params\band,default,,"0"
HKR, Ndi\params\BandPref, ParamDesc, 0, %BandPreference%
HKR, Ndi\params\BandPref, type, 0, "enum"
HKR, Ndi\params\BandPref\enum, "0", 0, %None%
HKR, Ndi\params\BandPref\enum, "1", 0, %Prefer80211a%
HKR, Ndi\params\BandPref\enum, "2", 0, %Prefer80211gb%
HKR, Ndi\params\BandPref,default,,"0"
HKR, Ndi\params\AssocRoamPref, ParamDesc, 0, %AssociationRoamPreference%
HKR, Ndi\params\AssocRoamPref, type, 0, "enum"
HKR, Ndi\params\AssocRoamPref\enum, "0", 0, %Disabled%
HKR, Ndi\params\AssocRoamPref\enum, "1", 0, %Enabled%
HKR, Ndi\params\AssocRoamPref,default,,"0"
HKR, Ndi\params\IBSSMode, ParamDesc, 0, %IBSS54gtmMode%
HKR, Ndi\params\IBSSMode, type, 0, "enum"
HKR, Ndi\params\IBSSMode\enum, "0", 0, %80211bOnly%
HKR, Ndi\params\IBSSMode\enum, "2", 0, %54gAuto%
HKR, Ndi\params\IBSSMode\enum, "4", 0, %54gPerformance%
HKR, Ndi\params\IBSSGProtection, ParamDesc, 0, %IBSS54gtmProtectionMode%
HKR, Ndi\params\IBSSGProtection, type, 0, "enum"
HKR, Ndi\params\IBSSGProtection\enum, "0", 0, %Disabled%
HKR, Ndi\params\IBSSGProtection\enum, "2", 0, %Auto%
HKR, Ndi\params\IBSSGProtection,default,,"2"
HKR, Ndi\params\RateA, ParamDesc, 0, %Rate_802_11a%
HKR, Ndi\params\RateA, type, 0, "enum"
HKR, Ndi\params\RateA\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\RateA\enum, "12", 0, " 6"
HKR, Ndi\params\RateA\enum, "18", 0, " 9"
HKR, Ndi\params\RateA\enum, "24", 0, "12"
HKR, Ndi\params\RateA\enum, "36", 0, "18"
HKR, Ndi\params\RateA\enum, "48", 0, "24"
HKR, Ndi\params\RateA\enum, "72", 0, "36"
HKR, Ndi\params\RateA\enum, "96", 0, "48"
HKR, Ndi\params\RateA\enum, "108",0, "54"
HKR, Ndi\params\RateA,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate_802_11bg%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108",0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Chanspec, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Chanspec, type, 0, "enum"
HKR, Ndi\params\Chanspec, default, 0, "11"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
[bagn.options.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"0"
HKR, Ndi\params\11HNetworks, ParamDesc, 0, "802.11h+d"
HKR, Ndi\params\11HNetworks, type, 0, "enum"
HKR, Ndi\params\11HNetworks\enum, "1", 0, %Loose_11h%
HKR, Ndi\params\11HNetworks\enum, "2", 0, %Strict_11h%
HKR, Ndi\params\11HNetworks\enum, "4", 0, %Loose_11h_and_11d%
HKR, Ndi\params\11HNetworks,default,,"1"
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "3", 0, %Auto%
HKR, Ndi\params\RoamTrigger\enum, "1", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "0", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "2", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"3"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\band, ParamDesc, 0, %DisableBands%
HKR, Ndi\params\band, type, 0, "enum"
HKR, Ndi\params\band\enum, "0", 0, %None%
HKR, Ndi\params\band\enum, "1", 0, %Disable80211gb%
HKR, Ndi\params\band\enum, "2", 0, %Disable80211a%
HKR, Ndi\params\band,default,,"0"
HKR, Ndi\params\BandPref, ParamDesc, 0, %BandPreference%
HKR, Ndi\params\BandPref, type, 0, "enum"
HKR, Ndi\params\BandPref\enum, "0", 0, %None%
HKR, Ndi\params\BandPref\enum, "1", 0, %Prefer80211a%
HKR, Ndi\params\BandPref\enum, "2", 0, %Prefer80211gb%
HKR, Ndi\params\BandPref,default,,"0"
HKR, Ndi\params\AssocRoamPref, ParamDesc, 0, %AssociationRoamPreference%
HKR, Ndi\params\AssocRoamPref, type, 0, "enum"
HKR, Ndi\params\AssocRoamPref\enum, "0", 0, %Disabled%
HKR, Ndi\params\AssocRoamPref\enum, "1", 0, %Enabled%
HKR, Ndi\params\AssocRoamPref,default,,"0"
HKR, Ndi\params\IBSSMode, ParamDesc, 0, %IBSSMode%
HKR, Ndi\params\IBSSMode, type, 0, "enum"
HKR, Ndi\params\IBSSMode\enum, "0", 0, %80211abOnly%
HKR, Ndi\params\IBSSMode\enum, "2", 0, %80211abgAuto%
HKR, Ndi\params\IBSSMode\enum, "4", 0, %80211abgPerf%
HKR, Ndi\params\IBSSMode\enum, "5", 0, %80211abgnAuto%
HKR, Ndi\params\IBSSMode,default,,"0"
HKR, Ndi\params\IBSSGProtection, ParamDesc, 0, %IBSS54gtmProtectionMode%
HKR, Ndi\params\IBSSGProtection, type, 0, "enum"
HKR, Ndi\params\IBSSGProtection\enum, "0", 0, %Disabled%
HKR, Ndi\params\IBSSGProtection\enum, "2", 0, %Auto%
HKR, Ndi\params\IBSSGProtection,default,,"2"
HKR, Ndi\params\RateA, ParamDesc, 0, %Rate_802_11a%
HKR, Ndi\params\RateA, type, 0, "enum"
HKR, Ndi\params\RateA\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\RateA\enum, "12", 0, " 6"
HKR, Ndi\params\RateA\enum, "18", 0, " 9"
HKR, Ndi\params\RateA\enum, "24", 0, "12"
HKR, Ndi\params\RateA\enum, "36", 0, "18"
HKR, Ndi\params\RateA\enum, "48", 0, "24"
HKR, Ndi\params\RateA\enum, "72", 0, "36"
HKR, Ndi\params\RateA\enum, "96", 0, "48"
HKR, Ndi\params\RateA\enum, "108",0, "54"
HKR, Ndi\params\RateA,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate_802_11bg%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108",0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Chanspec, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Chanspec, type, 0, "enum"
HKR, Ndi\params\Chanspec, default, 0, "11"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
HKR, Ndi\params\Intolerant, ParamDesc, 0, %Intolerant%
HKR, Ndi\params\Intolerant, type, 0, "enum"
HKR, Ndi\params\Intolerant\enum, "0", 0, %Disabled%
HKR, Ndi\params\Intolerant\enum, "1", 0, %Enabled%
HKR, Ndi\params\Intolerant,default,,"0"
HKR, Ndi\params\11NPreamble, ParamDesc, 0, "802.11n Preamble"
HKR, Ndi\params\11NPreamble, type, 0, "enum"
HKR, Ndi\params\11NPreamble\enum, "-1", 0, %Auto%
HKR, Ndi\params\11NPreamble\enum, "0", 0, %Mixed_Mode%
HKR, Ndi\params\11NPreamble,default,,"-1"
HKR, Ndi\params\ShortGI, ParamDesc, 0, "Short GI"
HKR, Ndi\params\ShortGI, type, 0, "enum"
HKR, Ndi\params\ShortGI\enum, "-1", 0, %Auto%
HKR, Ndi\params\ShortGI\enum, "0", 0, %Disabled%
HKR, Ndi\params\ShortGI,default,,"-1"
HKR, Ndi\params\BandwidthCap, ParamDesc, 0, "Bandwidth Capability"
HKR, Ndi\params\BandwidthCap, type, 0, "enum"
HKR, Ndi\params\BandwidthCap\enum, "0", 0, "11a/b/g:20MHz"
HKR, Ndi\params\BandwidthCap\enum, "1", 0, "11a/b/g:20/40MHz"
HKR, Ndi\params\BandwidthCap\enum, "2", 0, "11a:20/40;11bg:20MHz"
HKR, Ndi\params\BandwidthCap,default,,"2"
[strings]
V_BCM="Broadcom"
BCM430B_DeviceDesc="Broadcom 802.11b Network Adapter"
BCM430G_DeviceDesc="Broadcom 802.11g Network Adapter"
BCM430A_DeviceDesc="Broadcom 802.11a Network Adapter"
BCM430M_DeviceDesc="Broadcom 802.11 Multiband Network Adapter"
BCM43XX_HELP="The Broadcom 802.11 Network Adapter provides wireless local area networking."
BCM43XX_Service_DispName="Broadcom 802.11 Network Adapter Driver"
BCM43XX_DiskName="802.11 Network Adapter Install Disk"
BCM430N_DeviceDesc="Broadcom 802.11n Network Adapter"
BCMH43XX_Service_DispName="Broadcom 802.11 USB Network Adapter Driver"
54gAuto="54g - Auto"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g(tm) Mode"
IBSS54gtmProtectionMode="IBSS 54g(tm) Protection Mode"
IBSSMode="IBSS Mode"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
XPress_Technology="XPress (TM) Technology"
Fast="Fast"
MinimumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WMM"
Afterburner="Afterburner"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"
Manage_Wireless_Settings="Manage Wireless Settings"
DisableRadioUponWiredConnection="Disable Upon Wired Connect"
SSIDAutoPromote="SSID Autopromote"
IBSSChannelNumber="WZC IBSS Channel Number"
IbssAllowed="IBSS Allowed"
Loose_11h_and_11d="Loose 11h+d"
Loose_11h="Loose 11h"
Strict_11h="Strict 11h"
MixedCell="Mixed Cell Support"
vlan_mode="VLAN Priority Support"
80211abOnly="802.11a/b Only"
80211abgAuto="802.11a/b/g Auto"
80211abgPerf="802.11a/b/g Performance"
80211abgnAuto="802.11a/b/g/n Auto"
PriorityVLANTag="Priority & VLAN"
PriorityAndVLANDisabled="Priority & VLAN Disabled"
PriorityAndVLANEnabled="Priority & VLAN Enabled"
PriorityEnabled="Priority Enabled"
VLANEnabled="VLAN Enabled"
Lock_Wireless_Settings="Lock Wireless Settings"
Usebestrate="Best Rate"
WakeUpCapabilities="Wake-Up Mode"
MagicPacket="Magic Packet"
NetPattern="Wake Up Frame"
Intolerant="40MHz Intolerant"
All="All"
MagicNet="Magic & WakeUp Frame"
LossofAP="LossOfLink"
Mixed_Mode="Mixed Mode"
LossMagic="MagicPkt & LinkLoss"
LossNet="WakeUpPkt & LinkLoss"
