
[Version]
Signature="$Windows NT$"
Compatible=1
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318}
Provider=%MRVL%
CatalogFile=mrv8knet.cat
DriverVer=1/09/2004,2.3.0.1
[SourceDisksNames]
1="Marvell installation disk 1",,,
[SourceDisksFiles]
mrv8k51.sys =1
[DestinationDirs]
W8100PCI.XP.CopyFiles=12
DefaultDestDirs=11
[Manufacturer]
%MRVL%=DLINK
[DLINK]
%W8100PCIXPCB.DeviceDesc1%=W8100PCIXP.ndi, PCI\VEN_11AB&DEV_1FA6&SUBSYS_1FA411AB
%W8100PCIXPCB.DeviceDesc1%=W8100PCIXP.ndi, PCI\VEN_11AB&DEV_1FA6&SUBSYS_3B081186
%W8100PCIXPCB.DeviceDesc2%=W8100PCIXP.ndi, PCI\VEN_11AB&DEV_1FA6&SUBSYS_3B091186
[ControlFlags]
ExcludeFromSelect=PCI\VEN_11AB&DEV_1FA6&SUBSYS_1FA411AB
ExcludeFromSelect=PCI\VEN_11AB&DEV_1FA6&SUBSYS_3B081186
ExcludeFromSelect=PCI\VEN_11AB&DEV_1FA6&SUBSYS_3B091186
[W8100PCIXP.ndi]
Characteristics=0x84
BusType=5
AddReg=W8100PCI.reg, W8100PCIXP.reg, W8100PCI.zerocfg
;CpyFiles=W8100PCI.XP.CopyFiles
[W8100PCIXP.reg]
HKR, Ndi, Service, 0, "W8100PCI"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[W8100PCI.XP.CopyFiles]
mrv8k51.sys,,,2
[W8100PCIXP.ndi.Services]
AddService=W8100PCI, 2, W8100PCIXP.Service, CommonXP.EventLog
[W8100PCIXP.Service]
DisplayName=%W8100PCIXP.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\mrv8k51.sys
LoadOrderGroup=NDIS
[CommonXP.EventLog]
AddReg=CommonXP.AddEventLog.reg
[CommonXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[W8100PCI.reg]
HKR, Ndi\xparams\DesiredSSID,ParamDesc,,"%SSID%"
HKR, Ndi\xparams\DesiredSSID,default,,"default"
HKR, Ndi\xparams\DesiredSSID,type,,"edit"
HKR, Ndi\xparams\DesiredSSID,LimitText,,"32"
HKR, Ndi\xparams\DesiredSSID,UpperCase,,"0"
HKR, Ndi\xparams\DesiredSSID,Optional,,"1"
HKR, Ndi\xparams\AuthMode,ParamDesc,,"%AuthMode%"
HKR, Ndi\xparams\AuthMode,default,,"0"
HKR, Ndi\xparams\AuthMode,type,,enum
HKR, Ndi\xparams\AuthMode\enum,"0",,"Open"
HKR, Ndi\xparams\AuthMode\enum,"1",,"Shared"
HKR, Ndi\xparams\NetworkMode,ParamDesc,,"%NetworkMode%"
HKR, Ndi\xparams\NetworkMode,default,,"1"
HKR, Ndi\xparams\NetworkMode,type,,enum
HKR, Ndi\xparams\NetworkMode\enum,"0",,"Ad Hoc"
HKR, Ndi\xparams\NetworkMode\enum,"1",,"Infrastructure"
HKR, Ndi\xparams\FragThsd, ParamDesc,0 , "%FragThsds%"
HKR, Ndi\xparams\FragThsd, default, 0 , "2346"
HKR, Ndi\xparams\FragThsd, min, 0 , "256"
HKR, Ndi\xparams\FragThsd, max, 0 , "2346"
HKR, Ndi\xparams\FragThsd, step, 0 , "1"
HKR, Ndi\xparams\FragThsd, Base, 0 , "10"
HKR, Ndi\xparams\FragThsd, type, 0 ,"dword"
HKR, Ndi\xparams\Channel, ParamDesc,0 , "%Channel%"
HKR, Ndi\xparams\Channel, default, 0 , "6"
HKR, Ndi\xparams\Channel, min, 0 , "0"
HKR, Ndi\xparams\Channel, max, 0 , "14"
HKR, Ndi\xparams\Channel, step, 0 , "1"
HKR, Ndi\xparams\Channel, Base, 0 , "16"
HKR, Ndi\xparams\Channel, type, 0 ,"dword"
HKR, Ndi\xparams\TxAntenna, ParamDesc,0 , "%TxAntennaStr%"
HKR, Ndi\xparams\TxAntenna, default, 0 , "2"
HKR, Ndi\xparams\TxAntenna, min, 0 , "1"
HKR, Ndi\xparams\TxAntenna, max, 0 , "ffff"
HKR, Ndi\xparams\TxAntenna, step, 0 , "1"
HKR, Ndi\xparams\TxAntenna, Base, 0 , "16"
HKR, Ndi\xparams\TxAntenna, type, 0 ,"dword"
HKR, Ndi\xparams\RxAntenna, ParamDesc,0 , "%RxAntennaStr%"
HKR, Ndi\xparams\RxAntenna, default, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna, min, 0 , "1"
HKR, Ndi\xparams\RxAntenna, max, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna, step, 0 , "1"
HKR, Ndi\xparams\RxAntenna, Base, 0 , "16"
HKR, Ndi\xparams\RxAntenna, type, 0 ,"dword"
HKR, Ndi\xparams\RTSThsd, ParamDesc, 0, "%RTSThsds%"
HKR, Ndi\xparams\RTSThsd, default, 0, "2346"
HKR, Ndi\xparams\RTSThsd, min, 0, "0"
HKR, Ndi\xparams\RTSThsd, max, 0, "2346"
HKR, Ndi\xparams\RTSThsd, step, 0, "1"
HKR, Ndi\xparams\RTSThsd, Base, 0, "10"
HKR, Ndi\xparams\RTSThsd, type, 0, "dword"
HKR, Ndi\xparams\DataRate,ParamDesc,,"%DataRate%"
HKR, Ndi\xparams\DataRate,default,,"FF"
HKR, Ndi\xparams\DataRate,type,,enum
HKR, Ndi\xparams\DataRate\enum,"FF",,"Auto"
HKR, Ndi\xparams\DataRate\enum,"2",,"1 Mbps"
HKR, Ndi\xparams\DataRate\enum,"4",,"2 Mbps"
HKR, Ndi\xparams\DataRate\enum,"b",,"5.5 Mbps"
HKR, Ndi\xparams\DataRate\enum,"16",,"11 Mbps"
HKR, Ndi\xparams\DataRate\enum,"C",,"6 Mbps"
HKR, Ndi\xparams\DataRate\enum,"12",,"9 Mbps"
HKR, Ndi\xparams\DataRate\enum,"18",,"12 Mbps"
HKR, Ndi\xparams\DataRate\enum,"24",,"18 Mbps"
HKR, Ndi\xparams\DataRate\enum,"30",,"24 Mbps"
HKR, Ndi\xparams\DataRate\enum,"48",,"36 Mbps"
HKR, Ndi\xparams\DataRate\enum,"60",,"48 Mbps"
HKR, Ndi\xparams\DataRate\enum,"6C",,"54 Mbps"
HKR, Ndi\xparams\WepStatus,ParamDesc,,"%WepStatus%"
HKR, Ndi\xparams\WepStatus,default,,"1"
HKR, Ndi\xparams\WepStatus,type,,enum
HKR, Ndi\xparams\WepStatus\enum,"0",,"Enabled"
HKR, Ndi\xparams\WepStatus\enum,"1",,"Disabled"
HKR, Ndi\xparams\Preamble,ParamDesc,,"%PreambleStr%"
HKR, Ndi\xparams\Preamble,default,,"3"
HKR, Ndi\xparams\Preamble,type,,enum
HKR, Ndi\xparams\Preamble\enum,"1",,"Auto"
HKR, Ndi\xparams\Preamble\enum,"2",,"Short Preamble"
HKR, Ndi\xparams\Preamble\enum,"3",,"Long Preamble"
HKR,, TxWepKey, 2, ""
HKR,, WepKey1, 2, ""
HKR,, WepKey2, 2, ""
HKR,, WepKey3, 2, ""
HKR,, WepKey4, 2, ""
[Strings]
MRVL="D-Link"
TxAntennaStr="Tx Antenna Select"
RxAntennaStr="Rx Antenna Select"
Channel="Channel"
FragThsds="Fragamentation Threshold"
DataRate="Data Rate"
RTSThsds="RTS Threshold"
AuthMode="Authentication Mode"
NetworkMode="Operation Mode"
WepStatus="WEP Status"
SSID="SSID"
PreambleStr="Preamble Select"
W8100PCIXPCB.DeviceDesc1="D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter"
W8100PCIXPCB.DeviceDesc2="D-Link AirPlus G DWL-G510 Wireless PCI Card"
W8100PCIXP.Service.DispName="D-Link AirPlus G Wireless Driver"

