
[Version]
Signature="$CHICAGO$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%ATHEROS%
Compatible=1
DriverVer=09/27/2010,9.1.0.323
Catalogfile.nt=netathw.cat
[Manufacturer]
%ATHEROS%=Atheros
[ControlFlags]
ExcludeFromSelect=\ ;for win95 and legacy support
PCI\VEN_168C&DEV_0013
[Atheros]
%ATHER.DeviceDesc.3067%=ATHER_DEV_001C.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_303F103C
%ATHER.DeviceDesc.3067%=ATHER_DEV_001C.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_3040103C
%ATHER.DeviceDesc.3067%=ATHER_DEV_001C.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_137A103C
%ATHER.DeviceDesc.3067%=ATHER_DEV_001C.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_137B103C
%ATHER.DeviceDesc.2063%=ATHER_DEV_2063.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_1385103C
%ATHER.DeviceDesc.2063%=ATHER_DEV_2063.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_1386103C
%ATHER.DeviceDesc.3096%=ATHER_DEV_002A.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1381103C
%ATHER.DeviceDesc.3096%=ATHER_DEV_002A.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1382103C
%ATHER.DeviceDesc.3096%=ATHER_DEV_002A.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_3041103C
%ATHER.DeviceDesc.3096%=ATHER_DEV_002A.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_3042103C
%ATHER.DeviceDesc.30A1%=ATHER_DEV_30A1.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_303F103C
%ATHER.DeviceDesc.30A1%=ATHER_DEV_30A1.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_3040103C
%ATHER.DeviceDesc.30AB%=ATHER_DEV_30AB.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_1461103C
%ATHER.DeviceDesc.30A4%=ATHER_DEV_30A4.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_1462103C
%ATHER.DeviceDesc.30A4%=ATHER_DEV_3197.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_1626103C
[ATHER_DEV_001C.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
DelReg=5211.DelReg
AddReg=5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, ledcontrol.reg, uapsd.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_001C.ndi.NT.Services]
AddService=AR5416, 2, ATHER.Service, common.EventLog
[ATHER_DEV_2063.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
DelReg=5211.DelReg
AddReg=5211.reg, ATHER.reg, 5211.reg, ledcontrol3.reg, uapsd.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_2063.ndi.NT.Services]
AddService=AR5416, 2, ATHER.Service, common.EventLog
[ATHER_DEV_002A.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, sys.TcpParams.reg, ledcontrol2.reg, uapsd.reg, htAdhoc.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_002A.ndi.NT.Services]
AddService=AR5416, 2, ATHER.Service, common.EventLog
[ATHER_DEV_30A1.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, sys.TcpParams.reg, ledcontrol2.reg, uapsd.reg, htAdhoc.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_30A1.ndi.NT.Services]
AddService=AR5416, 2, ATHER.Service, common.EventLog
[ATHER_DEV_30AB.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, sys.TcpParams.reg, ledcontrol2.reg, uapsd.reg, htAdhoc.reg, janusda.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_30AB.ndi.NT.Services]
AddService=AR5416, 2, ATHER.Service, common.EventLog
[ATHER_DEV_30A4.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, sys.TcpParams.reg, ledcontrol4.reg, uapsd.reg, htAdhoc.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_30A4.ndi.NT.Services]
AddService=AR5416, 2, ATHER.Service, common.EventLog
[ATHER_DEV_3197.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
DelReg=5416.DelReg
AddReg=5416.reg, ATHER.reg, 5416.reg, sys.TcpParams.reg, ledcontrol4.reg, uapsd.reg, htAdhoc.reg, heliusda.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_3197.ndi.NT.Services]
AddService=AR5416, 2, ATHER.Service, common.EventLog
[5212.bgmp.reg]
HKR, , NetBand, 0x00002, "12"
HKR, CustomParams\Configurations, NicType, 0x10003, 2
[5211.DelReg]
HKR,,d3forcel1disable.reg
HKR,,pcieWaen
HKR,,radioEnable
HKR, Ndi\params\radioEnable
[5211.reg]
HKR, Ndi\params\MapRegisters, ParamDesc, 0, %MapRegisters%
HKR, Ndi\params\MapRegisters, default, 0, "256"
HKR, Ndi\params\MapRegisters, min, 0, "32"
HKR, Ndi\params\MapRegisters, max, 0, "512"
HKR, Ndi\params\MapRegisters, step, 0, "8"
HKR, Ndi\params\MapRegisters, base, 0, "10"
HKR, Ndi\params\MapRegisters, type, 0, "int"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\sleepMode, ParamDesc, 0, %sleepMode%
HKR, Ndi\params\sleepMode, Base, 0, "10"
HKR, Ndi\params\sleepMode, default, 0, "2"
HKR, Ndi\params\sleepMode, type, 0, "enum"
HKR, Ndi\params\sleepMode\enum, "0", 0, %sleepModeOff%
HKR, Ndi\params\sleepMode\enum, "2", 0, %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum, "1", 0, %sleepModeMax%
HKR, Ndi\params\shortPreamble, ParamDesc, 0, %shortPreamble%
HKR, Ndi\params\shortPreamble, Base, 0, "10"
HKR, Ndi\params\shortPreamble, default, 0, "1"
HKR, Ndi\params\shortPreamble, type, 0, "enum"
HKR, Ndi\params\shortPreamble\enum, "1", 0, %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0", 0, %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid, ParamDesc, 0, %scanTimeValid%
HKR, Ndi\params\scanTimeValid, default, 0, "60"
HKR, Ndi\params\scanTimeValid, min, 0, "20"
HKR, Ndi\params\scanTimeValid, max, 0, "120"
HKR, Ndi\params\scanTimeValid, step, 0, "5"
HKR, Ndi\params\scanTimeValid, base, 0, "10"
HKR, Ndi\params\scanTimeValid, type, 0, "int"
HKR, CustomParams\Configurations, MajorVersion, 0x10003, 2
HKR, CustomParams\Configurations, MinorVersion, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
[5416.DelReg]
HKR,,d3forcel1disable.reg
HKR,,pcieWaen
HKR,,radioEnable
HKR, Ndi\params\radioEnable
[5416.reg]
HKR, Ndi\params\MapRegisters, ParamDesc, 0, %MapRegisters%
HKR, Ndi\params\MapRegisters, default, 0, "256"
HKR, Ndi\params\MapRegisters, min, 0, "32"
HKR, Ndi\params\MapRegisters, max, 0, "512"
HKR, Ndi\params\MapRegisters, step, 0, "8"
HKR, Ndi\params\MapRegisters, base, 0, "10"
HKR, Ndi\params\MapRegisters, type, 0, "int"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\sleepMode, ParamDesc, 0, %sleepMode%
HKR, Ndi\params\sleepMode, Base, 0, "10"
HKR, Ndi\params\sleepMode, default, 0, "2"
HKR, Ndi\params\sleepMode, type, 0, "enum"
HKR, Ndi\params\sleepMode\enum, "0", 0, %sleepModeOff%
HKR, Ndi\params\sleepMode\enum, "2", 0, %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum, "1", 0, %sleepModeMax%
HKR, Ndi\params\shortPreamble, ParamDesc, 0, %shortPreamble%
HKR, Ndi\params\shortPreamble, Base, 0, "10"
HKR, Ndi\params\shortPreamble, default, 0, "1"
HKR, Ndi\params\shortPreamble, type, 0, "enum"
HKR, Ndi\params\shortPreamble\enum, "1", 0, %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0", 0, %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid, ParamDesc, 0, %scanTimeValid%
HKR, Ndi\params\scanTimeValid, default, 0, "60"
HKR, Ndi\params\scanTimeValid, min, 0, "20"
HKR, Ndi\params\scanTimeValid, max, 0, "120"
HKR, Ndi\params\scanTimeValid, step, 0, "5"
HKR, Ndi\params\scanTimeValid, base, 0, "10"
HKR, Ndi\params\scanTimeValid, type, 0, "int"
HKR, CustomParams\Configurations, MajorVersion, 0x10003, 2
HKR, CustomParams\Configurations, MinorVersion, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
[uapsd.reg]
HKR, Ndi\params\uapsdEnabledBE, ParamDesc, 0, %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledBE, default, 0, "0"
HKR, Ndi\params\uapsdEnabledBE, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledBE\enum, "1", 0, %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum, "0", 0, %uapsdEnabledBEOff%
HKR, Ndi\params\uapsdEnabledBK, ParamDesc, 0, %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledBK, default, 0, "0"
HKR, Ndi\params\uapsdEnabledBK, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledBK\enum, "1", 0, %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum, "0", 0, %uapsdEnabledBKOff%
HKR, Ndi\params\uapsdEnabledVI, ParamDesc, 0, %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledVI, default, 0, "0"
HKR, Ndi\params\uapsdEnabledVI, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledVI\enum, "1", 0, %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum, "0", 0, %uapsdEnabledVIOff%
HKR, Ndi\params\uapsdEnabledVO, ParamDesc, 0, %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO, Base, 0, "10"
HKR, Ndi\params\uapsdEnabledVO, default, 0, "0"
HKR, Ndi\params\uapsdEnabledVO, type, 0, "enum"
HKR, Ndi\params\uapsdEnabledVO\enum, "1", 0, %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum, "0", 0, %uapsdEnabledVOOff%
[ledcontrol.reg]
HKR, , gpioPinFunc0, 0x00002, "3"
HKR, , gpioFunc0ActHi, 0x00002, "0"
[ledcontrol2.reg]
HKR, , gpioPinFunc0, 0x00002, "1"
HKR, , gpioFunc0ActHi, 0x00002, "0"
HKR, , sharedGpioFunc0, 0x00002, "1"
[ledcontrol3.reg]
HKR, , gpioPinFunc0, 0x00002, "1"
HKR, , gpioFunc0ActHi, 0x00002, "0"
[ledcontrol4.reg]
HKR, , gpioPinFunc0, 0x00002, "8"
HKR, , gpioFunc0ActHi, 0x00002, "0"
HKR, , sharedGpioFunc0, 0x00002, "1"
[htAdhoc.reg]
HKR, Ndi\params\htAdhocEnable, ParamDesc, 0, %AdHoc11n%
HKR, Ndi\params\htAdhocEnable, Base, 0, "10"
HKR, Ndi\params\htAdhocEnable, default, 0, "0"
HKR, Ndi\params\htAdhocEnable, type, 0, "enum"
HKR, Ndi\params\htAdhocEnable\enum, "1", 0, %Enable%
HKR, Ndi\params\htAdhocEnable\enum, "0", 0, %Disable%
[janusda.reg]
HKR, , btCoexEnable, 0x00002, "4"
HKR, , btCoexAgent, 0x00002, "1"
[heliusda.reg]
HKR, , btCoexEnable, 0x00002, "4"
HKR, , btCoexAgent, 0x00002, "1"
HKR, , btModule, 0x00002, "2"
HKR, , txChainSelectLegacy, 0x00002, "2"
HKR, , rxChainSelectLegacy, 0x00002, "2"
[ATHER.reg]
HKR, Ndi, Service, 0, "AR5416"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[ATHER.Service]
DisplayName=%ATHER.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\athw.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[sys.TcpParams.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000003
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000
[ATHER.CopyFiles.nt]
athw.sys,,,2
[ATHER.DelIniFiles]
Athnic.ini,,,1
[SourceDisksNames]
1=%Atheros_Disk%,,,
[SourceDisksFiles]
ar52119x.sys=1,, ; on distribution disk 1
athw.sys=1,, ; on distribution disk 1
[DestinationDirs]
ATHER.CopyFiles.nt=12
ATHER.DelIniFiles=10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir=11
[DEFAULTDESTDIRS]
[Strings]
Atheros="Atheros"
MapRegisters="Map Registers"
NetworkAddress="Network Address"
sleepMode="Power Save Mode"
scanTimeValid="Scan Valid Interval"
sleepModeOff="Off"
sleepModeNormal="Normal"
sleepModeMax="Maximum"
shortPreamble="802.11b Preamble"
shortPreambleEnable="Long and Short"
shortPreambleDisable="Long only"
uapsdEnabledBE="Power Save Policy (Best Effort)"
uapsdEnabledBEOn="WMM Power Save (UAPSD)"
uapsdEnabledBEOff="Legacy Power Save"
uapsdEnabledBK="Power Save Policy (Background)"
uapsdEnabledBKOn="WMM Power Save (UAPSD)"
uapsdEnabledBKOff="Legacy Power Save"
uapsdEnabledVI="Power Save Policy (Voice)"
uapsdEnabledVIOn="WMM Power Save (UAPSD)"
uapsdEnabledVIOff="Legacy Power Save"
uapsdEnabledVO="Power Save Policy (Video)"
uapsdEnabledVOOn="WMM Power Save (UAPSD)"
uapsdEnabledVOOff="Legacy Power Save"
Atheros_Disk="Atheros Driver Disk 1"
AdHoc11n="AdHoc 11n"
Enable="Enable"
Disable="Disable"
ATHER.Service.DispName="Atheros Wireless Adapter Service"
ATHER.DeviceDesc.3067="Atheros AR5007 802.11b/g WiFi Adapter"
ATHER.DeviceDesc.2063="Atheros AR5006 802.11a/b/g WiFi Adapter"
ATHER.DeviceDesc.3096="Atheros AR5009 802.11a/g/n WiFi Adapter"
ATHER.DeviceDesc.30A1="Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHER.DeviceDesc.30AB="Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHER.DeviceDesc.30A4="Atheros AR9287 802.11b/g/n WiFi Adapter"
