
[version]
signature="$CHICAGO$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
provider=%V_CISCO%
MillenniumPreferred=.ME
DriverVer=09/20/2004, 3.9.16
CatalogFile=neta504.cat
[SourceDisksNames]
1= %Disk_1_Desc%,,,,
[SourceDisksFiles]
PCX504.sys =1,,
PCX504.51 =1,,
vxdx500.vxd =1,,
CInst16.dll =1,,
CUtil16.exe =1,,
[DestinationDirs]
CopySys_NT=12 ; Drivers directory (%windir%\system32\drivers)
CopySys_XP=12 ; Drivers directory (%windir%\system32\drivers)
CopyFW_a_NT=12 ; Drivers directory (%windir%\system32\drivers)
CopyFW_b_NT=12 ; Drivers directory (%windir%\system32\drivers)
CopyCoInst_NT=11
CopySys_9x=11 ; Win9x Only (%windir%\system)
CopyFW_a_9x=11 ; Win9x Only (%windir%\system)
CopyFW_b_9x=11 ; Win9x Only (%windir%\system)
CopyCoInst_9x=11 ; Win9x Only (%windir%\system)
DefaultDestDir=11 ; Win9x Only (%windir%\system)
[Manufacturer]
%V_CISCO%=CISCO,NT.5.1
[ControlFlags]
ExcludeFromSelect=*
[CISCO]
%PCX504_b.DevDesc%=PCX504_b.ndi, PCI\VEN_14B9&DEV_A504&SUBSYS_500014B9
%PCX504_a.DevDesc%=PCX504_a.ndi, PCI\VEN_14B9&DEV_A505&SUBSYS_640014B9
[CISCO.NT.5.1]
%PCX504_b.DevDesc%=PCX504_b_XP.ndi, PCI\VEN_14B9&DEV_A504&SUBSYS_500014B9
%PCX504_a.DevDesc%=PCX504_a_XP.ndi, PCI\VEN_14B9&DEV_A505&SUBSYS_640014B9
[PCX504_b_XP.ndi]
AddReg=NDI5, COMMON, DATARATE_b, SSID, RADIONAME_b, BUSPCI
Characteristics=0x84
BusType=5
;CpyFiles=CopySys_XP, CopyFW_b_NT
[PCX504_b_XP.ndi.Services]
AddService=PCX504, 2, PCX504.Service, common.AddEventLog
[PCX504_b_XP.ndi.CoInstallers]
AddReg=CoInstaller.NT.AddReg
;CpyFiles=CopyCoInst_NT
[PCX504_b.ndi.NT]
AddReg=NDI5, COMMON, DATARATE_b, SSID, RADIONAME_b, BUSPCI
Characteristics=0x84
BusType=5
;CpyFiles=CopySys_NT, CopyFW_b_NT
[PCX504_b.ndi.NT.Services]
AddService=PCX504, 2, PCX504.Service, common.AddEventLog
[PCX504_b.ndi.NT.CoInstallers]
AddReg=CoInstaller.NT.AddReg
;CpyFiles=CopyCoInst_NT
[PCX504_b.ndi.ME]
AddReg=NDI5_ME, COMMON, DATARATE_b, SSID, RADIONAME_b, BUSPCI, DEVID_b
Characteristics=0x84
BusType=5
;CpyFiles=CopyCoInst_9x,CopySys_9x,CopyFW_b_9x
[PCX504_b.ndi.ME.Services]
AddService=PCX504, 2, PCX504.Service, common.AddEventLog
[PCX504_b.ndi]
AddReg=NDI3, COMMON, DATARATE_b, SSID, RADIONAME_b, BUSPCI, DEVID_b
;CpyFiles=CopyCoInst_9x,CopySys_9x,CopyFW_b_9x
[PCX504_a_XP.ndi]
AddReg=NDI5, COMMON, DATARATE_a, SSID, RADIONAME_a, BUSCARDBUS
Characteristics=0x84
BusType=5
;CpyFiles=CopySys_XP, CopyFW_a_NT
[PCX504_a_XP.ndi.Services]
AddService=PCX504, 2, PCX504.Service, common.AddEventLog
[PCX504_a_XP.ndi.CoInstallers]
AddReg=CoInstaller.NT.AddReg
;CpyFiles=CopyCoInst_NT
[PCX504_a.ndi.NT]
AddReg=NDI5, COMMON, DATARATE_a, SSID, RADIONAME_a, BUSCARDBUS
Characteristics=0x84
BusType=5
;CpyFiles=CopySys_NT, CopyFW_a_NT
[PCX504_a.ndi.NT.Services]
AddService=PCX504, 2, PCX504.Service, common.AddEventLog
[PCX504_a.ndi.NT.CoInstallers]
AddReg=CoInstaller.NT.AddReg
;CpyFiles=CopyCoInst_NT
[PCX504_a.ndi.ME]
AddReg=NDI5_ME, COMMON, DATARATE_a, SSID, RADIONAME_a, BUSCARDBUS, DEVID_a
Characteristics=0x84
BusType=5
;CpyFiles=CopyCoInst_9x,CopySys_9x,CopyFW_a_9x
[PCX504_a.ndi.ME.Services]
AddService=PCX504, 2, PCX504.Service, common.AddEventLog
[PCX504_a.ndi]
AddReg=NDI3, COMMON, DATARATE_a, SSID, RADIONAME_a, BUSCARDBUS, DEVID_a
;CpyFiles=CopyCoInst_9x,CopySys_9x,CopyFW_a_9x
[DEVID_b]
HKR,Ndi,DeviceID,,"PCI\VEN_14B9&DEV_A504"
[DEVID_a]
HKR,Ndi,DeviceID,,"PCI\VEN_14B9&DEV_A505"
[NDI5]
HKR,Ndi,Service,0,"PCX504"
HKR,Ndi\Interfaces,DefUpper,0,"ndis5"
HKR,Ndi\Interfaces,DefLower,0,"ethernet"
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet"
HKR,,MediaDisconnectDamper,,"10"
HKR,,AdapterType,,"1"
[NDI5_ME]
HKR,Ndi,Service,0,"PCX504"
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,PCX504.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR,NDIS,LogDriverName,,"PCX504"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,Ndi\Interfaces,DefUpper,,"ndis5"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis5"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,,AdapterType,,1
HKR,Ndi,NdiInstaller,0,"CINST16.DLL,CiscoNdiProc"
[NDI3]
HKR,,PnPCapabilities,0x10001,0x138
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,PCX504.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR,NDIS,LogDriverName,,"PCX504"
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0A
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,,AdapterType,,1
HKR,Ndi,NdiInstaller,0,"CINST16.DLL,CiscoNdiProc"
[BUSPCI]
HKR,,FormFactor,,"PCI"
[BUSCARDBUS]
HKR,,FormFactor,,"CARDBUS"
[COMMON]
HKR,,NodeName,2,""
HKR,NDI\params\NodeName,ParamDesc,,%ClientName%
HKR,NDI\params\NodeName,flag,1,30,00,00,00
HKR,NDI\params\NodeName,type,,"edit"
HKR,NDI\params\NodeName,LimitText,,"16"
HKR,NDI\params\NodeName,default,2,""
HKR,NDI\params\NodeName,optional,0,"1"
HKR,,InfrastructureMode,2,"1"
HKR,NDI\params\InfrastructureMode,ParamDesc,,%InfraMode%
HKR,NDI\params\InfrastructureMode,flag,1,30,00,00,00
HKR,NDI\params\InfrastructureMode,type,,"enum"
HKR,NDI\params\InfrastructureMode,default,,"1"
HKR,NDI\params\InfrastructureMode\enum,0,0,%No%
HKR,NDI\params\InfrastructureMode\enum,1,0,%Yes%
HKR,,PowerSaveMode,2,"0"
HKR,NDI\params\PowerSaveMode,ParamDesc,,%PSP%
HKR,NDI\params\PowerSaveMode,flag,1,30,00,00,00
HKR,NDI\params\PowerSaveMode,type,,"enum"
HKR,NDI\params\PowerSaveMode,default,,"0"
HKR,NDI\params\PowerSaveMode\enum,0,,%CAM%
HKR,NDI\params\PowerSaveMode\enum,2,,%PSP-CAM%
HKR,NDI\params\PowerSaveMode\enum,3,,%MAXPSP%
[SSID]
HKR,, SSID1,2,""
HKR,NDI\params\SSID1,ParamDesc,0,"SSID"
HKR,NDI\params\SSID1,type,0,"edit"
HKR,NDI\params\SSID1,flag,1,30,0,0,0
HKR,NDI\params\SSID1,optional,0,"1"
HKR,NDI\params\SSID1,default,2,""
[DATARATE_b]
HKR,,SupportedRates,2,"0"
HKR,NDI\params\SupportedRates,ParamDesc,,%DataRates%
HKR,NDI\params\SupportedRates,flag,1,30,00,00,00
HKR,NDI\params\SupportedRates,type,,"enum"
HKR,NDI\params\SupportedRates,default,,"0"
HKR,NDI\params\SupportedRates\enum,0,,%Auto%
HKR,NDI\params\SupportedRates\enum,2,,%1Mb%
HKR,NDI\params\SupportedRates\enum,4,,%2Mb%
HKR,NDI\params\SupportedRates\enum,B,,%5Mb%
HKR,NDI\params\SupportedRates\enum,16,,%11Mb%
HKR,NDI\params\SupportedRates,base,0,"16"
[DATARATE_a]
HKR,,SupportedRates,2,"0"
HKR,NDI\params\SupportedRates,ParamDesc,,%DataRates%
HKR,NDI\params\SupportedRates,flag,1,30,00,00,00
HKR,NDI\params\SupportedRates,type,,"enum"
HKR,NDI\params\SupportedRates,default,,"0"
HKR,NDI\params\SupportedRates\enum,0,,%Auto%
HKR,NDI\params\SupportedRates\enum,C,,%6Mb%
HKR,NDI\params\SupportedRates\enum,12,,%9Mb%
HKR,NDI\params\SupportedRates\enum,18,,%12Mb%
HKR,NDI\params\SupportedRates\enum,24,,%18Mb%
HKR,NDI\params\SupportedRates\enum,30,,%24Mb%
HKR,NDI\params\SupportedRates\enum,48,,%36Mb%
HKR,NDI\params\SupportedRates\enum,60,,%48Mb%
HKR,NDI\params\SupportedRates\enum,6C,,%54Mb%
HKR,NDI\params\SupportedRates,base,0,"16"
[RADIONAME_b]
HKR,,RadioName,,"PCX504"
[RADIONAME_a]
HKR,,RadioName,,"PCX5045G"
[PCX504.Service]
DisplayName=%PCX504.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\PCX504.sys
LoadOrderGroup=NDIS
[CoInstaller.NT.AddReg]
[common.AddEventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\netevent.dll"
HKR,,TypesSupported,0x00010001,7
[CopySys_NT]
PCX504.sys,,,2
[CopySys_XP]
PCX504.sys,pcx504.51,,2
[CopyFW_b_NT]
[CopyFW_a_NT]
[CopySys_9x]
PCX504.sys,,,2
vxdX500.vxd,,,2
[CopyFW_a_9x]
[CopyFW_b_9x]
[CopyCoInst_NT]
[CopyCoInst_9x]
CUtil16.exe,,,2
CInst16.dll,,,2
[strings]
V_CISCO="Cisco"
ClientName="Client Name"
InfraMode="Infrastructure Mode"
No="No"
Yes="Yes"
Disabled="Disabled"
Enabled="Enabled"
PSP="Power Saving Mode(PSP)"
CAM="CAM"
PSP-CAM="PSP-CAM (FASTPSP)"
MAXPSP="Max Power Save/PSP"
DataRates="Data Rates"
Auto="Auto"
1Mb=" 1 Mb"
2Mb=" 2 Mb"
5Mb=" 5.5 Mb"
11Mb="11 Mb"
6Mb=" 6 Mb"
9Mb=" 9 Mb"
12Mb="12 Mb"
18Mb="18 Mb"
24Mb="24 Mb"
36Mb="36 Mb"
48Mb="48 Mb"
54Mb="54 Mb"
Disk_1_Desc="Cisco Systems Wireless LAN Adapter Installation Disk"
PCX504.Service.DispName="Cisco Systems Wireless LAN Adapter Driver"
PCX504_b.DevDesc="Cisco Systems PCI Wireless LAN Adapter"
PCX504_a.DevDesc="Cisco Systems AIR-CB20A 802.11a Wireless LAN Adapter"
