
[Version]
CatalogFile=smcwlan.cat
Signature="$Windows NT$"
Provider=%TI%
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=03/06/2003,3.0.0.1
[Manufacturer]
%TI%=SMCInstruments
[ControlFlags]
ExcludeFromSelect=PCI\VEN_104C&DEV_8400&SUBSYS_8402104C
ExcludeFromSelect=PCI\VEN_104C&DEV_8400&SUBSYS_850216AB
[SMCInstruments]
%SMC.DeviceDesc1%=SMC.8400, PCI\VEN_104C&DEV_8400&SUBSYS_8402104C
%SMC.DeviceDesc2%=SMC.8400, PCI\VEN_104C&DEV_8400&SUBSYS_850216AB
[TI3000P.ndi]
AddReg=SMC.ndi.reg
[SMC.8400.NT]
BusType=5
AddReg =SMC.ndi.reg.NT, TI.Param.Reg
Characteristics=0x84
;CpyFiles =SMC.8400.CopyFiles.NT, SMC.8400.BinFiles.NT
[SMC.ndi.reg.NT]
HKR, Ndi, Service, 0, "SMCLN"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[SMC.8400.NT.Services]
AddService=SMCLN, 2, SMCLN.Service, SMCLN.EventLog
[SMCLN.Service]
DisplayName=%SMCLN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\smcwlan.sys
LoadOrderGroup=NDIS
[SMCLN.EventLog]
AddReg=SMCLN.AddEventLog.reg
[SMCLN.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[SMC.8400.CopyFiles.NT]
SMCWLAN.sys
[SMC.8400.BinFiles.NT]
[SMC.8400]
AddReg=SMC.ndi.reg, TI.Param.Reg, SMC.8400.Install
[SMC.8400.Install]
HKR,Ndi\Install,,,"SMC.8400.Copy"
HKR,Ndi\Remove,,,"SMC.8400.Remove"
[SMC.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_8400"
HKR,Ndi,HelpText,0,%WLANAdapterHelpText%
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,SMCWLAN.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, , "SMCLN"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"
HKR,Ndi,InstallInf,,"SMCWLAN.INF"
[SMC.8400.Copy]
;CpyFiles=SMC.8400.CopyFiles
[SMC.8400.Remove]
;DlFiles=SMC.8400.CopyFiles
[SMC.8400.CopyFiles]
SMCWLAN.sys
[TI.Param.Reg]
HKR, ,Radio11_RxLevel,, "bc b3 a9 9a 90 89 80 79 70 68 64 61 60 55 00"
HKR, ,Radio11_LNA,, "01 01 01 01 01 01 01 01 01 01 01 01 01 01 01"
HKR, ,Radio11_RSSI,, "0a 0f 14 19 1e 23 28 2d 32 37 3c 41 46 4b c8"
HKR, ,Radio0D_RxLevel,, "55 4f 4a 43 3a 32 5d 56 4e 46 3e 37 2a 23 1f"
HKR, ,Radio0D_LNA,, "00 00 00 00 00 00 01 01 01 01 01 01 01 01 01"
HKR, ,Radio0D_RSSI,, "0a 0f 14 19 1e 23 28 2d 32 37 3c 41 46 4b 5a"
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x10001, 25200
HKR,,PermAddress,,112233
HKR, ,HardwareID, ,"ACX100"
HKR, ,NumACXRxDescriptors, ,10
HKR, ,NumACXTxDescriptors, ,10
HKR, ,LeapUserPassword, ,""
HKR, ,DriverDescription, ,"SMC EZ Connect Turbo WLAN Adapter"
HKR,NDI\params\dot11DesiredBSSType,ParamDesc,,"Desired BSS Type"
HKR,NDI\params\dot11DesiredBSSType,type,,"enum"
HKR,NDI\params\dot11DesiredBSSType,default,,"1"
HKR,NDI\params\dot11DesiredBSSType\enum,"0",,"Ad-Hoc"
HKR,NDI\params\dot11DesiredBSSType\enum,"1",,"Infrastructure"
HKR,NDI\params\dot11DesiredBSSType\enum,"2",,"Any"
HKR, Ndi\Params\dot11DesiredSSID, ParamDesc, ,"Desired SSID"
HKR, Ndi\Params\dot11DesiredSSID, Type, ,"edit"
HKR, Ndi\Params\dot11DesiredSSID, LimitText, ,"32"
HKR, Ndi\Params\dot11DesiredSSID, Default,,"ANY"
HKR, Ndi\Params\dot11DesiredSSID, UpperCase,,"0"
HKR,NDI\params\dot11PowerMode,ParamDesc,,"Power Mode"
HKR,NDI\params\dot11PowerMode,type,,"enum"
HKR,NDI\params\dot11PowerMode,default,,"0"
HKR,NDI\params\dot11PowerMode\enum,"0",,"Continuous Access Mode"
HKR,NDI\params\dot11PowerMode\enum,"1",,"Maximum Power Save"
HKR,NDI\params\dot11PowerMode\enum,"2",,"Fast Power Save"
HKR,NDI\params\dot11DesiredTxRate,ParamDesc,, "Desired Tx Rate"
HKR,NDI\params\dot11DesiredTxRate,type,,"enum"
HKR,NDI\params\dot11DesiredTxRate,default,,"0"
HKR,NDI\params\dot11DesiredTxRate\enum,"0",,"Auto"
HKR,NDI\params\dot11DesiredTxRate\enum,"1",,"1 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"2",,"2 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"3",,"5.5 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"4",,"5.5 Mbps PBCC"
HKR,NDI\params\dot11DesiredTxRate\enum,"5",,"11 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"6",,"11 Mbps PBCC"
HKR,NDI\params\dot11DesiredTxRate\enum,"7",,"22 Mbps PBCC"
HKR,NDI\params\dot11SupportedRateMask,ParamDesc,, "Desired Supported Rate Set"
HKR,NDI\params\dot11SupportedRateMask,type,,"enum"
HKR,NDI\params\dot11SupportedRateMask,default,,"2"
HKR,NDI\params\dot11SupportedRateMask\enum,"0",,"1,2 Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"1",,"1,2,5.5,11 Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"2",,"1,2,5.5,11,22 Mbps"
HKR,NDI\params\dot11BasicRateMask,ParamDesc,, "Desired Basic Rate Set"
HKR,NDI\params\dot11BasicRateMask,type,,"enum"
HKR,NDI\params\dot11BasicRateMask,default,,"0"
HKR,NDI\params\dot11BasicRateMask\enum,"0",,"1,2,5.5,11 Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"1",,"1,2 Mbps"
HKR, Ndi\Params\dot11FragmentationThreshold, ParamDesc, ,"Fragmentation Threshold"
HKR, Ndi\Params\dot11FragmentationThreshold, Type, , "int"
HKR, Ndi\Params\dot11FragmentationThreshold, Default, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Min, , "256"
HKR, Ndi\Params\dot11FragmentationThreshold, Max, , "6000"
HKR, Ndi\Params\dot11FragmentationThreshold, Step, , "1"
HKR, Ndi\Params\dot11FragmentationThreshold, Base, , "10"
HKR, Ndi\Params\dot11RTSThreshold, ParamDesc, ,"RTS Threshold"
HKR, Ndi\Params\dot11RTSThreshold, Type, , "int"
HKR, Ndi\Params\dot11RTSThreshold, Default, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Min, , "0"
HKR, Ndi\Params\dot11RTSThreshold, Max, , "6000"
HKR, Ndi\Params\dot11RTSThreshold, Step, , "1"
HKR, Ndi\Params\dot11RTSThreshold, Base, , "10"
HKR,NDI\params\dot11WEPStatus,ParamDesc,,"WEP Option"
HKR,NDI\params\dot11WEPStatus,type,,"enum"
HKR,NDI\params\dot11WEPStatus,default,,"1"
HKR,NDI\params\dot11WEPStatus\enum,"0",,"WEP Enabled"
HKR,NDI\params\dot11WEPStatus\enum,"1",,"WEP Disabled"
HKR,NDI\params\dot11AuthMode,ParamDesc,,"Authentication Mode"
HKR,NDI\params\dot11AuthMode,type,,"enum"
HKR,NDI\params\dot11AuthMode,default,,"2"
HKR,NDI\params\dot11AuthMode\enum,"0",,"Open Authentication"
HKR,NDI\params\dot11AuthMode\enum,"1",,"Shared Authentication"
HKR,NDI\params\dot11AuthMode\enum,"2",,"Auto Switch"
HKR,NDI\params\dot11ShortPreambleInvoked,ParamDesc,,"Short Preamble"
HKR,NDI\params\dot11ShortPreambleInvoked,type,,"enum"
HKR,NDI\params\dot11ShortPreambleInvoked,default,,"0"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"0",,"Off"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"1",,"On"
HKR,NDI\params\ELPSupport,ParamDesc,,"ELP Support"
HKR,NDI\params\ELPSupport,type,,"enum"
HKR,NDI\params\ELPSupport,default,,"0"
HKR,NDI\params\ELPSupport\enum,"1",,"Enabled"
HKR,NDI\params\ELPSupport\enum,"0",,"Disabled"
HKR, Ndi\Params\LeapUserName, ParamDesc, ,"LeapUserName"
HKR, Ndi\Params\LeapUserName, Type, ,"edit"
HKR, Ndi\Params\LeapUserName, LimitText, ,"32"
HKR, Ndi\Params\LeapUserName, Default,,"tiwlan"
HKR, Ndi\Params\LeapUserName, UpperCase,,"0"
HKR,NDI\params\LeapEnabled,ParamDesc,,"LeapEnabled"
HKR,NDI\params\LeapEnabled,type,,"enum"
HKR,NDI\params\LeapEnabled,default,,"0"
HKR,NDI\params\LeapEnabled\enum,"1",,"Enabled"
HKR,NDI\params\LeapEnabled\enum,"0",,"Disabled"
HKR,NDI\params\Mode4x,ParamDesc,,"Mode4x"
HKR,NDI\params\Mode4x,type,,"enum"
HKR,NDI\params\Mode4x,default,,"1"
HKR,NDI\params\Mode4x\enum,"0",,"Off"
HKR,NDI\params\Mode4x\enum,"1",,"On"
HKR,NDI\params\Mode4xMixed,ParamDesc,,"Mode4xMixed"
HKR,NDI\params\Mode4xMixed,type,,"enum"
HKR,NDI\params\Mode4xMixed,default,,"0"
HKR,NDI\params\Mode4xMixed\enum,"0",,"Off"
HKR,NDI\params\Mode4xMixed\enum,"1",,"On"
HKR,NDI\params\ackE4x,ParamDesc,,"4X Ack emulation"
HKR,NDI\params\ackE4x,type,,"enum"
HKR,NDI\params\ackE4x,default,,"1"
HKR,NDI\params\ackE4x\enum,"0",,"Off"
HKR,NDI\params\ackE4x\enum,"1",,"On"
HKR,NDI\params\dot11TxAntenna,ParamDesc,,"Antenna TX"
HKR,NDI\params\dot11TxAntenna,type,,"enum"
HKR,NDI\params\dot11TxAntenna,default,,"0"
HKR,NDI\params\dot11TxAntenna\enum,"0",,"Antenna 1"
HKR,NDI\params\dot11TxAntenna\enum,"1",,"Antenna 2"
HKR,NDI\params\dot11RxAntenna,ParamDesc,,"Antenna RX"
HKR,NDI\params\dot11RxAntenna,type,,"enum"
HKR,NDI\params\dot11RxAntenna,default,,"2"
HKR,NDI\params\dot11RxAntenna\enum,"0",,"Antenna 1"
HKR,NDI\params\dot11RxAntenna\enum,"1",,"Antenna 2"
HKR,NDI\params\dot11RxAntenna\enum,"2",,"Both"
HKR, Ndi\Params\dot11DesiredChannel, ParamDesc, ,"Desired Channel"
HKR, Ndi\Params\dot11DesiredChannel, Type, , "int"
HKR, Ndi\Params\dot11DesiredChannel, Default, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Min, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Max, , "11"
HKR, Ndi\Params\dot11DesiredChannel, Step, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Base, , "10"
[DestinationDirs]
DefaultDestDir=12 ; System Directory
SMC.8400.CopyFiles=11
SMC.8400.BinFiles.NT=10,system
[SourceDisksNames]
1=%DiskName%,,
[SourceDisksFiles]
SMCWLAN.sys=1
[Strings]
TI="SMC"
SMC.DeviceDesc1="SMC2435W 22 Mbps Wireless Cardbus Adapter"
SMC.DeviceDesc2="SMC2402W 22 Mbps Wireless PCI Adapter"
SMCLN.Service.DispName="SMC EZ Connect Turbo WLAN Adapter"
WLANAdapterHelpText= "A WLAN Adapter provides high speed connection to the Internet through 802.11b technology"
DiskName="SMC EZ Connect Turbo WLAN Installation Disk"
