
[Version]
CatalogFile=usrwlan.cat
Signature="$Windows NT$"
Provider=%TI%
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=02/25/2003,3.0.0.0
[Manufacturer]
%TI%=USR
[ControlFlags]
ExcludeFromSelect=PCI\VEN_104C&DEV_8400&SUBSYS_16EC00FC
ExcludeFromSelect=PCI\VEN_104C&DEV_8400&SUBSYS_16EC00FD
[USR]
%USR.DeviceDesc1%=USR.8400, PCI\VEN_104C&DEV_8400&SUBSYS_16EC00FC
%USR.DeviceDesc2%=USR.8400, PCI\VEN_104C&DEV_8400&SUBSYS_16EC00FD
[TI3000P.ndi]
AddReg=USR.ndi.reg
[USR.8400.NT]
BusType=5
AddReg =USR.ndi.reg.NT, TI.Param.Reg
Characteristics=0x84
;CpyFiles =USR.8400.CopyFiles.NT, USR.8400.BinFiles.NT
[USR.ndi.reg.NT]
HKR, Ndi, Service, 0, "USRLN"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[USR.8400.NT.Services]
AddService=USRLN, 2, USRLN.Service, USRLN.EventLog
[USRLN.Service]
DisplayName=%USRLN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\usrwlan.sys
LoadOrderGroup=NDIS
[USRLN.EventLog]
AddReg=USRLN.AddEventLog.reg
[USRLN.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[USR.8400.CopyFiles.NT]
[USR.8400.BinFiles.NT]
[USR.8400]
AddReg=USR.ndi.reg, TI.Param.Reg, USR.8400.Install
[USR.8400.Install]
HKR,Ndi\Install,,,"USR.8400.Copy"
HKR,Ndi\Remove,,,"USR.8400.Remove"
[USR.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_8400"
HKR,Ndi,HelpText,0,%WLANAdapterHelpText%
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,USRWLAN.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, , "USRLN"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"
HKR,Ndi,InstallInf,,"USRWLAN.INF"
[USR.8400.Copy]
;CpyFiles=USR.8400.CopyFiles
[USR.8400.Remove]
;DlFiles=USR.8400.CopyFiles
[USR.8400.CopyFiles]
[TI.Param.Reg]
HKR, ,Radio11_RxLevel,, "bc b3 a9 9a 90 89 80 79 70 68 64 61 60 55 00"
HKR, ,Radio11_LNA,, "01 01 01 01 01 01 01 01 01 01 01 01 01 01 01"
HKR, ,Radio11_RSSI,, "0a 0f 14 19 1e 23 28 2d 32 37 3c 41 46 4b c8"
HKR, ,Radio0D_RxLevel,, "55 4f 4a 43 3a 32 5d 56 4e 46 3e 37 2a 23 1f"
HKR, ,Radio0D_LNA,, "00 00 00 00 00 00 01 01 01 01 01 01 01 01 01"
HKR, ,Radio0D_RSSI,, "0a 0f 14 19 1e 23 28 2d 32 37 3c 41 46 4b 5a"
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x10001, 25200
HKR,,PermAddress,,112233
HKR, ,HardwareID, ,"ACX100"
HKR, ,NumACXRxDescriptors, ,10
HKR, ,NumACXTxDescriptors, ,10
HKR, ,LeapUserPassword, ,""
HKR, ,DriverDescription, ,"USR 22M WLAN Adapter"
HKR,NDI\params\dot11DesiredBSSType,ParamDesc,,"Desired BSS Type"
HKR,NDI\params\dot11DesiredBSSType,type,,"enum"
HKR,NDI\params\dot11DesiredBSSType,default,,"1"
HKR,NDI\params\dot11DesiredBSSType\enum,"0",,"Ad-Hoc"
HKR,NDI\params\dot11DesiredBSSType\enum,"1",,"Infrastructure"
HKR, Ndi\Params\dot11DesiredSSID, ParamDesc, ,"Desired SSID"
HKR, Ndi\Params\dot11DesiredSSID, Type, ,"edit"
HKR, Ndi\Params\dot11DesiredSSID, LimitText, ,"32"
HKR, Ndi\Params\dot11DesiredSSID, Default,,"ANY"
HKR, Ndi\Params\dot11DesiredSSID, UpperCase,,"0"
HKR,NDI\params\dot11PowerMode,ParamDesc,,"Power Mode"
HKR,NDI\params\dot11PowerMode,type,,"enum"
HKR,NDI\params\dot11PowerMode,default,,"0"
HKR,NDI\params\dot11PowerMode\enum,"0",,"Continuous Access Mode"
HKR,NDI\params\dot11PowerMode\enum,"1",,"Maximum Power Save"
HKR,NDI\params\dot11PowerMode\enum,"2",,"Fast Power Save"
HKR,NDI\params\dot11DesiredTxRate,ParamDesc,, "Desired Tx Rate"
HKR,NDI\params\dot11DesiredTxRate,type,,"enum"
HKR,NDI\params\dot11DesiredTxRate,default,,"0"
HKR,NDI\params\dot11DesiredTxRate\enum,"0",,"Auto"
HKR,NDI\params\dot11DesiredTxRate\enum,"1",,"1 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"2",,"2 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"3",,"5.5 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"4",,"5.5 Mbps PBCC"
HKR,NDI\params\dot11DesiredTxRate\enum,"5",,"11 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"6",,"11 Mbps PBCC"
HKR,NDI\params\dot11DesiredTxRate\enum,"7",,"22 Mbps PBCC"
HKR,NDI\params\dot11SupportedRateMask,ParamDesc,, "Desired Supported Rate Set"
HKR,NDI\params\dot11SupportedRateMask,type,,"enum"
HKR,NDI\params\dot11SupportedRateMask,default,,"2"
HKR,NDI\params\dot11SupportedRateMask\enum,"0",,"1,2 Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"1",,"1,2,5.5,11 Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"2",,"1,2,5.5,11,22 Mbps"
HKR,NDI\params\dot11BasicRateMask,ParamDesc,, "Desired Basic Rate Set"
HKR,NDI\params\dot11BasicRateMask,type,,"enum"
HKR,NDI\params\dot11BasicRateMask,default,,"0"
HKR,NDI\params\dot11BasicRateMask\enum,"0",,"1,2,5.5,11 Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"1",,"1,2 Mbps"
HKR, Ndi\Params\dot11FragmentationThreshold, ParamDesc, ,"Fragmentation Threshold"
HKR, Ndi\Params\dot11FragmentationThreshold, Type, , "int"
HKR, Ndi\Params\dot11FragmentationThreshold, Default, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Min, , "256"
HKR, Ndi\Params\dot11FragmentationThreshold, Max, , "6000"
HKR, Ndi\Params\dot11FragmentationThreshold, Step, , "1"
HKR, Ndi\Params\dot11FragmentationThreshold, Base, , "10"
HKR, Ndi\Params\dot11RTSThreshold, ParamDesc, ,"RTS Threshold"
HKR, Ndi\Params\dot11RTSThreshold, Type, , "int"
HKR, Ndi\Params\dot11RTSThreshold, Default, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Min, , "0"
HKR, Ndi\Params\dot11RTSThreshold, Max, , "6000"
HKR, Ndi\Params\dot11RTSThreshold, Step, , "1"
HKR, Ndi\Params\dot11RTSThreshold, Base, , "10"
HKR,NDI\params\dot11WEPStatus,ParamDesc,,"WEP Option"
HKR,NDI\params\dot11WEPStatus,type,,"enum"
HKR,NDI\params\dot11WEPStatus,default,,"1"
HKR,NDI\params\dot11WEPStatus\enum,"0",,"WEP Enabled"
HKR,NDI\params\dot11WEPStatus\enum,"1",,"WEP Disabled"
HKR,NDI\params\dot11AuthMode,ParamDesc,,"Authentication Mode"
HKR,NDI\params\dot11AuthMode,type,,"enum"
HKR,NDI\params\dot11AuthMode,default,,"2"
HKR,NDI\params\dot11AuthMode\enum,"0",,"Open Authentication"
HKR,NDI\params\dot11AuthMode\enum,"1",,"Shared Authentication"
HKR,NDI\params\dot11AuthMode\enum,"2",,"Auto Switch"
HKR,NDI\params\dot11ShortPreambleInvoked,ParamDesc,,"Short Preamble"
HKR,NDI\params\dot11ShortPreambleInvoked,type,,"enum"
HKR,NDI\params\dot11ShortPreambleInvoked,default,,"0"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"0",,"Off"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"1",,"On"
HKR,NDI\params\Mode4x,ParamDesc,,"Mode4x"
HKR,NDI\params\Mode4x,type,,"enum"
HKR,NDI\params\Mode4x,default,,"1"
HKR,NDI\params\Mode4x\enum,"0",,"Off"
HKR,NDI\params\Mode4x\enum,"1",,"On"
HKR,NDI\params\ackE4x,ParamDesc,,"4X Ack emulation"
HKR,NDI\params\ackE4x,type,,"enum"
HKR,NDI\params\ackE4x,default,,"1"
HKR,NDI\params\ackE4x\enum,"0",,"Off"
HKR,NDI\params\ackE4x\enum,"1",,"On"
HKR,NDI\params\dot11TxAntenna,ParamDesc,,"Antenna TX"
HKR,NDI\params\dot11TxAntenna,type,,"enum"
HKR,NDI\params\dot11TxAntenna,default,,"1"
HKR,NDI\params\dot11TxAntenna\enum,"0",,"Antenna 1"
HKR,NDI\params\dot11TxAntenna\enum,"1",,"Antenna 2"
HKR,NDI\params\dot11RxAntenna,ParamDesc,,"Antenna RX"
HKR,NDI\params\dot11RxAntenna,type,,"enum"
HKR,NDI\params\dot11RxAntenna,default,,"2"
HKR,NDI\params\dot11RxAntenna\enum,"0",,"Antenna 1"
HKR,NDI\params\dot11RxAntenna\enum,"1",,"Antenna 2"
HKR,NDI\params\dot11RxAntenna\enum,"2",,"Both"
HKR, Ndi\Params\dot11DesiredChannel, ParamDesc, ,"Desired Channel"
HKR, Ndi\Params\dot11DesiredChannel, Type, , "int"
HKR, Ndi\Params\dot11DesiredChannel, Default, , "11"
HKR, Ndi\Params\dot11DesiredChannel, Min, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Max, , "11"
HKR, Ndi\Params\dot11DesiredChannel, Step, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Base, , "10"
[DestinationDirs]
DefaultDestDir=12 ; System Directory
USR.8400.CopyFiles=11
USR.8400.BinFiles.NT=10,system
[SourceDisksNames]
1=%DiskName%,,
[SourceDisksFiles]
USRWLAN.sys=1
[Strings]
TI="U.S.Robotics"
USR.DeviceDesc1="U.S. Robotics 22Mbps Wireless Cardbus Adapter"
USR.DeviceDesc2="U.S. Robotics 22Mbps Wireless PCI Adapter"
USRLN.Service.DispName="U.S. Robotics 22Mbps Wireless Lan Adapter"
WLANAdapterHelpText="A U.S. Robotics 22Mbps Wireless Lan Adapter provides high speed connection to the Internet through 802.11b technology"
DiskName="U.S. Robotics 22Mbps Wireless Lan Adapter Installation Disk"
