
[Version]
Signature="$Chicago$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%D-Link%
Compatible=1
DriverVer=04/15/2009, 1.04.03.0000
CatalogFile=Drt2870.cat ;for WHQL certified
[ControlFlags]
[Manufacturer]
%D-Link%=D-Link
[D-Link]
%D-Link_3C09.DeviceDesc%=RTWLANSB.ndi, USB\VID_07D1&PID_3C09
%D-Link_3C11.DeviceDesc%=RTWLANH.ndi, USB\VID_07D1&PID_3C11
%D-Link_3C13.DeviceDesc%=RTWLANSB.ndi, USB\VID_07D1&PID_3C13
%D-Link_3C0A.DeviceDesc%=RTWLANSB.ndi, USB\VID_07D1&PID_3C0A
%D-Link_3C0B.DeviceDesc%=RTWLANSB.ndi, USB\VID_07D1&PID_3C0B
%D-Link_3C0D.DeviceDesc%=RTWLANSB.ndi, USB\VID_07D1&PID_3C0D
%D-Link_3C0E.DeviceDesc%=RTWLANSB.ndi, USB\VID_07D1&PID_3C0E
[RTWLANSB.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RTWLAN.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RTWLANR.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, RemoveFlag.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RTWLAND.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RTWLANRG.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg, RemoveFlag.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RTWLANH.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, IEEE80211H.reg ,CoInstOpt_DLink.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RTWLANHC.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, IEEE80211H.reg, CarrierDetect.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RTWLANS.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, SmartScan.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RTWLANSB.ndi.NT.Services]
AddService=rt2870, 2, Generic.Service, common.EventLog
[RTWLAN.ndi.NT.Services]
AddService=rt2870, 2, Generic.Service, common.EventLog
[RTWLANR.ndi.NT.Services]
AddService=rt2870, 2, Generic.Service, common.EventLog
[RTWLAND.ndi.NT.Services]
AddService=rt2870, 2, Generic.Service, common.EventLog
[RTWLANRG.ndi.NT.Services]
AddService=rt2870, 2, Generic.Service, common.EventLog
[RTWLANH.ndi.NT.Services]
AddService=rt2870, 2, Generic.Service, common.EventLog
[RTWLANHC.ndi.NT.Services]
AddService=rt2870, 2, Generic.Service, common.EventLog
[RTWLANS.ndi.NT.Services]
AddService=rt2870, 2, Generic.Service, common.EventLog
[RTWLANSB.ndi.NT.CoInstallers]
;CpyFiles=CoInstaller.CopyFiles
AddReg=CoInstaller_AddReg
[RTWLAN.ndi.NT.CoInstallers]
;CpyFiles=CoInstaller.CopyFiles
AddReg=CoInstaller_AddReg
[RTWLANR.ndi.NT.CoInstallers]
;CpyFiles=CoInstaller.CopyFiles
AddReg=CoInstaller_AddReg
[RTWLAND.ndi.NT.CoInstallers]
;CpyFiles=CoInstaller.CopyFiles
AddReg=CoInstaller_AddReg
[RTWLANRG.ndi.NT.CoInstallers]
;CpyFiles=CoInstaller.CopyFiles
AddReg=CoInstaller_AddReg
[RTWLANH.ndi.NT.CoInstallers]
;CpyFiles=CoInstaller.CopyFiles
AddReg=CoInstaller_AddReg
[RTWLANHC.ndi.NT.CoInstallers]
;CpyFiles=CoInstaller.CopyFiles
AddReg=CoInstaller_AddReg
[RTWLANS.ndi.NT.CoInstallers]
;CpyFiles=CoInstaller.CopyFiles
AddReg=CoInstaller_AddReg
[Common.reg]
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
HKR, , Radio, 0, "0"
HKR, NDI\params\Radio, ParamDesc, 0, %RadioOnOff%
HKR, NDI\params\Radio, type, 0, "enum"
HKR, NDI\params\Radio, default, 0, "0"
HKR, NDI\params\Radio\enum, 1, 0, %Disable%
HKR, NDI\params\Radio\enum, 0, 0, %Enable%
HKR, , AutoReconnect, 0, "1"
HKR, , ShowHiddenSSID, 0, "0" ; 0=disable(default), 1=enable
HKR, , OpMode, 0, "0"
HKR, , WirelessMode, 0, "5"
HKR, , TGnWifiTest, 0, "0"
HKR, , ShortSlot, 0, "1"
HKR, , TurboRate, 0, "0"
HKR, , AdhocOfdm, 0, "1"
HKR, , Adhoc5GDisable, 0, "0"
HKR, , TXBurst, 0, "1"
HKR, , BGProtection, 0, "0"
HKR, , FrameAggregation,0, "1"
HKR, , IEEE80211H, 0, "0"
HKR, NDI\params\IEEE80211H, ParamDesc, 0, %IEEE802_11h%
HKR, NDI\params\IEEE80211H, type, 0, "enum"
HKR, NDI\params\IEEE80211H, default, 0, "0"
HKR, NDI\params\IEEE80211H\enum, 0, 0, %Disable%
HKR, NDI\params\IEEE80211H\enum, 1, 0, %Enable%
HKR, , CarrierDetect, 0, "0"
HKR, , AutoChannelSelect, 0, "0"
HKR, , WMMCapable, 0, "1"
HKR, , APSDCapable, 0, "0"
HKR, , APSDAC_BE, 0, "0"
HKR, , APSDAC_BK, 0, "0"
HKR, , APSDAC_VI, 0, "0"
HKR, , APSDAC_VO, 0, "0"
HKR, , MaxSPLength, 0, "0"
HKR, Default, MaxSPLength, 0, "0"
HKR, , DLSCapable, 0, "0"
HKR, , RDG, 0, "1"
HKR, , PSControl, 0x00010001, 0x00000000
HKR, , ProhibitTKIPonHT, 0, "1"
HKR, , SmartScan, 0, "0"
HKR, NDI\params\SmartScan, ParamDesc, 0, %SmartScan%
HKR, NDI\params\SmartScan, type, 0, "enum"
HKR, NDI\params\SmartScan, default, 0, "0"
HKR, NDI\params\SmartScan\enum, 0, 0, %Disable%
HKR, NDI\params\SmartScan\enum, 1, 0, %Enable%
HKR, , AllowBW40InBGBand, 0, "1"
HKR, , PSPXlink, 0, "0"
HKR, NDI\params\PSPXlink, ParamDesc, 0, %PSPXlink%
HKR, NDI\params\PSPXlink, type, 0, "enum"
HKR, NDI\params\PSPXlink, default, 0, "0"
HKR, NDI\params\PSPXlink\enum, 0, 0, %Disable%
HKR, NDI\params\PSPXlink\enum, 1, 0, %Enable%
HKR, , CCX2Control, 0x00010001, 0x00fa4600
HKR, , BACapability, 0x10001, "0x0b034020"
HKR, Default, BACapability, 0x10001, "0x0b034020"
HKR, , TransmitSetting, 0x10001, "0x2ba15"
HKR, Default, TransmitSetting, 0x10001, "0x2ba15"
HKR, , VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, Default, VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, , WPSDevName, 0, %WPS_DEVNAME_DEF_STR%
HKR, Default, WPSDevName, 0, %WPS_DEVNAME_DEF_STR%
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, Default, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, , NetworkAddress, 0, ""
HKR, Default, NetworkAddress, 0, ""
HKR, NDI\params\NetworkAddress, ParamDesc, 0, %LocalNetworkAddress%
HKR, NDI\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, limitText, 0, "12"
HKR, NDI\params\NetworkAddress, default, 0, ""
HKR, NDI\params\Networkaddress, optional, 0, "1"
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, %PSMode%
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, %CAM%
HKR, NDI\params\PSMode\enum, 1, 0, %MAXPSP%
HKR, , ACPowerCam, 0, "0"
HKR, Default, ACPowerCam, 0, "0"
HKR, , PreambleType, 0, "0"
HKR, Default, PreambleType, 0, "0"
HKR, , RTSThresh, 0, "2347"
HKR, Default, RTSThresh, 0, "2347"
HKR, , FragThresh, 0, "2346"
HKR, Default, FragThresh, 0, "2346"
HKR, , AuthenType, 0, "0" ; Open System
HKR, Default, AuthenType, 0, "0"
HKR, , Encryption, 0, "1" ; Disable
HKR, Default, Encryption, 0, "1"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
HKR, , BssidRepositTime, 0, "120"
[RemoveFlag.reg]
HKR, , SafelyRemoveOff, 0, "1"
[IEEE80211H.reg]
HKR, , IEEE80211H, 0, "1"
[CarrierDetect.reg]
HKR, , CarrierDetect, 0, "1"
[SmartScan.reg]
HKR, , SmartScan, 0, "1"
[AdhocN.reg]
HKR, , AdhocNMode, 0, "0"
HKR, NDI\params\AdhocNMode, ParamDesc, 0, %AdhocNMode%
HKR, NDI\params\AdhocNMode, type, 0, "enum"
HKR, NDI\params\AdhocNMode, default, 0, "0"
HKR, NDI\params\AdhocNMode\enum, 0, 0, %Disable%
HKR, NDI\params\AdhocNMode\enum, 1, 0, %Enable%
[InitChn14Disabled.reg]
HKR, , InitChn14Disabled, 0,"1"
[SingleBand.reg]
HKR, , CountryRegion, 0, "0"
HKR, NDI\params\CountryRegion, ParamDesc, 0, %CountryRegion24G%
HKR, NDI\params\CountryRegion, type, 0, "enum"
HKR, NDI\params\CountryRegion, default, 0, "0"
HKR, NDI\params\CountryRegion\enum, 0, 0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum, 1, 0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum, 2, 0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum, 3, 0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum, 4, 0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum, 5, 0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum, 6, 0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum, 7, 0, %CountryRegion24G_7%
[DefaultBand.reg]
HKR, , CountryRegion, 0, "0"
HKR, NDI\params\CountryRegion, ParamDesc, 0, %CountryRegion24G%
HKR, NDI\params\CountryRegion, type, 0, "enum"
HKR, NDI\params\CountryRegion, default, 0, "0"
HKR, NDI\params\CountryRegion\enum, 0, 0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum, 1, 0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum, 2, 0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum, 3, 0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum, 4, 0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum, 5, 0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum, 6, 0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum, 7, 0, %CountryRegion24G_7%
HKR, , CountryRegionABand, 0, "0"
HKR, NDI\params\CountryRegionABand, ParamDesc, 0, %CountryRegion5G%
HKR, NDI\params\CountryRegionABand, type, 0, "enum"
HKR, NDI\params\CountryRegionABand, default, 0, "0"
HKR, NDI\params\CountryRegionABand\enum,0, 0, %CountryRegion5G_0%
HKR, NDI\params\CountryRegionABand\enum,1, 0, %CountryRegion5G_1%
HKR, NDI\params\CountryRegionABand\enum,2, 0, %CountryRegion5G_2%
HKR, NDI\params\CountryRegionABand\enum,3, 0, %CountryRegion5G_3%
HKR, NDI\params\CountryRegionABand\enum,4, 0, %CountryRegion5G_4%
HKR, NDI\params\CountryRegionABand\enum,5, 0, %CountryRegion5G_5%
HKR, NDI\params\CountryRegionABand\enum,6, 0, %CountryRegion5G_6%
HKR, NDI\params\CountryRegionABand\enum,7, 0, %CountryRegion5G_7%
HKR, NDI\params\CountryRegionABand\enum,8, 0, %CountryRegion5G_8%
HKR, NDI\params\CountryRegionABand\enum,9, 0, %CountryRegion5G_9%
HKR, NDI\params\CountryRegionABand\enum,10, 0, %CountryRegion5G_10%
HKR, NDI\params\CountryRegionABand\enum,11, 0, %CountryRegion5G_11%
HKR, NDI\params\CountryRegionABand\enum,12, 0, %CountryRegion5G_12%
HKR, NDI\params\CountryRegionABand\enum,13, 0, %CountryRegion5G_13%
HKR, NDI\params\CountryRegionABand\enum,14, 0, %CountryRegion5G_14%
HKR, NDI\params\CountryRegionABand\enum,15, 0, %CountryRegion5G_15%
HKR, NDI\params\CountryRegionABand\enum,16, 0, %CountryRegion5G_16%
[CoInstOpt_DLink.reg]
HKR, , RaCoInstOpt, 0,"00001111"
HKR, , WirelessMode, 0, "5"
HKR, , CountryWirelessMode, 0x10001, "0x11101110"
[CoInstOpt_Az.reg]
HKR, , RaCoInstOpt, 0,"00001111"
HKR, , WirelessMode, 0, "3"
[CoInstaller_AddReg]
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
CoInstaller.CopyFiles=11
[NT.CopyFiles]
rt2870.sys ; NT Installation
[CoInstaller.CopyFiles]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
rt2870.sys=1
[RTUSB.ndi.NT.reg]
HKR, Ndi, Service, 0, "rt2870"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[Generic.Service]
DisplayName=%Generic.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2870.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2870.sys"
HKR, , TypesSupported, 0x00010001, 7
[strings]
D-Link="D-Link Corporation"
D-Link_3C09.DeviceDesc="D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc="D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc="D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc="D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc="D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc="D-Link DWA-125 Wireless 150 USB Adapter"
D-Link_3C0E.DeviceDesc="D-Link WUA-2340 USB Adapter(rev.B)"
INSTALL_DISK_STR="D-Link Wireless 11n USB Installation Disk"
Generic.Service.DispName="D-Link 802.11n USB Wireless LAN Card Driver"
VENDOR_DESC_DEF_STR="IEEE 802.11 Wireless Card."
NETWORK_TYPE_DEF_STR="1"
CHANNEL="1"
WPS_DEVNAME_DEF_STR="D-Link Client"
RadioOnOff="Radio On/Off"
Disable="Disable"
Enable="Enable"
CountryRegion24G="Country Region (2.4GHz)"
CountryRegion24G_0="#0 (1 - 11)"
CountryRegion24G_1="#1 (1 - 13)"
CountryRegion24G_2="#2 (10 - 11)"
CountryRegion24G_3="#3 (10 - 13)"
CountryRegion24G_4="#4 (14)"
CountryRegion24G_5="#5 (1 - 14)"
CountryRegion24G_6="#6 (3 - 9)"
CountryRegion24G_7="#7 (5 - 13)"
CountryRegion5G="Country Region (5GHz)"
CountryRegion5G_0="#0 (36 - 64,149 - 165)"
CountryRegion5G_1="#1 (36 - 140)"
CountryRegion5G_2="#2 (36 - 64)"
CountryRegion5G_3="#3 (52 - 64,149 - 161)"
CountryRegion5G_4="#4 (149 - 165)"
CountryRegion5G_5="#5 (149 - 161)"
CountryRegion5G_6="#6 (36 - 48)"
CountryRegion5G_7="#7 (36 - 165)"
CountryRegion5G_8="#8 (52 - 64)"
CountryRegion5G_9="#9 (36 - 116,132 - 165)"
CountryRegion5G_10="#10 (36 - 48,149 - 165)"
CountryRegion5G_11="#11 (36 - 120,149 - 161)"
CountryRegion5G_12="#12 (36 - 140)"
CountryRegion5G_13="#13 (52 - 161)"
CountryRegion5G_14="#14 (36 - 116,136 - 165)"
CountryRegion5G_15="#15 (149 - 173)"
CountryRegion5G_16="#16 (36 - 173)"
IEEE802_11h="IEEE802.11h"
SmartScan="Multimedia/Gaming Environment"
PSPXlink="PSP Xlink Mode"
LocalNetworkAddress="Local MAC Network Address"
PSMode="Power Saving Mode"
CAM="CAM"
MAXPSP="Max_PSP"
AdhocNMode="Adhoc support 802.11n"

