
[version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Realtek% ;;
CatalogFile.NT=net8192ce.cat ;; for WHQL certified
DriverVer=12/22/2011,1005.31.1222.2011
[Manufacturer]
%Realtek%=Realtek,NTx86
%Lenovo%=Lenovo,NTx86
%ASUS%=ASUS,NTx86
%EDIMAX%=EDIMAX,NTx86
[ControlFlags]
ExcludeFromSelect=*
[Realtek.NTx86]
%RTL8192ceT.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8191
%RTL8192ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_817810EC
%RTL8192ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_818610EC
%RTL8192ce.DeviceDesc%=INTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_818310EC
%RTL8192ce.DeviceDesc%=INTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_819110EC
%RTL8192ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_11781A3B
%RTL8192ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_818910EC
%RTL8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_762210EC
%RTL8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_14001B9A
%RTL8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_14011B9A
%RTL8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_14021B9A
%RTL8192ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_717810EC
%RTL8192ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_71791025
%RTL8192ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_71801025
%RTL8192ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_917810EC
%RTL8192ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_91791025
%RTL8192ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_91801025
%RTL8192ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_617810EC
%RTL8192ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_61791025
%RTL8192ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_61801025
%RTL8191ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8177
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_817610EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_817510EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818110EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818210EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818410EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818510EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821910EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820710EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820810EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820910EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821010EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_822010EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821110EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821210EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821310EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821410EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_822110EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821510EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821610EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821710EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821810EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_822210EC
%RTL8188ce.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819110EC
%RTL8188ce.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819210EC
%RTL8188ce.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819310EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_11391A3B
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81941028
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819710EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_829710EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_38241462
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81981028
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_8176185F
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820610EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_03151A32
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_7185144F
%HP8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_1629103C
%RTL8188ce.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819910EC
%RTL8188ce.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820310EC
%RTL8188ce.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820410EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_23151A32
%RTL8188ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_761110EC
%RTL8188ce.DeviceDesc%=INTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818A10EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_815010EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_717610EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_717710EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_717810EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_717910EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_718010EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_71811025
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_71821025
%RTL8188ceG.DeviceDesc%=SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_719110EC
%RTL8188ceG.DeviceDesc%=SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_719210EC
%RTL8188ceG.DeviceDesc%=SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_719310EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_1A391A3B
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_824A1462
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_715010EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_917610EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_917510EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_918110EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_918210EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_918410EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_918510EC
%HP8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_169F103C
%HP8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_1786103C
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_16B310CF
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_91861025
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_91871025
%RTL8188ceC.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919110EC
%RTL8188ceC.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919210EC
%RTL8188ceC.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919310EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_20571A3B
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_20781A3B
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_917410EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919410EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919610EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_91971028
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_38741462
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_91981028
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920110EC
%RTL8188ceC.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920210EC
%RTL8188ceC.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920310EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_915010EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_617610EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_617710EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_617810EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_617910EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_618010EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_61811025
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_61821025
%RTL8188ceCG.DeviceDesc%= SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619110EC
%RTL8188ceCG.DeviceDesc%= SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619210EC
%RTL8188ceCG.DeviceDesc%= SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619310EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_2A571A3B
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_874A1462
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619410EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619510EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_615010EC
%RTL8188ce.DeviceDesc%=XAVI8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_24811B9A
%RTL8188ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81861025
%RTL8188ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81871025
%RTL8188ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81301025
%RTL8188ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81311025
%RTL8192ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_81791025
%RTL8192ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_81801025
[Lenovo.NTx86]
%LNV8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819510EC
%LNV8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820010EC
%LNV8188ce.DeviceDesc%=LNVG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_719410EC
%LNV8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919510EC
%LNV8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919910EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920010EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920410EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820110EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820210EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820510EC
[ASUS.NTx86]
%ASUSEdimax8188ce.DeviceDesc%=ASED8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_84B51043
%ASUSEdimax8192ce.DeviceDesc%=ASED8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_84B61043
[EDIMAX.NTx86]
%EDI8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_76227392
[Realtek.NTamd64]
%RTL8192ceT.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8191
%RTL8192ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_817810EC
%RTL8192ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_818610EC
%RTL8192ce.DeviceDesc%=INTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_818310EC
%RTL8192ce.DeviceDesc%=INTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_819110EC
%RTL8192ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_11781A3B
%RTL8192ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_818910EC
%RTL8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_762210EC
%RTL8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_14001B9A
%RTL8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_14011B9A
%RTL8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_14021B9A
%RTL8192ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_717810EC
%RTL8192ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_71791025
%RTL8192ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_71801025
%RTL8192ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_917810EC
%RTL8192ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_91791025
%RTL8192ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_91801025
%RTL8192ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_617810EC
%RTL8192ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_61791025
%RTL8192ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_61801025
%RTL8191ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8177
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_817610EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_817510EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818110EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818210EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818410EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818510EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821910EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820710EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820810EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820910EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821010EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_822010EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821110EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821210EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821310EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821410EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_822110EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821510EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821610EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821710EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_821810EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_822210EC
%RTL8188ce.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819110EC
%RTL8188ce.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819210EC
%RTL8188ce.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819310EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_11391A3B
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81941028
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819710EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_829710EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_38241462
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81981028
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_8176185F
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820610EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_03151A32
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_7185144F
%HP8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_1629103C
%RTL8188ce.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819910EC
%RTL8188ce.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820310EC
%RTL8188ce.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820410EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_23151A32
%RTL8188ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_761110EC
%RTL8188ce.DeviceDesc%=INTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_818A10EC
%RTL8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_815010EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_717610EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_717710EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_717810EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_717910EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_718010EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_71811025
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_71821025
%RTL8188ceG.DeviceDesc%=SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_719110EC
%RTL8188ceG.DeviceDesc%=SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_719210EC
%RTL8188ceG.DeviceDesc%=SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_719310EC
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_1A391A3B
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_824A1462
%RTL8188ceG.DeviceDesc%=RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_715010EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_917610EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_917510EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_918110EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_918210EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_918410EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_918510EC
%HP8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_169F103C
%HP8188ce.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_1786103C
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_16B310CF
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_91861025
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_91871025
%RTL8188ceC.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919110EC
%RTL8188ceC.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919210EC
%RTL8188ceC.DeviceDesc%=SS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919310EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_20571A3B
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_20781A3B
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_917410EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919410EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919610EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_91971028
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_38741462
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_91981028
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920110EC
%RTL8188ceC.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920210EC
%RTL8188ceC.DeviceDesc%=ASUS8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920310EC
%RTL8188ceC.DeviceDesc%=RTL8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_915010EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_617610EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_617710EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_617810EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_617910EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_618010EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_61811025
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_61821025
%RTL8188ceCG.DeviceDesc%= SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619110EC
%RTL8188ceCG.DeviceDesc%= SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619210EC
%RTL8188ceCG.DeviceDesc%= SSG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619310EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_2A571A3B
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_874A1462
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619410EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_619510EC
%RTL8188ceCG.DeviceDesc%= RTLG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_615010EC
%RTL8188ce.DeviceDesc%=XAVI8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_24811B9A
%RTL8188ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81861025
%RTL8188ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81871025
%RTL8188ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81301025
%RTL8188ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_81311025
%RTL8192ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_81791025
%RTL8192ce.DeviceDesc%=ACER8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_81801025
[Lenovo.NTamd64]
%LNV8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_819510EC
%LNV8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820010EC
%LNV8188ce.DeviceDesc%=LNVG8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_719410EC
%LNV8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919510EC
%LNV8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_919910EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920010EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_920410EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820110EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820210EC
%LNVC8188ce.DeviceDesc%=LNV8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_820510EC
[ASUS.NTamd64]
%ASUSEdimax8188ce.DeviceDesc%=ASED8192Ce.ndi, PCI\VEN_10EC&DEV_8176&SUBSYS_84B51043
%ASUSEdimax8192ce.DeviceDesc%=ASED8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_84B61043
[EDIMAX.NTamd64]
%EDI8192ce.DeviceDesc%=EDI8192Ce.ndi, PCI\VEN_10EC&DEV_8178&SUBSYS_76227392
[RTL8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11nWirelessMode.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[RTL8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[RTLG8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11gWirelessMode.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[RTLG8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[LNV8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11nWirelessMode.reg, ShowRxRate.reg, LPS.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[LNV8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[LNVG8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11gWirelessMode.reg, ShowRxRate.reg, LPS.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[LNVG8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[SS8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11nWirelessMode.reg, RxWorkItem.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[SS8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[SSG8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11gWirelessMode.reg, RxWorkItem.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[SSG8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[ASUS8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11nWirelessMode.reg, 11nAdhoc.reg, 11nTKIP.reg, 11nWEP.reg, ShowMaxRxRate.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[ASUS8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[ASED8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11nWirelessMode.reg, 11nAdhoc.reg, 11nTKIP.reg, 11nWEP.reg, ShowMaxRxRate.reg, HWWPSPBC.reg, Xlink.reg, NO_GPIORFSW.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[ASED8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[EDI8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11nWirelessMode.reg, HWWPSPBC.reg, Xlink.reg, NO_GPIORFSW.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[EDI8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[INTL8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11nWirelessMode.reg, MinFwLPS.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[INTL8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[XAVI8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11nWirelessMode.reg, HWWPSPBC.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[XAVI8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[ACER8192Ce.ndi.NT]
AddReg=RTL8192Ce.reg, 11nWirelessMode.reg, WoWLAN.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8192Ce.CopyFiles
[ACER8192Ce.ndi.NT.Services]
AddService=RTL8192Ce, 2, RTL8192Ce.Service, RTL8192Ce.EventLog
[RTL8192Ce.reg]
HKR, Ndi, Service, 0, "RTL8192Ce"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR,defaults, AH_BcnIntv, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, default, 0, "100"
HKR,Ndi\params\AH_BcnIntv, ParamDesc, 0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, type, 0, "int"
HKR,Ndi\params\AH_BcnIntv, min, 0, "20"
HKR,Ndi\params\AH_BcnIntv, max, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, step, 0, "1"
HKR,Ndi\params\Dot11dEnable, ParamDesc, 0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable, type, 0, "enum"
HKR,Ndi\params\Dot11dEnable, default, 0, "0"
HKR,Ndi\params\Dot11dEnable\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum, "1", 0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, %ROAMING_SENSITIVITY_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel, Type, 0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default, 0, "80"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "127", 0, %DISABLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "65", 0, %HIGH_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "70", 0, %MIDDLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "80", 0, %LOW_STR%
HKR,Ndi\params\PreambleMode, ParamDesc, 0, %PREAMBLE_MODE_STR%
HKR,Ndi\params\PreambleMode, type, 0, "enum"
HKR,Ndi\params\PreambleMode, default, 0, "2"
HKR,Ndi\params\PreambleMode\enum, "1", 0, %LONG_PREAMBLE_STR%
HKR,Ndi\params\PreambleMode\enum, "2", 0, %LONG_SHORT_PREAMBLE_STR%
HKR,defaults,PreambleMode,0,"2"
HKR,,PreambleMode,0,"2"
HKR,Ndi\params\TxPowerLevel, ParamDesc, 0, %TX_POWER_LEVEL_STR%
HKR,Ndi\params\TxPowerLevel, type, 0, "enum"
HKR,Ndi\params\TxPowerLevel, default, 0, "0"
HKR,Ndi\params\TxPowerLevel\enum, "0", 0, %AUTO_STR%
HKR,Ndi\params\TxPowerLevel\enum, "1", 0, %HIGH_TX_POWER_STR%
HKR,Ndi\params\TxPowerLevel\enum, "2", 0, %MIDDLE_TX_POWER_STR%
HKR,Ndi\params\TxPowerLevel\enum, "3", 0, %LOW_TX_POWER_STR%
HKR,Ndi\params\TxPowerLevel\enum, "4", 0, %VERY_LOW_TX_POWER_STR%
HKR,defaults,TxPowerLevel,0,"0"
HKR,,TxPowerLevel,0,"0"
HKR,,Channel,0,"10"
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"
HKR,,LPSIntvl,0,"5"
HKR,,HwSwRfOffD3,0,"0"
HKR,defaults,PciASPM,0,"0"
HKR,,PciASPM,0,"0"
HKR,,LPS2RDisable,0,"1"
HKR,,GPIORFSW,0,"1"
HKR,,KeepAliveLevel,0,"1"
HKR,,bRegDefaultAntenna,0,"1"
HKR,,IODvName,0,"0"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
HKR,,WiFiConfg,,"0"
[Xlink.reg]
HKR,Ndi\params\PSPXlinkMode, ParamDesc, 0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode, type, 0, "enum"
HKR,Ndi\params\PSPXlinkMode, default, 0, "0"
HKR,Ndi\params\PSPXlinkMode\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum, "1", 0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"
[11nAdhoc.reg]
HKR,Ndi\params\11nAdhoc, ParamDesc, 0, %11NADHOC_ENABLE_STR%
HKR,Ndi\params\11nAdhoc, type, 0, "enum"
HKR,Ndi\params\11nAdhoc, default, 0, "0"
HKR,Ndi\params\11nAdhoc\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\11nAdhoc\enum, "1", 0, %ENABLE_STR%
HKR,defaults,11nAdhoc,0,"0"
HKR,,11nAdhoc,0,"0"
[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, type, 0, "enum"
HKR,Ndi\params\WirelessMode, default, 0, "8"
HKR,Ndi\params\WirelessMode\enum, "2", 0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, "4", 0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"
[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, type, 0, "enum"
HKR,Ndi\params\WirelessMode, default, 0, "8"
HKR,Ndi\params\WirelessMode\enum, "2", 0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, "4", 0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, "8", 0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"
[LPS.reg]
HKR,Ndi\params\bLeisurePs, ParamDesc, 0, %LEISURE_POWER_SAVE_STR%
HKR,Ndi\params\bLeisurePs, type, 0, "enum"
HKR,Ndi\params\bLeisurePs, default, 0, "2"
HKR,Ndi\params\bLeisurePs\enum, "2", 0, %LEISURE_POWER_SAVE_AUTO%
HKR,Ndi\params\bLeisurePs\enum, "0", 0, %LEISURE_POWER_SAVE_DISABLE%
HKR,Ndi\params\bLeisurePs\enum, "1", 0, %LEISURE_POWER_SAVE_ENABLE%
[ShowRxRate.reg]
HKR,,ShowRate,0,"2"
[RxWorkItem.reg]
HKR,,UseRxInterruptWorkItem,0,"1"
[ShowMaxRxRate.reg]
HKR,,ShowRate,0,"3"
[11nTKIP.reg]
HKR,,TKIPinNmode,0,"1"
[11nWEP.reg]
HKR,,WEPinNmode,0,"1"
[HWWPSPBC.reg]
HKR,,GPIOHWPBC,0,"1"
[NO_GPIORFSW.reg]
HKR,,GPIORFSW,0,"0"
[MinFwLPS.reg]
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"
[WoWLAN.reg]
HKR,defaults,WoWLANMode,0,"1"
HKR,,WoWLANMode,0,"1"
[RTL8192Ce.Service]
DisplayName=%Realtek.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rtl8192Ce.sys
LoadOrderGroup=NDIS
[RTL8192Ce.EventLog]
AddReg=RTL8192Ce.AddEventLog.reg
[RTL8192Ce.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[RTL8192Ce.CopyFiles]
rtl8192Ce.sys,,,2
[DestinationDirs]
RTL8192Ce.CopyFiles=12
DefaultDestDir=11 ; LDID_SYS
[SourceDisksNames]
1=%DISKNAME%,,,
[SourceDisksFiles]
rtl8192Ce.sys=1
[Strings]
Realtek="Realtek Semiconductor Corp."
Lenovo="Lenovo Corp."
ASUS="ASUSTeK Computer Inc."
EDIMAX="Edimax Technology Co., Ltd"
SSID_STR="SSID"
CHANNEL_STR="Channel"
NETWORK_TYPE_STR="Network Type"
LED_CONTROL_STR="LED Control"
POWER_SAVE_STR="Power Save Mode"
WIFI_IBSS_STR="IBSS Default 11b Mode"
RATE_ADAPTIVE_STR="Rate Adaptive"
QOS_STR="QoS"
WMM_APSD="WMM APSD"
CCX_RM_STR="CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR="CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR="Forced Priority"
HW_PARA_STR="Init from HwParaFile"
THREE_WIRE_MODE_STR="Three Wire Programming Mode"
BOARD_TYPE_STR="Board Type"
PROTECTION_MODE_STR="Protection Mode"
TPC_STR="Transmit Power Control"
TPC_POLARITY_STR="TPC Polarity Select"
HIGH_POWER_STR="High Power Mechanism"
INIT_GAIN_STR="Initial Gain State"
CW_MAX_MIN_STR="Contention Window"
PSP_XLINK_STR="PSP XLink Mode"
CHANNEL_PLAN_STR="Channel Plan"
WL_MODE_STR="Wireless Mode"
PREAMBLE_MODE_STR="Preamble Mode"
FRAGTHRESH_STR="Fragmentation Threshold"
RTSTHRESH_STR="RTS Threshold"
DOT11_ENABLE_STR="802.11d"
11NADHOC_ENABLE_STR="11n AdHoc"
DISABLE_STR="Disable"
ENABLE_STR="Enable"
CAM_STR="CAM"
MAX_PSP_STR="MAX_PSP"
FAST_PSP_STR="Fast_PSP"
AD_HOC_STR="Ad Hoc"
INFRASTRUCTURE_STR="Infrastructure"
AUTO_SELECT_STR="Auto select"
DOMAIN_FROM_EEPROM_STR="DOMAIN_FROM_EEPROM"
AUTO_STR="Auto"
LONG_PREAMBLE_STR="Long only"
LONG_SHORT_PREAMBLE_STR="Short & long"
SHORT_PREAMBLE_STR="Short Preamble"
FCC_STR="FCC"
IC_STR="IC"
ETSI_STR="ETSI"
SPAIN_STR="Spain"
FRANCE_STR="France"
MKK_STR="MKK"
MKK1_STR="MKK1"
ISRAEL_STR="Israel"
TELEC_STR="TELEC"
IEEE_802_11A_STR="IEEE 802.11a"
IEEE_802_11B_STR="IEEE 802.11b"
IEEE_802_11BG_STR="IEEE 802.11b/g"
IEEE_802_11BGN_STR="IEEE 802.11b/g/n"
Roam_Retry_Limit_STR="Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR="Associated Power Save"
LEISURE_POWER_SAVE_AUTO="AUTO"
LEISURE_POWER_SAVE_ENABLE="ENABLE"
LEISURE_POWER_SAVE_DISABLE="DISABLE"
AH_BCNINTV_STR="Beacon Interval"
ROAMING_SENSITIVITY_STR="Roaming Sensitivity Level"
HIGH_STR="High"
MIDDLE_STR="Middle"
LOW_STR="Low"
TX_POWER_LEVEL_STR="TX Power Level"
HIGH_TX_POWER_STR="100 %"
MIDDLE_TX_POWER_STR="75 %"
LOW_TX_POWER_STR="50 %"
VERY_LOW_TX_POWER_STR="20 %"
DISKNAME=" Realtek Wireless LAN PCI-E Driver Disk "
Realtek.Service.DispName ="Realtek Wireless LAN 802.11n PCI-E NIC Driver"
RTL8192CeT.DeviceDesc ="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC(TEST)"
RTL8192Ce.DeviceDesc ="Realtek RTL8192CE Wireless LAN 802.11n PCI-E NIC"
RTL8191Ce.DeviceDesc ="Realtek RTL8191CE Wireless LAN 802.11n PCI-E NIC"
RTL8188Ce.DeviceDesc ="Realtek RTL8188CE Wireless LAN 802.11n PCI-E NIC"
RTL8192CeG.DeviceDesc ="Realtek RTL8192CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8191CeG.DeviceDesc ="Realtek RTL8191CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8188CeG.DeviceDesc ="Realtek RTL8188CE Wireless LAN 802.11b/g PCI-E NIC FOR RUSSIA SKU"
RTL8192CeC.DeviceDesc ="Realtek RTL8192CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8191CeC.DeviceDesc ="Realtek RTL8191CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8188CeC.DeviceDesc ="Realtek RTL8188CE Wireless LAN 802.11n COMBO PCI-E NIC"
RTL8192CeCG.DeviceDesc ="Realtek RTL8192CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8191CeCG.DeviceDesc ="Realtek RTL8191CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
RTL8188CeCG.DeviceDesc ="Realtek RTL8188CE Wireless LAN 802.11b/g COMBO PCI-E NIC FOR RUSSIA SKU"
LNV8188ce.DeviceDesc ="1x1 11b/g/n Wireless LAN PCI Express Half Mini Card Adapter"
LNVC8188ce.DeviceDesc ="1x1 11b/g/n Wireless LAN PCI Express Adapter"
HP8188ce.DeviceDesc ="Realtek RTL8188CE 802.11b/g/n WiFi Adapter"
ASUSEdimax8188ce.DeviceDesc ="ASUS PCE-N10 11n Wireless LAN PCI-E Card"
ASUSEdimax8192ce.DeviceDesc ="ASUS PCE-N15 11n Wireless LAN PCI-E Card"
EDI8192ce.DeviceDesc ="Edimax 802.11n Wireless Adapter"

