
[Version]
DriverVer=05/16/2002, 1.7.37.1098
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
CatalogFile=WMP11NDS.CAT
[Manufacturer]
%V_Provider%=Adapters
[ControlFlags]
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_38741737
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_38711737
[Adapters]
%WMP11.DeviceDesc%=WMP11.ndi, PCI\VEN_1260&DEV_3873&SUBSYS_38741737
%WMP11_1.DeviceDesc%=WMP11_1.ndi, PCI\VEN_1260&DEV_3873&SUBSYS_38711737
[WMP11.ndi]
AddReg=WMP11.ndi.reg, Pci9x.reg, Advanced.reg, Common.reg
;CpyFiles=win9x.CopyFiles
[WMP11_1.ndi]
AddReg=WMP11.ndi.reg, Pci9x_1.reg, Advanced.reg, Common.reg
;CpyFiles=win9x.CopyFiles
[WMP11.ndi.reg]
HKR, , NTMPDriver, 0, "WMP11NDS.sys"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, WMP11NDS.sys
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, 0, "WMP11"
HKR, NDIS, MajorNdisVersion,1, "03"
HKR, NDIS, MinorNdisVersion,1, "0A"
HKR, , BusType, 0, "5"
HKR, NDI, CardType, 0, "PCI"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[win9x.CopyFiles]
WMP11NDS.sys ; Win9x Installation
[Pci9x.reg]
HKR, , IOBaseAddress, 1, "02","00","00","00"
HKR, , InterruptNumber, 1, "04","00","00","00"
HKR, , EnableIRQSharing,1, "01","00","00","00"
HKR, , VendorDesc, 0, "Instant Wireless PCI Card"
HKR, Ndi, DeviceID, 0, "PCI\VEN_1260&DEV_3873&SUBSYS_38741737"
[Pci9x_1.reg]
HKR, , IOBaseAddress, 1, "02","00","00","00"
HKR, , InterruptNumber, 1, "04","00","00","00"
HKR, , EnableIRQSharing,1, "01","00","00","00"
HKR, , VendorDesc, 0, "Instant Wireless PCI Card"
HKR, Ndi, DeviceID, 0, "PCI\VEN_1260&DEV_3873&SUBSYS_38711737"
[WMP11.ndi.NT]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
[WMP11.ndi.NT.Services]
AddService=WMP11, 2, WMP11.Service, common.EventLog
[WMP11.Service]
DisplayName=%WMP11.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\WMP11NDS.sys
LoadOrderGroup=NDIS
[WMP11_1.ndi.NT]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
[WMP11_1.ndi.NT.Services]
AddService=WMP11, 2, WMP11_1.Service, common.EventLog
[WMP11_1.Service]
DisplayName=%WMP11_1.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\WMP11NDS.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\WMP11NDS.sys
HKR, , TypesSupported, 0x00010001, 7
[nt.reg]
HKR, Ndi, Service, 0, "WMP11"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[Common.reg]
HKR, , APDensity, 0, "1"
HKR, defaults, APDensity, 0, "1"
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, defaults, SSID, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, ParamDesc, 0, "SSID"
HKR, NDI\params\SSID, type, 0, "edit"
HKR, NDI\params\SSID, limitText, 0, "32"
HKR, NDI\params\SSID, default, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, flag, 1, "30","00","00","00"
HKR, , StationName, 0, "Client"
HKR, defaults, StationName, 0, "Client"
HKR, , DSChannel, 0, %CHANNEL%
HKR, defaults, DSChannel, 0, %CHANNEL%
HKR, NDI\params\DSChannel, ParamDesc, 0, "Channel"
HKR, NDI\params\DSChannel, type, 0, "enum"
HKR, NDI\params\DSChannel, default, 0, %CHANNEL%
HKR, NDI\params\DSChannel, flag, 1, "30","00","00","00"
HKR, NDI\params\DSChannel\enum, 1, 0, "1"
HKR, NDI\params\DSChannel\enum, 2, 0, "2"
HKR, NDI\params\DSChannel\enum, 3, 0, "3"
HKR, NDI\params\DSChannel\enum, 4, 0, "4"
HKR, NDI\params\DSChannel\enum, 5, 0, "5"
HKR, NDI\params\DSChannel\enum, 6, 0, "6"
HKR, NDI\params\DSChannel\enum, 7, 0, "7"
HKR, NDI\params\DSChannel\enum, 8, 0, "8"
HKR, NDI\params\DSChannel\enum, 9, 0, "9"
HKR, NDI\params\DSChannel\enum, 10, 0, "10"
HKR, NDI\params\DSChannel\enum, 11, 0, "11"
HKR, , Encapsulation, 0, "1"
HKR, defaults, Encapsulation, 0, "1"
HKR, , TxRate, 0, "15"
HKR, defaults, TxRate, 0, "15"
HKR, NDI\params\TxRate, ParamDesc, 0, "Transmit Rate"
HKR, NDI\params\TxRate, type, 0, "enum"
HKR, NDI\params\TxRate, default, 0, "15"
HKR, NDI\params\TxRate, flag, 1, "30","00","00","00"
HKR, NDI\params\TxRate\enum, 1, 0, "Fixed 1 Mb/s"
HKR, NDI\params\TxRate\enum, 2, 0, "Fixed 2 Mb/s"
HKR, NDI\params\TxRate\enum, 3, 0, "Auto Select 1 or 2"
HKR, NDI\params\TxRate\enum, 4, 0, "Fixed 5.5 Mb/s"
HKR, NDI\params\TxRate\enum, 8, 0, "Fixed 11 Mb/s"
HKR, NDI\params\TxRate\enum, 15, 0, "Fully Auto"
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, defaults, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, flag, 1, "30","00","00","00"
HKR, NDI\params\NetworkType\enum, 0, 0, "Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , WepReq, 0, %WEP_REQUIRED_DEF_STR%
HKR, defaults, WepReq, 0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq, ParamDesc, 0, "Encryption"
HKR, NDI\params\WepReq, flag, 1, "30","00","00","00"
HKR, NDI\params\WepReq, type, 0, "enum"
HKR, Ndi\params\WepReq, default, 0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq\enum, 0, 0, "Disabled"
HKR, NDI\params\WepReq\enum, 2, 0, "64 bit"
HKR, NDI\params\WepReq\enum, 6, 0, "128 bit"
HKR, NDI\params\WepReq, optional, 0, "0"
HKR, , EncryptInDriver, 0, "1"
HKR, defaults, EncryptInDriver, 0, "1"
HKR, , DecryptInDriver, 0, "1"
HKR, defaults, DecryptInDriver, 0, "1"
HKR, , WEPFactor, 0, "3"
HKR, defaults, WEPFactor, 0, "3"
HKR, , Esarhpssap, 0, %PASSPHRASE_DEF_STR%
HKR, defaults, Esarhpssap, 0, %PASSPHRASE_DEF_STR%
HKR, NDI\params\Esarhpssap, ParamDesc, 0, "WEP Passphrase"
HKR, NDI\params\Esarhpssap, type, 0, "edit"
HKR, NDI\params\Esarhpssap, limitText, 0, "64"
HKR, NDI\params\Esarhpssap, default, 0, %PASSPHRASE_DEF_STR%
HKR, NDI\params\Esarhpssap, flag, 1, "30","00","00","00"
HKR, , IBSSInDriver, 0, "0"
HKR, defaults, IBSSInDriver, 0, "0"
HKR,, WEP64_KEY_1, 0,"0000000000"
HKR,, WEP64_KEY_2, 0,"0000000000"
HKR,, WEP64_KEY_3, 0,"0000000000"
HKR,, WEP64_KEY_4, 0,"0000000000"
HKR,, WEP128_KEY_1, 0,"00000000000000000000000000"
HKR,, WEP128_KEY_2, 0,"00000000000000000000000000"
HKR,, WEP128_KEY_3, 0,"00000000000000000000000000"
HKR,, WEP128_KEY_4, 0,"00000000000000000000000000"
HKR,, CurProfile, 0,"default"
[Advanced.reg]
HKR, , ListenInterval, 0, "3"
HKR, defaults, ListenInterval, 0, "3"
HKR, NDI\params\ListenInterval, ParamDesc, 0, "Maximum Listen Interval"
HKR, NDI\params\ListenInterval, flag, 1, "30","00","00","00"
HKR, NDI\params\ListenInterval, type, 0, "int"
HKR, Ndi\params\ListenInterval, default, 0, "3"
HKR, NDI\params\ListenInterval, min, 0, "0"
HKR, NDI\params\ListenInterval, max, 0, "77"
HKR, NDI\params\ListenInterval, step, 0, "1"
HKR, NDI\params\ListenInterval, optional, 0, "0"
HKR, , RTSThresh, 0, "2432"
HKR, defaults, RTSThresh, 0, "2432"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2432"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2432"
HKR, NDI\params\RTSThresh, step, 0, "64"
HKR, NDI\params\RTSThresh, flag, 1, "20","00","00","00"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2432"
HKR, defaults, FragThresh, 0, "2432"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragmentation Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2432"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2432"
HKR, NDI\params\FragThresh, step, 0, "128"
HKR, NDI\params\FragThresh, flag, 1, "20","00","00","00"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , PreambleMode, 0, "1"
HKR, defaults, PreambleMode, 0, "1"
HKR, NDI\params\PreambleMode, ParamDesc, 0, %SHORT_PREAM_STR%
HKR, NDI\params\PreambleMode, flag, 1, "30","00","00","00"
HKR, NDI\params\PreambleMode, type, 0, "enum"
HKR, Ndi\params\PreambleMode, default, 0, "1"
HKR, NDI\params\PreambleMode\enum,1, 0, "Long Tx Preamble"
HKR, NDI\params\PreambleMode\enum,2, 0, "Short Tx Preamble"
HKR, NDI\params\PreambleMode, optional, 0, "0"
HKR, , AuthentAlg, 0, %AUTHENT_TYPE_DEF_STR%
HKR, defaults, AuthentAlg, 0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg, ParamDesc, 0, "Authentication Algorithm"
HKR, NDI\params\AuthentAlg, type, 0, "enum"
HKR, NDI\params\AuthentAlg, default, 0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg, flag, 1, "30","00","00","00"
HKR, NDI\params\AuthentAlg\enum, 1, 0, "WECA Compliant (always use Open)"
HKR, NDI\params\AuthentAlg\enum, 2, 0, "Must use Shared with WEP"
HKR, NDI\params\AuthentAlg\enum, 65535, 0, "Automatic based on WEP setting"
HKR, , PSMode, 0, "1"
HKR, defaults, PSMode, 0, "1"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Save Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "1"
HKR, NDI\params\PSMode, flag, 1, "30","00","00","00"
HKR, NDI\params\PSMode\enum, 1, 0, "Disabled"
HKR, NDI\params\PSMode\enum, 2, 0, "Enabled"
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
win9x.CopyFiles=11 ; system32 subdirectory on win9x
[NT.CopyFiles]
WMP11NDS.sys,,,2 ; NT Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
WMP11NDS.sys=1
[strings]
Provider="Linksys"
V_Provider="The Linksys Group, Inc."
WMP11.DeviceDesc="Instant Wireless PCI Card"
WMP11_1.DeviceDesc="Instant Wireless PCI Card"
WMP11.Service.DispName="Instant Wireless PCI Card Driver"
WMP11_1.Service.DispName="Instant Wireless PCI Card Driver"
INSTALL_DISK_STR="Instant Wireless PCI Card Installation Disk"
SSID_DEF_STR="linksys"
NETWORK_TYPE_DEF_STR=1
CHANNEL=6
AUTHENT_TYPE_DEF_STR="65535"
PASSPHRASE_DEF_STR=""
WEP_REQUIRED_DEF_STR="0"
SHORT_PREAM_STR="Preamble Mode"

