
[Version]
DriverVer=11/28/2002, 2.1.0
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=AmPsmNIC.cat
[Strings]
VER_VENDOR_STR="Proxim Corporation"
VER_VENDOR_NAME_STR="Proxim Corporation"
PRISM_SERVICE_DISPLAY_USB="ORiNOCO 802.11b USB Driver"
INSTALL_DISK_STR="ORiNOCO 802.11b USB Driver Disk"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"
LOAD_FIRMWARE_STR="Firmware Download"
PDWELL_STR="Passive Scan Dwell Time"
USB_DESC_STR_GOLD="ORiNOCO 802.11b USB"
USB_DESC_STR_SILVER="ORiNOCO 802.11b USB"
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%USB_DESC_STR_GOLD%=PRISM_USB1, USB\VID_0BB2&PID_0304
%USB_DESC_STR_SILVER%=PRISM_USB2, USB\VID_0BB2&PID_0305
[PRISM_USB1] ; Win9x
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_USB1.NT] ; Win2k
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_USB1.NT.Services]
AddService=PRISM_USB, 2, PRISM_DRIVER_USB.Service, PRISM_DRIVER.EventLog
[PRISM_USB1.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_0BB2&PID_0304"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%USB_DESC_STR_GOLD%
HKR, ,LoadFirmware,0,"0"
[PRISM_USB2] ; Win9x
AddReg=PRISM_USB2.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_USB2.NT] ; Win2k
AddReg=PRISM_USB2.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_USB2.NT.Services]
AddService=PRISM_USB, 2, PRISM_DRIVER_USB.Service, PRISM_DRIVER.EventLog
[PRISM_USB2.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_0BB2&PID_0305"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%USB_DESC_STR_SILVER%
HKR, ,LoadFirmware,0,"0"
[PRISM_DRIVER_USB.Service]
DisplayName=%PRISM_SERVICE_DISPLAY_USB%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\EXPSUSB.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_USB.reg]
HKR,NDI ,Service ,0 ,"PRISM_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"EXPSUSB.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,"1"
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,"enum"
HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,"1"
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,"1"
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,"enum"
HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
HKR,NDI\params\PSMode,optional,0,"1"
[COMMON.reg]
HKR, ,LanExpress ,0 ,"1"
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,3
HKR,Ndi\params\ListenInterval,default,0,"3"
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,"int"
HKR,NDI\params\ListenInterval,flag,1,"30","00","00","00"
HKR,NDI\params\ListenInterval,min,0,"0"
HKR,NDI\params\ListenInterval,max,0,"77"
HKR,NDI\params\ListenInterval,step,0,"1"
HKR,NDI\params\ListenInterval,optional,0,"1"
HKR,defaults,RTSThresh,0,2432
HKR,Ndi\params\RTSThresh,default,0,"2432"
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,"int"
HKR,NDI\params\RTSThresh,flag,1,"20","00","00","00"
HKR,NDI\params\RTSThresh,min,0,"0"
HKR,NDI\params\RTSThresh,max,0,"2432"
HKR,NDI\params\RTSThresh,step,0,"64"
HKR,NDI\params\RTSThresh,optional,0,"1"
HKR,defaults,FragThresh,0,2432
HKR,Ndi\params\FragThresh,default,0,"2432"
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,"int"
HKR,NDI\params\FragThresh,flag,1,"20","00","00","00"
HKR,NDI\params\FragThresh,min,0,"256"
HKR,NDI\params\FragThresh,max,0,"2432"
HKR,NDI\params\FragThresh,step,0,"128"
HKR,NDI\params\FragThresh,optional,0,"1"
HKR,defaults,PreambleMode,0,1
HKR,Ndi\params\PreambleMode,default,0,"1"
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,"enum"
HKR,NDI\params\PreambleMode,flag,1,"30","00","00","00"
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,"1"
HKR,defaults,AuthentAlg,0,65535
HKR,NDI\params\AuthentAlg,default,0,"65535"
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,"enum"
HKR,NDI\params\AuthentAlg,flag,1,"30","00","00","00"
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,"1"
HKR,defaults,LoadFirmware,0,0
HKR,Ndi\params\LoadFirmware,default,0,"0"
HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
HKR,NDI\params\LoadFirmware,type,,"enum"
HKR,NDI\params\LoadFirmware,flag,1,"30","00","00","00"
HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
HKR,NDI\params\LoadFirmware,optional,0,"1"
HKR,defaults,PDwellTime,0,"120"
HKR,Ndi\params\PDwellTime,default,0,"120"
HKR,NDI\params\PDwellTime,ParamDesc,0,%PDWELL_STR%
HKR,NDI\params\PDwellTime,type,0,"int"
HKR,NDI\params\PDwellTime,flag,1,"20","00","00","00"
HKR,NDI\params\PDwellTime,min,0,"0"
HKR,NDI\params\PDwellTime,max,0,"1000"
HKR,NDI\params\PDwellTime,step,0,"10"
HKR,NDI\params\PDwellTime,optional,0,"1"
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_DRIVER.copy]
EXPSUSB.sys
[PRISM_DRIVER.copy.NT]
EXPSUSB.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
EXPSUSB.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
EXPSUSB.sys=1
