
[Version]
Signature="$Chicago$"
CatalogFile=cw51usb.cat
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
DriverVer=06/21/2002,1.5.24.7
[Manufacturer]
%Provider%=Adapters,NT.5.1
[ControlFlags]
ExcludeFromSelect=USB\VID_2474&PID_3642 ; Intersil
ExcludeFromSelect=USB\VID_8086&PID_1110 ; Intel
ExcludeFromSelect=USB\VID_8086&PID_1111 ; Intel Windansea
ExcludeFromSelect=USB\VID_049F&PID_0033 ; Compaq
ExcludeFromSelect=USB\VID_05E0&PID_0800 ; Symbol Windansea
[Adapters.NT.5.1]
%CW10USB_ISIL.DeviceDescUSB%=CW10_USB.ndi, USB\VID_2474&PID_3642
%CW10USB_INTEL.DeviceDescUSB%=CW10_USB.ndi, USB\VID_8086&PID_1110
%CW10USB_INTEL1.DeviceDescUSB%=CW10_USB.ndi, USB\VID_8086&PID_1111
%CW10USB_CPQ.DeviceDescUSB%=CW10_USB1.ndi, USB\VID_049F&PID_0033
%CW10USB_SYMBOL.DeviceDescUSB%=CW10_USB2.ndi, USB\VID_05E0&PID_0800
[Adapters]
[CW10_USB.ndi]
AddReg=USB_ID.reg, Common.reg, win9x.reg, USB.reg
;CpyFiles=win9x.USBCopyFiles
[CW10_USB1.ndi]
AddReg=USB_ID.reg, Common.reg, win9x.reg, USB.reg, CPQ.reg
;CpyFiles=win9x.USBCopyFiles
[CW10_USB2.ndi]
AddReg=USB_ID.reg, Common.reg, win9x.reg, USB.reg, SYM.reg
;CpyFiles=win9x.USBCopyFiles
[CW10_USB.ndi.NT]
AddReg=Common.reg, nt.reg, USB.reg, CW51_USB.CoInstallers_AddReg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;
;CpyFiles=NT.USBCopyFiles, NT.CW51_USBCopyFilesSection
[CW10_USB.ndi.NT.Services]
AddService=CW10, 2, CW51_USB.Service, common.EventLog
DelService=cw10, 0x4
[CW10_USB1.ndi.NT]
AddReg=Common.reg, nt.reg, USB.reg, CPQ.reg, CW51_USB.CoInstallers_AddReg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;
;CpyFiles=NT.USBCopyFiles, NT.CW51_USBCopyFilesSection
[CW10_USB1.ndi.NT.Services]
AddService=CW10, 2, CW51_USB.Service, common.EventLog
DelService=cw10, 0x4
[CW10_USB2.ndi.NT]
AddReg=Common.reg, nt.reg, USB.reg, SYM.reg, CW51_USB.CoInstallers_AddReg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;
;CpyFiles=NT.USBCopyFiles, NT.CW51_USBCopyFilesSection
[CW10_USB2.ndi.NT.Services]
AddService=CW10, 2, CW51_USB.Service, common.EventLog
DelService=cw10, 0x4
[DestinationDirs]
DefaultDestDir=11
NT.USBCopyFiles=12 ; system32\drivers subdirectory on NT
win9x.USBCopyFiles=11 ; system subdirectory on win9x
[NT.USBCopyFiles]
cw51usb.sys ; NT Installation
[win9x.USBCopyFiles]
cw10usb.sys ; win9x Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
cw51usb.sys=1
[CPQ.reg]
HKR, , VendorDesc, 0, "Compaq 802.11b MultiPort Module"
[SYM.reg]
HKR, , VendorDesc, 0, "Symbol Spectrum24 Wireless LAN USB Adapter"
[NT.CW51_USBCopyFilesSection]
[CW51_USB.CoInstallers_AddReg]
[Common.reg]
HKR, , VendorDesc, 0, "Intel(R) PRO/Wireless 2011B LAN USB"
HKR, , APDensity, 0, "1"
HKR, defaults, APDensity, 0, 1
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, defaults, SSID, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, ParamDesc, 0, "SSID"
HKR, NDI\params\SSID, type, 0, "edit"
HKR, NDI\params\SSID, limitText, 0, "32"
HKR, NDI\params\SSID, default, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, flag, 1, "30","00","00","00"
HKR, , StationName, 0, "Client"
HKR, defaults, StationName, 0, "Client"
HKR, , ListenInterval, 0, "3"
HKR, defaults, ListenInterval, 0, 3
HKR, NDI\params\ListenInterval, ParamDesc, 0, "Maximum Listen Interval"
HKR, NDI\params\ListenInterval, flag, 1, "30","00","00","00"
HKR, NDI\params\ListenInterval, type, 0, "int"
HKR, Ndi\params\ListenInterval, default, 0, "3"
HKR, NDI\params\ListenInterval, min, 0, "0"
HKR, NDI\params\ListenInterval, max, 0, "77"
HKR, NDI\params\ListenInterval, step, 0, "1"
HKR, NDI\params\ListenInterval, optional, 0, "0"
HKR, , DSChannel, 0, "10"
HKR, defaults, DSChannel, 0, 10
HKR, , Encapsulation, 0, "1"
HKR, defaults, Encapsulation, 0, 1
HKR, , TxRate, 0, "15"
HKR, defaults, TxRate, 0, 15
HKR, NDI\params\TxRate, ParamDesc, 0, "Transmit Rate"
HKR, NDI\params\TxRate, type, 0, "enum"
HKR, NDI\params\TxRate, default, 0, "15"
HKR, NDI\params\TxRate, flag, 1, "30","00","00","00"
HKR, NDI\params\TxRate\enum, 1, 0, "Fixed 1 Mb/s"
HKR, NDI\params\TxRate\enum, 2, 0, "Fixed 2 Mb/s"
HKR, NDI\params\TxRate\enum, 3, 0, "Auto Select 1 or 2"
HKR, NDI\params\TxRate\enum, 4, 0, "Fixed 5.5 Mb/s"
HKR, NDI\params\TxRate\enum, 8, 0, "Fixed 11 Mb/s"
HKR, NDI\params\TxRate\enum, 15, 0, "Fully Auto"
HKR, , RTSThresh, 0, "2432"
HKR, defaults, RTSThresh, 0, 2432
HKR, NDI\params\RTSThresh, ParamDesc, 0, "Medium Reservation"
HKR, NDI\params\RTSThresh, type, 0, "enum"
HKR, NDI\params\RTSThresh, default, 0, "2432"
HKR, NDI\params\RTSThresh, flag, 1, "30","00","00","00"
HKR, NDI\params\RTSThresh\enum, 2432, 0, "Off"
HKR, NDI\params\RTSThresh\enum, 500, 0, "Hidden Stations"
HKR, , FragThresh, 0, "2432"
HKR, defaults, FragThresh, 0, 2432
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragmentation Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2432"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2432"
HKR, NDI\params\FragThresh, step, 0, "128"
HKR, NDI\params\FragThresh, flag, 1, "20","00","00","00"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, defaults, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, flag, 1, "30","00","00","00"
HKR, NDI\params\NetworkType\enum, 0, 0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , PSMode, 0, "1"
HKR, defaults, PSMode, 0, 1
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Save Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "1"
HKR, NDI\params\PSMode, flag, 1, "30","00","00","00"
HKR, NDI\params\PSMode\enum, 1, 0, "Disabled"
HKR, NDI\params\PSMode\enum, 2, 0, "Enabled"
HKR, , WepReq, 0, %WEP_REQUIRED_DEF_STR%
HKR, defaults, WepReq, 0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq, ParamDesc, 0, "Encryption"
HKR, NDI\params\WepReq, flag, 1, "30","00","00","00"
HKR, NDI\params\WepReq, type, 0, "enum"
HKR, Ndi\params\WepReq, default, 0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq\enum, 0, 0, "Disabled"
HKR, NDI\params\WepReq\enum, 2, 0, "64 bit"
HKR, NDI\params\WepReq\enum, 6, 0, "128 bit"
HKR, NDI\params\WepReq, optional, 0, "0"
HKR, , EncryptInDriver, 0, "1"
HKR, defaults, EncryptInDriver, 0, 1
HKR, , DecryptInDriver, 0, "1"
HKR, defaults, DecryptInDriver, 0, 1
HKR, , WEPFactor, 0, "3"
HKR, defaults, WEPFactor, 0, 3
HKR, , PreambleMode, 0, "1"
HKR, defaults, PreambleMode, 0, 1
HKR, NDI\params\PreambleMode, ParamDesc, 0, %SHORT_PREAM_STR%
HKR, NDI\params\PreambleMode, flag, 1, "30","00","00","00"
HKR, NDI\params\PreambleMode, type, 0, "enum"
HKR, Ndi\params\PreambleMode, default, 0, "1"
HKR, NDI\params\PreambleMode\enum,1, 0, "Long Tx Preamble"
HKR, NDI\params\PreambleMode\enum,2, 0, "Short Tx Preamble"
HKR, NDI\params\PreambleMode, optional, 0, "0"
HKR, , AuthentAlg, 0, %AUTHENT_TYPE_DEF_STR%
HKR, defaults, AuthentAlg, 0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg, ParamDesc, 0, "Authentication Algorithm"
HKR, NDI\params\AuthentAlg, type, 0, "enum"
HKR, NDI\params\AuthentAlg, default, 0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg, flag, 1, "30","00","00","00"
HKR, NDI\params\AuthentAlg\enum, 1, 0, "WECA Compliant (always use Open)"
HKR, NDI\params\AuthentAlg\enum, 2, 0, "Must use Shared with WEP"
HKR, , IBSSInDriver, 0, "1"
HKR, defaults, IBSSInDriver, 0, 1
HKR, NDI\params\IBSSInDriver, ParamDesc, 0, "Driver based IBSS"
HKR, NDI\params\IBSSInDriver, type, 0, "enum"
HKR, NDI\params\IBSSInDriver, default, 0, "1"
HKR, NDI\params\IBSSInDriver, flag, 1, "30","00","00","00"
HKR, NDI\params\IBSSInDriver\enum,0, 0, "Disabled"
HKR, NDI\params\IBSSInDriver\enum,1, 0, "Enabled"
[USB.reg]
HKR, , BusType, 0, "15"
HKR, NDI, CardType, 0, "PNP"
[win9x.reg]
HKR, , DevLoader, 0, "*ndis,*ntkern"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, , OSVersion, 0, "1"
HKR, NDIS, LogDriverName, 0, "cw10usb"
HKR, NDIS, MajorNdisVersion,1, 03
HKR, NDIS, MinorNdisVersion,1, 0A
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[USB_ID.reg]
HKR, , DeviceVxDs, 0, "cw10usb.sys"
HKR, , NTMPDriver, 0, "cw10usb.sys"
HKR, Ndi, DeviceID, 0, "USB\VID_2474&PID_3642"
[nt.reg]
HKR, Ndi, Service, 0, "CW10"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, , OSVersion, 0, "2"
[CW51_USB.Service]
DisplayName=%CW10_USB.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\CW51Usb.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,%%SystemRoot%%"\System32\netevent.dll",%%SystemRoot%%"\System32\drivers\CW51usb.sys"
HKR, , TypesSupported, 0x00010001, 7
[Strings]
Provider="Intel Corporation"
CW10USB_ISIL.DeviceDescUSB="Intersil IEEE 802.11 LAN USB Adapter"
CW10USB_INTEL.DeviceDescUSB="Intel(R) PRO/Wireless LAN Module"
CW10USB_INTEL1.DeviceDescUSB="Intel(R) PRO/Wireless 2011B LAN USB Device"
CW10USB_CPQ.DeviceDescUSB="Compaq 802.11b MultiPort Module"
CW10USB_SYMBOL.DeviceDescUSB="Symbol Spectrum24 Wireless LAN USB Adapter"
CW10_USB.Service.DispName="Intel(R) PRO/Wireless LAN Module Driver"
SHORT_PREAM_STR="Preamble Mode"
INSTALL_DISK_STR="Wireless LAN Installation Disk"
SSID_DEF_STR="101"
NETWORK_TYPE_DEF_STR="1"
AUTHENT_TYPE_DEF_STR="2"
PASSPHRASE_DEF_STR="INTEL"
WEP_REQUIRED_DEF_STR="0"
