; R5C592.inf
; Windows XP/2000 installation file
; for installing RICOH SD/MM Card and Memory Stick driver
; Copyright (c) 2001-2003 RICOH Company Ltd.,   All rights Reserved
; This Driver supports R5C592/R5C576 RICOH Bay Controller
; 

[Version] 
Signature = "$Windows NT$" 
;Class=System
;ClassGUID={4d36e97d-e325-11ce-bfc1-08002be10318} 
Class=hdc
ClassGUID={4d36e96a-e325-11ce-bfc1-08002be10318} 
Provider=%Ricoh% 
CatalogFile=R5C592.cat
DriverVer= 01/20/2004, 1.01.07.02

[DestinationDirs] 
R5C592.Files.x86_11 = 11 
R5C592.Files.x86_12 = 12 
R5C576.Files.x86_12 = 12 

[SourceDisksNames.x86]
0=%Desc_x860%

[SourceDisksNames.ia64]


[SourceDisksFiles.x86]
R592.sys=0,, 
snymsico.dll=0,, 

[SourceDisksFiles.ia64]


[Manufacturer] 
%Ricoh%=Ricoh

[Ricoh]
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592&SUBSYS_81F51033
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592&SUBSYS_81F61033
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592&SUBSYS_81FE1033
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592&SUBSYS_81FF1033
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592&SUBSYS_820D1033
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592&SUBSYS_82291033
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592&SUBSYS_82311033
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592&SUBSYS_82371033
%R5C592Desc%=R5C592_Inst,PCI\VEN_1180&DEV_0592&SUBSYS_82591033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576&SUBSYS_81F51033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576&SUBSYS_81F61033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576&SUBSYS_81FE1033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576&SUBSYS_81FF1033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576&SUBSYS_820D1033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576&SUBSYS_82291033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576&SUBSYS_82311033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576&SUBSYS_82371033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0576&SUBSYS_82591033
%R5C576Desc%=R5C576_Inst,PCI\VEN_1180&DEV_0575

[R5C592_Inst.ntx86] 
CopyFiles = R5C592.Files.x86_11, R5C592.Files.x86_12 

[R5C592_Inst.ntx86.Services] 
AddService = R592,0x00000002,R5C592_Service_Instx86, 

[R5C592_Service_Instx86] 
ServiceType = %SERVICE_KERNEL_DRIVER% 
StartType = %SERVICE_BOOT_START% 
ErrorControl = %SERVICE_ERROR_NORMAL% 
ServiceBinary = %12%\R592.sys 
LoadOrderGroup = "MemoryStick"
AddReg        = MsDiskAddReg

[MsDiskAddReg]
HKR, "Parameters", "MSSystemWaitTime",		%REG_DWORD%, 0x00000002
HKR, "Parameters", "PROSystemWaitTime",		%REG_DWORD%, 0x00000002



[R5C592.Files.x86_11] 
snymsico.dll
[R5C592.Files.x86_12] 
R592.sys

[R5C592_Inst.ntx86.HW] 
AddReg = R5C592_Inst.AddReg 
 
[R5C592_Inst.AddReg] 
HKR,,DeviceGroup,,"MemoryStick"
HKR,,Icons,0x00010000,"%SystemRoot%\system32\snymsico.dll,0"
HKR,,Label,,"MemoryStick"
HKR,,NoSoftEject,0x00010001,"00000001"
HKR,,FriendlyName,,%R5C592Desc%
HKR,,DeviceCharacteristics,0x10001,0x00000101
HKR,,DeviceType,0x10001,0x00000007

[R5C576_Inst.ntx86] 
CopyFiles = R5C576.Files.x86_12 

[R5C576_Inst.ntx86.Services] 
AddService = R592,0x00000002,R5C576_Service_Instx86, 

[R5C576_Service_Instx86] 
ServiceType = %SERVICE_KERNEL_DRIVER% 
StartType = %SERVICE_BOOT_START% 
ErrorControl = %SERVICE_ERROR_NORMAL% 
ServiceBinary = %12%\R592.sys 
AddReg        = SDDiskAddReg

[SDDiskAddReg]
HKR, "Parameters", "SDSystemWaitTime",		%REG_DWORD%, 0x00000001 


[R5C576.Files.x86_12] 
R592.sys

[R5C576_Inst.ntx86.HW] 
AddReg = R5C576_Inst.AddReg 
 
[R5C576_Inst.AddReg] 
HKR,,Icons,0x00010000,"%SystemRoot%\system32\shell32.dll,-305"
HKR,,Label,,"SD / MMC"
HKR,,NoSoftEject,0x00010001,"00000001"
HKR,,FriendlyName,,%R5C576Desc%
HKR,,DeviceCharacteristics,0x10001,0x00000101
HKR,,DeviceType,0x10001,0x00000007

[Strings] 

;  *******Localizable Strings******* 
Ricoh= "Ricoh Company" 
Desc_x860= "Ricoh SD/MM Card and Memory Stick Controller" 
R5C592Desc= "Ricoh Memory Stick Bus Host Adapter" 
R5C576Desc= "Ricoh SD Bus Host Adapter" 
DeviceGroups = "Software\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups"

;  *******Non Localizable Strings******* 

SERVICE_BOOT_START = 0x0 
SERVICE_SYSTEM_START = 0x1 
SERVICE_AUTO_START = 0x2 
SERVICE_DEMAND_START = 0x3 
SERVICE_DISABLED = 0x4 

SERVICE_KERNEL_DRIVER = 0x1 
SERVICE_ERROR_IGNORE = 0x0 
SERVICE_ERROR_NORMAL = 0x1 
SERVICE_ERROR_SEVERE = 0x2 
SERVICE_ERROR_CRITICAL = 0x3 

REG_EXPAND_SZ = 0x00020000 
REG_DWORD = 0x00010001 
