;Monitor INF file for Fujitsu Display B27-8 TE Pro
;Copyright 2017 Fujitsu Technology Solutions

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%FTS_Mfg%
CatalogFile=B27-8_TE_Pro.cat
DriverVer=08/24/2017,1.0.0.0


[ControlFlags]
ExcludeFromSelect.nt=Monitor\FUS08AC
ExcludeFromSelect.nt=Monitor\FUS08AA
ExcludeFromSelect.nt=Monitor\FUS08AB

[DestinationDirs]
DefaultDestDir=11
B27-8 TE Pro_a.CopyFiles=23
B27-8 TE Pro_h.CopyFiles=23
B27-8 TE Pro_dp.CopyFiles=23

[SourceDisksNames]
1=%DiskName%,,,

[SourceDisksFiles]
B27-8_TE_Pro.icm=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys


[Manufacturer]
%FTS_Mfg%=FTS_Mfg,NTAMD64

[FTS_Mfg] 
%B27-8 TE Pro_a%=B27-8 TE Pro_a.Install, Monitor\FUS08AC
%B27-8 TE Pro_h%=B27-8 TE Pro_h.Install, Monitor\FUS08AA
%B27-8 TE Pro_dp%=B27-8 TE Pro_dp.Install, Monitor\FUS08AB

[FTS_Mfg.NTAMD64] 
%B27-8 TE Pro_a%=B27-8 TE Pro_a.Install, Monitor\FUS08AC
%B27-8 TE Pro_h%=B27-8 TE Pro_h.Install, Monitor\FUS08AA
%B27-8 TE Pro_dp%=B27-8 TE Pro_dp.Install, Monitor\FUS08AB


[B27-8 TE Pro_a.Install]
DELReg=DEL_CURRENT_REG    
AddReg=B27-8 TE Pro_a.AddReg
CopyFiles=B27-8 TE Pro_a.CopyFiles

[B27-8 TE Pro_a.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[B27-8 TE Pro_h.Install]
DELReg=DEL_CURRENT_REG    
AddReg=B27-8 TE Pro_h.AddReg
CopyFiles=B27-8 TE Pro_h.CopyFiles

[B27-8 TE Pro_h.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install

[B27-8 TE Pro_dp.Install]
DELReg=DEL_CURRENT_REG    
AddReg=B27-8 TE Pro_dp.AddReg
CopyFiles=B27-8 TE Pro_dp.CopyFiles

[B27-8 TE Pro_dp.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install


[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile


[B27-8 TE Pro_a.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,48.0-76.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"B27-8_TE_Pro.icm"


[B27-8 TE Pro_h.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,48.0-76.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"B27-8_TE_Pro.icm"

[B27-8 TE Pro_dp.AddReg]
HKR,"MODES\1920,1080",Mode1,,"30.0-82.0,48.0-76.0,+,+"
HKR,,MaxResolution,,"1920,1080"
HKR,,DPMS,,1
HKR,,ICMProfile,0,"B27-8_TE_Pro.icm"


[B27-8 TE Pro_a.CopyFiles]
B27-8_TE_Pro.icm

[B27-8 TE Pro_h.CopyFiles]
B27-8_TE_Pro.icm

[B27-8 TE Pro_dp.CopyFiles]
B27-8_TE_Pro.icm


[Strings]
SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

DiskName="Fujitsu Driver & Utilities CD B27-8 TE Pro"
FTS_Mfg="Fujitsu Technology Solutions"	

B27-8 TE Pro_a="Fujitsu B27-8 TE Pro (Analog)"
B27-8 TE Pro_h="Fujitsu B27-8 TE Pro (HDMI)"
B27-8 TE Pro_dp="Fujitsu B27-8 TE Pro (DP)"