
[Version]
DriverVer=03/27/2002,1.7.37.1096
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
CatalogFile=LSWLNDS.CAT
[Manufacturer]
%V_Provider%=Adapters, NT.5.1
[ControlFlags]
ExcludeFromSelect=PCMCIA\THE_LINKSYS_GROUP__INC.-INSTANT_WIRELESS_NETWORK_PC_CARD-FA61
ExcludeFromSelect=PCMCIA\THE_LINKSYS_GROUP__INC.-WIRELESS_NETWORK_CF_CARD-C7C7
ExcludeFromSelect=PCMCIA\THE_LINKSYS_GROUP__INC.-INSTANT_WIRELESS_NETWORK_PC_CARD-0C0B
ExcludeFromSelect=PCMCIA\INSTANT_WIRELESS_-_NETWORK_PC_CARD-317F
[Adapters]
%WPC11.DeviceDesc%=WPC11.ndi, PCMCIA\THE_LINKSYS_GROUP__INC.-INSTANT_WIRELESS_NETWORK_PC_CARD-FA61
%WPC11_1.DeviceDesc%=WPC11_1.ndi, PCMCIA\THE_LINKSYS_GROUP__INC.-WIRELESS_NETWORK_CF_CARD-C7C7
%WPC11_2.DeviceDesc%=WPC11_2.ndi, PCMCIA\THE_LINKSYS_GROUP__INC.-INSTANT_WIRELESS_NETWORK_PC_CARD-0C0B
%WPC11_3.DeviceDesc%=WPC11_3.ndi, PCMCIA\INSTANT_WIRELESS_-_NETWORK_PC_CARD-317F
[Adapters.NT.5.1]
%WPC11.DeviceDesc%=WPC11.NT51.ndi, PCMCIA\THE_LINKSYS_GROUP__INC.-INSTANT_WIRELESS_NETWORK_PC_CARD-FA61
%WPC11_1.DeviceDesc%=WPC11_1.NT51.ndi, PCMCIA\THE_LINKSYS_GROUP__INC.-WIRELESS_NETWORK_CF_CARD-C7C7
%WPC11_2.DeviceDesc%=WPC11_2.NT51.ndi, PCMCIA\THE_LINKSYS_GROUP__INC.-INSTANT_WIRELESS_NETWORK_PC_CARD-0C0B
%WPC11_3.DeviceDesc%=WPC11_3.NT51.ndi, PCMCIA\INSTANT_WIRELESS_-_NETWORK_PC_CARD-317F
[WPC11.ndi]
AddReg=WPC11.ndi.reg, Pcmcia9x.reg, Advanced.reg, Common.reg
;CpyFiles=win9x.CopyFiles
DriverVer=05/16/2002,1.7.37.1098
[WPC11_1.ndi]
AddReg=WPC11.ndi.reg, Pcmcia9x_1.reg, Advanced.reg, Common.reg
;CpyFiles=win9x.CopyFiles
DriverVer=05/16/2002,1.7.37.1098
[WPC11_2.ndi]
AddReg=WPC11.ndi.reg, Pcmcia9x_2.reg, Advanced.reg, Common.reg
;CpyFiles=win9x.CopyFiles
DriverVer=05/16/2002,1.7.37.1098
[WPC11_3.ndi]
AddReg=WPC11.ndi.reg, Pcmcia9x_3.reg, Advanced.reg, Common.reg
;CpyFiles=win9x.CopyFiles
DriverVer=05/16/2002,1.7.37.1098
[WPC11.ndi.reg]
HKR, , NTMPDriver, 0, LSWLNDS.sys
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, LSWLNDS.sys
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, 0, "WPC11"
HKR, NDIS, MajorNdisVersion,1, 03
HKR, NDIS, MinorNdisVersion,1, 0A
HKR, , BusType, 0, 8
HKR, NDI, CardType, 0, "PCMCIA"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[Pcmcia9x.reg]
HKR, , IOBaseAddress, 1, 02,00,00,00
HKR, , InterruptNumber, 1, 04,00,00,00
HKR, , EnableIRQSharing,1, 01,00,00,00
HKR, , VendorDesc, 0, "Instant Wireless Network PC Card V2.5"
HKR, Ndi, DeviceID, 0, "PCMCIA\THE_LINKSYS_GROUP__INC.-INSTANT_WIRELESS_NETWORK_PC_CARD-FA61"
[Pcmcia9x_1.reg]
HKR, , IOBaseAddress, 1, 02,00,00,00
HKR, , InterruptNumber, 1, 04,00,00,00
HKR, , EnableIRQSharing,1, 01,00,00,00
HKR, , VendorDesc, 0, "Instant Wireless Network CF Card"
HKR, Ndi, DeviceID, 0, "PCMCIA\THE_LINKSYS_GROUP__INC.-WIRELESS_NETWORK_CF_CARD-C7C7"
[Pcmcia9x_2.reg]
HKR, , IOBaseAddress, 1, 02,00,00,00
HKR, , InterruptNumber, 1, 04,00,00,00
HKR, , EnableIRQSharing,1, 01,00,00,00
HKR, , VendorDesc, 0, "Instant Wireless Network PC Card V3.0"
HKR, Ndi, DeviceID, 0, "PCMCIA\THE_LINKSYS_GROUP__INC.-INSTANT_WIRELESS_NETWORK_PC_CARD-0C0B"
[Pcmcia9x_3.reg]
HKR, , IOBaseAddress, 1, 02,00,00,00
HKR, , InterruptNumber, 1, 04,00,00,00
HKR, , EnableIRQSharing,1, 01,00,00,00
HKR, , VendorDesc, 0, "Instant Wireless Network PC Card V2.0"
HKR, Ndi, DeviceID, 0, "PCMCIA\INSTANT_WIRELESS_-_NETWORK_PC_CARD-317F"
[WPC11.ndi.NT]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
DriverVer=05/16/2002,1.7.37.1098
[WPC11.ndi.NT.Services]
AddService=WPC11, 2, WPC11.Service, common.EventLog
[WPC11.Service]
DisplayName=%WPC11.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\LSWLNDS.sys
LoadOrderGroup=NDIS
[WPC11_1.ndi.NT]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
DriverVer=05/16/2002,1.7.37.1098
[WPC11_1.ndi.NT.Services]
AddService=WPC11, 2, WPC11_1.Service, common.EventLog
[WPC11_1.Service]
DisplayName=%WPC11_1.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\LSWLNDS.sys
LoadOrderGroup=NDIS
[WPC11_2.ndi.NT]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
DriverVer=05/16/2002,1.7.37.1098
[WPC11_2.ndi.NT.Services]
AddService=WPC11, 2, WPC11_2.Service, common.EventLog
[WPC11_2.Service]
DisplayName=%WPC11_2.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\LSWLNDS.sys
LoadOrderGroup=NDIS
[WPC11_3.ndi.NT]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT.CopyFiles
DriverVer=05/16/2002,1.7.37.1098
[WPC11_3.ndi.NT.Services]
AddService=WPC11, 2, WPC11_3.Service, common.EventLog
[WPC11_3.Service]
DisplayName=%WPC11_3.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\LSWLNDS.sys
LoadOrderGroup=NDIS
[WPC11.NT51.ndi]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT51.CopyFiles
DriverVer=03/27/2002,1.7.37.1096
[WPC11.NT51.ndi.Services]
AddService=WPC11, 2, WPC11.Service, common.EventLog
[WPC11_1.NT51.ndi]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT51.CopyFiles
DriverVer=03/27/2002,1.7.37.1096
[WPC11_1.NT51.ndi.Services]
AddService=WPC11, 2, WPC11_1.Service, common.EventLog
[WPC11_2.NT51.ndi]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT51.CopyFiles
DriverVer=03/27/2002,1.7.37.1096
[WPC11_2.NT51.ndi.Services]
AddService=WPC11, 2, WPC11_2.Service, common.EventLog
[WPC11_3.NT51.ndi]
AddReg=Advanced.reg, Common.reg, nt.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
;CpyFiles=NT51.CopyFiles
DriverVer=03/27/2002,1.7.37.1096
[WPC11_3.NT51.ndi.Services]
AddService=WPC11, 2, WPC11_3.Service, common.EventLog
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\LSWLNDS.sys
HKR, , TypesSupported, 0x00010001, 7
[nt.reg]
HKR, Ndi, Service, 0, "WPC11"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[Common.reg]
HKR, , APDensity, 0, "1"
HKR, defaults, APDensity, 0, "1"
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, defaults, SSID, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, ParamDesc, 0, "SSID"
HKR, NDI\params\SSID, type, 0, "edit"
HKR, NDI\params\SSID, limitText, 0, "32"
HKR, NDI\params\SSID, default, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, flag, 1, "30","00","00","00"
HKR, , StationName, 0, "Client"
HKR, defaults, StationName, 0, "Client"
HKR, , DSChannel, 0, %CHANNEL%
HKR, defaults, DSChannel, 0, %CHANNEL%
HKR, NDI\params\DSChannel, ParamDesc, 0, "Channel"
HKR, NDI\params\DSChannel, type, 0, "enum"
HKR, NDI\params\DSChannel, default, 0, %CHANNEL%
HKR, NDI\params\DSChannel, flag, 1, "30","00","00","00"
HKR, NDI\params\DSChannel\enum, 1, 0, "1"
HKR, NDI\params\DSChannel\enum, 2, 0, "2"
HKR, NDI\params\DSChannel\enum, 3, 0, "3"
HKR, NDI\params\DSChannel\enum, 4, 0, "4"
HKR, NDI\params\DSChannel\enum, 5, 0, "5"
HKR, NDI\params\DSChannel\enum, 6, 0, "6"
HKR, NDI\params\DSChannel\enum, 7, 0, "7"
HKR, NDI\params\DSChannel\enum, 8, 0, "8"
HKR, NDI\params\DSChannel\enum, 9, 0, "9"
HKR, NDI\params\DSChannel\enum, 10, 0, "10"
HKR, NDI\params\DSChannel\enum, 11, 0, "11"
HKR, , Encapsulation, 0, "1"
HKR, defaults, Encapsulation, 0, "1"
HKR, , TxRate, 0, "15"
HKR, defaults, TxRate, 0, "15"
HKR, NDI\params\TxRate, ParamDesc, 0, "Transmit Rate"
HKR, NDI\params\TxRate, type, 0, "enum"
HKR, NDI\params\TxRate, default, 0, "15"
HKR, NDI\params\TxRate, flag, 1, "30","00","00","00"
HKR, NDI\params\TxRate\enum, 1, 0, "Fixed 1 Mb/s"
HKR, NDI\params\TxRate\enum, 2, 0, "Fixed 2 Mb/s"
HKR, NDI\params\TxRate\enum, 3, 0, "Auto Select 1 or 2"
HKR, NDI\params\TxRate\enum, 4, 0, "Fixed 5.5 Mb/s"
HKR, NDI\params\TxRate\enum, 8, 0, "Fixed 11 Mb/s"
HKR, NDI\params\TxRate\enum, 15, 0, "Fully Auto"
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, defaults, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, flag, 1, "30","00","00","00"
HKR, NDI\params\NetworkType\enum, 0, 0, "Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , WepReq, 0, %WEP_REQUIRED_DEF_STR%
HKR, defaults, WepReq, 0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq, ParamDesc, 0, "Encryption"
HKR, NDI\params\WepReq, flag, 1, "30","00","00","00"
HKR, NDI\params\WepReq, type, 0, "enum"
HKR, Ndi\params\WepReq, default, 0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq\enum, 0, 0, "Disabled"
HKR, NDI\params\WepReq\enum, 2, 0, "64 bit"
HKR, NDI\params\WepReq\enum, 6, 0, "128 bit"
HKR, NDI\params\WepReq, optional, 0, "0"
HKR, , EncryptInDriver, 0, "1"
HKR, defaults, EncryptInDriver, 0, "1"
HKR, , DecryptInDriver, 0, "1"
HKR, defaults, DecryptInDriver, 0, "1"
HKR, , WEPFactor, 0, "3"
HKR, defaults, WEPFactor, 0, "3"
HKR, , Esarhpssap, 0, %PASSPHRASE_DEF_STR%
HKR, defaults, Esarhpssap, 0, %PASSPHRASE_DEF_STR%
HKR, NDI\params\Esarhpssap, ParamDesc, 0, "WEP Passphrase"
HKR, NDI\params\Esarhpssap, type, 0, "edit"
HKR, NDI\params\Esarhpssap, limitText, 0, "64"
HKR, NDI\params\Esarhpssap, default, 0, %PASSPHRASE_DEF_STR%
HKR, NDI\params\Esarhpssap, flag, 1, "30","00","00","00"
HKR, , IBSSInDriver, 0, "0"
HKR, defaults, IBSSInDriver, 0, "0"
HKR,, WEP64_KEY_1, 0,"0000000000"
HKR,, WEP64_KEY_2, 0,"0000000000"
HKR,, WEP64_KEY_3, 0,"0000000000"
HKR,, WEP64_KEY_4, 0,"0000000000"
HKR,, WEP128_KEY_1, 0,"00000000000000000000000000"
HKR,, WEP128_KEY_2, 0,"00000000000000000000000000"
HKR,, WEP128_KEY_3, 0,"00000000000000000000000000"
HKR,, WEP128_KEY_4, 0,"00000000000000000000000000"
HKR,, CurProfile, 0,"default"
[Advanced.reg]
HKR, , ListenInterval, 0, "3"
HKR, defaults, ListenInterval, 0, "3"
HKR, NDI\params\ListenInterval, ParamDesc, 0, "Maximum Listen Interval"
HKR, NDI\params\ListenInterval, flag, 1, "30","00","00","00"
HKR, NDI\params\ListenInterval, type, 0, "int"
HKR, Ndi\params\ListenInterval, default, 0, "3"
HKR, NDI\params\ListenInterval, min, 0, "0"
HKR, NDI\params\ListenInterval, max, 0, "77"
HKR, NDI\params\ListenInterval, step, 0, "1"
HKR, NDI\params\ListenInterval, optional, 0, "0"
HKR, , RTSThresh, 0, "2432"
HKR, defaults, RTSThresh, 0, "2432"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2432"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2432"
HKR, NDI\params\RTSThresh, step, 0, "64"
HKR, NDI\params\RTSThresh, flag, 1, "20","00","00","00"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2432"
HKR, defaults, FragThresh, 0, "2432"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragmentation Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2432"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2432"
HKR, NDI\params\FragThresh, step, 0, "128"
HKR, NDI\params\FragThresh, flag, 1, "20","00","00","00"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , PreambleMode, 0, "1"
HKR, defaults, PreambleMode, 0, "1"
HKR, NDI\params\PreambleMode, ParamDesc, 0, %SHORT_PREAM_STR%
HKR, NDI\params\PreambleMode, flag, 1, "30","00","00","00"
HKR, NDI\params\PreambleMode, type, 0, "enum"
HKR, Ndi\params\PreambleMode, default, 0, "1"
HKR, NDI\params\PreambleMode\enum,1, 0, "Long Tx Preamble"
HKR, NDI\params\PreambleMode\enum,2, 0, "Short Tx Preamble"
HKR, NDI\params\PreambleMode, optional, 0, "0"
HKR, , AuthentAlg, 0, %AUTHENT_TYPE_DEF_STR%
HKR, defaults, AuthentAlg, 0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg, ParamDesc, 0, "Authentication Algorithm"
HKR, NDI\params\AuthentAlg, type, 0, "enum"
HKR, NDI\params\AuthentAlg, default, 0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg, flag, 1, "30","00","00","00"
HKR, NDI\params\AuthentAlg\enum, 1, 0, "WECA Compliant (always use Open)"
HKR, NDI\params\AuthentAlg\enum, 2, 0, "Must use Shared with WEP"
HKR, NDI\params\AuthentAlg\enum, 65535, 0, "Automatic based on WEP setting"
HKR, , PSMode, 0, "1"
HKR, defaults, PSMode, 0, "1"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Save Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "1"
HKR, NDI\params\PSMode, flag, 1, "30","00","00","00"
HKR, NDI\params\PSMode\enum, 1, 0, "Disabled"
HKR, NDI\params\PSMode\enum, 2, 0, "Enabled"
[DestinationDirs]
DefaultDestDir=11
NT.CopyFiles=12 ; system32\drivers subdirectory on 2000
NT51.CopyFiles=12 ; system32\drivers subdirectory on XP
win9x.CopyFiles=11 ; system32 subdirectory on win9x
[NT.CopyFiles]
LSWLNDS.sys,,,2
[NT51.CopyFiles]
LSWLNDS.sys,LSWLNDSX.SYS,,2
[win9x.CopyFiles]
LSWLNDS.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
LSWLNDS.sys=1
LSWLNDSX.sys=1
[strings]
Provider="Linksys"
V_Provider="The Linksys Group, Inc."
WPC11.DeviceDesc="Instant Wireless Network PC Card V2.5"
WPC11_1.DeviceDesc="Instant Wireless Network CF Card"
WPC11_2.DeviceDesc="Instant Wireless Network PC Card V3.0"
WPC11_3.DeviceDesc="Instant Wireless Network PC Card V2.0"
WPC11.Service.DispName="Instant Wireless Network PC Card V2.5 Driver"
WPC11_1.Service.DispName="Instant Wireless Network CF Card Driver"
WPC11_2.Service.DispName="Instant Wireless Network PC Card V3.0 Driver"
WPC11_3.Service.DispName="Instant Wireless Network PC Card V2.0 Driver"
INSTALL_DISK_STR="Instant Wireless Network PC Card Installation Disk"
SSID_DEF_STR="linksys"
NETWORK_TYPE_DEF_STR=1
CHANNEL=6
AUTHENT_TYPE_DEF_STR="65535"
PASSPHRASE_DEF_STR=""
WEP_REQUIRED_DEF_STR="0"
SHORT_PREAM_STR="Preamble Mode"

