
[Version]
CatalogFile=LSTINDS.cat
Signature="$Windows NT$"
Provider=%TI%
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=03/10/2004,6.0.0.18
[Manufacturer]
%TI%=TexasInstruments,NT.5.1
[ControlFlags]
ExcludeFromSelect=PCI\VEN_104C&DEV_9066&SUBSYS_00331737
[TexasInstruments.NT.5.1]
%TIACX.DeviceDesc%=TIACXXP, PCI\VEN_104C&DEV_9066&SUBSYS_00331737 ; B & G
[TexasInstruments]
%TIACX.DeviceDesc%=TIACX, PCI\VEN_104C&DEV_9066&SUBSYS_00331737 ; B & G
[TIACXXP]
BusType=5
AddReg =TIACXXP.ndi.reg.NT, TI.Param.Reg, BG.Param.Reg, WXP.Param.Reg
Characteristics=0x84
;CpyFiles =TIACXXP.CopyFiles
[TIACXXP.ndi.reg.NT]
HKR, Ndi, Service, 0, "TNET1130x"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[TIACXXP.Services]
AddService=TNET1130x, 2, TIACXLNXP.Service, TIACXLNXP.EventLog
[TIACXXP.CopyFiles]
TNET1130x.sys
[TIACXLNXP.Service]
DisplayName=%TIACXLN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\tnet1130x.sys
LoadOrderGroup=NDIS
[TIACXLNXP.EventLog]
AddReg=TIACXLNXP.AddEventLog.reg
[TIACXLNXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[WXP.Param.Reg]
HKR, ,PrivacyMode,, "2"
HKR, ,utlPrivacyMode,, "0"
HKR, ,utlAuthenticationMode,, "0"
[TIACX.NT]
BusType=5
AddReg =TIACX.ndi.reg.NT, TI.Param.Reg, BG.Param.Reg, W2K.Param.Reg
Characteristics=0x84
;CpyFiles =TIACX.CopyFiles.NT, TIACX.BinFiles.NT
[TIACX.ndi.reg.NT]
HKR, Ndi, Service, 0, "TNET1130"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[TIACX.NT.Services]
AddService=TNET1130, 2, TIACXLN.Service, TIACXLN.EventLog
[TIACX.CopyFiles.NT]
TNET1130.sys
[TIACX.BinFiles.NT]
[TIACXLN.Service]
DisplayName=%TIACXLN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\tnet1130.sys
LoadOrderGroup=NDIS
[TIACXLN.EventLog]
AddReg=TIACXLN.AddEventLog.reg
[TIACXLN.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[W2K.Param.Reg]
HKR, ,PrivacyMode,, "2"
HKR, ,utlPrivacyMode,, "0"
HKR, ,utlAuthenticationMode,, "0"
[TIACX]
AddReg=TIACX.ndi.reg, TI.Param.Reg, TIACX.Install, BG.Param.Reg, W98.Param.Reg
[TIACX.Copy]
;CpyFiles=TIACX.CopyFiles
[TIACX.Install]
HKR,Ndi\Install,,,"TIACX.Copy"
HKR,Ndi\Remove,,,"TIACX.Remove"
[TIACX.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_9066"
HKR,Ndi,HelpText,0,%WLANAdapterHelpText%
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,LSTINDS4.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, , "LSTINDS4"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"
[TIACX.CopyFiles]
LSTINDS4.sys
[W98.Param.Reg]
HKR, ,PrivacyMode,, "2"
HKR, ,utlPrivacyMode,, "0"
HKR, ,utlAuthenticationMode,, "0"
[BG.Param.Reg]
HKR, ,dot11SupportedRateMask,, "8"
HKR, ,dot11BasicRateMask,, "1"
HKR,NDI\params\dot11NetworkType,ParamDesc,, "Network Type"
HKR,NDI\params\dot11NetworkType,type,,"enum"
HKR,NDI\params\dot11NetworkType,default,,"3"
HKR,NDI\params\dot11NetworkType\enum,"1",,"11b"
HKR,NDI\params\dot11NetworkType\enum,"2",,"11a"
HKR,NDI\params\dot11NetworkType\enum,"3",,"11g"
HKR,NDI\params\dot11NetworkType\enum,"4",,"11a&g"
HKR, ,dot11DesiredChannel, ,1
[TI.Param.Reg]
HKR, ,dot11DesiredBSSType,, "1"
HKR, ,WiFiAdhoc,, "0"
HKR, ,DisableSsidPending,, "1"
HKR,NDI\params\dot11PowerMode,ParamDesc,,"Power Mode"
HKR,NDI\params\dot11PowerMode,type,,"enum"
HKR,NDI\params\dot11PowerMode,default,,"0"
HKR,NDI\params\dot11PowerMode\enum,"0",,"Continuous Access Mode"
HKR,NDI\params\dot11PowerMode\enum,"1",,"Maximum Power Save"
HKR, Ndi\Params\dot11FragmentationThreshold, ParamDesc, ,"Fragmentation Threshold"
HKR, Ndi\Params\dot11FragmentationThreshold, Type, , "int"
HKR, Ndi\Params\dot11FragmentationThreshold, Default, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Min, , "256"
HKR, Ndi\Params\dot11FragmentationThreshold, Max, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Step, , "1"
HKR, Ndi\Params\dot11FragmentationThreshold, Base, , "10"
HKR, Ndi\Params\dot11RTSThreshold, ParamDesc, ,"RTS Threshold"
HKR, Ndi\Params\dot11RTSThreshold, Type, , "int"
HKR, Ndi\Params\dot11RTSThreshold, Default, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Min, , "0"
HKR, Ndi\Params\dot11RTSThreshold, Max, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Step, , "1"
HKR, Ndi\Params\dot11RTSThreshold, Base, , "10"
HKR,NDI\params\Mode4x,ParamDesc,,"Mode4x"
HKR,NDI\params\Mode4x,type,,"enum"
HKR,NDI\params\Mode4x,default,,"1"
HKR,NDI\params\Mode4x\enum,"0",,"Off"
HKR,NDI\params\Mode4x\enum,"1",,"On"
[DestinationDirs]
DefaultDestDir=12 ; Windows\System32\Drivers
TIACXXP.CopyFiles=12 ; Winnt\System32\Drivers Directory ; WinXP
TIACXAGXP.CopyFiles=12 ; Winnt\System32\Drivers Directory ; WinXP
TIACX.CopyFiles=11 ; Windows\System or Winnt\System32 Directory ; Win98/ME
TIACX.BinFiles.NT=10,system
TIACXAG.CopyFiles=11 ; Windows\System or Winnt\System32 Directory ; Win98/ME
TIACXAG.BinFiles.NT=10,system
[SourceDisksNames]
1=%DiskName%,,
[SourceDisksFiles]
TNET1130x.sys=1
TNET1130.sys=1
LSTINDS4.sys=1
[Strings]
TI="Linksys"
TIACX.DeviceDesc="Wireless-G Notebook Adapter v.2.0"
TIACXLN.Service.DispName="Wireless-G Notebook Adapter v.2.0"
WLANAdapterHelpText= "A WLAN Adapter provides high speed connection to the Internet through 802.11b technology"
DiskName="Linksys Wireless-G Notebook Adapter Installation Disk"
