
[Version]
Signature="$Windows NT$"
Provider=%TI%
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=06/28/2004,6.0.1.6
[Manufacturer]
%TI%=USR
[ControlFlags]
ExcludeFromSelect=PCI\VEN_104C&DEV_9066&SUBSYS_16EC010D
ExcludeFromSelect=PCI\VEN_104C&DEV_9066&SUBSYS_16EC010E
[USR.NT.5.1]
%USR11G.DeviceDesc%=USR11GXP, PCI\VEN_104C&DEV_9066&SUBSYS_16EC010D
%USR11G.DeviceDesc%=USR11GXP, PCI\VEN_104C&DEV_9066&SUBSYS_16EC010E
[USR]
%USR11G.DeviceDesc%=USR11G, PCI\VEN_104C&DEV_9066&SUBSYS_16EC010D
%USR11G.DeviceDesc%=USR11G, PCI\VEN_104C&DEV_9066&SUBSYS_16EC010E
[USR11GXP]
BusType=5
AddReg =USR11GXP.ndi.reg.NT, TI.Param.Reg, BG.Param.Reg
Characteristics=0x84
;CpyFiles =USR11GXP.CopyFiles
[USR11GXP.ndi.reg.NT]
HKR, Ndi, Service, 0, "USR11G"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[USR11GXP.Services]
AddService=USR11G, 2, USR11GXP.Service, USR11GXP.EventLog
[USR11GXP.CopyFiles]
[USR11GAGXP]
BusType=5
AddReg =USR11GAGXP.ndi.reg.NT, TI.Param.Reg, AG.Param.Reg
Characteristics=0x84
;CpyFiles =USR11GAGXP.CopyFiles
[USR11GAGXP.ndi.reg.NT]
HKR, Ndi, Service, 0, "USR11G"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[USR11GAGXP.Services]
AddService=USR11G, 2, USR11GXP.Service, USR11GXP.EventLog
[USR11GAGXP.CopyFiles]
[USR11GXP.Service]
DisplayName=%USR11G.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\USR11G.sys
LoadOrderGroup=NDIS
[USR11GXP.EventLog]
AddReg=USR11GXP.AddEventLog.reg
[USR11GXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[USR11G.NT]
BusType=5
AddReg =USR11G.ndi.reg.NT, TI.Param.Reg, BG.Param.Reg
Characteristics=0x84
;CpyFiles =USR11G.CopyFiles.NT, USR11G.BinFiles.NT
[USR11G.ndi.reg.NT]
HKR, Ndi, Service, 0, "USR11G"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[USR11G.NT.Services]
AddService=USR11G, 2, USR11G.Service, USR11G.EventLog
[USR11G.CopyFiles.NT]
[USR11G.BinFiles.NT]
[USR11GAG.NT]
BusType=5
AddReg =USR11GAG.ndi.reg.NT, TI.Param.Reg, AG.Param.Reg
Characteristics=0x84
;CpyFiles =USR11GAG.CopyFiles.NT, USR11GAG.BinFiles.NT
[USR11GAG.ndi.reg.NT]
HKR, Ndi, Service, 0, "USR11G"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[USR11GAG.NT.Services]
AddService=USR11G, 2, USR11G.Service, USR11G.EventLog
[USR11GAG.CopyFiles.NT]
[USR11GAG.BinFiles.NT]
[USR11G.Service]
DisplayName=%USR11G.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\USR11G.sys
LoadOrderGroup=NDIS
[USR11G.EventLog]
AddReg=USR11G.AddEventLog.reg
[USR11G.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[USR11G]
AddReg=USR11G.ndi.reg, TI.Param.Reg, USR11G.Install, BG.Param.Reg
[USR11G.Copy]
;CpyFiles=USR11G.CopyFiles
[USR11G.Install]
HKR,Ndi\Install,,,"USR11G.Copy"
HKR,Ndi\Remove,,,"USR11G.Remove"
[USR11G.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_9066"
HKR,Ndi,HelpText,0,%WLANAdapterHelpText%
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,USR11G.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, , "USR11G"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"
[USR11G.CopyFiles]
[USR11GAG]
AddReg=USR11GAG.ndi.reg, TI.Param.Reg, USR11GAG.Install, AG.Param.Reg
[USR11GAG.Copy]
;CpyFiles=USR11G.CopyFiles
[USR11GAG.Install]
HKR,Ndi\Install,,,"USR11G.Copy"
HKR,Ndi\Remove,,,"USR11G.Remove"
[USR11GAG.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_9066"
HKR,Ndi,HelpText,0,%WLANAdapterHelpText%
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,USR11G.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, , "USR11G"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"
[USR11GAG.CopyFiles]
[BG.Param.Reg]
HKR, ,dot11NetworkType,, "3"
HKR, ,dot11SupportedRateMask, ,"8"
HKR, ,dot11BasicRateMask, ,"1"
[AG.Param.Reg]
HKR, ,dot11NetworkType,, "4"
HKR, ,dot11SupportedRateMask, ,"8"
HKR, ,dot11BasicRateMask, ,"0"
[TI.Param.Reg]
HKR, ,MultiRegulatoryDomain, ,"0"
HKR, ,SpectrumManagement, ,"0"
HKR, ,TxPower, ,"1"
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, ,60480
HKR,NDI\params\dot11DesiredBSSType,ParamDesc,,"Desired BSS Type"
HKR,NDI\params\dot11DesiredBSSType,type,,"enum"
HKR,NDI\params\dot11DesiredBSSType,default,,"1"
HKR,NDI\params\dot11DesiredBSSType\enum,"0",,"Ad-Hoc"
HKR,NDI\params\dot11DesiredBSSType\enum,"1",,"Infrastructure"
HKR, Ndi\Params\dot11DesiredSSID, ParamDesc, ,"Desired SSID"
HKR, Ndi\Params\dot11DesiredSSID, Type, ,"edit"
HKR, Ndi\Params\dot11DesiredSSID, LimitText, ,"32"
HKR, Ndi\Params\dot11DesiredSSID, Default,,"Any"
HKR, Ndi\Params\dot11DesiredSSID, UpperCase,,"0"
HKR, ,dot11PowerMode, ,"0"
HKR, ,IbssProtectionType, ,"0"
HKR,NDI\params\dot11DesiredTxRate,ParamDesc,, "Desired Tx Rate"
HKR,NDI\params\dot11DesiredTxRate,type,,"enum"
HKR,NDI\params\dot11DesiredTxRate,default,,"0"
HKR,NDI\params\dot11DesiredTxRate\enum,"0",,"Auto"
HKR,NDI\params\dot11DesiredTxRate\enum,"1",,"1 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"2",,"2 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"3",,"5.5 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"4",,"6 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"5",,"9 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"6",,"11 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"7",,"12 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"8",,"18 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"9",,"22 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"10",,"24 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"11",,"36 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"12",,"48 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"13",,"54 Mbps"
HKR, ,dot11FragmentationThreshold, ,"4096"
HKR, ,dot11RTSThreshold, ,"4096"
HKR, ,dot11WEPStatus, ,"1"
HKR, ,dot11AuthenticationMode, ,"0"
HKR, ,dot11ShortPreambleInvoked, ,"0"
HKR, ,ELPSupport, ,"0"
HKR, ,LeapUserName, ,"usrwlan"
HKR, ,LeapEnabled, ,"0"
HKR, ,Mode4x, ,"1"
HKR, ,g80211DraftNumber, ,"6"
HKR, ,PrivacyMode, ,"0"
HKR, ,CCXSecurityType, ,"0"
HKR, ,MixedMode, ,"0"
HKR, Ndi\Params\dot11DesiredChannel, ParamDesc, ,"Desired Channel"
HKR, Ndi\Params\dot11DesiredChannel, Type, , "int"
HKR, Ndi\Params\dot11DesiredChannel, Default, , "11"
HKR, Ndi\Params\dot11DesiredChannel, Min, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Max, , "11"
HKR, Ndi\Params\dot11DesiredChannel, Step, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Base, , "10"
HKR, ,EnergyDetection, ,"1"
HKR, ,FBLongInterval,, "100"
HKR, ,FBShortInterval,, "2000"
HKR, ,dot11MaxSiteLifetime, ,"3"
HKR, ,TxOpContinuation, ,"1"
[DestinationDirs]
DefaultDestDir=12 ; Windows\System32\Drivers
USR11GXP.CopyFiles=12 ; Winnt\System32\Drivers Directory ; WinXP
USR11GAGXP.CopyFiles=12 ; Winnt\System32\Drivers Directory ; WinXP
USR11G.CopyFiles=11 ; Windows\System or Winnt\System32 Directory ; Win98/ME
USR11G.BinFiles.NT=10,system
USR11GAG.CopyFiles=11 ; Windows\System or Winnt\System32 Directory ; Win98/ME
USR11GAG.BinFiles.NT=10,system
[SourceDisksNames]
1=%DiskName%,,
[SourceDisksFiles]
USR11G.sys=1
[Strings]
TI="U.S. Robotics"
USR11G.DeviceDesc="U.S. Robotics 802.11g Wireless Turbo Adapter"
USR11G.Service.DispName="U.S. Robotics 802.11g Wireless Turbo Adapter"
WLANAdapterHelpText= "A WLAN Adapter provides high speed connection to the Internet through 802.11g technology"
DiskName="USR WLAN Installation Disk"
