
[Version]
DriverVer=02/12/2009, 2.01.01.0015
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
CatalogFile=rt2500usb.CAT ;for WHQL certified
[ControlFlags]
[Manufacturer]
%Ralink%=Ralink
%Amigo%=Amigo
%MSI%=MSI
%SMC%=SMC
%ASUS%=ASUS
%ZINWELL%=ZINWELL
%VTech%=VTech
%SURECOM%=SURECOM
%Gigabyte%=Gigabyte
%Siemens%=Siemens
%BUFFALO%=BUFFALO
%Sagem%=Sagem
%Conceptronic%=Conceptronic
%CNet%=CNet
[Ralink]
%Ralink.DeviceDesc%=RALINK.ndi, USB\VID_148F&PID_2570
[Amigo]
%Amigo_1.DeviceDesc%=AMIGO_1.ndi, USB\VID_148F&PID_9020
%Amigo_2.DeviceDesc%=AMIGO_2.ndi, USB\VID_0EB0&PID_9020
[MSI]
%m2500usb_6861.DeviceDesc%=m2500usb_6861.ndi, USB\VID_0DB0&PID_6861
%m2500usb_6865.DeviceDesc%=m2500usb_6865.ndi, USB\VID_0DB0&PID_6865
%m2500usb_6869.DeviceDesc%=m2500usb_6869.ndi, USB\VID_0DB0&PID_6869
[SMC]
%SMC.DeviceDesc%=SMC.ndi, USB\VID_0707&PID_EE13
[ASUS]
%ASUS.DeviceDesc%=ASUS.ndi, USB\VID_0B05&PID_1706
%ASUSGEN.DeviceDesc%=ASUSGEN.ndi, USB\VID_0B05&PID_1707
[ZINWELL]
%ZINWELLUSB.DeviceDesc%=ZINWELLUSB.ndi, USB\VID_5A57&PID_0260
[VTech]
%VTechUSB.DeviceDesc%=VTech.ndi, USB\VID_0F88&PID_3012
[SURECOM]
%SURECOM.DeviceDesc%=SURECOM.ndi, USB\VID_0769&PID_11F3
[Gigabyte]
%Gigabyte.DeviceDesc%=Gigabyte.ndi, USB\VID_1044&PID_8007
[Siemens]
%Siemens.DeviceDesc%=SIEMENS.ndi, USB\VID_0681&PID_3C06
[BUFFALO]
%BUFFALO_5E.DeviceDesc%=BUFFALO_5E.ndi, USB\VID_0411&PID_005E
%BUFFALO_66.DeviceDesc%=BUFFALO_66.ndi, USB\VID_0411&PID_0066
%BUFFALO_67.DeviceDesc%=BUFFALO_67.ndi, USB\VID_0411&PID_0067
%BUFFALO_97.DeviceDesc%=BUFFALO_97.ndi, USB\VID_0411&PID_0097
[Sagem]
%Sagem.DeviceDesc%=Sagem.ndi, USB\VID_079B&PID_004B
[Conceptronic]
%Conceptronic.DeviceDesc%=Conceptronic.ndi, USB\VID_14B2&PID_3C02
[CNet]
%CNet.DeviceDesc%=CNet.ndi, USB\VID_1371&PID_9022
[RALINK.ndi]
AddReg=USB_184F_2570.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[AMIGO_1.ndi]
AddReg=USB_148F_9020.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[AMIGO_2.ndi]
AddReg=USB_0EB0_9020.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[m2500usb_6861.ndi]
AddReg=USB_0DB0_6861.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[m2500usb_6865.ndi]
AddReg=USB_0DB0_6865.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[m2500usb_6869.ndi]
AddReg=USB_0DB0_6869.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[SMC.ndi]
AddReg=USB_0707_EE13.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[ASUS.ndi]
AddReg=USB_0B05_1706.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[ASUSGEN.ndi]
AddReg=USB_0B05_1707.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[ZINWELLUSB.ndi]
AddReg=USB_5A57_0260.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[VTech.ndi]
AddReg=USB_0F88_3012.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[SURECOM.ndi]
AddReg=USB_0769_11F3.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[Gigabyte.ndi]
AddReg=USB_1044_8007.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[SIEMENS.ndi]
AddReg=USB_0681_3C06.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[BUFFALO_5E.ndi]
AddReg=USB_0411_005E.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[BUFFALO_66.ndi]
AddReg=USB_0411_0066.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[BUFFALO_67.ndi]
AddReg=USB_0411_0067.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[BUFFALO_97.ndi]
AddReg=USB_0411_0097.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[Sagem.ndi]
AddReg=USB_079B_004B.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[Conceptronic.ndi]
AddReg=USB_14B2_3C02.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[CNet.ndi]
AddReg=USB_1371_9022.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[RALINK.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[AMIGO_1.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[AMIGO_2.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[m2500usb_6861.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[m2500usb_6865.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[m2500usb_6869.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[SMC.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[ASUS.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[ASUSGEN.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[ZINWELLUSB.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[VTech.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[SURECOM.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[Gigabyte.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[SIEMENS.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[BUFFALO_5E.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[BUFFALO_66.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[BUFFALO_67.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[BUFFALO_97.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[Sagem.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[Conceptronic.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[CNet.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RALINK.ndi.NT.Services]
AddService=RT2500USB, 2, RALINK.Service, common.EventLog
[AMIGO_1.ndi.NT.Services]
AddService=RT2500USB, 2, AMIGO.Service, common.EventLog
[AMIGO_2.ndi.NT.Services]
AddService=RT2500USB, 2, AMIGO.Service, common.EventLog
[m2500usb_6861.ndi.NT.Services]
AddService=RT2500USB, 2, m2500usb.Service, common.EventLog
[m2500usb_6865.ndi.NT.Services]
AddService=RT2500USB, 2, m2500usb.Service, common.EventLog
[m2500usb_6869.ndi.NT.Services]
AddService=RT2500USB, 2, m2500usb.Service, common.EventLog
[SMC.ndi.NT.Services]
AddService=RT2500USB, 2, SMC.Service, common.EventLog
[ASUS.ndi.NT.Services]
AddService=RT2500USB, 2, ASUS.Service, common.EventLog
[ASUSGEN.ndi.NT.Services]
AddService=RT2500USB, 2, ASUS.Service, common.EventLog
[ZINWELLUSB.ndi.NT.Services]
AddService=RT2500USB, 2, ZINWELLUSB.Service, common.EventLog
[VTech.ndi.NT.Services]
AddService=RT2500USB, 2, VTech.Service, common.EventLog
[SURECOM.ndi.NT.Services]
AddService=RT2500USB, 2, SURECOM.Service, common.EventLog
[Gigabyte.ndi.NT.Services]
AddService=RT2500USB, 2, Gigabyte.Service, common.EventLog
[SIEMENS.ndi.NT.Services]
AddService=RT2500USB, 2, SIEMENS.Service, common.EventLog
[BUFFALO_5E.ndi.NT.Services]
AddService=RT2500USB, 2, BUFFALO.Service, common.EventLog
[BUFFALO_66.ndi.NT.Services]
AddService=RT2500USB, 2, BUFFALO.Service, common.EventLog
[BUFFALO_67.ndi.NT.Services]
AddService=RT2500USB, 2, BUFFALO.Service, common.EventLog
[BUFFALO_97.ndi.NT.Services]
AddService=RT2500USB, 2, BUFFALO.Service, common.EventLog
[Sagem.ndi.NT.Services]
AddService=RT2500USB, 2, Sagem.Service, common.EventLog
[Conceptronic.ndi.NT.Services]
AddService=RT2500USB, 2, Conceptronic.Service, common.EventLog
[CNet.ndi.NT.Services]
AddService=RT2500USB, 2, CNet.Service, common.EventLog
[Common.reg]
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
HKR, , Radio, 0, "0"
HKR, NDI\params\Radio, ParamDesc, 0, "Radio On/Off"
HKR, NDI\params\Radio, type, 0, "enum"
HKR, NDI\params\Radio, default, 0, "0"
HKR, NDI\params\Radio\enum, 1, 0, "Disable"
HKR, NDI\params\Radio\enum, 0, 0, "Enable"
HKR, , AutoReconnect, 0, "1"
HKR, NDI\params\AutoReconnect, ParamDesc, 0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect, type, 0, "enum"
HKR, NDI\params\AutoReconnect, default, 0, "1"
HKR, NDI\params\AutoReconnect\enum, 0, 0, "Disable"
HKR, NDI\params\AutoReconnect\enum, 1, 0, "Enable"
HKR, , ShowHiddenSSID, 0, "0" ; 0=disable(default), 1=enable
HKR, , ConfigSelect, 0, "0" ; 0=RaConfig, 1=ZeroConfig
HKR, , CountryRegion, 0, "0"
HKR, , WirelessMode, 0, "0"
HKR, , TXBurst, 0, "0"
HKR, , ShortSlot, 0, "0"
HKR, , TurboRate, 0, "0"
HKR, , AdhocOfdm, 0, "0"
HKR, , BGProtection, 0, "0"
HKR, , VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, Default, VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, , PSPXlink, 0, "0"
HKR, NDI\params\PSPXlink, ParamDesc, 0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink, type, 0, "enum"
HKR, NDI\params\PSPXlink, default, 0, "0"
HKR, NDI\params\PSPXlink\enum, 0, 0, "Disable"
HKR, NDI\params\PSPXlink\enum, 1, 0, "Enable"
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, Default, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0, 0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, , NetworkAddress, 0, ""
HKR, Default, NetworkAddress, 0, ""
HKR, NDI\params\NetworkAddress, ParamDesc, 0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, limitText, 0, "12"
HKR, NDI\params\NetworkAddress, default, 0, ""
HKR, NDI\params\NetworkAddress, optional, 0, "1"
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Saving Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum, 1, 0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum, 2, 0, "Fast_PSP (Power Save Mode)"
HKR, , ACPowerCam, 0, "0"
HKR, Default, ACPowerCam, 0, "0"
HKR, NDI\params\ACPowerCam, ParamDesc, 0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam, type, 0, "enum"
HKR, NDI\params\ACPowerCam, default, 0, "0"
HKR, NDI\params\ACPowerCam\enum, 0, 0, "Disable"
HKR, NDI\params\ACPowerCam\enum, 1, 0, "Enable"
HKR, , PreambleType, 0, "0"
HKR, Default, PreambleType, 0, "0"
HKR, , TXPower, 0, "0"
HKR, Default, TXPower, 0, "0"
HKR, , RTSThresh, 0, "2347"
HKR, Default, RTSThresh, 0, "2347"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2347"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2347"
HKR, NDI\params\RTSThresh, step, 0, "1"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2346"
HKR, Default, FragThresh, 0, "2346"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragment Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2346"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2346"
HKR, NDI\params\FragThresh, step, 0, "1"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , AuthenType, 0, "0" ; Open System
HKR, Default, AuthenType, 0, "0"
HKR, , Encryption, 0, "1" ; Disable
HKR, Default, Encryption, 0, "1"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
HKR, , WPAPSK, 0, ""
HKR, Default, WPAPSK, 0, ""
HKR, , Use8021X, 0, "0"
HKR, Default, Use8021X, 0, "0"
HKR, , AuthenProtocol, 0, "0"
HKR, Default, AuthenProtocol, 0, "0"
HKR, , TunnelProtocol, 0, "3"
HKR, Default, TunnelProtocol, 0, "3"
HKR, , ID, 0, ""
HKR, Default, ID, 0, ""
HKR, , Password, 0, ""
HKR, Default, Password, 0, ""
HKR, , TunnelID, 0, ""
HKR, Default, TunnelID, 0, ""
HKR, , TunnelPassword, 0, ""
HKR, Default, TunnelPassword, 0, ""
HKR, , SessionResumption, 0, "0"
HKR, Default, SessionResumption, 0, "0"
HKR, , PasswordMode, 0, "1"
HKR, Default, PasswordMode, 0, "1"
HKR, , UseClientCert, 0, "0"
HKR, Default, UseClientCert, 0, "0"
HKR, , UseServerCert, 0, "0"
HKR, Default, UseServerCert, 0, "0"
HKR, , ClientCertLen, 0, "0"
HKR, Default, ClientCertLen, 0, "0"
HKR, , ClientCertData, 0, ""
HKR, Default, ClientCertData, 0, ""
HKR, , ServerCertLen, 0, "0"
HKR, Default, ServerCertLen, 0, "0"
HKR, , ServerCertData, 0, ""
HKR, Default, ServerCertData, 0, ""
HKR, , ServerName, 0, ""
HKR, Default, ServerName, 0, ""
HKR, , NameRule, 0, "0"
HKR, Default, NameRule, 0, "0"
HKR, , IntermediateCert, 0, "0"
HKR, Default, IntermediateCert, 0, "0"
HKR, , LeapEnabled, 0, "0"
HKR, Default, LeapEnabled, 0, "0"
HKR, , LeapUserName, 0, ""
HKR, Default, LeapUserName, 0, ""
HKR, , LeapPassword, 0, ""
HKR, Default, LeapPassword, 0, ""
HKR, , RekeyInterval, 0, "60"
HKR, , RekeyMethod, 0, "0"
[USB_184F_2570.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_148F&PID_2570"
[USB_148F_9020.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_148F&PID_9020"
[USB_0EB0_9020.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0EB0&PID_9020"
[USB_0DB0_6861.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0DB0&PID_6861"
[USB_0DB0_6865.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0DB0&PID_6865"
[USB_0DB0_6869.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0DB0&PID_6869"
[USB_0707_EE13.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0707&PID_EE13"
[USB_0B05_1706.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0B05&PID_1706"
[USB_0B05_1707.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0B05&PID_1707"
[USB_5A57_0260.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_5A57&PID_0260"
[USB_0F88_3012.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0F88&PID_3012"
[USB_0769_11F3.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0769&PID_11F3"
[USB_1044_8007.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_1044&PID_8007"
[USB_0681_3C06.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0681&PID_3C06"
[USB_0411_005E.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0411&PID_005E"
[USB_0411_0066.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0411&PID_0066"
[USB_0411_0067.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0411&PID_0067"
[USB_0411_0097.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0411&PID_0097"
[USB_079B_004B.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_079B&PID_004B"
[USB_14B2_3C02.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_14B2&PID_3C02"
[USB_1371_9022.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_1371&PID_9022"
[USB9X.ndi.reg]
HKR, , NTMPDriver, 0, rt25u98.sys
HKR, , BusType, 0, 15
HKR, NDI, CardType, 0, "PNP"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "rt25u98.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "rt25u98"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
win9x.CopyFiles=11 ; system32 subdirectory on win9x
[NT.CopyFiles]
rt2500usb.sys ; NT Installation
[win9x.CopyFiles]
rt25u98.sys ; Win9x Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
rt2500usb.sys=1
rt25u98.sys=1
[RTUSB.ndi.NT.reg]
HKR, Ndi, Service, 0, "rt2500usb"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[Ralink.Service]
DisplayName=%Ralink.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[AMIGO.Service]
DisplayName=%AMIGO.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[m2500usb.Service]
DisplayName=%m2500usb.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[SMC.Service]
DisplayName=%SMC.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[ASUS.Service]
DisplayName=%ASUS.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[ZINWELLUSB.Service]
DisplayName=%ZINWELL.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[VTech.Service]
DisplayName=%VTech.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[SURECOM.Service]
DisplayName=%SURECOM.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[Gigabyte.Service]
DisplayName=%Gigabyte.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[SIEMENS.Service]
DisplayName=%SIEMENS.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[BUFFALO.Service]
DisplayName=%BUFFALO.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[Sagem.Service]
DisplayName=%Sagem.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[Conceptronic.Service]
DisplayName=%Conceptronic.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[CNet.Service]
DisplayName=%CNet.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2500usb.sys"
HKR, , TypesSupported, 0x00010001, 7
[strings]
Provider="Ralink"
Ralink="Ralink Technology Corp."
Amigo="Amigo Technology Inc."
MSI="802.11 Wireless"
SMC="SMC Networks, Inc"
ASUS="ASUSTeK Computer Inc."
ZINWELL="ZINWELL"
VTech="VTech Telecommunications Ltd"
SURECOM="SURECOM Technology Corp"
Gigabyte="Gigabyte Technology Corp."
Siemens="Siemens"
BUFFALO="BUFFALO INC."
Sagem="Sagem, SA"
Conceptronic="2L (Conceptronic)"
CNet="CNet Technology Inc."
RALINK.DeviceDesc="RT2500 USB Wireless LAN Card"
Amigo_1.DeviceDesc="Wireless USB Card"
Amigo_2.DeviceDesc="IEEE 802.11g Wireless Pocket USB"
m2500usb_6861.DeviceDesc="Wireless 11g USB 2.0 Stick"
m2500usb_6865.DeviceDesc="Wireless 11g MiniUSB 2.0 Adapter"
m2500usb_6869.DeviceDesc="Wireless 11g MiniUSB 2.0 Bluetooth Combo"
SMC.DeviceDesc="EZ Connect g 2.4GHz 802.11g Wireless USB Adapter"
ASUS.DeviceDesc="ASUS USB Wireless Network Adapter"
ASUSGEN.DeviceDesc="802.11b/g USB Wireless Network Adapter"
ZINWELLUSB.DeviceDesc="802.11g USB Adapter"
VTechUSB.DeviceDesc="VTech Wireless 802.11g USB 2.0 Adapter"
SURECOM.DeviceDesc="SURECOM 802.11g WLAN USB Adapter"
Gigabyte.DeviceDesc="Gigabyte WBKG USB WLAN Card"
Siemens.DeviceDesc="Siemens 802.11g USB Wireless Network Adapter"
BUFFALO_5E.DeviceDesc="BUFFALO WLI-U2-KG54-YB Wireless LAN Adapter"
BUFFALO_66.DeviceDesc="BUFFALO WLI-U2-KG54 Wireless LAN Adapter"
BUFFALO_67.DeviceDesc="BUFFALO WLI-U2-KG54-AI Wireless LAN Adapter"
BUFFALO_97.DeviceDesc="BUFFALO WLI-U2-KG54-BB Wireless LAN Adapter"
Sagem.DeviceDesc="SAGEM Wi-Fi 11g USB adapter"
Conceptronic.DeviceDesc="Conceptronic 54Mbps USB adapter"
CNet.DeviceDesc="CNet Wireless-G USB dongle"
INSTALL_DISK_STR="Wireless 11g USB Installation Disk"
RALINK.Service.DispName="RT2500 USB Wireless LAN Driver"
AMIGO.Service.DispName="AMIGO RT2500 USB Wieless Driver"
m2500usb.Service.DispName="Wireless 11g RT2500 USB 2.0 Network Driver"
SMC.Service.DispName="SMC RT2500 USB Wireless LAN Driver"
ASUS.Service.DispName="ASUS RT2500 USB Wireless LAN Driver"
ZINWELL.Service.DispName="ZINWELL RT2500 USB 802.11g Wireless Driver"
VTech.Service.DispName="VTech RT2500 USB 802.11g Wireless Driver"
SURECOM.Service.DispName="SURECOM RT2500 USB 802.11g WLAN Driver"
Gigabyte.Service.DispName="Gigabyte RT2500 USB WLAN Driver"
SIEMENS.Service.DispName="Siemens 802.11g RT2500 USB Wireless Driver"
BUFFALO.Service.DispName="BUFFALO RT2500 USB Wireless Driver"
Sagem.Service.DispName="SAGEM Wi-Fi 11g RT2500 USB adapter Driver"
Conceptronic.Service.DispName="Conceptronic 54Mbps RT2500 USB adapter Driver"
CNet.Service.DispName="CNet RT2500 USB Wireless Driver"
VENDOR_DESC_DEF_STR=""
NETWORK_TYPE_DEF_STR="1"
CHANNEL="1"
