
[Version]
DriverVer=01/17/2003, 3.0.2
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%USB_DESC_STR%=WLAN_USB, USB\VID_09AA&PID_3642
%USB_DESC_STR%=WLAN_USB, USB\VID_0707&PID_EE04
[WLAN_USB]
AddReg=WLAN_USB.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=WLAN_DRIVER_USB, WLAN_CONFIG
[WLAN_USB.ME]
AddReg=WLAN_USB.reg, COMMON_USB.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=WLAN_DRIVER_USB, WLAN_CONFIG
[WLAN_USB.NT]
AddReg=WLAN_USB.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=WLAN_DRIVER_USB.NT
BusType=0
Characteristics= 0x84
[WLAN_USB.NT.Services]
AddService= "PRISM_USB", 2, WLAN_DRIVER_USB.Service, WLAN_DRIVER.EventLog
[WLAN_USB.NT.CoInstallers]
AddReg=WLAN_COINSTALL.reg.NT
[WLAN_USB.reg]
HKR,Ndi,DeviceID,0,"USB\VID_09AA&PID_3642"
HKR,,PlatformId,0,"0"
HKR,,VendorDesc,0,%USB_DESC_STR%
HKR,,LoadFirmware,0,1
HKR,NDI\params\LoadFirmware,,0,1
[WLAN_COINSTALL.reg.NT]
[WLAN_DRIVER.Service]
DisplayName=%WLAN_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\WLANNDS.sys
LoadOrderGroup=NDIS
[WLAN_DRIVER_USB.Service]
DisplayName=%WLAN_SERVICE_DISPLAY_USB%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\SMCWUSB.sys
LoadOrderGroup=NDIS
[WLAN_DRIVER.EventLog]
AddReg=WLAN_DRIVER.EventLog.reg
[WLAN_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_USB.reg]
HKR,NDI ,Service ,0 ,"PRISM_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"SMCWUSB.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON.reg]
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,3
HKR,NDI\params\ListenInterval,,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,1
HKR,defaults,RTSThresh,0,2432
HKR,NDI\params\RTSThresh,,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,NDI\params\RTSThresh,optional,0,1
HKR,defaults,FragThresh,0,2432
HKR,NDI\params\FragThresh,,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,NDI\params\FragThresh,optional,0,1
HKR,defaults,PreambleMode,0,1
HKR,NDI\params\PreambleMode,,0,1
HKR,Ndi\params\PreambleMode,default,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,1
HKR,defaults,AuthentAlg,0,65535
HKR,NDI\params\AuthentAlg,,0,65535
HKR,NDI\params\AuthentAlg,default,0,65535
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,1
HKR,defaults,AdhocDemoMode,0,0
HKR,NDI\params\AdhocDemoMode,,0,0
HKR,Ndi\params\AdhocDemoMode,default,0,0
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,enum
HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
HKR,NDI\params\AdhocDemoMode,optional,0,1
HKR,defaults,LoadFirmware,0,1
HKR,Ndi\params\LoadFirmware,default,0,1
HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
HKR,NDI\params\LoadFirmware,type,,enum
HKR,NDI\params\LoadFirmware,flag,1,30,00,00,00
HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
HKR,NDI\params\LoadFirmware,optional,0,1
HKR,defaults,PDwellTime,0,120
HKR,NDI\params\PDwellTime,,0,120
HKR,Ndi\params\PDwellTime,default,0,120
HKR,NDI\params\PDwellTime,ParamDesc,0,%PDWELL_STR%
HKR,NDI\params\PDwellTime,type,0,int
HKR,NDI\params\PDwellTime,flag,1,20,00,00,00
HKR,NDI\params\PDwellTime,min,0,0
HKR,NDI\params\PDwellTime,max,0,1000
HKR,NDI\params\PDwellTime,step,0,10
HKR,NDI\params\PDwellTime,optional,0,1
HKR,defaults,11dMode,0,0
HKR,NDI\params\11dMode,,0,0
HKR,Ndi\params\11dMode,default,0,0
HKR,NDI\params\11dMode,ParamDesc,,%MDC_CONTROL_STR%
HKR,NDI\params\11dMode,type,,enum
HKR,NDI\params\11dMode,flag,1,30,00,00,00
HKR,NDI\params\11dMode\enum,0,,"None"
HKR,NDI\params\11dMode\enum,1,,"Strict"
HKR,NDI\params\11dMode\enum,2,,"Flexible"
HKR,NDI\params\11dMode,optional,0,1
[DestinationDirs]
;CpyFiles Section=Destination Directory ID -- see layout.inf
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
WLAN_DRIVER=11 ; Win9x=%windir%\system
WLAN_DRIVER_USB=11 ; Win9x=%windir%\system
WLAN_CONFIG=11 ; Win9x=%windir%\system
WLAN_DRIVER.NT=12 ; Win2k=%windir%\system32\drivers
WLAN_DRIVER_USB.NT=12 ; Win2k=%windir%\system32\drivers
[WLAN_CONFIG]
PRISMCFG.dll ; Win9x NDI
[WLAN_DRIVER]
WLANNDS.sys
[WLAN_DRIVER_USB]
SMCWUSB.sys
[WLAN_DRIVER.NT]
WLANNDS.sys
[WLAN_DRIVER_USB.NT]
SMCWUSB.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
PRISMCFG.dll=1
SMCWUSB.sys=1
[SourceDisksFiles.ME] ; WinMe
PRISMCFG.dll=1
SMCWUSB.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
SMCWUSB.sys=1
[Strings]
VER_VENDOR_STR=" "
VER_VENDOR_NAME_STR=" "
WLAN_SERVICE_DISPLAY="Wireless LAN Driver"
WLAN_SERVICE_DISPLAY_USB="Wireless LAN USB Driver"
INSTALL_DISK_STR="Wireless LAN Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"
LOAD_FIRMWARE_STR="Firmware Download"
PDWELL_STR="Passive Scan Dwell Time"
MDC_CONTROL_STR="802.11D Control"
USB_DESC_STR="SMCWUSB32 802.11b Wireless LAN USB Card"

