
[Version]
Signature="$CHICAGO$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%DLink%
Compatible=1
DriverVer=06/12/2008,1.5.206.2
Catalogfile=netA5AGU.cat
[Manufacturer]
%DLink%=DLink
[ControlFlags]
ExcludeFromSelect=VID_2001&PID_3A01
ExcludeFromSelect=VID_2001&PID_3A03
ExcludeFromSelect=VID_2001&PID_3A05
ExcludeFromSelect=VID_07D1&PID_3A08
ExcludeFromSelect=VID_07D1&PID_3A0B
[DLink]
%DWLAG132%=DAG132_DEV.ndi, USB\VID_2001&PID_3A01
%DWLG132C%=DG132C_DEV.ndi, USB\VID_2001&PID_3A03
%WUA2340%=WUA2340_DEV.ndi, USB\VID_07D1&PID_3A08
%DWLAG122%=DAG122_DEV.ndi, USB\VID_2001&PID_3A05
%ALICEG132%=ITG132_DEV.ndi, USB\VID_07D1&PID_3A0B
%DWA120%=DWA120_DEV.ndi, USB\VID_07D1&PID_3A0D
[DAG132_DEV.ndi]
AddReg=DAG132_DEV.id.reg, 5523.reg, DLink.win.reg, 5523.abg.reg, UpDom.reg
;CpyFiles=DLink.win.CopyFiles, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[DG132C_DEV.ndi]
AddReg=DG132C_DEV.id.reg, 5523.reg, DLink.win.reg, 5523.bg.reg, TIWmm.reg
;CpyFiles=DLink.win.CopyFiles, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[WUA2340_DEV.ndi]
AddReg=WUA2340_DEV.id.reg, 5523.reg, DLink.win.reg, 5523.bg.reg
;CpyFiles=DLink.win.CopyFiles, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[DAG122_DEV.ndi]
AddReg=DAG122_DEV.id.reg, 5523.reg, DLink.win.reg, 5523.nsabg.reg
;CpyFiles=DLink.win.CopyFiles, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[ITG132_DEV.ndi]
AddReg=ITG132_DEV.id.reg, 5523.reg, DLink.win.reg, 5523.bg.reg, TIWmm.reg
;CpyFiles=DLink.win.CopyFiles, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[DWA120_DEV.ndi]
AddReg=DWA120_DEV.id.reg, 5523.reg, DLink.win.reg, 5523.bg.reg
;CpyFiles=DLink.win.CopyFiles, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[DAG132_DEV.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
AddReg=5523.reg, DLink.reg, 5523.reg, 5523.abg.reg, UpDom.reg
;CpyFiles=DLink.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[DG132C_DEV.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
AddReg=5523.reg, DLink.reg, 5523.reg, 5523.bg.reg, TIWmm.reg
;CpyFiles=DLink.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[WUA2340_DEV.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
AddReg=5523.reg, DLink.reg, 5523.reg, 5523.bg.reg
;CpyFiles=DLink.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[DAG122_DEV.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
AddReg=5523.reg, DLink.reg, 5523.reg, 5523.nsabg.reg
;CpyFiles=DLink.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[ITG132_DEV.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
AddReg=5523.reg, DLink.reg, 5523.reg, 5523.bg.reg, TIWmm.reg
;CpyFiles=DLink.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[DWA120_DEV.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
AddReg=5523.reg, DLink.reg, 5523.reg, 5523.bg.reg
;CpyFiles=DLink.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=DLink.DelIniFiles
DelReg=5523.DelReg
[DAG132_DEV.ndi.NT.Services]
AddService=A5AGU, 2, DLink.Service, common.EventLog
[DAG132_DEV.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
;CpyFiles=CoInstallers_CopyFiles
[DG132C_DEV.ndi.NT.Services]
AddService=A5AGU, 2, DLink.Service, common.EventLog
[DG132C_DEV.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
;CpyFiles=CoInstallers_CopyFiles
[WUA2340_DEV.ndi.NT.Services]
AddService=A5AGU, 2, DLink.Service, common.EventLog
[WUA2340_DEV.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
;CpyFiles=CoInstallers_CopyFiles
[DAG122_DEV.ndi.NT.Services]
AddService=A5AGU, 2, DLink.Service, common.EventLog
[DAG122_DEV.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
;CpyFiles=CoInstallers_CopyFiles
[ITG132_DEV.ndi.NT.Services]
AddService=A5AGU, 2, DLink.Service, common.EventLog
[ITG132_DEV.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
;CpyFiles=CoInstallers_CopyFiles
[DWA120_DEV.ndi.NT.Services]
AddService=A5AGU, 2, DLink.Service, common.EventLog
[DWA120_DEV.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
;CpyFiles=CoInstallers_CopyFiles
[CoInstallers_AddReg]
[DAG132_DEV.id.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_2001&PID_3A01"
[DG132C_DEV.id.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_2001&PID_3A03"
[WUA2340_DEV.id.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_07D1&PID_3A08"
[DAG122_DEV.id.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_2001&PID_3A05"
[ITG132_DEV.id.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_07D1&PID_3A0B"
[DWA120_DEV.id.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_07D1&PID_3A0D"
[5523.abg.reg]
HKR, , NetBand, 0x00002, "31"
HKR, , AdHocBand, 0x00002, "0"
HKR, , NicType, 0x10003, "2"
HKR, , abolt, 0x00002, "3"
[5523.bg.reg]
HKR, , NetBand, 0x00002, "28"
HKR, , AdHocBand, 0x00002, "0"
HKR, , NicType, 0x10003, "0"
HKR, , abolt, 0x00002, "3"
[5523.nsabg.reg]
HKR, , NetBand, 0x00002, "13"
HKR, , AdHocBand, 0x00002, "0"
HKR, , NicType, 0x10003, "2"
HKR, , abolt, 0x00002, "0"
[5523.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
[5523.reg]
HKR, , SSID, 0x00002, "default"
HKR, , AdHocChannel, 0x00002, "2437"
HKR, , RTSThreshold, 0x00002, "2346"
HKR, , FragThreshold, 0x00002, "2346"
HKR, Ndi\params\MapRegisters, ParamDesc, 0, %MapRegisters%
HKR, Ndi\params\MapRegisters, default, 0, "256"
HKR, Ndi\params\MapRegisters, min, 0, "32"
HKR, Ndi\params\MapRegisters, max, 0, "512"
HKR, Ndi\params\MapRegisters, step, 0, "8"
HKR, Ndi\params\MapRegisters, base, 0, "10"
HKR, Ndi\params\MapRegisters, type, 0, "int"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\sleepMode, ParamDesc, 0, %sleepMode%
HKR, Ndi\params\sleepMode, Base, 0, "10"
HKR, Ndi\params\sleepMode, default, 0, "0"
HKR, Ndi\params\sleepMode, type, 0, "enum"
HKR, Ndi\params\sleepMode\enum, "0", 0, %sleepModeOff%
HKR, Ndi\params\sleepMode\enum, "2", 0, %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum, "1", 0, %sleepModeMax%
HKR, Ndi\params\tpc, ParamDesc, 0, %tpc%
HKR, Ndi\params\tpc, Base, 0, "10"
HKR, Ndi\params\tpc, default, 0, "0"
HKR, Ndi\params\tpc, type, 0, "enum"
HKR, Ndi\params\tpc\enum, "0", 0, %tpc100%
HKR, Ndi\params\tpc\enum, "1", 0, %tpc50%
HKR, Ndi\params\tpc\enum, "2", 0, %tpc25%
HKR, Ndi\params\tpc\enum, "3", 0, %tpc12%
HKR, Ndi\params\tpc\enum, "4", 0, %tpcLowest%
HKR, Ndi\params\shortPreamble, ParamDesc, 0, %shortPreamble%
HKR, Ndi\params\shortPreamble, Base, 0, "10"
HKR, Ndi\params\shortPreamble, default, 0, "1"
HKR, Ndi\params\shortPreamble, type, 0, "enum"
HKR, Ndi\params\shortPreamble\enum, "1", 0, %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0", 0, %shortPreambleDisable%
HKR, Ndi\params\radioEnable, ParamDesc, 0, %radioEnable%
HKR, Ndi\params\radioEnable, Base, 0, "10"
HKR, Ndi\params\radioEnable, default, 0, "1"
HKR, Ndi\params\radioEnable, type, 0, "enum"
HKR, Ndi\params\radioEnable\enum, "1", 0, %radioEnableOn%
HKR, Ndi\params\radioEnable\enum, "0", 0, %radioEnableOff%
HKR, Ndi\params\authTypeUseOnly, ParamDesc, 0, %authTypeUseOnly%
HKR, Ndi\params\authTypeUseOnly, Base, 0, "10"
HKR, Ndi\params\authTypeUseOnly, default, 0, "0"
HKR, Ndi\params\authTypeUseOnly, type, 0, "enum"
HKR, Ndi\params\authTypeUseOnly\enum, "0", 0, %authAuto%
HKR, Ndi\params\authTypeUseOnly\enum, "1", 0, %authOpen%
HKR, Ndi\params\authTypeUseOnly\enum, "2", 0, %authShared%
HKR, , pciDetectEnable, 0x00002, "0"
HKR, CustomParams\Configurations, MajorVersion, 0x10003, 2
HKR, CustomParams\Configurations, MinorVersion, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
[TIWmm.reg]
HKR, Ndi\params\eneConfigEnable, ParamDesc, 0, %DSCP0_OFF%
HKR, Ndi\params\eneConfigEnable, Base, 0, "10"
HKR, Ndi\params\eneConfigEnable, default, 0, "0"
HKR, Ndi\params\eneConfigEnable, type, 0, "enum"
HKR, Ndi\params\eneConfigEnable\enum, "1", 0, %AC_BK%
HKR, Ndi\params\eneConfigEnable\enum, "0", 0, %AC_BE%
[UpDom.reg]
HKR, , eneConfigEnable, 0x00002, "0"
[5523.reg.security]
"D:ARAI(A;;GA;;;BA)(A;;GA;;;SY)(A;CI;GA;;;IU)"
[DLink.reg]
HKR, Ndi, Service, 0, "A5AGU"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[DLink.Service]
DisplayName=%DLink.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\A5AGU.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[DLink.win.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "A5AGU9x.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "A5AGU9x"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, Ndi\Install, ndis3, 0, "DLink.install"
[DLink.win.CopyFiles]
A5AGU9x.sys,,,2
[DLink.CopyFiles.nt]
A5AGU.sys,,,2
[CoInstallers_CopyFiles]
[DLink.DelIniFiles]
Athnic.ini,,,1
[SourceDisksNames]
1=%DLink_Disk%,,,
[SourceDisksFiles]
A5AGU9x.sys=1,, ; on distribution disk 1
A5AGU.sys=1,, ; on distribution disk 1
[DestinationDirs]
DLink.CopyFiles.nt=12
DLink.win.CopyFiles=10,system32\drivers ; %SystemRoot%\system32\drivers
DLink.DelIniFiles=10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir=11
[DEFAULTDESTDIRS]
[Strings]
DLink="D-Link"
authTypeUseOnly="802.11 Authentication Type"
authAuto="Auto"
authOpen="Open"
authShared="Shared"
MapRegisters="Map Registers"
NetworkAddress="Network Address"
sleepMode="Power Save Mode"
sleepModeOff="Off"
sleepModeNormal="Normal"
sleepModeMax="Maximum"
tpc="Transmit Power"
tpcLowest="Lowest"
tpc12="12.5%"
tpc25="25%"
tpc50="50%"
tpc100="100%"
shortPreamble="802.11b Preamble"
shortPreambleEnable="Long and Short"
shortPreambleDisable="Long only"
radioEnable="Radio On/Off"
radioEnableOn="On"
radioEnableOff="Off"
DSCP0_OFF="DSCP0"
AC_BK="AC_BK"
AC_BE="AC_BE"
DLink_Disk="D-Link Wireless Driver Disk"
DLink.Service.DispName="D-Link USB Wireless Network Adapter Service"
DWLAG132="D-Link AirPremier DWL-AG132 Wireless USB Adapter(rev.B)"
DWLG132C="D-Link AirPlus Xtreme G DWL-G132 Wireless USB Adapter(rev.A)"
DWLAG122="D-Link AirPlus AG DWL-AG122 Wireless USB Adapter(rev.A)"
WUA2340="D-Link WUA-2340 USB Adapter"
ALICEG132="Alice G-132"
DWA120="D-Link Wireless 108G DWA-120 USB Adapter"
