[Version]
DriverVer=03/30/2004, 3.00.12.0
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=PRISMA02.cat
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%A021_DESC_STR%=PRISM_A021, USB\VID_1435&PID_0210
%A022_DESC_STR%=PRISM_A022, USB\VID_1435&PID_0427
[PRISM_A021] ; Win9x
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
[PRISM_A021.ME] ; WinMe
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
[PRISM_A021.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
[PRISM_A021.NT] ; Win2k and WinXP
AddReg=PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
BusType=15 ; PNP (allows USB)
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_A021.NT.Services]
AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog
[PRISM_A021.NT.CoInstallers]
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_A021.reg]
HKR,Ndi,DeviceID,0,"USB\VID_1435&PID_0210"
HKR,,PlatformID,0,14480
HKR,,UsbVariant,0,8832
HKR,,VendorDesc,0,%A021_DESC_STR%
HKR,,FWFileName,0,"PRISMA02.arm"
[PRISM_A022] ; Win9x
AddReg=PRISM_A022.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
[PRISM_A022.ME] ; WinMe
AddReg=PRISM_A022.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
[PRISM_A022.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_A022.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
[PRISM_A022.NT] ; Win2k
AddReg=PRISM_A022.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
BusType=15 ; PNP (allows USB)
Characteristics= 0x84
[PRISM_A022.NT.Services]
AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog
[PRISM_A022.NT.CoInstallers]
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_A022.reg]
HKR,Ndi,DeviceID,0,"USB\VID_1435&PID_0427"
HKR,,PlatformID,0,14480
HKR,,UsbVariant,0,14471
HKR,,VendorDesc,0,%A022_DESC_STR%
HKR,,FWFileName,0,"PRISMA02.arm"
[PRISM_COINSTALL.reg.NT]
[PRISM_DRIVER_A02.Service]
DisplayName=%A02_SERVICE_STR%
Description="%HelpText%"
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\PRISMA02u.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_A02_DEL.reg]
HKR, ,FWFileName
[COMMON_A02.reg]
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0" ; Inconsistency with earlier definition is needed.
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR, ,DeviceVxDs ,0 ,"PRISMA02u.sys"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,04
HKR,NDIS ,MinorNdisVersion ,1 ,00
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR, ,DeviceVxDs ,0 ,"PRISMA02u.sys"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis5"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,04
HKR,NDIS ,MinorNdisVersion ,1 ,00
[COMMON_NDIS.reg.NT]
HKR,NDI ,Service ,0 ,"PRISM_A02"
HKR,Ndi ,HelpText ,0 ,"%HelpText%"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,SSID ,0 ,"ANY"
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,,ConfigProfile,0,256
HKR,NDI\params\ConfigProfile,default,0,256
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,0,"enum"
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile,default,0,"256"
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
HKR,NDI\params\ConfigProfile,optional,0,1
HKR,,NitroMode,0,"1"
HKR,NDI\params\NitroMode,default,0,1
HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
HKR,NDI\params\NitroMode,type,0,"enum"
HKR,NDI\params\NitroMode,flag,1,30,00,00,00
HKR,NDI\params\NitroMode,default,0,"1"
HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
HKR,NDI\params\NitroMode,optional,0,1
HKR,,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,0,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,0,"enum"
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode,default,0,"1"
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode,optional,0,1
HKR,NDI\params\PpePdlpEnable,default,0,1
HKR,NDI\params\PpePdlpEnable,ParamDesc,,%PPE_PDLP%
HKR,NDI\params\PpePdlpEnable,type,,enum
HKR,NDI\params\PpePdlpEnable,flag,1,30,00,00,00
HKR,NDI\params\PpePdlpEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpePdlpEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpePdlpEnable,optional,0,1
HKR,NDI\params\PpeCompressEnable,default,0,1
HKR,NDI\params\PpeCompressEnable,ParamDesc,,%PPE_COMPRESS%
HKR,NDI\params\PpeCompressEnable,type,,enum
HKR,NDI\params\PpeCompressEnable,flag,1,30,00,00,00
HKR,NDI\params\PpeCompressEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpeCompressEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpeCompressEnable,optional,0,1
HKR,NDI\params\PpeConcatEnable,default,0,1
HKR,NDI\params\PpeConcatEnable,ParamDesc,,%PPE_CONCAT%
HKR,NDI\params\PpeConcatEnable,type,,enum
HKR,NDI\params\PpeConcatEnable,flag,1,30,00,00,00
HKR,NDI\params\PpeConcatEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpeConcatEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpeConcatEnable,optional,0,1
HKR,NDI\params\PpePiggyBackEnable,default,0,1
HKR,NDI\params\PpePiggyBackEnable,ParamDesc,,%PPE_PIGGYBACK%
HKR,NDI\params\PpePiggyBackEnable,type,,enum
HKR,NDI\params\PpePiggyBackEnable,flag,1,30,00,00,00
HKR,NDI\params\PpePiggyBackEnable\enum,0,,%OFF_STR%
HKR,NDI\params\PpePiggyBackEnable\enum,1,,%ON_STR%
HKR,NDI\params\PpePiggyBackEnable,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.ME=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_NDI.copy]
[PRISM_NDI.copy.ME]
[PRISM_COINSTALL.copy.NT]
[PRISM_DRIVER.copy]
PRISMA02u.sys
PRISMIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.ME]
PRISMA02u.sys
PRISMIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.NT]
PRISMA02u.sys
[PRISM_APPLET.copy]
[PRISM_APPLET.copy.ME]
[PRISM_APPLET.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
PRISMA02u.sys=1
PRISMIOC.vxd=1,win9x
[SourceDisksFiles.ME] ; WinMe
PRISMA02u.sys=1
PRISMIOC.vxd=1,win9x
[SourceDisksFiles.X86] ; Win2k/Xp
PRISMA02u.sys=1
[Strings]
VER_VENDOR_STR="Conexant"
VER_VENDOR_NAME_STR="Conexant Systems, Inc."
INSTALL_DISK_STR="Wireless LAN Install Disk"
A021_DESC_STR="802.11g USB 2.0 adapter"
A022_DESC_STR="802.11g USB 2.0 adapter"
A02_SERVICE_STR="802.11g USB 2.0 adapter"
HelpText="The 802.11g USB 2.0 Adapter provides wireless local area networking."
ON_STR="On"
OFF_STR="Off"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WiFi"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"
NITRO_MODE="Nitro Mode"
PPE_PDLP="Direct Link"
PPE_COMPRESS="Compression"
PPE_CONCAT="Concatenation"
PPE_PIGGYBACK="PiggyBack"

